
[Version]
DriverVer=07/01/2002, 1.31.7.0
Signature="$Chicago$"
Compatible=1
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%VER_VENDOR_STR%
CatalogFile=MSWPCC.cat
[ControlFlags]
ExcludeFromSelect=PCMCIA\Microsoft-Wireless_Notebook_Adapter_MN-520-2E27
[Manufacturer]
%VER_VENDOR_NAME_STR%=DeviceList,NTx86.5.1
[DeviceList]
%PRISM_PCMCIA1_STR%=PRISM_PCMCIA1, PCMCIA\Microsoft-Wireless_Notebook_Adapter_MN-520-2E27
[DeviceList.NTx86.5.1]
%PRISM_PCMCIA1_STR%=PRISM_PCMCIA_XP1, PCMCIA\Microsoft-Wireless_Notebook_Adapter_MN-520-2E27
[PRISM_PCMCIA1] ; Win9x
AddReg=PRISM_PCMCIA1.reg, COMMON_PCMCIA.reg, COMMON_NDIS.reg, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy
[PRISM_PCMCIA1.NT] ; Win2k
AddReg=PRISM_PCMCIA1.reg, COMMON_PCMCIA.reg, COMMON_NDIS.reg.NT, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.NT
BusType=8 ; PCMCIA
Characteristics= 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[PRISM_PCMCIA1.NT.Services]
AddService="MSW", 2, PRISM_DRIVER.Service, PRISM_DRIVER.EventLog
[PRISM_PCMCIA1.reg]
HKR,Ndi ,DeviceID,0,"PCMCIA\Microsoft-Wireless_Notebook_Adapter_MN-520-2E27"
[PRISM_PCMCIA_XP1] ; WinXP
AddReg=PRISM_PCMCIA_XP1.reg, COMMON_PCMCIA_XP1.reg, COMMON_NDIS.reg.NT, COMMON.reg, COMMON_NDIS.reg.XP
;CpyFiles=PRISM_DRIVER.copy.XP
BusType=8 ; PCMCIA
Characteristics= 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[PRISM_PCMCIA_XP1.Services]
AddService="MSW", 2, PRISM_DRIVER_XP1.Service, PRISM_DRIVER.EventLog
[PRISM_PCMCIA_XP1.reg]
HKR,Ndi ,DeviceID,0,"PCMCIA\Microsoft-Wireless_Notebook_Adapter_MN-520-2E27"
[PRISM_DRIVER.Service]
DisplayName=%PRISM_SERVICE_DISPLAY%
ServiceType=1 ; SERVICE_KERNEL_DRIVER
StartType=3 ; SERVICE_DEMAND_START
ErrorControl=1 ; NORMAL
ServiceBinary=%12%\MSWNDS50.sys
LoadOrderGroup=NDIS
[PRISM_DRIVER_XP1.Service]
DisplayName=%PRISM_SERVICE_DISPLAY%
ServiceType=1 ; SERVICE_KERNEL_DRIVER
StartType=3 ; SERVICE_DEMAND_START
ErrorControl=1 ; NORMAL
ServiceBinary=%12%\MSWNDS51.sys
LoadOrderGroup=NDIS
[PRISM_DRIVER.EventLog]
AddReg=PRISM_DRIVER.EventLog.reg
[PRISM_DRIVER.EventLog.reg]
HKR, ,EventMessageFile ,0x00020000 ,"%%SystemRoot%%\System32\netevent.dll"
HKR, ,TypesSupported ,0x00010001 ,7
[COMMON_PCMCIA.reg]
HKR,NDI ,Service ,0 ,"MSW"
HKR,NDI ,CardType ,0 ,"PCMCIA"
HKR, ,BusType ,0 ,"8"
HKR, ,DeviceVxDs ,0 ,"MSWNDS50.sys"
HKR, ,EnableIRQSharing ,1 ,01,00,00,00
HKR, ,IOBaseAddress ,1 ,02,00,00,00
HKR, ,InterruptNumber ,1 ,04,00,00,00
[COMMON_PCMCIA_XP1.reg]
HKR,NDI ,Service ,0 ,"MSW"
HKR,NDI ,CardType ,0 ,"PCMCIA"
HKR, ,BusType ,0 ,"8"
HKR, ,DeviceVxDs ,0 ,"MSWNDS51.sys"
HKR, ,EnableIRQSharing ,1 ,01,00,00,00
HKR, ,IOBaseAddress ,1 ,02,00,00,00
HKR, ,InterruptNumber ,1 ,04,00,00,00
[COMMON_NDIS.reg]
HKR, ,RunningWin9X ,0 ,"1"
HKR, ,DevLoader ,0 ,"*ndis"
HKR,NDI\Interfaces ,UpperRange ,0 ,"ndis3"
HKR,NDI\Interfaces ,LowerRange ,0 ,"ethernet"
HKR,NDI\Interfaces ,DefUpper ,0 ,"ndis3"
HKR,NDI\Interfaces ,DefLower ,0 ,"ethernet"
HKR,NDIS ,LogDriverName ,0 ,"MSW"
HKR,NDIS ,MajorNdisVersion ,1 ,03
HKR,NDIS ,MinorNdisVersion ,1 ,0a
HKR,defaults,PSMode,0,1
HKR,Ndi\params\PSMode,default,0,1
HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
HKR,NDI\params\PSMode,type,,enum
HKR,NDI\params\PSMode,flag,1,30,00,00,00
HKR,NDI\params\PSMode\enum,1,,"Disable"
HKR,NDI\params\PSMode\enum,2,,"Always Enable"
[COMMON_NDIS.reg.NT]
HKR,NDI\Interfaces ,UpperRange ,0 ,"ndis5"
HKR,NDI\Interfaces ,LowerRange ,0 ,"ethernet"
HKR,defaults,PSMode,0,1
HKR,Ndi\params\PSMode,default,0,1
HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
HKR,NDI\params\PSMode,type,,enum
HKR,NDI\params\PSMode,flag,1,30,00,00,00
HKR,NDI\params\PSMode\enum,1,,"Disable"
HKR,NDI\params\PSMode\enum,2,,"Always Enable"
[COMMON_NDIS.reg.XP]
HKR,NDI\params\PSMode\enum,3,,"Auto Enable"
[COMMON.reg]
HKR, ,MSWIOC ,0 ,"1"
HKR, ,SilentInstall ,0 ,"1"
HKR,defaults,RTSThresh,0,2432
HKR,Ndi\params\RTSThresh,default,0,2432
HKR,NDI\params\RTSThresh,ParamDesc,0,%RTSTHRESH_STR%
HKR,NDI\params\RTSThresh,type,0,int
HKR,NDI\params\RTSThresh,flag,1,20,00,00,00
HKR,NDI\params\RTSThresh,min,0,0
HKR,NDI\params\RTSThresh,max,0,2432
HKR,NDI\params\RTSThresh,step,0,64
HKR,defaults,FragThresh,0,2432
HKR,Ndi\params\FragThresh,default,0,2432
HKR,NDI\params\FragThresh,ParamDesc,0,%FRAGTHRESH_STR%
HKR,NDI\params\FragThresh,type,0,int
HKR,NDI\params\FragThresh,flag,1,20,00,00,00
HKR,NDI\params\FragThresh,min,0,256
HKR,NDI\params\FragThresh,max,0,2432
HKR,NDI\params\FragThresh,step,0,128
HKR,defaults,PreambleMode,0,1
HKR,Ndi\params\PreambleMode,default,0,1
HKR,NDI\params\PreambleMode,ParamDesc,,%SHORT_PREAM_STR%
HKR,NDI\params\PreambleMode,type,,enum
HKR,NDI\params\PreambleMode,flag,1,30,00,00,00
HKR,NDI\params\PreambleMode\enum,1,,"Long Tx Preamble"
HKR,NDI\params\PreambleMode\enum,2,,"Short Tx Preamble"
HKR,NDI\params\PreambleMode\enum,3,,"Auto Tx Preamble"
HKR,defaults,DSChannel,0,6
HKR,NDI\params\DSChannel,default,0,6
HKR,NDI\params\DSChannel,ParamDesc,0,%DSCHANNEL_STR%
HKR,NDI\params\DSChannel,type,0,"enum"
HKR,NDI\params\DSChannel\enum,1,0,"1"
HKR,NDI\params\DSChannel\enum,2,0,"2"
HKR,NDI\params\DSChannel\enum,3,0,"3"
HKR,NDI\params\DSChannel\enum,4,0,"4"
HKR,NDI\params\DSChannel\enum,5,0,"5"
HKR,NDI\params\DSChannel\enum,6,0,"6"
HKR,NDI\params\DSChannel\enum,7,0,"7"
HKR,NDI\params\DSChannel\enum,8,0,"8"
HKR,NDI\params\DSChannel\enum,9,0,"9"
HKR,NDI\params\DSChannel\enum,10,0,"10"
HKR,NDI\params\DSChannel\enum,11,0,"11"
HKR,defaults,NetworkType,0,1
HKR,NDI\params\NetworkType,default,0,1
HKR,NDI\params\NetworkType,ParamDesc,0,%NETWORKTYPE_STR%
HKR,NDI\params\NetworkType,type,0,"enum"
HKR,NDI\params\NetworkType\enum,0,0,%NETWORKTYPE_P0_STR%
HKR,NDI\params\NetworkType\enum,1,0,%NETWORKTYPE_P1_STR%
HKR,defaults,SSID,0,%DEFAULT_SSID_STR%
HKR,NDI\params\SSID,default,0,%DEFAULT_SSID_STR%
HKR,NDI\params\SSID,ParamDesc,0,%SSID_STR%
HKR,NDI\params\SSID,type,0,"edit"
HKR,NDI\params\SSID,limitText,0,"32"
HKR,NDI\params\SSID,flag,1,"30","00","00","00"
HKR,defaults,TxRate,0,15
HKR,NDI\params\TxRate,default,0,15
HKR,NDI\params\TxRate,ParamDesc,0,%TXRATE_STR%
HKR,NDI\params\TxRate,type,0,"enum"
HKR,NDI\params\TxRate\enum,3,0,%TXRATE_P3_STR%
HKR,NDI\params\TxRate\enum,4,0,%TXRATE_P4_STR%
HKR,NDI\params\TxRate\enum,8,0,%TXRATE_P8_STR%
HKR,NDI\params\TxRate\enum,15,0,%TXRATE_P15_STR%
HKR,defaults,DecryptInDriver,0,1
HKR, ,DecryptInDriver, 0, "1" ;1:Enable 0:Disable
HKR,defaults,EncryptInDriver,0,1
HKR, ,EncryptInDriver, 0, "1" ;1:Enable 0:Disable
HKR,defaults,WEPFactor,0,0
HKR, ,WEPFactor, 0, "0" ;Range:0~3
HKR,defaults,EnableRadio,0,1
HKR,NDI\params\EnableRadio,,0,1
HKR,NDI\params\EnableRadio,default,0,1
HKR,NDI\params\EnableRadio,ParamDesc,0,%ENABLERADIO_STR%
HKR,NDI\params\EnableRadio,type,0,"enum"
HKR,NDI\params\EnableRadio\enum,0,0,%ENABLERADIO_P0_STR%
HKR,NDI\params\EnableRadio\enum,1,0,%ENABLERADIO_P1_STR%
HKR,defaults,IBSSInDriver,0,0
HKR, ,IBSSInDriver, 0, "0" ;1:Enable 0:Disable
HKR,defaults,BeaconPeriod,0,100
HKR, ,BeaconPeriod, 0, "100" ;Range:100~1000
HKR,defaults,BasicRates,0,15
HKR, ,BasicRates, 0, "15" ;bit0:1Mbps, bit1:2Mbps, bit2:5.5Mbps bit3:11Mbps
[DestinationDirs]
DefaultDestDir=11 ; Win9x=%windir%\system Win2k=%windir%\system32 WinXP=%windir%\system32
PRISM_DRIVER.copy=11 ; Win9x=%windir%\system
PRISM_DRIVER.copy.NT=12 ; Win2k=%windir%\system32\drivers
PRISM_DRIVER.copy.XP=12 ; WinXP=%windir%\system32\drivers
[PRISM_DRIVER.copy]
MSWNDS50.sys,MSWNDS50.sys,,
MSWIOC.vxd ; Win9x Ioctl interface
[PRISM_DRIVER.copy.NT]
MSWNDS50.sys,MSWNDS50.sys,,
[PRISM_DRIVER.copy.XP]
MSWNDS51.sys,MSWNDS51.sys,,
[SourceDisksNames]
1=%INSTALL_DISK_STR%,,,
[SourceDisksFiles]
MSWIOC.vxd=1
MSWNDS50.sys=1
MSWNDS51.sys=1
[Strings]
VER_VENDOR_STR="Microsoft(R)"
VER_VENDOR_NAME_STR="Microsoft(R) Corporation"
PRISM_PCMCIA1_STR="Microsoft Broadband Networking Wireless Notebook Adapter"
PRISM_SERVICE_DISPLAY="Microsoft Broadband Networking Driver"
INSTALL_DISK_STR="Microsoft Broadband Networking Install Disk"
SHORT_PREAM_STR="Preamble Mode"
RTSTHRESH_STR="RTS Threshold"
FRAGTHRESH_STR="Fragmentation Threshold"
POWER_SAVE_STR="Power Save Mode"
DSCHANNEL_STR="Channel"
NETWORKTYPE_STR="Network Type"
NETWORKTYPE_P0_STR="Peer to Peer"
NETWORKTYPE_P1_STR="Access Point"
SSID_STR="SSID"
DEFAULT_SSID_STR="MSHOME"
TXRATE_STR="Transmit Rate"
TXRATE_P3_STR="Auto 1 or 2 Mb"
TXRATE_P4_STR="5.5 Mb"
TXRATE_P8_STR="11 Mb"
TXRATE_P15_STR="Fully Automatic"
ENABLERADIO_STR="Enable Radio"
ENABLERADIO_P0_STR="Radio Off"
ENABLERADIO_P1_STR="Radio On"
