
[version]
Signature="$Chicago$"
Compatible=1
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%Realtek% ;;
CatalogFile.NT=net8185.cat ;; for WHQL certified
DriverVer=09/17/2009,5.1114.0917.2009
[Manufacturer]
%Realtek%=Realtek
%Surecom%=Surecom
[ControlFlags]
ExcludeFromSelect=PCI\VEN_10EC&DEV_8185&REV_20
ExcludeFromSelect=PCI\VEN_10EC&DEV_8185&SUBSYS_818510EC&REV_20
ExcludeFromSelect=PCI\VEN_10EC&DEV_8185&SUBSYS_616510E8
ExcludeFromSelect=PCI\VEN_10EC&DEV_8185&SUBSYS_13F210BD&REV_20
ExcludeFromSelect=PCI\VEN_10EC&DEV_8185&SUBSYS_14F210BD&REV_20
[Realtek]
%RTL8185.DeviceDesc%=RTL8185.ndi, PCI\VEN_10EC&DEV_8185&REV_20
%RTL8185.DeviceDesc%=RTL8185.ndi, PCI\VEN_10EC&DEV_8185&SUBSYS_818510EC&REV_20
%RTL8185.DeviceDesc%=RTL8185.ndi, PCI\VEN_10EC&DEV_8185&SUBSYS_616518E8
[Surecom]
%RTL8185.DeviceDesc_SURECOME_EP9321%=RTL8185.ndi, PCI\VEN_10EC&DEV_8185&SUBSYS_13F210BD&REV_20
%RTL8185.DeviceDesc_SURECOME_EP9428%=RTL8185.ndi, PCI\VEN_10EC&DEV_8185&SUBSYS_14F210BD&REV_20
[RTL8185.ndi]
DriverVer=09/17/2009,1114
AddReg=rtl8185.id.reg, RTL8185.common.reg, RTL8185.win.reg
;CpyFiles=RTL8185.CopyFiles98
[RTL8185.ndi.NT]
AddReg=RTL8185.common.reg, RTL8185.reg
Characteristics=0x84
BusType=5
;CpyFiles=RTL8185.CopyFiles
[RTL8185.ndi.NT.Services]
AddService=rtl8185, 2, rtl8185.Service, RTL8185.EventLog
[RTL8185.CopyFiles]
rtl8185.sys,,,2
[RTL8185.CopyFiles98]
rtl8185.sys,,,2
[rtl8185.id.reg]
HKR, Ndi, DeviceID, 0, "PCI\VEN_10EC&DEV_8185"
HKR, Ndi\Install, , 0, rtsnt.install
HKR, NDI\Params\NetworkAddress, flag, 1, 30, 00, 00, 00
[RTL8185.win.reg]
HKR, , DriverDesc, 0, "Realtek RTL8185 54M Wireless LAN Network Adapter"
HKR, , DevLoader, 0, *ndis
HKR, , DeviceVxDs, 0, rtl8185.sys
HKR, , EnumPropPages, 0, netdi.dll, EnumPropPages
HKR, , MediaType, 0, 1
HKR, , AdapterType, 0, 5
HKR, , BusType, 0, 5
HKR, NDIS, MajorNdisVersion, 1, 03
HKR, NDIS, MinorNdisVersion, 1, 0a
HKR, NDIS, LogDriverName, 0, "RTL8185"
HKR, Ndi\Interfaces, DefLower, , "ethernet"
HKR, Ndi\Interfaces, LowerRange, , "ethernet"
HKR, Ndi\Interfaces, DefUpper, , "ndis3"
HKR, Ndi\Interfaces, UpperRange, , "ndis3"
HKR, Ndi\Install, ndis3, 0, "rtl185.ndis5"
[RTL8185.common.reg]
HKR,defaults,FragThresh, 0, "2432"
HKR,Ndi\params\FragThresh, default, 0, "2432"
HKR,Ndi\params\FragThresh, ParamDesc, 0, %FRAGTHRESH_STR%
HKR,Ndi\params\FragThresh, type, 0, "int"
HKR,Ndi\params\FragThresh, min, 0, "256"
HKR,Ndi\params\FragThresh, max, 0, "2432"
HKR,Ndi\params\FragThresh, step, 0, "1"
HKR,defaults,Channel,0,"1"
HKR,Ndi\params\Channel,default, 0,"1"
HKR,Ndi\params\Channel,ParamDesc,,%CHANNEL_STR%
HKR,Ndi\params\Channel,type, ,"int"
HKR,Ndi\params\Channel,flag, 1,"30","00","00","00"
HKR,Ndi\params\Channel,min, 0,"1"
HKR,Ndi\params\Channel,max, 0,"14"
HKR,Ndi\params\Channel,step, 0,"1"
HKR,defaults,PowerSaveMode,0,"0"
HKR,Ndi\params\PowerSaveMode,default,0,"0"
HKR,NDI\params\PowerSaveMode,ParamDesc,,%POWER_SAVE_STR%
HKR,NDI\params\PowerSaveMode,type,,"enum"
HKR,NDI\params\PowerSaveMode,flag,1,"30","00","00","00"
HKR,NDI\params\PowerSaveMode\enum,0,,"None"
HKR,NDI\params\PowerSaveMode\enum,2,,"Min"
HKR,NDI\params\PowerSaveMode\enum,1,,"Max"
HKR,Ndi\params\SSID, ParamDesc, 0, %SSID_STR%
HKR,defaults, SSID, 0, "ANY"
HKR,Ndi\params\SSID, type, 0, "edit"
HKR,Ndi\params\SSID, default, 0, "ANY"
HKR,Ndi\params\SSID, LimitText, 0, "32"
HKR,Ndi\Params\ChannelPlan, ParamDesc, 0, "Channel Plan"
HKR,Ndi\Params\ChannelPlan, Type, 0, "enum"
HKR,Ndi\Params\ChannelPlan, Default, 0, "15"
HKR,Ndi\Params\ChannelPlan\enum, "0", 0, "FCC"
HKR,Ndi\Params\ChannelPlan\enum, "1", 0, "IC"
HKR,Ndi\Params\ChannelPlan\enum, "2", 0, "ETSI"
HKR,Ndi\Params\ChannelPlan\enum, "3", 0, "Spain"
HKR,Ndi\Params\ChannelPlan\enum, "4", 0, "France"
HKR,Ndi\Params\ChannelPlan\enum, "5", 0, "MKK"
HKR,Ndi\Params\ChannelPlan\enum, "6", 0, "MKK1"
HKR,Ndi\Params\ChannelPlan\enum, "7", 0, "Israel"
HKR,Ndi\Params\ChannelPlan\enum, "8", 0, "TELEC"
HKR,Ndi\Params\ChannelPlan\enum, "15", 0, "DOMAIN_FROM_EEPROM"
HKR,Ndi\Params\PSPXLINKMode, ParamDesc, 0, "PSP XLINK Mode"
HKR,Ndi\Params\PSPXLINKMode, Type, 0, "enum"
HKR,Ndi\Params\PSPXLINKMode, Default, 0, "0"
HKR,Ndi\Params\PSPXLINKMode\enum, "0", 0, "Disable"
HKR,Ndi\Params\PSPXLINKMode\enum, "1", 0, "Enable"
HKR,defaults,NetworkType,0,"1"
HKR,Ndi\params\NetworkType,default,0,"1"
HKR,NDI\params\NetworkType,ParamDesc,,%NETWORK_TYPE_STR%
HKR,NDI\params\NetworkType,type,,"enum"
HKR,NDI\params\NetworkType,flag,1,"30","00","00","00"
HKR,NDI\params\NetworkType\enum,0,,"Ad Hoc"
HKR,NDI\params\NetworkType\enum,1,,"Infrastructure"
HKR,NDI\params\NetworkType\enum,2,,"Auto select"
HKR,Ndi\Params\bRateAdaptive, ParamDesc, 0, %RATE_ADAPTIVE_STR%
HKR,Ndi\Params\bRateAdaptive, Type, 0, "enum"
HKR,Ndi\Params\bRateAdaptive, Default, 0, "1"
HKR,Ndi\Params\bRateAdaptive\enum, "0", 0, "Disable"
HKR,Ndi\Params\bRateAdaptive\enum, "1", 0, "Enable"
HKR,Ndi\Params\AdhocWirelessMode, ParamDesc, 0, %DEFAULY_ADHOC_MODE_STR%
HKR,Ndi\Params\AdhocWirelessMode, Type, 0, "enum"
HKR,Ndi\Params\AdhocWirelessMode, Default, 0, "2"
HKR,Ndi\Params\AdhocWirelessMode\enum, "2", 0, "WIRELESS_MODE_B"
HKR,Ndi\Params\AdhocWirelessMode\enum, "4", 0, "WIRELESS_MODE_G"
HKR,Ndi\Params\SupportWOL, ParamDesc, 0, "Wireless WakeOnLan"
HKR,Ndi\Params\SupportWOL, Type, 0, "enum"
HKR,Ndi\Params\SupportWOL, Default, 0, "0"
HKR,Ndi\Params\SupportWOL\enum, "0", 0, "Disable"
HKR,Ndi\Params\SupportWOL\enum, "1", 0, "Enable"
HKR,,DefaultKeyID,,"0"
HKR,,DefaultKey0,,""
HKR,,DefaultKey1,,""
HKR,,DefaultKey2,,""
HKR,,DefaultKey3,,""
[RTL8185.reg]
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5,mdcwifi"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi, Service, 0, "RTL8185"
[rtl8185.Service]
DisplayName=%RTL8185.Service.DispName%
ServiceType=1 ; %SERVICE_KERNEL_DRIVER%
StartType=3 ; %SERVICE_DEMAND_START%
ErrorControl=1 ; %SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\rtl8185.sys
LoadOrderGroup=NDIS
[RTL8185.EventLog]
Addreg=RTL8185.AddEventLog.reg
[RTL8185.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported, 0x00010001, 7
[DestinationDirs]
RTL8185.CopyFiles=12
RTL8185.CopyFiles98=11
DefaultDestDir=11 ; LDID_SYS
[SourceDisksNames]
1=%DISKNAME%,,,
[SourceDisksFiles]
rtl8185.sys=1
[Strings]
Realtek="Realtek"
Surecom="Surecom"
DISKNAME=" Realtek RTL8185 54M Wireless LAN Network Adapter Driver Disk "
SHORT_PREAM_STR="Preamble Mode"
FRAGTHRESH_STR="Fragmentation Threshold"
CHANNEL_STR="Channel"
POWER_SAVE_STR="Power Save Mode"
SSID_STR="SSID"
NETWORK_TYPE_STR="Network Type"
RATE_ADAPTIVE_STR="Rate Adaptive"
DEFAULY_ADHOC_MODE_STR="Default Adhoc WirelessMode"
RTL8185.DeviceDesc="Realtek RTL8185 54M Wireless LAN Network Adapter"
RTL8185.Service.DispName="Realtek RTL8185 54M Wireless LAN Network Adapter Driver"
RTL8185.DeviceDesc_SURECOME_EP9321="SURECOM EP-9321-g/g1 802.11g 54M WLAN PCI Adapter"
RTL8185.DeviceDesc_SURECOME_EP9428="SURECOM EP-9428-g 802.11g 54M WLAN CardBus Adapter"
