
[version]
Signature="$CHICAGO$"
Compatible=1
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%DLink%
CatalogFile=DWL520.cat ;; for WHQL certified
DriverVer=07/02/2003, 1.80.0702.2003
[Manufacturer]
%DLink%=DLink
[ControlFlags]
ExcludeFromSelect=\
PCI\VEN_1317&DEV_8201&SUBSYS_35031186
[DLink]
%DWL520.DeviceDesc%=DWL520.ndi, PCI\VEN_1317&DEV_8201&SUBSYS_35031186
[DWL520.ndi]
AddReg=DWL520.Reg, DLink.common.Reg, DLink.pci.reg, DLink.con.reg
;CpyFiles=DLink.ndis.copyfiles
[DWL520.ndi.NT]
Characteristics=0x84
BusType=5
AddReg=DWL520.ndi.reg, DLink.ndi.common.reg, DLink.pci.reg, DLink.con.reg
;CpyFiles=DLink.ndis.copyfiles.NT
[DWL520.ndi.NT.Services]
AddService=DWL520, 2, DLink.Service, DLink.EventLog
[DLink.ndis.copyfiles]
DWL520.sys,,,2
[DLink.ndis.copyfiles.NT]
DWL520.sys,,,2
[DWL520.Reg]
HKR, NDI, DeviceID, , "PCI\VEN_1317&DEV_8201"
HKR, , AdapterCFID, , 82011317
[DLink.common.Reg]
HKR, , DevLoader, , *ndis
HKR, , DeviceVxDs, , DWL520.sys
HKR, , AdapterType, , 5
HKR, , BusType, , 5
HKR, NDIS, MajorNdisVersion, 1, 04
HKR, NDIS, MinorNdisVersion, 1, 00
HKR, NDIS, LogDriverName, , "DWL520"
HKR, Ndi\Interfaces, DefUpper, , "ndis3"
HKR, Ndi\Interfaces, DefLower, , "ethernet"
HKR, Ndi\Interfaces, UpperRange, , "ndis3"
HKR, Ndi\Interfaces, LowerRange, , "ethernet"
HKR, Ndi\Install, ndis3, 0, "DLink.Install"
HKR, , OSModel, , "0"
[DWL520.ndi.reg]
HKR, , AdapterCFID, 0, "82011317"
[DLink.ndi.common.reg]
HKR, Ndi, Service, 0, "DWL520"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, , OSModel, , "1"
[DLink.pci.reg]
HKR, , AdapterType, 0, "5"
HKR, , PacketsPerTxInt, , "1" ; 0x0a
HKR, , PacketsPerRxInd, , "10" ; 0x0a
HKR, , BurstLength, , "0" ; 0(Unlimited), 1 DW, 2 DW, 3 DW,...
HKR, , TxPacketDesc, , "300"
HKR, , RxPacketDesc, , "80" ; 0x78
HKR, , TxDmaDesc, , "600"
HKR, , RxDmaDesc, , "40" ; 0x28
HKR, , SupportFH, , "0" ; not support
HKR, , SupportDS, , "1" ; support
HKR, , BeaconInterval, , "100" ;
HKR, , ATIMWindow, , "0" ;
HKR, , StaEntryAmount, , "48" ; size of station base
HKR, , MaxFragedMSDU, , "40" ;
HKR, , MaxTxBuffer, , "100" ;
HKR, , HardwareWepTx, , "1" ;
HKR, , Promiscuous, , "0" ;
HKR, , FragThreshold, , "2346" ;
HKR, , RadioStatus, , "0" ;
[DLink.con.reg]
HKR, Ndi\Params\SelectedChannel, ParamDesc, , "Channel"
HKR, Ndi\Params\SelectedChannel, default, , "6"
HKR, Ndi\Params\SelectedChannel, type, , "enum"
HKR, Ndi\Params\SelectedChannel\enum, 0, , "Automatic"
HKR, Ndi\Params\SelectedChannel\enum, 1, , "01"
HKR, Ndi\Params\SelectedChannel\enum, 2, , "02"
HKR, Ndi\Params\SelectedChannel\enum, 3, , "03"
HKR, Ndi\Params\SelectedChannel\enum, 4, , "04"
HKR, Ndi\Params\SelectedChannel\enum, 5, , "05"
HKR, Ndi\Params\SelectedChannel\enum, 6, , "06"
HKR, Ndi\Params\SelectedChannel\enum, 7, , "07"
HKR, Ndi\Params\SelectedChannel\enum, 8, , "08"
HKR, Ndi\Params\SelectedChannel\enum, 9, , "09"
HKR, Ndi\Params\SelectedChannel\enum, 10, , "10"
HKR, Ndi\Params\SelectedChannel\enum, 11, , "11"
HKR, Ndi\Params\SelectedChannel\enum, 12, , "12"
HKR, Ndi\Params\SelectedChannel\enum, 13, , "13"
HKR, Ndi\Params\SelectedChannel\enum, 14, , "14"
HKR, Ndi\Params\SelectedChannel, flag, 1, "20","00","00","00"
HKR, Ndi\Params\DataRate, ParamDesc, , "Data Rate"
HKR, Ndi\Params\DataRate, default, , "0"
HKR, Ndi\Params\DataRate, type, , "enum"
HKR, Ndi\Params\DataRate\enum, 0, , "Auto"
HKR, Ndi\Params\DataRate\enum, 10, , "1M"
HKR, Ndi\Params\DataRate\enum, 20, , "2M"
HKR, Ndi\Params\DataRate\enum, 55, , "5.5M"
HKR, Ndi\Params\DataRate\enum, 110, , "11M"
HKR, Ndi\Params\DataRate, flag, 1, "20","00","00","00"
HKR, Ndi\Params\OperationMode, ParamDesc, , "Network Type"
HKR, Ndi\Params\OperationMode, default, , "0"
HKR, Ndi\Params\OperationMode, type, , "enum"
HKR, Ndi\Params\OperationMode\enum, 0, , "Infrastructure"
HKR, Ndi\Params\OperationMode\enum, 1, , "AdHoc Mode"
HKR, Ndi\Params\OperationMode, flag, 1, "20","00","00","00"
HKR, Ndi\params\SSID, ParamDesc, , "SSID"
HKR, Ndi\params\SSID, type, , "edit"
HKR, NDI\params\SSID, limitText, , "32"
HKR, NDI\params\SSID, default, , "default"
HKR, NDI\params\SSID, flag, 1, "20","00","00","00"
HKR, Ndi\params\RTSThreshold, ParamDesc, 0, "RTS Threshold"
HKR, Ndi\params\RTSThreshold, type, 0, "int"
HKR, Ndi\params\RTSThreshold, default, 0, "2346"
HKR, Ndi\params\RTSThreshold, min, 0, "0"
HKR, Ndi\params\RTSThreshold, max, 0, "2346"
HKR, Ndi\params\RTSThreshold, step, 0, "1"
HKR, , RTSThreshold, 0, "2346"
HKR, Ndi\Params\WepEnabled, ParamDesc, , "WEP"
HKR, Ndi\Params\WepEnabled, default, , "0"
HKR, Ndi\Params\WepEnabled, type, , "enum"
HKR, Ndi\Params\WepEnabled\enum, 0, , "Disabled"
HKR, Ndi\Params\WepEnabled\enum, 1, , "WEP key 64 bit"
HKR, Ndi\Params\WepEnabled\enum, 2, , "WEP key 128 bit"
HKR, Ndi\Params\WepEnabled, flag, 1, "20","00","00","00"
HKR, Ndi\Params\SharedKeyIndex, ParamDesc, , "Select SharedKey Index"
HKR, Ndi\Params\SharedKeyIndex, default, , "0"
HKR, Ndi\Params\SharedKeyIndex, type, , "enum"
HKR, Ndi\Params\SharedKeyIndex\enum, 0, , "No Selection"
HKR, Ndi\Params\SharedKeyIndex\enum, 1, , "1"
HKR, Ndi\Params\SharedKeyIndex\enum, 2, , "2"
HKR, Ndi\Params\SharedKeyIndex\enum, 3, , "3"
HKR, Ndi\Params\SharedKeyIndex\enum, 4, , "4"
HKR, Ndi\Params\SharedKeyIndex, flag, 1, "20","00","00","00"
HKR, Ndi\params\SharedKey1, ParamDesc, , "ShareKey1"
HKR, Ndi\params\SharedKey1, type, , "edit"
HKR, NDI\params\SharedKey1, limitText, , "26"
HKR, NDI\params\SharedKey1, default, , ""
HKR, NDI\params\SharedKey1, flag, 1, "20","00","00","00"
HKR, Ndi\params\SharedKey2, ParamDesc, , "ShareKey2"
HKR, Ndi\params\SharedKey2, type, , "edit"
HKR, NDI\params\SharedKey2, limitText, , "26"
HKR, NDI\params\SharedKey2, default, , ""
HKR, NDI\params\SharedKey2, flag, 1, "20","00","00","00"
HKR, Ndi\params\SharedKey3, ParamDesc, , "ShareKey3"
HKR, Ndi\params\SharedKey3, type, , "edit"
HKR, NDI\params\SharedKey3, limitText, , "26"
HKR, NDI\params\SharedKey3, default, , ""
HKR, NDI\params\SharedKey3, flag, 1, "20","00","00","00"
HKR, Ndi\params\SharedKey4, ParamDesc, , "ShareKey4"
HKR, Ndi\params\SharedKey4, type, , "edit"
HKR, NDI\params\SharedKey4, limitText, , "26"
HKR, NDI\params\SharedKey4, default, , ""
HKR, NDI\params\SharedKey4, flag, 1, "20","00","00","00"
HKR, Ndi\Params\AntennaSelection, ParamDesc, , "Antenna"
HKR, Ndi\Params\AntennaSelection, default, , "128"
HKR, Ndi\Params\AntennaSelection, type, , "enum"
HKR, Ndi\Params\AntennaSelection\enum, 0, , "Antenna A"
HKR, Ndi\Params\AntennaSelection\enum, 64, , "Antenna B"
HKR, Ndi\Params\AntennaSelection\enum, 128, , "Diversity"
HKR, Ndi\Params\AntennaSelection, flag, 1, "20","00","00","00"
HKR, Ndi\Params\PreambleMode, ParamDesc, , "Preamble Mode"
HKR, Ndi\Params\PreambleMode, default, , "0"
HKR, Ndi\Params\PreambleMode, type, , "enum"
HKR, Ndi\Params\PreambleMode\enum, 1, , "Long Preamble"
HKR, Ndi\Params\PreambleMode\enum, 2, , "Short Preamble"
HKR, Ndi\Params\PreambleMode, flag, 1, "20","00","00","00"
[DLink.Service]
DisplayName=%DLink.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_AUTO_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\DWL520.sys
LoadOrderGroup=NDIS
AddReg=TextModeFlags.reg
[DLink.EventLog]
AddReg=DLink.AddEventLog.reg
[DLink.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, %%SystemRoot%%\System32\netevent.dll
HKR, , TypesSupported, 0x00010001, 7
[TextModeFlags.reg]
HKR, , TextModeFlags, 0x00010001, 0x0001
[DestinationDirs]
DLink.ndis.copyfiles=11
DLink.ndis.copyfiles.NT=12
DefaultDestDir=11 ; LDID_SYS
[SourceDisksNames]
1=%DISKNAME%,,,
[SourceDisksFiles]
DWL520.sys=1
netdwl.inf=1
[Strings]
DLink="D-Link Corporation"
DISKNAME="D-Link Air DWL-520 Wireless PCI Adapter Driver Diskette "
DWL520.DeviceDesc="D-Link Air DWL-520 Wireless PCI Adapter"
DLink.Service.DispName="D-Link Air DWL-520 Wireless PCI Adapter"

