
[version]
Signature="$Chicago$"
Compatible=1
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%Realtek% ;;
DriverVer=07/08/2003,5.145.0708.2003
[Manufacturer]
%Realtek%=Realtek
[ControlFlags]
ExcludeFromSelect=PCI\VEN_1799&DEV_6001
ExcludeFromSelect=PCI\VEN_1799&DEV_6001&SUBSYS_60011799
[Realtek]
%RTL8180.DeviceDesc%=RTL8180.ndi, PCI\VEN_1799&DEV_6001
%RTL8180.DeviceDesc%=RTL8180.ndi, PCI\VEN_1799&DEV_6001&SUBSYS_60011799
[rtl8180.ndi]
DriverVer=07/08/2003,145
AddReg=rtl8180.id.reg, RTL8180.common.reg, RTL8180.win.reg
;CpyFiles=RTL8180.CopyFiles98
[RTL8180.ndi.NT]
AddReg=RTL8180.common.reg, RTL8180.reg
Characteristics=0x84
BusType=5
;CpyFiles=RTL8180.CopyFiles
[RTL8180.ndi.NT.Services]
AddService=rtl8180, 2, rtsnt.Service, RTL8180.EventLog
[RTL8180.CopyFiles]
Bel6001.sys,,,2
[RTL8180.CopyFiles98]
Bel6001.sys,,,2
[rtl8180.id.reg]
HKR, Ndi, DeviceID, 0, "PCI\VEN_1799&DEV_6001"
HKR, Ndi\Install, , 0, rtsnt.install
HKR, NDI\Params\NetworkAddress, flag, 1, 30, 00, 00, 00
[RTL8180.win.reg]
HKR, , DriverDesc, 0, "Belkin 11Mbps Wireless Desktop Network Card"
HKR, , DevLoader, 0, *ndis
HKR, , DeviceVxDs, 0, Bel6001.sys
HKR, , EnumPropPages, 0, netdi.dll, EnumPropPages
HKR, , MediaType, 0, 1
HKR, , AdapterType, 0, 5
HKR, , BusType, 0, 5
HKR, NDIS, MajorNdisVersion, 1, 03
HKR, NDIS, MinorNdisVersion, 1, 0a
HKR, NDIS, LogDriverName, 0, "RTL8180"
HKR, Ndi\Interfaces, DefLower, , "ethernet"
HKR, Ndi\Interfaces, LowerRange, , "ethernet"
HKR, Ndi\Interfaces, DefUpper, , "ndis3"
HKR, Ndi\Interfaces, UpperRange, , "ndis3"
HKR, Ndi\Install, ndis3, 0, "rtl180.ndis5"
[RTL8180.common.reg]
HKR,Ndi\params\NetworkAddress, ParamDesc, 0, %NetworkAddress%
HKR,Ndi\params\NetworkAddress, type, 0, "edit"
HKR,Ndi\params\NetworkAddress, default, 0, "000000000000"
HKR,Ndi\params\NetworkAddress, LimitText, 0, "12"
HKR,Ndi\params\NetworkAddress, UpperCase, 0, "1"
HKR,Ndi\params\NetworkAddress, Optional, 0, "1"
HKR,defaults,Channel,0,"11"
HKR,Ndi\params\Channel,default, 0,"11"
HKR,NDI\params\Channel,ParamDesc,,%CHANNEL_STR%
HKR,NDI\params\Channel,type, ,"int"
HKR,NDI\params\Channel,flag, 1,"30","00","00","00"
HKR,NDI\params\Channel,min, 0,"1"
HKR,NDI\params\Channel,max, 0,"14"
HKR,NDI\params\Channel,step, 0,"1"
HKR,defaults,PowerSaveMode,0,"0"
HKR,Ndi\params\PowerSaveMode,default,0,"0"
HKR,NDI\params\PowerSaveMode,ParamDesc,,%POWER_SAVE_STR%
HKR,NDI\params\PowerSaveMode,type,,"enum"
HKR,NDI\params\PowerSaveMode,flag,1,"30","00","00","00"
HKR,NDI\params\PowerSaveMode\enum,0,,"OFF"
HKR,NDI\params\PowerSaveMode\enum,1,,"Maximum"
HKR,NDI\params\PowerSaveMode\enum,2,,"Minimum"
HKR,Ndi\params\SSID, ParamDesc, 0, %SSID_STR%
HKR,defaults, SSID, 0, "ANY"
HKR,Ndi\params\SSID, type, 0, "edit"
HKR,Ndi\params\SSID, default, 0, "ANY"
HKR,Ndi\params\SSID, LimitText, 0, "32"
HKR,defaults,NetworkType,0,"1"
HKR,Ndi\params\NetworkType,default,0,"1"
HKR,NDI\params\NetworkType,ParamDesc,,%NETWORK_TYPE_STR%
HKR,NDI\params\NetworkType,type,,"enum"
HKR,NDI\params\NetworkType,flag,1,"30","00","00","00"
HKR,NDI\params\NetworkType\enum,0,,"Ad Hoc"
HKR,NDI\params\NetworkType\enum,1,,"Infrastructure"
HKR,NDI\params\NetworkType\enum,2,,"Auto select"
HKR,,DefaultKeyID,,"0"
HKR,,DefaultKey0,,""
HKR,,DefaultKey1,,""
HKR,,DefaultKey2,,""
HKR,,DefaultKey3,,""
[RTL8180.reg]
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi, Service, 0, "RTL8180"
[rtsnt.Service]
DisplayName=%RTL8180.Service.DispName%
ServiceType=1 ; %SERVICE_KERNEL_DRIVER%
StartType=3 ; %SERVICE_DEMAND_START%
ErrorControl=1 ; %SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\Bel6001.sys
LoadOrderGroup=NDIS
[RTL8180.EventLog]
Addreg=RTL8180.AddEventLog.reg
[RTL8180.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported, 0x00010001, 7
[DestinationDirs]
RTL8180.CopyFiles=12
RTL8180.CopyFiles98=11
DefaultDestDir=11 ; LDID_SYS
[SourceDisksNames]
1=%DISKNAME%,,,
[SourceDisksFiles]
Bel6001.sys=1
[Strings]
Realtek="Belkin"
DISKNAME=" Belkin 11Mbps Wireless Desktop Network Card Driver Disk "
NetworkAddress="Network Address"
ADHOC_DEMO_STR="Adhoc Demo Mode"
SHORT_PREAM_STR="Preamble Mode"
AH_BCNINTV_STR="Beacon Interval"
AH_ATIMINTV_STR="Atim Window"
RTSTHRESH_STR="RTS Threshold"
FRAGTHRESH_STR="Fragmentation Threshold"
AUTHENT_TYPE_STR="Authentication Algorithm"
LISTENINTERVAL_STR="Listen Interval"
CHANNEL_STR="Channel"
DATA_RATE_STR="Data Rate"
POWER_SAVE_STR="Power Save Mode"
SSID_STR="SSID"
NETWORK_TYPE_STR="Network Type"
RTL8180.DeviceDesc="Belkin 11Mbps Wireless Desktop Network Card"
RTL8180.Service.DispName= "Belkin 11Mbps Wireless Desktop Network Card Driver"

