
[version]
Signature="$CHICAGO$"
Compatible=1
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%VER_VENDOR_STR%
CatalogFile=WLANPCI.cat ;; for WHQL certified
DriverVer=02/26/2004, 1.80.0226.2004
[Manufacturer]
%VER_VENDOR_STR%=DeviceList
[ControlFlags]
ExcludeFromSelect=PCI\VEN_1317&DEV_8201&SUBSYS_82011317
ExcludeFromSelect=PCI\VEN_1317&DEV_8201&SUBSYS_AB5013D1
ExcludeFromSelect=PCI\VEN_1317&DEV_8201&SUBSYS_AB6013D1
ExcludeFromSelect=PCI\VEN_1317&DEV_8201&SUBSYS_AB7013D1
ExcludeFromSelect=PCI\VEN_1317&DEV_8201&SUBSYS_0705152D
[DeviceList]
%ADM8211_CardBus.DeviceDesc%=ADM8211.ndi, PCI\VEN_1317&DEV_8201&SUBSYS_82011317
%ADM8211_CardBus.DeviceDesc%=ADM8211.ndi, PCI\VEN_1317&DEV_8201&SUBSYS_AB5013D1
%ADM8211_PCI.DeviceDesc%=ADM8211.ndi, PCI\VEN_1317&DEV_8201&SUBSYS_AB6013D1
%ADM8211_MiniPCI.DeviceDesc%=ADM8211.ndi, PCI\VEN_1317&DEV_8201&SUBSYS_AB7013D1
%ADM8211_MiniPCI.DeviceDesc%=ADM8211.ndi, PCI\VEN_1317&DEV_8201&SUBSYS_0705152D
[ADM8211.ndi]
AddReg=ADM8211.Reg, ADMtek.common.Reg, ADMtek.pci.reg, ADMtek.con.reg
;CpyFiles=ADMtek.ndis.copyfiles
[ADM8211.ndi.NT]
Characteristics=0x84
BusType=5
AddReg=ADM8211.ndi.reg, ADMtek.ndi.common.reg, ADMtek.pci.reg, ADMtek.con.reg
;CpyFiles=ADMtek.ndis.copyfiles.NT
[ADM8211.ndi.NT.Services]
AddService=ADM8211, 2, ADMtek.Service, ADM8211.EventLog
[ADMtek.ndis.copyfiles]
WLANPCI.sys,,,2
[ADMtek.ndis.copyfiles.NT]
WLANPCI.sys,,,2
[ADM8211.Reg]
HKR, NDI, DeviceID, , "PCI\VEN_1317&DEV_8201"
HKR, , AdapterCFID, , 82011317
[ADMtek.common.Reg]
HKR, , DevLoader, , *ndis
HKR, , DeviceVxDs, , WLANPCI.sys
HKR, , AdapterType, , 5
HKR, , BusType, , 5
HKR, NDIS, MajorNdisVersion, 1, 04
HKR, NDIS, MinorNdisVersion, 1, 00
HKR, NDIS, LogDriverName, , "ADM8211"
HKR, Ndi\Interfaces, DefUpper, , "ndis3"
HKR, Ndi\Interfaces, DefLower, , "ethernet"
HKR, Ndi\Interfaces, UpperRange, , "ndis3"
HKR, Ndi\Interfaces, LowerRange, , "ethernet"
HKR, Ndi\Install, ndis3, 0, "ADMtek.Install"
[ADM8211.ndi.reg]
HKR, , AdapterCFID, 0, "82011317"
[ADMtek.ndi.common.reg]
HKR, Ndi, Service, 0, "ADM8211"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
[ADMtek.pci.reg]
HKR, , AdapterType, 0, "5"
HKR, , PacketsPerTxInt, , "1" ; 0x0a
HKR, , PacketsPerRxInd, , "10" ; 0x0a
HKR, , BurstLength, , "0" ; 0(Unlimited), 1 DW, 2 DW, 3 DW,...
HKR, , TxPacketDesc, , "300"
HKR, , RxPacketDesc, , "80" ; 0x78
HKR, , TxDmaDesc, , "600"
HKR, , RxDmaDesc, , "40" ; 0x28
HKR, , SupportFH, , "0" ; not support
HKR, , SupportDS, , "1" ; support
HKR, , BeaconInterval, , "100" ;
HKR, , ATIMWindow, , "0" ;
HKR, , StaEntryAmount, , "48" ; size of station base
HKR, , MaxFragedMSDU, , "40" ;
HKR, , MaxTxBuffer, , "100" ;
HKR, , HardwareWepTx, , "1" ;
HKR, , Promiscuous, , "0" ;
HKR, , FragThreshold, , "2346" ;
HKR, , RadioStatus, , "0" ;
[ADMtek.con.reg]
HKR, Ndi\Params\SelectedChannel, ParamDesc, , "Channel"
HKR, Ndi\Params\SelectedChannel, default, , "0"
HKR, Ndi\Params\SelectedChannel, type, , "enum"
HKR, Ndi\Params\SelectedChannel\enum, 0, , "Automatic"
HKR, Ndi\Params\SelectedChannel\enum, 1, , "01"
HKR, Ndi\Params\SelectedChannel\enum, 2, , "02"
HKR, Ndi\Params\SelectedChannel\enum, 3, , "03"
HKR, Ndi\Params\SelectedChannel\enum, 4, , "04"
HKR, Ndi\Params\SelectedChannel\enum, 5, , "05"
HKR, Ndi\Params\SelectedChannel\enum, 6, , "06"
HKR, Ndi\Params\SelectedChannel\enum, 7, , "07"
HKR, Ndi\Params\SelectedChannel\enum, 8, , "08"
HKR, Ndi\Params\SelectedChannel\enum, 9, , "09"
HKR, Ndi\Params\SelectedChannel\enum, 10, , "10"
HKR, Ndi\Params\SelectedChannel\enum, 11, , "11"
HKR, Ndi\Params\SelectedChannel\enum, 12, , "12"
HKR, Ndi\Params\SelectedChannel\enum, 13, , "13"
HKR, Ndi\Params\SelectedChannel\enum, 14, , "14"
HKR, Ndi\Params\SelectedChannel, flag, 1, "20","00","00","00"
HKR, Ndi\Params\DataRate, ParamDesc, , "Data Rate"
HKR, Ndi\Params\DataRate, default, , "110"
HKR, Ndi\Params\DataRate, type, , "enum"
HKR, Ndi\Params\DataRate\enum, 0, , "AutoDetect"
HKR, Ndi\Params\DataRate\enum, 10, , "1M"
HKR, Ndi\Params\DataRate\enum, 20, , "2M"
HKR, Ndi\Params\DataRate\enum, 55, , "5.5M"
HKR, Ndi\Params\DataRate\enum, 110, , "11M"
HKR, Ndi\Params\DataRate, flag, 1, "20","00","00","00"
HKR, Ndi\Params\OperationMode, ParamDesc, , "Network Type"
HKR, Ndi\Params\OperationMode, default, , "0"
HKR, Ndi\Params\OperationMode, type, , "enum"
HKR, Ndi\Params\OperationMode\enum, 0, , "Infrastructure"
HKR, Ndi\Params\OperationMode\enum, 1, , "AdHoc Mode"
HKR, Ndi\Params\OperationMode, flag, 1, "20","00","00","00"
HKR, Ndi\params\SSID, ParamDesc, , "SSID"
HKR, Ndi\params\SSID, type, , "edit"
HKR, NDI\params\SSID, limitText, , "32"
HKR, NDI\params\SSID, default, , "ANY"
HKR, NDI\params\SSID, flag, 1, "20","00","00","00"
HKR, Ndi\params\RTSThreshold, ParamDesc, 0, "RTS Threshold"
HKR, Ndi\params\RTSThreshold, type, 0, "int"
HKR, Ndi\params\RTSThreshold, default, 0, "2346"
HKR, Ndi\params\RTSThreshold, min, 0, "0"
HKR, Ndi\params\RTSThreshold, max, 0, "2346"
HKR, Ndi\params\RTSThreshold, step, 0, "1"
HKR, , RTSThreshold, 0, "2346"
HKR, Ndi\Params\WepEnabled, ParamDesc, , "WEP"
HKR, Ndi\Params\WepEnabled, default, , "0"
HKR, Ndi\Params\WepEnabled, type, , "enum"
HKR, Ndi\Params\WepEnabled\enum, 0, , "Disabled"
HKR, Ndi\Params\WepEnabled\enum, 1, , "WEP key 64 bit"
HKR, Ndi\Params\WepEnabled\enum, 2, , "WEP key 128 bit"
HKR, Ndi\Params\WepEnabled, flag, 1, "20","00","00","00"
HKR, Ndi\Params\SharedKeyIndex, ParamDesc, , "Select SharedKey Index"
HKR, Ndi\Params\SharedKeyIndex, default, , "0"
HKR, Ndi\Params\SharedKeyIndex, type, , "enum"
HKR, Ndi\Params\SharedKeyIndex\enum, 0, , "No Selection"
HKR, Ndi\Params\SharedKeyIndex\enum, 1, , "1"
HKR, Ndi\Params\SharedKeyIndex\enum, 2, , "2"
HKR, Ndi\Params\SharedKeyIndex\enum, 3, , "3"
HKR, Ndi\Params\SharedKeyIndex\enum, 4, , "4"
HKR, Ndi\Params\SharedKeyIndex, flag, 1, "20","00","00","00"
HKR, Ndi\params\SharedKey1, ParamDesc, , "ShareKey1"
HKR, Ndi\params\SharedKey1, type, , "edit"
HKR, NDI\params\SharedKey1, limitText, , "26"
HKR, NDI\params\SharedKey1, default, , ""
HKR, NDI\params\SharedKey1, flag, 1, "20","00","00","00"
HKR, Ndi\params\SharedKey2, ParamDesc, , "ShareKey2"
HKR, Ndi\params\SharedKey2, type, , "edit"
HKR, NDI\params\SharedKey2, limitText, , "26"
HKR, NDI\params\SharedKey2, default, , ""
HKR, NDI\params\SharedKey2, flag, 1, "20","00","00","00"
HKR, Ndi\params\SharedKey3, ParamDesc, , "ShareKey3"
HKR, Ndi\params\SharedKey3, type, , "edit"
HKR, NDI\params\SharedKey3, limitText, , "26"
HKR, NDI\params\SharedKey3, default, , ""
HKR, NDI\params\SharedKey3, flag, 1, "20","00","00","00"
HKR, Ndi\params\SharedKey4, ParamDesc, , "ShareKey4"
HKR, Ndi\params\SharedKey4, type, , "edit"
HKR, NDI\params\SharedKey4, limitText, , "26"
HKR, NDI\params\SharedKey4, default, , ""
HKR, NDI\params\SharedKey4, flag, 1, "20","00","00","00"
HKR, Ndi\Params\AntennaSelection, ParamDesc, , "Antenna"
HKR, Ndi\Params\AntennaSelection, default, , "128"
HKR, Ndi\Params\AntennaSelection, type, , "enum"
HKR, Ndi\Params\AntennaSelection\enum, 0, , "Antenna A"
HKR, Ndi\Params\AntennaSelection\enum, 64, , "Antenna B"
HKR, Ndi\Params\AntennaSelection\enum, 128, , "Diversity"
HKR, Ndi\Params\AntennaSelection, flag, 1, "20","00","00","00"
HKR, Ndi\params\CR03, ParamDesc, 0, "CR03"
HKR, Ndi\params\CR03, type, , "edit"
HKR, NDI\params\CR03, limitText, , "2"
HKR, NDI\params\CR03, default, , "80"
HKR, NDI\params\CR03, flag, 1, "20","00","00","00"
HKR, Ndi\params\CR17, ParamDesc, 0, "CR17"
HKR, Ndi\params\CR17, type, , "edit"
HKR, NDI\params\CR17, limitText, , "2"
HKR, NDI\params\CR17, default, , "74"
HKR, NDI\params\CR17, flag, 1, "20","00","00","00"
HKR, Ndi\params\CR20, ParamDesc, 0, "CR20"
HKR, Ndi\params\CR20, type, 0, "edit"
HKR, Ndi\params\CR20, default, 0, "0A"
HKR, Ndi\params\CR20, LimitText, 0, "2"
HKR, NDI\params\CR20, flag, 1, "20","00","00","00"
HKR, Ndi\params\CR21, ParamDesc, 0, "CR21"
HKR, Ndi\params\CR21, type, 0, "edit"
HKR, Ndi\params\CR21, default, 0, "46"
HKR, Ndi\params\CR21, LimitText, 0, "2"
HKR, NDI\params\CR21, flag, 1, "20","00","00","00"
HKR, Ndi\params\CR28, ParamDesc, 0, "CR28"
HKR, Ndi\params\CR28, type, 0, "edit"
HKR, Ndi\params\CR28, default, 0, "00"
HKR, Ndi\params\CR28, LimitText, 0, "2"
HKR, NDI\params\CR28, flag, 1, "20","00","00","00"
HKR, Ndi\params\CR29, ParamDesc, 0, "CR29"
HKR, Ndi\params\CR29, type, 0, "edit"
HKR, Ndi\params\CR29, default, 0, "84"
HKR, Ndi\params\CR28, LimitText, 0, "2"
HKR, NDI\params\CR29, flag, 1, "20","00","00","00"
HKR, Ndi\params\CardType, ParamDesc, , "CardType"
HKR, Ndi\params\CardType, type, , "edit"
HKR, NDI\params\CardType, limitText, , "6"
HKR, NDI\params\CardType, default, , "abocom"
HKR, NDI\params\CardType, flag, 1, "20","00","00","00"
[ADMtek.Service]
DisplayName=%ADMtek.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_AUTO_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\WLANPCI.sys
LoadOrderGroup=NDIS
AddReg=TextModeFlags.reg
[ADM8211.EventLog]
AddReg=ADMtek.AddEventLog.reg
[ADMTek.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, %%SystemRoot%%\System32\netevent.dll
HKR, , TypesSupported, 0x00010001, 7
[TextModeFlags.reg]
HKR, , TextModeFlags, 0x00010001, 0x0001
[DestinationDirs]
ADMtek.ndis.copyfiles=11
ADMtek.ndis.copyfiles.NT=12
DefaultDestDir=11 ; LDID_SYS
[SourceDisksNames]
1=%DISKNAME%,,,
[SourceDisksFiles]
WLANPCI.sys=1
WLANPCI.inf=1
[Strings]
VER_VENDOR_STR ="Wireless LAN"
DISKNAME="802.11b Wireless PC Card Driver Diskette"
ADM8211_CardBus.DeviceDesc="802.11b Wireless CardBus PC Card"
ADM8211_PCI.DeviceDesc="802.11b Wireless PCI Card"
ADM8211_MiniPCI.DeviceDesc="802.11b Wireless MiniPCI Card"
ADMtek.Service.DispName="Wireless PC Card"

