[version]
Signature="$Chicago$" ; Combined Win9x/Win2k inf
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%V_MSI%
Compatible=1
DriverVer=07/17/2003, 3.30.15.0
CatalogFile=ms68bm.CAT
[Manufacturer]
%V_MSI%=Minitar
[ControlFlags]
ExcludeFromSelect=*
[Minitar]
%MS68XX.CARDBUS%=MS68XX, PCI\VEN_14E4&DEV_4301&SUBSYS_68021462
%MS68XX.miniPCI%=MS68XX, PCI\VEN_14E4&DEV_4301&SUBSYS_68041462
%MS68XX.PCI%=MS68XX, PCI\VEN_14E4&DEV_4301&SUBSYS_68071462
%MS68XG.CARDBUS%=MS68XG, PCI\VEN_14E4&DEV_4320&SUBSYS_68191462
%MS68XG.miniPCI%=MS68XG, PCI\VEN_14E4&DEV_4320&SUBSYS_68201462
%MS68XG.PCI%=MS68XG, PCI\VEN_14E4&DEV_4320&SUBSYS_68251462
%MS68XM.CARDBUS%=MS68XM, PCI\VEN_14E4&DEV_4324
[MS68XX]
AddReg=MS68XX.win.reg, common.reg, b.options.reg, bg.options.reg
;CpyFiles=MS68XX.sys.files
[MS68XG]
AddReg=MS68XX.win.reg, common.reg, g.options.reg, bg.options.reg
;CpyFiles=MS68XX.sys.files
[BCM43XM]
AddReg=MS68XX.win.reg, common.reg, bag.options.reg
;CpyFiles=MS68XX.sys.files
[MS68XX.win.reg]
HKR, Ndi, DeviceID, , "PCI\VEN_14E4&DEV_4307"
HKR, , EnumPropPages, 0, "netdi.dll,EnumPropPages"
HKR, NDIS, MajorNdisVersion, 1, 03
HKR, NDIS, MinorNdisVersion, 1, 0A
HKR, NDIS, LogDriverName, , "MS68XX"
HKR, NDIS, MajorDriverVersion, 1, 1
HKR, NDIS, MinorDriverVersion, 1, 0
HKR, Ndi\Install, , , "MS68XX.ndi.install"
HKR, Ndi\Interfaces, DefUpper, 0, "ndis3"
HKR, Ndi\Interfaces, DefLower, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis3"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi, HelpText, , %MS68XX_HELP%
[MS68XX.ndi.install]
AddReg=MS68XX.ndi.reg
[MS68XX.ndi.reg]
HKR, , DevLoader, 0, "*ndis"
HKR, , DeviceVxDs, 0, %DEFAULT_WIN9X_SYS%
[MS68XX.sys.files]
ms68bm.SYS,,,18
[MS68XX.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=MS68XX.reg, common.reg, b.options.reg, bg.options.reg
;CpyFiles=MS68XX.files.NT
[MS68XG.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=MS68XX.reg, common.reg, g.options.reg, bg.options.reg
;CpyFiles=MS68XX.files.NT
[MS68XM.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=MS68XX.reg, common.reg, bag.options.reg
;CpyFiles=MS68XX.files.NT
[MS68XX.NT.Services]
AddService=MS68XX, 2, MS68XX.Service, common.EventLog
[MS68XG.NT.Services]
AddService=MS68XX, 2, MS68XX.Service, common.EventLog
[MS68XM.NT.Services]
AddService=MS68XX, 2, MS68XX.Service, common.EventLog
[MS68XX.reg]
HKR, Ndi\Interfaces, UpperRange, , "ndis5"
HKR, Ndi\Interfaces, LowerRange, , "ethernet"
HKR, Ndi, HelpText, , %MS68XX_HELP%
HKR, Ndi, Service, 0, "MS68XX"
[MS68XX.Service]
DisplayName=%MS68XX.Service.DispName%
ServiceType=1 ; %SERVICE_KERNEL_DRIVER%
StartType=3 ; %SERVICE_DEMAND_START%
ErrorControl=1 ; %SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\ms68bm.sys
LoadOrderGroup=NDIS
[common.EventLog]
AddReg=common.AddEventLog.reg
[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported, 0x00010001, 7
[MS68XX.files.NT]
ms68bm.SYS,,,2
[common.reg]
HKR, ,"EnableSoftAP", 0, "0"
HKR, ,"EnableLeap", 0, "0"
HKR, ,"EnableAutoConnect", 0, "0"
HKR, Ndi\params\RadioState, ParamDesc, 0, "Radio Enable/Disable"
HKR, Ndi\params\RadioState, type, 0, "enum"
HKR, Ndi\params\RadioState\enum, "1", 0, "Disabled"
HKR, Ndi\params\RadioState\enum, "0", 0, "Enabled"
HKR, Ndi\params\RadioState,default,,"0"
HKR, Ndi\params\PowerSaveMode, ParamDesc, 0, "Power Save Mode"
HKR, Ndi\params\PowerSaveMode, type, 0, "enum"
HKR, Ndi\params\PowerSaveMode\enum, "0", 0, "Disabled"
HKR, Ndi\params\PowerSaveMode\enum, "1", 0, "Enabled"
HKR, Ndi\params\PowerSaveMode,default,,"0"
HKR, Ndi\params\PLCPHeader, ParamDesc, 0, "PLCP Header"
HKR, Ndi\params\PLCPHeader, type, 0, "enum"
HKR, Ndi\params\PLCPHeader\enum, "-1", 0, "Long"
HKR, Ndi\params\PLCPHeader\enum, "0", 0, "Auto (Short/Long)"
HKR, Ndi\params\PLCPHeader,default,,"0"
HKR, Ndi\params\frag, ParamDesc, 0, "Fragmentation Threshold"
HKR, Ndi\params\frag,type,0,"dword"
HKR, Ndi\params\frag,min,,"256"
HKR, Ndi\params\frag,max,,"2346"
HKR, Ndi\params\frag,default,,"2346"
HKR, Ndi\params\rts, ParamDesc, 0, "RTS Threshold"
HKR, Ndi\params\rts,type,0,"dword"
HKR, Ndi\params\rts,min,,"0"
HKR, Ndi\params\rts,max,,"2347"
HKR, Ndi\params\rts,default,,"2347"
HKR, Ndi\params\NetworkAddress, ParamDesc, 0, "Locally Administered MAC Address"
HKR, Ndi\params\NetworkAddress, type, 0, "edit"
HKR, Ndi\params\NetworkAddress, LimitText, 0, "12"
HKR, Ndi\params\NetworkAddress, UpperCase, 0, "1"
HKR, Ndi\params\NetworkAddress, default, 0, ""
HKR, Ndi\params\NetworkAddress, optional, 0, "1"
HKR, Ndi\params\PwrOut, ParamDesc, 0, "Power Output"
HKR, Ndi\params\PwrOut, type, 0, "enum"
HKR, Ndi\params\PwrOut\enum, "100", 0, "100%"
HKR, Ndi\params\PwrOut\enum, "75", 0, "75%"
HKR, Ndi\params\PwrOut\enum, "50", 0, "50%"
HKR, Ndi\params\PwrOut\enum, "25", 0, "25%"
HKR, Ndi\params\PwrOut,default,,"100"
HKR, Ndi\params\FrameBursting, ParamDesc, 0, "XPress (TM) Technology"
HKR, Ndi\params\FrameBursting, type, 0, "enum"
HKR, Ndi\params\FrameBursting\enum, "0", 0, "Disabled"
HKR, Ndi\params\FrameBursting\enum, "1", 0, "Enabled"
HKR, Ndi\params\FrameBursting,default,,"0"
HKR, Ndi\params\BTCoexist, ParamDesc, 0, "Bluetooth Collaboration"
HKR, Ndi\params\BTCoexist, type, 0, "enum"
HKR, Ndi\params\BTCoexist\enum, "1", 0, "Enable"
HKR, Ndi\params\BTCoexist\enum, "0", 0, "Disable"
HKR, Ndi\params\BTCoexist,default,,"1"
HKR, ,"WEP", 0, ""
HKR, ,"NetworkType", 0, "-1"
HKR, ,"SSID", 0, ""
HKR, ,"gpio0", 0, "-1"
HKR, ,"gpio1", 0, "-1"
HKR, ,"gpio2", 0, "-1"
HKR, ,"gpio3", 0, "-1"
HKR, ,"scan_channel_time", 0, "-1"
HKR, ,"scan_unassoc_time", 0, "-1"
HKR, ,"scan_home_time", 0, "-1"
HKR, ,"scan_passes", 0, "-1"
HKR, ,"BadFramePreempt", 0, "0"
HKR, ,"Interference_Mode", 0, "-1"
HKR, Ndi\params\antdiv, ParamDesc, 0, "Antenna Diversity"
HKR, Ndi\params\antdiv, type, 0, "enum"
HKR, Ndi\params\antdiv\enum, "-1", 0, "Auto"
HKR, Ndi\params\antdiv,default,,"-1"
[b.options.reg]
HKR, Ndi\params\Rate, ParamDesc, 0, "Rate"
HKR, Ndi\params\Rate, type, 0, "enum"
HKR, Ndi\params\Rate\enum, "0", 0, "Use best rate"
HKR, Ndi\params\Rate\enum, "2", 0, " 1"
HKR, Ndi\params\Rate\enum, "4", 0, " 2"
HKR, Ndi\params\Rate\enum, "11", 0, " 5.5"
HKR, Ndi\params\Rate\enum, "22", 0, "11"
HKR, Ndi\params\Rate,default,,"0"
HKR, Ndi\params\Locale, ParamDesc, 0, "Locale"
HKR, Ndi\params\Locale, type, 0, "enum"
HKR, Ndi\params\Locale\enum, "0", 0, "Worldwide"
HKR, Ndi\params\Locale\enum, "5", 0, "Japan"
HKR, Ndi\params\Locale,default,,"15"
[g.options.reg]
HKR, Ndi\params\RoamTrigger, ParamDesc, 0, "Roaming Decision"
HKR, Ndi\params\RoamTrigger, type, 0, "enum"
HKR, Ndi\params\RoamTrigger\enum, "-60", 0, "Optimize Bandwidth"
HKR, Ndi\params\RoamTrigger\enum, "-70", 0, "Default"
HKR, Ndi\params\RoamTrigger\enum, "-80", 0, "Optimize Distance"
HKR, Ndi\params\RoamTrigger,default,,"-70"
HKR, Ndi\params\IBSSGMode, ParamDesc, 0, "IBSS 54g(tm) Mode"
HKR, Ndi\params\IBSSGMode, type, 0, "enum"
HKR, Ndi\params\IBSSGMode\enum, "0", 0, "802.11b Only"
HKR, Ndi\params\IBSSGMode\enum, "1", 0, "54g LRS"
HKR, Ndi\params\IBSSGMode\enum, "2", 0, "54g Auto"
HKR, Ndi\params\IBSSGMode\enum, "4", 0, "54g Only"
HKR, Ndi\params\IBSSGMode,default,,"2"
HKR, Ndi\params\Locale, ParamDesc, 0, "Locale"
HKR, Ndi\params\Locale, type, 0, "enum"
HKR, Ndi\params\Locale\enum, "0", 0, "Worldwide"
HKR, Ndi\params\Locale\enum, "5", 0, "Japan"
HKR, Ndi\params\Locale\enum, "6", 0, "USA"
HKR, Ndi\params\Locale,default,,"15"
HKR, Ndi\params\Rate, ParamDesc, 0, "Rate"
HKR, Ndi\params\Rate, type, 0, "enum"
HKR, Ndi\params\Rate\enum, "0", 0, "Use best rate"
HKR, Ndi\params\Rate\enum, "2", 0, " 1"
HKR, Ndi\params\Rate\enum, "4", 0, " 2"
HKR, Ndi\params\Rate\enum, "11", 0, " 5.5"
HKR, Ndi\params\Rate\enum, "12", 0, " 6"
HKR, Ndi\params\Rate\enum, "18", 0, " 9"
HKR, Ndi\params\Rate\enum, "22", 0, "11"
HKR, Ndi\params\Rate\enum, "24", 0, "12"
HKR, Ndi\params\Rate\enum, "36", 0, "18"
HKR, Ndi\params\Rate\enum, "48", 0, "24"
HKR, Ndi\params\Rate\enum, "72", 0, "36"
HKR, Ndi\params\Rate\enum, "96", 0, "48"
HKR, Ndi\params\Rate\enum, "108",0, "54"
HKR, Ndi\params\Rate,default,,"0"
[bg.options.reg]
HKR, Ndi\params\Channel, ParamDesc, 0, "IBSS Channel Number"
HKR, Ndi\params\Channel, default, 0, "11"
HKR, Ndi\params\Channel, min, 0, "1"
HKR, Ndi\params\Channel, max, 0, "14"
HKR, Ndi\params\Channel, step, 0, "1"
HKR, Ndi\params\Channel, base, 0, "10"
HKR, Ndi\params\Channel, type, 0, "int"
[bag.options.reg]
HKR, Ndi\params\RoamTrigger, ParamDesc, 0, "Roaming Decision"
HKR, Ndi\params\RoamTrigger, type, 0, "enum"
HKR, Ndi\params\RoamTrigger\enum, "-60", 0, "Optimize Bandwidth"
HKR, Ndi\params\RoamTrigger\enum, "-70", 0, "Default"
HKR, Ndi\params\RoamTrigger\enum, "-80", 0, "Optimize Distance"
HKR, Ndi\params\RoamTrigger,default,,"-70"
HKR, Ndi\params\PLCPHeader, ParamDesc, 0, "BSS PLCP Header"
HKR, Ndi\params\PLCPHeader, type, 0, "enum"
HKR, Ndi\params\PLCPHeader\enum, "-1", 0, "Long"
HKR, Ndi\params\PLCPHeader\enum, "0", 0, "Auto (Short/Long)"
HKR, Ndi\params\PLCPHeader,default,,"0"
HKR, Ndi\params\band, ParamDesc, 0, "Disable Bands"
HKR, Ndi\params\band, type, 0, "enum"
HKR, Ndi\params\band\enum, "0", 0, "None"
HKR, Ndi\params\band\enum, "1", 0, "Disable 802.11g/b"
HKR, Ndi\params\band\enum, "2", 0, "Disable 802.11a"
HKR, Ndi\params\band,default,,"0"
HKR, Ndi\params\Locale, ParamDesc, 0, "Locale"
HKR, Ndi\params\Locale, type, 0, "enum"
HKR, Ndi\params\Locale\enum, "0", 0, "Worldwide"
HKR, Ndi\params\Locale\enum, "5", 0, "Japan"
HKR, Ndi\params\Locale\enum, "6", 0, "USA"
HKR, Ndi\params\Locale,default,,"15"
HKR, Ndi\params\AssocPref, ParamDesc, 0, "Association Preference"
HKR, Ndi\params\AssocPref, type, 0, "enum"
HKR, Ndi\params\AssocPref\enum, "0", 0, "None"
HKR, Ndi\params\AssocPref\enum, "1", 0, "Prefer 802.11a"
HKR, Ndi\params\AssocPref\enum, "2", 0, "Prefer 802.11g/b"
HKR, Ndi\params\AssocPref,default,,"0"
HKR, Ndi\params\RoamPref, ParamDesc, 0, "Roaming Preference"
HKR, Ndi\params\RoamPref, type, 0, "enum"
HKR, Ndi\params\RoamPref\enum, "0", 0, "None"
HKR, Ndi\params\RoamPref\enum, "1", 0, "Stay In Band"
HKR, Ndi\params\RoamPref,default,,"0"
HKR, Ndi\params\IBSSGMode, ParamDesc, 0, "IBSS 54g(tm) Mode"
HKR, Ndi\params\IBSSGMode, type, 0, "enum"
HKR, Ndi\params\IBSSGMode\enum, "0", 0, "802.11b Only"
HKR, Ndi\params\IBSSGMode\enum, "1", 0, "54g LRS"
HKR, Ndi\params\IBSSGMode\enum, "2", 0, "54g Auto"
HKR, Ndi\params\IBSSGMode\enum, "4", 0, "54g Only"
HKR, Ndi\params\IBSSGMode,default,,"0"
HKR, Ndi\params\IBSSGProtection, ParamDesc, 0, "IBSS 54g(tm) Protection Mode"
HKR, Ndi\params\IBSSGProtection, type, 0, "enum"
HKR, Ndi\params\IBSSGProtection\enum, "0", 0, "Disabled"
HKR, Ndi\params\IBSSGProtection\enum, "2", 0, "Auto"
HKR, Ndi\params\IBSSGProtection,default,,"2"
HKR, Ndi\params\Rate, ParamDesc, 0, "Rate"
HKR, Ndi\params\Rate, type, 0, "enum"
HKR, Ndi\params\Rate\enum, "0", 0, "Use best rate"
HKR, Ndi\params\Rate\enum, "2", 0, " 1"
HKR, Ndi\params\Rate\enum, "4", 0, " 2"
HKR, Ndi\params\Rate\enum, "11", 0, " 5.5"
HKR, Ndi\params\Rate\enum, "12", 0, " 6"
HKR, Ndi\params\Rate\enum, "18", 0, " 9"
HKR, Ndi\params\Rate\enum, "22", 0, "11"
HKR, Ndi\params\Rate\enum, "24", 0, "12"
HKR, Ndi\params\Rate\enum, "36", 0, "18"
HKR, Ndi\params\Rate\enum, "48", 0, "24"
HKR, Ndi\params\Rate\enum, "72", 0, "36"
HKR, Ndi\params\Rate\enum, "96", 0, "48"
HKR, Ndi\params\Rate\enum, "108",0, "54"
HKR, Ndi\params\Rate,default,,"0"
HKR, Ndi\params\Channel, ParamDesc, 0, "IBSS Channel Number"
HKR, Ndi\params\Channel, type, 0, "enum"
HKR, Ndi\params\Channel\enum, "1", 0, " 1"
HKR, Ndi\params\Channel\enum, "2", 0, " 2"
HKR, Ndi\params\Channel\enum, "3", 0, " 3"
HKR, Ndi\params\Channel\enum, "4", 0, " 4"
HKR, Ndi\params\Channel\enum, "5", 0, " 5"
HKR, Ndi\params\Channel\enum, "6", 0, " 6"
HKR, Ndi\params\Channel\enum, "7", 0, " 7"
HKR, Ndi\params\Channel\enum, "8", 0, " 8"
HKR, Ndi\params\Channel\enum, "9", 0, " 9"
HKR, Ndi\params\Channel\enum, "10", 0, " 10"
HKR, Ndi\params\Channel\enum, "11", 0, " 11"
HKR, Ndi\params\Channel\enum, "12", 0, " 12"
HKR, Ndi\params\Channel\enum, "13", 0, " 13"
HKR, Ndi\params\Channel\enum, "14", 0, " 14"
HKR, Ndi\params\Channel\enum, "36", 0, " 36"
HKR, Ndi\params\Channel\enum, "40", 0, " 40"
HKR, Ndi\params\Channel\enum, "44", 0, " 44"
HKR, Ndi\params\Channel\enum, "48", 0, " 48"
HKR, Ndi\params\Channel\enum, "52", 0, " 52"
HKR, Ndi\params\Channel\enum, "56", 0, " 56"
HKR, Ndi\params\Channel\enum, "60", 0, " 60"
HKR, Ndi\params\Channel\enum, "64", 0, " 64"
HKR, Ndi\params\Channel\enum, "100", 0, "100"
HKR, Ndi\params\Channel\enum, "104", 0, "104"
HKR, Ndi\params\Channel\enum, "108", 0, "108"
HKR, Ndi\params\Channel\enum, "112", 0, "112"
HKR, Ndi\params\Channel\enum, "116", 0, "116"
HKR, Ndi\params\Channel\enum, "120", 0, "120"
HKR, Ndi\params\Channel\enum, "124", 0, "124"
HKR, Ndi\params\Channel\enum, "128", 0, "128"
HKR, Ndi\params\Channel\enum, "132", 0, "132"
HKR, Ndi\params\Channel\enum, "136", 0, "136"
HKR, Ndi\params\Channel\enum, "140", 0, "140"
HKR, Ndi\params\Channel\enum, "184", 0, "184"
HKR, Ndi\params\Channel\enum, "188", 0, "188"
HKR, Ndi\params\Channel\enum, "192", 0, "192"
HKR, Ndi\params\Channel\enum, "196", 0, "196"
HKR, Ndi\params\Channel\enum, "200", 0, "200"
HKR, Ndi\params\Channel\enum, "204", 0, "204"
HKR, Ndi\params\Channel\enum, "208", 0, "208"
HKR, Ndi\params\Channel\enum, "212", 0, "212"
HKR, Ndi\params\Channel\enum, "216", 0, "216"
HKR, Ndi\params\Channel, default, 0, "11"
[DestinationDirs]
DefaultDestDir=11
MS68XX.sys.files=11
MS68XX.files.NT=12
[SourceDisksNames]
[SourceDisksFiles]
ms68bm.SYS=1
[strings]
V_MSI="Minitar"
MS68XX.CARDBUS="IEEE802.11b Wireless Cardbus Adapter"
MS68XX.miniPCI="IEEE802.11b Wireless miniPCI Adapter"
MS68XX.PCI="IEEE802.11b Wireless PCI Adapter"
MS68XG.CARDBUS="IEEE802.11g Wireless Cardbus Adapter"
MS68XG.miniPCI="IEEE802.11g Wireless miniPCI Adapter"
MS68XG.PCI="IEEE802.11g Wireless PCI Adapter"
MS68XM.CARDBUS="IEEE802.11 Multiband Wireless Cardbus Adapter"
MS68XX_HELP="802.11bg Wireless network adapter."
DEFAULT_WIN9X_SYS="ms68bm.SYS"
MS68XX.Service.DispName="802.11bg Wireless Network Adapter"
MS68XX.DiskName="802.11bg Wireless LAN Network Adapter Install Disk"

