
[Version]
Signature="$Chicago$"
Compatible=1
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%Realtek%
CatalogFile.NT=netrtuw.cat ;; for WHQL certified
DriverVer=06/13/2008,5.1313.0613.2008
[Manufacturer]
%Realtek%=Realtek,NTx86
[ControlFlags]
ExcludeFromSelect=USB\VID_0BDA&PID_8187&REV_0100
ExcludeFromSelect=USB\VID_0769&PID_11F2&REV_0100
[Realtek.NTx86]
%RTL8187.DeviceDesc%=RTL8187.ndi,USB\VID_0BDA&PID_8187&REV_0100
%RTL8187.DeviceDesc%=RTL8187.ndi,USB\VID_13D1&PID_ABE6&REV_0100 ;
%RTL8187.DeviceDesc%=RTL8187.ndi,USB\VID_1371&PID_9401&REV_0100 ;
%RTL8187.DeviceDesc%=RTL8187.ndi,USB\VID_114B&PID_0150&REV_0100 ;
%RTL8187.DeviceDesc%=RTL8187.ndi,USB\VID_18E8&PID_6232&REV_0100 ;
%RTL8187.DeviceDesc%=RTL8187.ndi,USB\VID_0789&PID_010C&REV_0100 ;
%RTL8187.DeviceDesc.Surecom%=RTL8187.ndi,USB\VID_0769&PID_11F2&REV_0100 ;
%RTL8187.DeviceDesc.Sitecom%=RTL8187.ndi,USB\VID_0DF6&PID_000D&REV_0100 ;
[Realtek]
%RTL8187.DeviceDesc%=RTL8187.ndi,USB\VID_0BDA&PID_8187&REV_0100
%RTL8187.DeviceDesc%=RTL8187.ndi,USB\VID_13D1&PID_ABE6&REV_0100 ;
%RTL8187.DeviceDesc%=RTL8187.ndi,USB\VID_1371&PID_9401&REV_0100 ;
%RTL8187.DeviceDesc%=RTL8187.ndi,USB\VID_114B&PID_0150&REV_0100 ;
%RTL8187.DeviceDesc%=RTL8187.ndi,USB\VID_18E8&PID_6232&REV_0100 ;
%RTL8187.DeviceDesc%=RTL8187.ndi,USB\VID_0789&PID_010C&REV_0100 ;
%RTL8187.DeviceDesc.Surecom%=RTL8187.ndi,USB\VID_0769&PID_11F2&REV_0100 ;
%RTL8187.DeviceDesc.Sitecom%=RTL8187.ndi,USB\VID_0DF6&PID_000D&REV_0100 ;
[RTL8187.ndi]
DriverVer=06/13/2008,1313
AddReg=RTL8187.Reg, RTL8187.common.reg
;CpyFiles=RTL8187.CopyFiles98
[RTL8187.ndi.NT]
AddReg=RTL8187.NT.Reg, RTL8187.common.reg
Characteristics=0x84
BusType=15
;CpyFiles=RTL8187.CopyFiles
[RTL8187.ndi.NT.Services]
AddService=RTLWUSB, 2, rtsnt.Service, RTL8187.EventLog
[RTL8187.Reg]
HKR, Ndi, DeviceID, 0, USB\VID_0BDA&PID_8187&REV_0100
HKR,Ndi,CardType,,"PNP"
HKR, , DriverDesc, 0, "Realtek RTL8187 Wireless USB 2.0 Adapter"
HKR, , DevLoader,,*ndis,*ntkern,*ndis
HKR, , DeviceVxDs,,RTL8187.sys
HKR, , EnumPropPages, 0, netdi.dll, EnumPropPages
HKR,NDIS,MajorNdisVersion,1,03
HKR,NDIS,MinorNdisVersion,1,0a
HKR,NDIS,LogDriverName,,RTLWUSB
HKR,Ndi\Interfaces,DefLower,,"ethernet"
HKR,Ndi\Interfaces,LowerRange,,"ethernet"
HKR,Ndi\Interfaces,DefUpper,,"ndis3"
HKR,Ndi\Interfaces,UpperRange,,"ndis3"
[RTL8187.common.reg]
HKR,Ndi\params\SSID, ParamDesc, 0, %SSID_STR%
HKR,Ndi\params\SSID, type, 0, "edit"
HKR,Ndi\params\SSID, default, 0, "ANY"
HKR,Ndi\params\SSID, LimitText, 0, "32"
HKR,defaults,SSID,0,"ANY"
HKR,,SSID,0,"ANY"
HKR,Ndi\params\Channel, ParamDesc, 0, %CHANNEL_STR%
HKR,Ndi\params\Channel, type, 0, "int"
HKR,Ndi\params\Channel, default, 0, "1"
HKR,Ndi\params\Channel, Min, 0, "1"
HKR,Ndi\params\Channel, Max, 0, "14"
HKR,Ndi\params\Channel, Step, 0, "1"
HKR,Ndi\params\Channel, Base, 0, "10"
HKR,defaults,Channel,0,"1"
HKR,,Channel,0,"1"
HKR,Ndi\params\NetworkType, ParamDesc, 0, %NETWORK_TYPE_STR%
HKR,Ndi\params\NetworkType, type, 0, "enum"
HKR,Ndi\params\NetworkType, default, 0, "1"
HKR,Ndi\params\NetworkType\enum, "0", 0, "Ad Hoc"
HKR,Ndi\params\NetworkType\enum, "1", 0, "Infrastructure"
HKR,Ndi\params\NetworkType\enum, "2", 0, "Auto select"
HKR,defaults,NetworkType,0,"1"
HKR,,NetworkType,0,"1"
HKR,Ndi\params\LedCtrl, ParamDesc, 0, %LED_CONTROL_STR%
HKR,Ndi\params\LedCtrl, type, 0, "enum"
HKR,Ndi\params\LedCtrl, default, 0, "1"
HKR,Ndi\params\LedCtrl\enum, "0", 0, "Disable"
HKR,Ndi\params\LedCtrl\enum, "1", 0, "Enable"
HKR,defaults,LedCtrl,0,"1"
HKR,,LedCtrl,0,"1"
HKR,NDI\params\PowerSaveMode, ParamDesc, 0, %POWER_SAVE_STR%
HKR,NDI\params\PowerSaveMode, type, 0, "enum"
HKR,Ndi\params\PowerSaveMode, default, 0, "0"
HKR,NDI\params\PowerSaveMode\enum, "0", 0, "CAM"
HKR,NDI\params\PowerSaveMode\enum, "1", 0, "MAX_PSP"
HKR,NDI\params\PowerSaveMode\enum, "2", 0, "Fast_PSP"
HKR,defaults,PowerSaveMode,0,"0"
HKR,,PowerSaveMode,0,"0"
HKR,Ndi\params\WiFi11bIbss, ParamDesc, 0, %WIFI_IBSS_STR%
HKR,Ndi\params\WiFi11bIbss, type, 0, "enum"
HKR,Ndi\params\WiFi11bIbss, default, 0, "0"
HKR,Ndi\params\WiFi11bIbss\enum, "0", 0, "Disable"
HKR,Ndi\params\WiFi11bIbss\enum, "1", 0, "Enable"
HKR,defaults,WiFi11bIbss,0,"0"
HKR,,WiFi11bIbss,0,"0"
HKR,Ndi\params\bRateAdaptive, ParamDesc, 0, %RATE_ADAPTIVE_STR%
HKR,Ndi\params\bRateAdaptive, type, 0, "enum"
HKR,Ndi\params\bRateAdaptive, default, 0, "1"
HKR,Ndi\params\bRateAdaptive\enum, "0", 0, "Disable"
HKR,Ndi\params\bRateAdaptive\enum, "1", 0, "Enable"
HKR,defaults,bRateAdaptive,0,"1"
HKR,,bRateAdaptive,0,"1"
HKR,Ndi\params\MaxPktSize, ParamDesc, 0, %MAX_PKTSIZE_STR%
HKR,Ndi\params\MaxPktSize, type, 0, "int"
HKR,Ndi\params\MaxPktSize, default, 0, "1514"
HKR,Ndi\params\MaxPktSize, min, 0, "256"
HKR,Ndi\params\MaxPktSize, max, 0, "2304"
HKR,Ndi\params\MaxPktSize, step, 0, "1"
HKR,defaults,MaxPktSize, 0, "1514"
HKR,,MaxPktSize, 0, "1514"
HKR,Ndi\params\ChannelPlan, ParamDesc, 0, %CHANNEL_PLAN_STR%
HKR,Ndi\params\ChannelPlan, type, 0, "enum"
HKR,Ndi\params\ChannelPlan, default, 0, "15"
HKR,Ndi\params\ChannelPlan\enum, "0", 0, "FCC"
HKR,Ndi\params\ChannelPlan\enum, "1", 0, "IC"
HKR,Ndi\params\ChannelPlan\enum, "2", 0, "ETSI"
HKR,Ndi\params\ChannelPlan\enum, "3", 0, "Spain"
HKR,Ndi\params\ChannelPlan\enum, "4", 0, "France"
HKR,Ndi\params\ChannelPlan\enum, "5", 0, "MKK"
HKR,Ndi\params\ChannelPlan\enum, "6", 0, "MKK1"
HKR,Ndi\params\ChannelPlan\enum, "7", 0, "Israel"
HKR,Ndi\params\ChannelPlan\enum, "8", 0, "TELEC"
HKR,Ndi\params\ChannelPlan\enum, "15", 0, "DOMAIN_FROM_EEPROM"
HKR,defaults,ChannelPlan, 0, "15"
HKR,,ChannelPlan, 0, "15"
HKR,Ndi\params\ShortRetryLimit, ParamDesc, 0, %SHORT_RETRY_LIMIT%
HKR,Ndi\params\ShortRetryLimit, default, 0, "7"
HKR,Ndi\params\ShortRetryLimit, type, 0, "int"
HKR,Ndi\params\ShortRetryLimit, min, 0, "0"
HKR,Ndi\params\ShortRetryLimit, max, 0, "255"
HKR,Ndi\params\ShortRetryLimit, step, 0, "1"
HKR,defaults,ShortRetryLimit, 0, "7"
HKR,,ShortRetryLimit, 0, "7"
HKR,Ndi\params\LongRetryLimit, ParamDesc, 0, %LONG_RETRY_LIMIT%
HKR,Ndi\params\LongRetryLimit, default, 0, "7"
HKR,Ndi\params\LongRetryLimit, type, 0, "int"
HKR,Ndi\params\LongRetryLimit, min, 0, "0"
HKR,Ndi\params\LongRetryLimit, max, 0, "255"
HKR,Ndi\params\LongRetryLimit, step, 0, "1"
HKR,defaults,LongRetryLimit, 0, "7"
HKR,,LongRetryLimit, 0, "7"
HKR,Ndi\params\FragThresh, ParamDesc, 0, %FRAGTHRESH_STR%
HKR,Ndi\params\FragThresh, default, 0, "2346"
HKR,Ndi\params\FragThresh, type, 0, "int"
HKR,Ndi\params\FragThresh, min, 0, "256"
HKR,Ndi\params\FragThresh, max, 0, "2346"
HKR,Ndi\params\FragThresh, step, 0, "1"
HKR,defaults,FragThresh, 0, "2346"
HKR,,FragThresh, 0, "2346"
HKR,Ndi\params\RTSThresh, ParamDesc, 0, %RTSTHRESH_STR%
HKR,Ndi\params\RTSThresh, default, 0, "2347"
HKR,Ndi\params\RTSThresh, type, 0, "int"
HKR,Ndi\params\RTSThresh, min, 0, "0"
HKR,Ndi\params\RTSThresh, max, 0, "2347"
HKR,Ndi\params\RTSThresh, step, 0, "1"
HKR,defaults,RTSThresh, 0, "2347"
HKR,,RTSThresh, 0, "2347"
HKR,Ndi\params\PSPXlinkMode, ParamDesc, 0, %PSP_XLINK_STR%
HKR,Ndi\params\PSPXlinkMode, type, 0, "enum"
HKR,Ndi\params\PSPXlinkMode, default, 0, "0"
HKR,Ndi\params\PSPXlinkMode\enum, "0", 0, "Disable"
HKR,Ndi\params\PSPXlinkMode\enum, "1", 0, "Enable"
HKR,defaults,PSPXlinkMode,0,"0"
HKR,,PSPXlinkMode,0,"0"
HKR,,DefaultKeyID,,"0"
HKR,,DefaultKey0,,""
HKR,,DefaultKey1,,""
HKR,,DefaultKey2,,""
HKR,,DefaultKey3,,""
[RTL8187.CopyFiles98]
RTL8187.sys,,,2
[RTL8187.NT.Reg]
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5,mdcwifi,wifipro"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi, Service, 0, "RTLWUSB"
[rtsnt.Service]
DisplayName=%RTL8187.DeviceDesc.DispName%
ServiceType=1 ; %SERVICE_KERNEL_DRIVER%
StartType=3 ; %SERRVICE_DEMAND_START%
ErrorControl=1 ; %SERRVICE_ERROR_NORMAL%
ServiceBinary=%12%\RTL8187.sys
LoadOrderGroup=NDIS
[RTL8187.EventLog]
AddReg=RTL8187.AddEventLog.reg
[RTL8187.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported , 0x00010001, 7
[RTL8187.CopyFiles]
RTL8187.sys,,,2
[DestinationDirs]
RTL8187.CopyFiles98=11
RTL8187.CopyFiles=12
[SourceDisksNames]
1=%DISKNAME%,,,
[SourceDisksFiles]
RTL8187.sys=1
[Strings]
Realtek="Realtek Semiconductor Corp."
SSID_STR="SSID"
CHANNEL_STR="Channel"
NETWORK_TYPE_STR="Network Type"
LED_CONTROL_STR="LED Control"
POWER_SAVE_STR="Power Save Mode"
WIFI_IBSS_STR="IBSS Default 11b Mode"
RATE_ADAPTIVE_STR="Rate Adaptive"
MAX_PKTSIZE_STR="Maximum Packet Size"
CHANNEL_PLAN_STR="Channel Plan"
SHORT_RETRY_LIMIT="Short Retry Limit"
LONG_RETRY_LIMIT="Long Retry Limit"
FRAGTHRESH_STR="Fragmentation Threshold"
RTSTHRESH_STR="RTS Threshold"
PSP_XLINK_STR="PSP XLink Mode"
DISKNAME="Realtek RTL8187 Wireless 802.11b/g 54Mbps USB 2.0 Network Adapter Driver Disk"
RTL8187.DeviceDesc="Realtek RTL8187 Wireless 802.11b/g 54Mbps USB 2.0 Network Adapter"
RTL8187.DeviceDesc.DispName="Realtek RTL8187 Wireless 802.11b/g 54Mbps USB 2.0 Network Adapter"
RTL8187.DeviceDesc.Surecom="SURECOM EP-9001-g 802.11g 54M WLAN USB Adapter"
RTL8187.DeviceDesc.Sitecom="SITECOM WL-168 Wireless Network USB Adapter 54g"
