
[version]
Signature="$Chicago$"
Compatible=1
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%Realtek% ;;
CatalogFile.NT=net819xp.cat ;; for WHQL certified
DriverVer=12/22/2010,1682.0.1222.2010
[Manufacturer]
%Realtek%=Realtek,NTx86
%DLink%=DLink,NTx86
%Corega%=Corega,NTx86
[ControlFlags]
ExcludeFromSelect=*
[Realtek.NTx86]
%RTL8190p.DeviceDesc%=RTL8190p.ndi, PCI\VEN_10EC&DEV_8190&SUBSYS_819010EC
%RTL8192e.DeviceDesc.RTK%=RTL8192e.ndi, PCI\VEN_10EC&DEV_8192&SUBSYS_819210EC
%RTL8192e.DeviceDesc.TOSHIBA_LITEON_H%=RTL8192e.ndi, PCI\VEN_10EC&DEV_8192&SUBSYS_818110EC
%RTL8192e.DeviceDesc.TOSHIBA_LITEON_F%=RTL8192e.ndi, PCI\VEN_10EC&DEV_8192&SUBSYS_815110EC
%RTL8192e.DeviceDesc.TOSHIBA_ASKEY_H%=RTL8192e.ndi, PCI\VEN_10EC&DEV_8192&SUBSYS_818210EC
%RTL8192e.DeviceDesc.TOSHIBA_ASKEY_F%=RTL8192e.ndi, PCI\VEN_10EC&DEV_8192&SUBSYS_815210EC
%RTL8192e.DeviceDesc.TOSHIBA_FOXCONN_H%=RTL8192e.ndi, PCI\VEN_10EC&DEV_8192&SUBSYS_818310EC
%RTL8192e.DeviceDesc.TOSHIBA_FOXCONN_F%=RTL8192e.ndi, PCI\VEN_10EC&DEV_8192&SUBSYS_815310EC
%RTL8192e.DeviceDesc.TOSHIBA_ARCADYAN_H%=RTL8192e.ndi, PCI\VEN_10EC&DEV_8192&SUBSYS_818410EC
%RTL8192e.DeviceDesc.TOSHIBA_ARCADYAN_F%=RTL8192e.ndi, PCI\VEN_10EC&DEV_8192&SUBSYS_815410EC
%RTL8192e.DeviceDesc.AZUREWAVE%=RTL8192e.ndi, PCI\VEN_10EC&DEV_8192&SUBSYS_818610EC
%RTL8192e.DeviceDesc.MSI%=RTL8192e.ndi, PCI\VEN_10EC&DEV_8192&SUBSYS_68961462
%RTL8192e.DeviceDesc.PEGATRON%=RTL8192e.ndi, PCI\VEN_10EC&DEV_8192&SUBSYS_005e1b0a
%RTL8192e.DeviceDesc.SAMSUNG_FOXCONN_H%=RTL8192e.ndi, PCI\VEN_10EC&DEV_8192&SUBSYS_E01C105B
%RTL8192e.DeviceDesc.SAMSUNG_FOXCONN_F%=RTL8192e.ndi, PCI\VEN_10EC&DEV_8192&SUBSYS_E01D105B
%RTL8192e.DeviceDesc.SAMSUNG_ASKEY_H%=RTL8192e.ndi, PCI\VEN_10EC&DEV_8192&SUBSYS_7160144F
%RTL8192e.DeviceDesc%=RTL8192e.ndi, PCI\VEN_10EC&DEV_8192
[DLink.NTx86]
%DLink.DeviceDesc%=RTL8190p.ndi, PCI\VEN_10EC&DEV_8190&SUBSYS_33041186
[Corega.NTx86]
%CG-WLPCI300N.DeviceDesc%=RTL8190p.ndi, PCI\VEN_10EC&DEV_8190&SUBSYS_C12D1259
%CG-WLCB300N.DeviceDesc%=RTL8190p.ndi, PCI\VEN_07AA&DEV_0046
%CG-WLPCIE300N.DeviceDesc%=RTL8192e.ndi, PCI\VEN_07AA&DEV_0044
%CG-WLEC300N.DeviceDesc%=RTL8192e.ndi, PCI\VEN_07AA&DEV_0047
[Realtek.NTamd64]
%RTL8190p.DeviceDesc%=RTL8190p.ndi, PCI\VEN_10EC&DEV_8190&SUBSYS_819010EC
%RTL8192e.DeviceDesc.RTK%=RTL8192e.ndi, PCI\VEN_10EC&DEV_8192&SUBSYS_819210EC
%RTL8192e.DeviceDesc.TOSHIBA_LITEON_H%=RTL8192e.ndi, PCI\VEN_10EC&DEV_8192&SUBSYS_818110EC
%RTL8192e.DeviceDesc.TOSHIBA_LITEON_F%=RTL8192e.ndi, PCI\VEN_10EC&DEV_8192&SUBSYS_815110EC
%RTL8192e.DeviceDesc.TOSHIBA_ASKEY_H%=RTL8192e.ndi, PCI\VEN_10EC&DEV_8192&SUBSYS_818210EC
%RTL8192e.DeviceDesc.TOSHIBA_ASKEY_F%=RTL8192e.ndi, PCI\VEN_10EC&DEV_8192&SUBSYS_815210EC
%RTL8192e.DeviceDesc.TOSHIBA_FOXCONN_H%=RTL8192e.ndi, PCI\VEN_10EC&DEV_8192&SUBSYS_818310EC
%RTL8192e.DeviceDesc.TOSHIBA_FOXCONN_F%=RTL8192e.ndi, PCI\VEN_10EC&DEV_8192&SUBSYS_815310EC
%RTL8192e.DeviceDesc.TOSHIBA_ARCADYAN_H%=RTL8192e.ndi, PCI\VEN_10EC&DEV_8192&SUBSYS_818410EC
%RTL8192e.DeviceDesc.TOSHIBA_ARCADYAN_F%=RTL8192e.ndi, PCI\VEN_10EC&DEV_8192&SUBSYS_815410EC
%RTL8192e.DeviceDesc.AZUREWAVE%=RTL8192e.ndi, PCI\VEN_10EC&DEV_8192&SUBSYS_818610EC
%RTL8192e.DeviceDesc.MSI%=RTL8192e.ndi, PCI\VEN_10EC&DEV_8192&SUBSYS_68961462
%RTL8192e.DeviceDesc.PEGATRON%=RTL8192e.ndi, PCI\VEN_10EC&DEV_8192&SUBSYS_005e1b0a
%RTL8192e.DeviceDesc.SAMSUNG_FOXCONN_H%=RTL8192e.ndi, PCI\VEN_10EC&DEV_8192&SUBSYS_E01C105B
%RTL8192e.DeviceDesc.SAMSUNG_FOXCONN_F%=RTL8192e.ndi, PCI\VEN_10EC&DEV_8192&SUBSYS_E01D105B
%RTL8192e.DeviceDesc.SAMSUNG_ASKEY_H%=RTL8192e.ndi, PCI\VEN_10EC&DEV_8192&SUBSYS_7160144F
%RTL8192e.DeviceDesc%=RTL8192e.ndi, PCI\VEN_10EC&DEV_8192
[DLink.NTamd64]
%DLink.DeviceDesc%=RTL8190p.ndi, PCI\VEN_10EC&DEV_8190&SUBSYS_33041186
[Corega.NTamd64]
%CG-WLPCI300N.DeviceDesc%=RTL8190p.ndi, PCI\VEN_10EC&DEV_8190&SUBSYS_C12D1259
%CG-WLCB300N.DeviceDesc%=RTL8190p.ndi, PCI\VEN_07AA&DEV_0046
%CG-WLPCIE300N.DeviceDesc%=RTL8192e.ndi, PCI\VEN_07AA&DEV_0044
%CG-WLEC300N.DeviceDesc%=RTL8192e.ndi, PCI\VEN_07AA&DEV_0047
[RTL8190p.ndi.NT]
AddReg=RTL8190p.common.reg, RTL8190p.reg
Characteristics=0x84
BusType=5
;CpyFiles=RTL819xp.CopyFiles
[RTL8192e.ndi.NT]
AddReg=RTL8192e.common.reg, RTL8192e.reg
Characteristics=0x84
BusType=5
;CpyFiles=RTL819xp.CopyFiles
[RTL8190p.ndi.NT.Services]
AddService =RTL819xp, 2, RTL819xp.Service, RTL819xp.EventLog
[RTL8192e.ndi.NT.Services]
AddService=RTL819xp, 2, RTL819xp.Service, RTL819xp.EventLog
[RTL819xp.CopyFiles]
rtl819xp.sys,,,2
[RTL8190p.common.reg]
HKR,defaults, AH_BcnIntv, 0, "1000"
HKR,Ndi\params\AH_BcnIntv, default, 0, "100"
HKR,Ndi\params\AH_BcnIntv, ParamDesc, 0, %AH_BCNINTV_STR%
HKR,Ndi\params\AH_BcnIntv, type, 0, "int"
HKR,Ndi\params\AH_BcnIntv, min, 0, "20"
HKR,Ndi\params\AH_BcnIntv, max, 0, "1000"
HKR,Ndi\params\AH_BcnIntv, step, 0, "1"
HKR,Ndi\params\Dot11dEnable, ParamDesc, 0, %DOT11_ENABLE_STR%
HKR,Ndi\params\Dot11dEnable, type, 0, "enum"
HKR,Ndi\params\Dot11dEnable, default, 0, "0"
HKR,Ndi\params\Dot11dEnable\enum, "0", 0, %DISABLE_STR%
HKR,Ndi\params\Dot11dEnable\enum, "1", 0, %ENABLE_STR%
HKR,defaults,Dot11dEnable,0,"0"
HKR,,Dot11dEnable,0,"0"
HKR,Ndi\params\PSPXlinkMode, ParamDesc, 0, %PSP_XLINK_STR%
HKR,Ndi\params\PSPXlinkMode, type, 0, "enum"
HKR,Ndi\params\PSPXlinkMode, default, 0, "0"
HKR,Ndi\params\PSPXlinkMode\enum, "0", 0, %DISABLE_STR%
HKR,Ndi\params\PSPXlinkMode\enum, "1", 0, %ENABLE_STR%
HKR,defaults,PSPXlinkMode,0,"0"
HKR,,PSPXlinkMode,0,"0"
HKR,Ndi\params\WirelessMode, ParamDesc, 0, %WL_MODE_STR%
HKR,Ndi\params\WirelessMode, type, 0, "enum"
HKR,Ndi\params\WirelessMode, default, 0, "8"
HKR,Ndi\params\WirelessMode\enum, "2", 0, %IEEE_802_11B_STR%
HKR,Ndi\params\WirelessMode\enum, "4", 0, %IEEE_802_11BG_STR%
HKR,Ndi\params\WirelessMode\enum, "8", 0, %IEEE_802_11BGN_STR%
HKR,defaults,WirelessMode, 0, "8"
HKR,,WirelessMode, 0, "8"
HKR,,DefaultKeyID,,"0"
HKR,,DefaultKey0,,""
HKR,,DefaultKey1,,""
HKR,,DefaultKey2,,""
HKR,,DefaultKey3,,""
HKR,,WiFiConfg,,"0"
[RTL8192e.common.reg]
HKR,defaults,AH_BcnIntv, 0, "1000"
HKR,Ndi\params\AH_BcnIntv, default, 0, "100"
HKR,Ndi\params\AH_BcnIntv, ParamDesc, 0, %AH_BCNINTV_STR%
HKR,Ndi\params\AH_BcnIntv, type, 0, "int"
HKR,Ndi\params\AH_BcnIntv, min, 0, "20"
HKR,Ndi\params\AH_BcnIntv, max, 0, "1000"
HKR,Ndi\params\AH_BcnIntv, step, 0, "1"
HKR,Ndi\params\Dot11dEnable, ParamDesc, 0, %DOT11_ENABLE_STR%
HKR,Ndi\params\Dot11dEnable, type, 0, "enum"
HKR,Ndi\params\Dot11dEnable, default, 0, "0"
HKR,Ndi\params\Dot11dEnable\enum, "0", 0, %DISABLE_STR%
HKR,Ndi\params\Dot11dEnable\enum, "1", 0, %ENABLE_STR%
HKR,defaults,Dot11dEnable,0,"0"
HKR,,Dot11dEnable,0,"0"
HKR,Ndi\params\PSPXlinkMode, ParamDesc, 0, %PSP_XLINK_STR%
HKR,Ndi\params\PSPXlinkMode, type, 0, "enum"
HKR,Ndi\params\PSPXlinkMode, default, 0, "0"
HKR,Ndi\params\PSPXlinkMode\enum, "0", 0, %DISABLE_STR%
HKR,Ndi\params\PSPXlinkMode\enum, "1", 0, %ENABLE_STR%
HKR,defaults,PSPXlinkMode,0,"0"
HKR,,PSPXlinkMode,0,"0"
HKR,Ndi\params\WirelessMode, ParamDesc, 0, %WL_MODE_STR%
HKR,Ndi\params\WirelessMode, type, 0, "enum"
HKR,Ndi\params\WirelessMode, default, 0, "8"
HKR,Ndi\params\WirelessMode\enum, "2", 0, %IEEE_802_11B_STR%
HKR,Ndi\params\WirelessMode\enum, "4", 0, %IEEE_802_11BG_STR%
HKR,Ndi\params\WirelessMode\enum, "8", 0, %IEEE_802_11BGN_STR%
HKR,defaults,WirelessMode, 0, "8"
HKR,,WirelessMode, 0, "8"
HKR,defaults,LeisurePsMode,0,"2"
HKR,,LeisurePsMode,0,"2"
HKR,,InactivePs,0,"2"
HKR,,HwSwRfOffD3,0,"1"
HKR,,KeepAliveLevel,0,"2"
HKR,,DefaultKeyID,,"0"
HKR,,DefaultKey0,,""
HKR,,DefaultKey1,,""
HKR,,DefaultKey2,,""
HKR,,DefaultKey3,,""
HKR,,WiFiConfg,,"0"
HKR,,Channel,0,"10"
HKR,,PcieWork,0,"0"
HKR,,WepMode,0,"0"
[RTL8190p.reg]
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5,mdcwifi,wifipro"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi, Service, 0, "RTL8190p"
[RTL8192e.reg]
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5,mdcwifi,wifipro"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi, Service, 0, "RTL8192e"
[RTL819xp.Service]
DisplayName=%RTL819xp.Service.DispName%
ServiceType=1 ; %SERVICE_KERNEL_DRIVER%
StartType=3 ; %SERVICE_DEMAND_START%
ErrorControl=1 ; %SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\rtl819xp.sys
LoadOrderGroup=NDIS
[RTL819xp.EventLog]
Addreg=RTL819xp.AddEventLog.reg
[RTL819xp.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported, 0x00010001, 7
[DestinationDirs]
RTL819xp.CopyFiles=12
RTL819xp.CopyFiles98=11
DefaultDestDir=11 ; LDID_SYS
[SourceDisksNames]
1=%DISKNAME%,rtl819xp.sys,,
[SourceDisksFiles]
rtl819xp.sys=1,,
[Strings]
Realtek="Realtek Semiconductor Corp."
DLink="D-Link"
Corega="corega K.K."
SSID_STR="SSID"
CHANNEL_STR="Channel"
NETWORK_TYPE_STR="Network Type"
LED_CONTROL_STR="LED Control"
POWER_SAVE_STR="Power Save Mode"
WIFI_IBSS_STR="IBSS Default 11b Mode"
RATE_ADAPTIVE_STR="Rate Adaptive"
QOS_STR="QoS"
WMM_APSD="WMM APSD"
CCX_RM_STR="CCX Radio Measurement"
CCX_OFF_LINE_DUR_UP_LIMIT_STR="CCX Max Off-Line Measurement (0: unlimited)"
FORCE_PRIORITY_STR="Forced Priority"
HW_PARA_STR="Init from HwParaFile"
THREE_WIRE_MODE_STR="Three Wire Programming Mode"
BOARD_TYPE_STR="Board Type"
PROTECTION_MODE_STR="Protection Mode"
TPC_STR="Transmit Power Control"
TPC_POLARITY_STR="TPC Polarity Select"
HIGH_POWER_STR="High Power Mechanism"
INIT_GAIN_STR="Initial Gain State"
CW_MAX_MIN_STR="Contention Window"
PSP_XLINK_STR="PSP XLink Mode"
CHANNEL_PLAN_STR="Channel Plan"
WL_MODE_STR="Wireless Mode"
PREAMBLE_MODE_STR="Preamble Mode"
FRAGTHRESH_STR="Fragmentation Threshold"
RTSTHRESH_STR="RTS Threshold"
DOT11_ENABLE_STR="802.11d"
DISABLE_STR="Disable"
ENABLE_STR="Enable"
CAM_STR="CAM"
MAX_PSP_STR="MAX_PSP"
FAST_PSP_STR="Fast_PSP"
AD_HOC_STR="Ad Hoc"
INFRASTRUCTURE_STR="Infrastructure"
AUTO_SELECT_STR="Auto select"
DOMAIN_FROM_EEPROM_STR="DOMAIN_FROM_EEPROM"
AUTO_STR="Auto"
LONG_PREAMBLE_STR="Long Preamble"
SHORT_PREAMBLE_STR="Short Preamble"
FCC_STR="FCC"
IC_STR="IC"
ETSI_STR="ETSI"
SPAIN_STR="Spain"
FRANCE_STR="France"
MKK_STR="MKK"
MKK1_STR="MKK1"
ISRAEL_STR="Israel"
TELEC_STR="TELEC"
IEEE_802_11A_STR="IEEE 802.11a"
IEEE_802_11B_STR="IEEE 802.11b"
IEEE_802_11BG_STR="IEEE 802.11b/g"
IEEE_802_11BGN_STR="IEEE 802.11b/g/n"
Roam_Retry_Limit_STR="Roam Retry Limit(sec)"
LEISURE_POWER_SAVE_STR="Leisure Power Save"
AH_BCNINTV_STR="Beacon Interval"
DISKNAME="Realtek RTL819xP Wireless LAN (Mini-)PCI/PCI-E Driver Disk"
RTL8190p.DeviceDesc="Realtek RTL8190 802.11n Wireless LAN (Mini-)PCI NIC"
DLink.DeviceDesc="D-Link Wireless N DWA-532 Desktop Adapter"
RTL8192e.DeviceDesc.TOSHIBA_LITEON_H="Realtek RTL8192E Wireless LAN 802.11n PCI-E NIC"
RTL8192e.DeviceDesc.TOSHIBA_LITEON_F="Realtek RTL8192E Wireless LAN 802.11n PCI-E NIC"
RTL8192e.DeviceDesc.TOSHIBA_ASKEY_H="Realtek RTL8192E Wireless LAN 802.11n PCI-E NIC"
RTL8192e.DeviceDesc.TOSHIBA_ASKEY_F="Realtek RTL8192E Wireless LAN 802.11n PCI-E NIC"
RTL8192e.DeviceDesc.TOSHIBA_FOXCONN_H="Realtek RTL8192E Wireless LAN 802.11n PCI-E NIC"
RTL8192e.DeviceDesc.TOSHIBA_FOXCONN_F="Realtek RTL8192E Wireless LAN 802.11n PCI-E NIC"
RTL8192e.DeviceDesc.TOSHIBA_ARCADYAN_H="Realtek RTL8192E Wireless LAN 802.11n PCI-E NIC"
RTL8192e.DeviceDesc.TOSHIBA_ARCADYAN_F="Realtek RTL8192E Wireless LAN 802.11n PCI-E NIC"
RTL8192e.DeviceDesc.RTK="Realtek RTL8192E Wireless LAN 802.11n PCI-E NIC"
RTL8192e.DeviceDesc.AZUREWAVE="Realtek RTL8192E Wireless LAN 802.11n PCI-E NIC"
RTL8192e.DeviceDesc.MSI="802.11bgn 1T2R Mini Card Wireless Adapter"
RTL8192e.DeviceDesc.PEGATRON="Realtek RTL8192E/8256 802.11 b/g/n WLAN HMC Network"
RTL8192e.DeviceDesc.SAMSUNG_FOXCONN_H="Realtek RTL8192E Wireless LAN 802.11n PCI-E NIC"
RTL8192e.DeviceDesc.SAMSUNG_FOXCONN_F="Realtek RTL8192E Wireless LAN 802.11n PCI-E NIC"
RTL8192e.DeviceDesc.SAMSUNG_ASKEY_H="Realtek RTL8192E Wireless LAN 802.11n PCI-E NIC"
RTL8192e.DeviceDesc="Realtek RTL8192E Wireless LAN 802.11n PCI-E NIC"
CG-WLPCIE300N.DeviceDesc="CG-WLPCIE300N"
CG-WLEC300N.DeviceDesc="CG-WLEC300N"
CG-WLPCI300N.DeviceDesc="CG-WLPCI300N"
CG-WLCB300N.DeviceDesc="CG-WLCB300N"
RTL819xp.Service.DispName="Realtek RTL8190\RTL8192E 802.11n Wireless LAN (Mini-)PCI NIC NT Driver"

