
[Version]
DriverVer=04/29/2004, 3.0.11.1
Signature="$Chicago$"
Compatible=1
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%VER_VENDOR_STR%
CatalogFile=SMC2835W.cat
[ControlFlags]
ExcludeFromSelect=*
[Manufacturer]
%VER_VENDOR_NAME_STR%=DeviceList,NTx86.5.1
[DeviceList.NTx86.5.1]
%DCB1_DESC_STR%=NIC_DCB1_XP, PCI\VEN_1260&DEV_3890&SUBSYS_A83510B8
%DCB2_DESC_STR%=NIC_DCB2_XP, PCI\VEN_1260&DEV_3890&SUBSYS_EE081113
[DeviceList]
%DCB1_DESC_STR%=NIC_DCB1, PCI\VEN_1260&DEV_3890&SUBSYS_A83510B8
%DCB2_DESC_STR%=NIC_DCB2, PCI\VEN_1260&DEV_3890&SUBSYS_EE081113
[NIC_DCB1] ; Win9x
DelReg=COMMON_AMAC_DEL.reg
AddReg=NIC_DCB1.reg, NIC_DCB1.reg1, COMMON_ICB.reg, COMMON_NDIS.reg, COMMON.reg, COMMON_PSMODE.reg, COMMON_AMAC.reg
;CpyFiles=NIC_DRIVER.copy, NIC_CCU.copy
[NIC_DCB1.NT] ; Win2k
DelReg=COMMON_AMAC_DEL.reg
AddReg=NIC_DCB1.reg, COMMON_ICB.reg, COMMON_NDIS.reg.NT, COMMON.reg, COMMON_PS_MODE_XP.reg, COMMON_AMAC.reg
;CpyFiles=NIC_DRIVER.copy.NT, NIC_CCU.copy
BusType=5 ; PCI
Characteristics= 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[NIC_DCB1.NT.Services]
AddService="SMC2835W_PCI", 2, NIC_DRIVER_DCB.Service, NIC_DRIVER.EventLog
[NIC_DCB1.NT.CoInstallers]
;CpyFiles=NIC_COINSTALL.copy.NT
AddReg=NIC_COINSTALL.reg.NT
[NIC_DCB1_XP] ; Winxp
DelReg=COMMON_AMAC_DEL.reg
AddReg=NIC_DCB1.reg, COMMON_ICB.reg, COMMON_NDIS.reg.NT, COMMON.reg, COMMON_PS_MODE_XP.reg, COMMON_AMAC.reg
;CpyFiles=NIC_DRIVER.copy.XP, NIC_CCU.copy
BusType=5 ; PCI
Characteristics= 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[NIC_DCB1_XP.Services]
AddService="SMC2835W_PCI", 2, NIC_DRIVER_DCB.Service, NIC_DRIVER.EventLog
[NIC_DCB1_XP.CoInstallers]
;CpyFiles=NIC_COINSTALL.copy.NT
AddReg=NIC_COINSTALL.reg.NT
[NIC_DCB1.reg1]
[NIC_DCB1.reg]
HKR,Ndi,DeviceID,0,"PCI\VEN_1260&DEV_3890&SUBSYS_A83510B8"
HKR,,PlatformID,0,14480
HKR,,VendorDesc,0,%DCB1_DESC_STR%
HKR,,11dMode,0,0
HKR,,EnableRadio,0,1
HKR,,CountryName,0,"US "
[NIC_DCB2] ; Win9x
DelReg=COMMON_AMAC_DEL.reg
AddReg=NIC_DCB2.reg, NIC_DCB2.reg1, COMMON_ICB.reg, COMMON_NDIS.reg, COMMON.reg, COMMON_PSMODE.reg, COMMON_AMAC.reg
;CpyFiles=NIC_DRIVER.copy, NIC_CCU.copy
[NIC_DCB2.NT] ; Win2k
DelReg=COMMON_AMAC_DEL.reg
AddReg=NIC_DCB2.reg, COMMON_ICB.reg, COMMON_NDIS.reg.NT, COMMON.reg, COMMON_PS_MODE_XP.reg, COMMON_AMAC.reg
;CpyFiles=NIC_DRIVER.copy.NT, NIC_CCU.copy
BusType=5 ; PCI
Characteristics= 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[NIC_DCB2.NT.Services]
AddService="SMC2835W_PCI", 2, NIC_DRIVER_DCB.Service, NIC_DRIVER.EventLog
[NIC_DCB2.NT.CoInstallers]
;CpyFiles=NIC_COINSTALL.copy.NT
AddReg=NIC_COINSTALL.reg.NT
[NIC_DCB2_XP] ; Winxp
DelReg=COMMON_AMAC_DEL.reg
AddReg=NIC_DCB2.reg, COMMON_ICB.reg, COMMON_NDIS.reg.NT, COMMON.reg, COMMON_PS_MODE_XP.reg, COMMON_AMAC.reg
;CpyFiles=NIC_DRIVER.copy.XP, NIC_CCU.copy
BusType=5 ; PCI
Characteristics= 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[NIC_DCB2_XP.Services]
AddService="SMC2835W_PCI", 2, NIC_DRIVER_DCB.Service, NIC_DRIVER.EventLog
[NIC_DCB2_XP.CoInstallers]
;CpyFiles=NIC_COINSTALL.copy.NT
AddReg=NIC_COINSTALL.reg.NT
[NIC_DCB2.reg1]
[NIC_DCB2.reg]
HKR,Ndi,DeviceID,0,"PCI\VEN_1260&DEV_3890&SUBSYS_EE081113"
HKR,,PlatformID,0,14480
HKR,,VendorDesc,0,%DCB2_DESC_STR%
HKR,,11dMode,0,0
HKR,,EnableRadio,0,1
HKR,,CountryName,0,"US "
[NIC_COINSTALL.reg.NT]
[NIC_DRIVER_DCB.Service]
DisplayName=%NIC_SERVICE_DISPLAY_DCB%
ServiceType=1 ; SERVICE_KERNEL_DRIVER
StartType=3 ; SERVICE_DEMAND_START
ErrorControl=1 ; NORMAL
ServiceBinary=%12%\2835WICB.sys
LoadOrderGroup=NDIS
[NIC_DRIVER.EventLog]
AddReg=NIC_DRIVER.EventLog.reg
[NIC_DRIVER.EventLog.reg]
HKR, ,EventMessageFile ,0x00020000 ,"%%SystemRoot%%\System32\netevent.dll"
HKR, ,TypesSupported ,0x00010001 ,7
[COMMON_ICB.reg]
HKR,NDI ,Service ,0 ,"SMC2835W_PCI"
HKR, ,BusType ,0 ,"5"
HKR, ,DeviceVxDs ,0 ,"2835WICB.sys"
HKR, ,CardBusBridgeLatencyTimer ,0 ,"0"
HKR, ,CardBusBridgeCacheLineSize ,0 ,"0"
[COMMON_NDIS.reg]
HKR, ,RunningWin9X ,0 ,"1"
HKR, ,DevLoader ,0 ,"*ndis"
HKR, ,EnumPropPages ,0 ,"netdi.dll,EnumPropPages"
HKR,NDI\Interfaces ,UpperRange ,0 ,"ndis3"
HKR,NDI\Interfaces ,LowerRange ,0 ,"ethernet"
HKR,NDI\Interfaces ,DefUpper ,0 ,"ndis3"
HKR,NDI\Interfaces ,DefLower ,0 ,"ethernet"
HKR,NDIS ,LogDriverName ,0 ,"2835WICB"
HKR,NDIS ,MajorNdisVersion ,1 ,04
HKR,NDIS ,MinorNdisVersion ,1 ,00
[COMMON_NDIS.reg.NT]
HKR,NDI\Interfaces ,UpperRange ,0 ,"ndis5"
HKR,NDI\Interfaces ,LowerRange ,0 ,"ethernet"
[COMMON.reg]
HKR, ,SSID ,0 ,"ANY"
HKR, ,PpePdlpEnable ,0 ,"0"
HKR, ,PpeConcatEnable ,0 ,"0"
HKR, ,PpePdlpEnable ,0 ,"0"
HKR, ,PpePiggyBackEnable ,0 ,"0"
HKR, ,PRISMIOC ,0 ,"1"
HKR, ,SilentInstall ,0 ,"1"
HKR, ,NitroMode ,0 ,"0"
HKR, ,NitroTime ,0 ,"650"
HKR,Ndi\params\RTSThresh,default,0,2347
HKR,NDI\params\RTSThresh,ParamDesc,0,%RTSTHRESH_STR%
HKR,NDI\params\RTSThresh,type,0,int
HKR,NDI\params\RTSThresh,flag,1,20,00,00,00
HKR,NDI\params\RTSThresh,min,0,0
HKR,NDI\params\RTSThresh,max,0,2347
HKR,NDI\params\RTSThresh,step,0,1
HKR,Ndi\params\FragThresh,default,0,2346
HKR,NDI\params\FragThresh,ParamDesc,0,%FRAGTHRESH_STR%
HKR,NDI\params\FragThresh,type,0,int
HKR,NDI\params\FragThresh,flag,1,20,00,00,00
HKR,NDI\params\FragThresh,min,0,256
HKR,NDI\params\FragThresh,max,0,2346
HKR,NDI\params\FragThresh,step,0,2
[COMMON_AMAC_DEL.reg]
HKR,defaults,DataRates
HKR,NDI\params\DataRates
HKR,NDI\params\DataRate
HKR,DSChannel
HKR,defaults,DSChannel
HKR,NDI\params\DSChannel
[COMMON_AMAC.reg]
HKR,NDI\params\ShortRetryLimit,default,0,7
HKR,NDI\params\ShortRetryLimit,ParamDesc,,%SHORT_RETRY_STR%
HKR,NDI\params\ShortRetryLimit,type,,int
HKR,NDI\params\ShortRetryLimit,min,0,1
HKR,NDI\params\ShortRetryLimit,max,0,255
HKR,NDI\params\ShortRetryLimit,step,0,1
HKR,NDI\params\LongRetryLimit,default,0,4
HKR,NDI\params\LongRetryLimit,ParamDesc,,%LONG_RETRY_STR%
HKR,NDI\params\LongRetryLimit,type,0,int
HKR,NDI\params\LongRetryLimit,min,0,1
HKR,NDI\params\LongRetryLimit,max,0,255
HKR,NDI\params\LongRetryLimit,step,0,1
HKR,NDI\params\ConfigProfile,default,0,1
HKR,NDI\params\ConfigProfile,ParamDesc,,%CONFIG_PROFILE%
HKR,NDI\params\ConfigProfile,type,,enum
HKR,NDI\params\ConfigProfile,flag,1,30,00,00,00
HKR,NDI\params\ConfigProfile\enum,0,,%CONFIG_PROF_B_ONLY%
HKR,NDI\params\ConfigProfile\enum,1,,%CONFIG_PROF_MIXED%
HKR,NDI\params\ConfigProfile\enum,2,,%CONFIG_PROF_MIXED_LONG%
HKR,NDI\params\ConfigProfile\enum,3,,%CONFIG_PROF_G_ONLY%
HKR,NDI\params\ConfigProfile\enum,4,,%CONFIG_PROF_TEST%
HKR,NDI\params\ConfigProfile\enum,5,,%CONFIG_PROF_B_WIFI%
HKR,NDI\params\ConfigProfile\enum,6,,%CONFIG_PROF_MIXED_SHORT%
HKR,NDI\params\ConfigProfile\enum,256,,%CONFIG_PROF_WIFI_SPEC%
[COMMON_PSMODE.reg]
HKR,Ndi\params\PSMode,default,0,1
HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
HKR,NDI\params\PSMode,type,,enum
HKR,NDI\params\PSMode,flag,1,30,00,00,00
HKR,NDI\params\PSMode\enum,1,,%POWER_SAVE_OFF_STR%
HKR,NDI\params\PSMode\enum,2,,%POWER_SAVE_DYN_STR%
HKR,NDI\params\PSMode\enum,3,,%POWER_SAVE_MAX_STR%
[COMMON_PS_MODE_XP.reg]
HKR,Ndi\params\PSMode,default,0,1
HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
HKR,NDI\params\PSMode,type,,enum
HKR,NDI\params\PSMode,flag,1,30,00,00,00
HKR,NDI\params\PSMode\enum,1,,%POWER_SAVE_OFF_STR%
HKR,NDI\params\PSMode\enum,2,,%POWER_SAVE_DYN_STR%
HKR,NDI\params\PSMode\enum,3,,%POWER_SAVE_MAX_STR%
[DestinationDirs]
DefaultDestDir=11 ; Win9x=%windir%\system Win2k=%windir%\system32
NIC_DRIVER.copy=11 ; Win9x=%windir%\system
NIC_DRIVER.copy.NT=12 ; Win2k=%windir%\system32\drivers
NIC_DRIVER.copy.XP=12 ; Winxp=%windir%\system32\drivers
NIC_CCU.copy=11 ; Win9x=%windir%\system
[NIC_CCU.copy]
[NIC_DRIVER.copy]
2835WICB.sys
[NIC_DRIVER.copy.NT]
2835WICB.sys
[NIC_DRIVER.copy.XP]
2835WICB.sys,2835WC51.sys
[NIC_COINSTALL.copy.NT]
[SourceDisksNames]
1=%INSTALL_DISK_STR%,,,
[SourceDisksFiles] ; Win9x
2835WICB.sys=1
[SourceDisksFiles.X86] ; Win2k/Xp
2835WICB.sys=1
2835WC51.sys=1
[Strings]
VER_VENDOR_STR="SMC"
VER_VENDOR_NAME_STR="SMC Networks, Inc."
NIC_SERVICE_DISPLAY_DCB="SMC2835W 2.4GHz 54 Mbps Wireless Cardbus Driver"
INSTALL_DISK_STR="SMC2835W 2.4GHz 54 Mbps Wireless Cardbus adapter Install Disk"
ON_STR="On"
OFF_STR="Off"
RTSTHRESH_STR="RTS Threshold"
FRAGTHRESH_STR="Fragmentation Threshold"
AUTHENT_TYPE_STR="Authentication Algorithm"
POWER_SAVE_STR="Power Save Mode"
POWER_SAVE_OFF_STR="Disabled"
POWER_SAVE_DYN_STR="Dynamic"
POWER_SAVE_MAX_STR="Maximum"
LOAD_FIRMWARE_STR="Firmware Download"
SHORT_RETRY_STR="Short Retry Limit"
LONG_RETRY_STR="Long Retry Limit"
ANTENNA_TX_STR="Antenna Tx"
ANTENNA_RX_STR="Antenna Rx"
ANTENNA_DIVERSITY_STR="Antenna Diversity"
CHANNEL_STR="Channel"
DATARATES_STR="Data Rate"
DATARATES_AUTO="Fully Automatic"
ALSR_STR="Auto Long Slot Reassociation"
CONFIG_PROFILE="Configuration Profile"
CONFIG_PROF_B_ONLY="B only"
CONFIG_PROF_MIXED="Mixed"
CONFIG_PROF_MIXED_LONG="Mixed Long"
CONFIG_PROF_G_ONLY="G only"
CONFIG_PROF_TEST="Test"
CONFIG_PROF_B_WIFI="B WIFI"
CONFIG_PROF_MIXED_SHORT="Mixed Short"
CONFIG_PROF_WIFI_SPEC="WiFi Spec"
DCB1_DESC_STR="SMC2835W 2.4GHz 54 Mbps Wireless CardBus Adapter"
DCB2_DESC_STR="SMC2835W 2.4GHz 54 Mbps Wireless CardBus Adapter"

