
[Version]
DriverVer=05/29/2003, 1.0.17.65
Signature="$Chicago$"
Compatible=1
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%VER_VENDOR_STR%
MillenniumPreferred=.ME
[ControlFlags]
ExcludeFromSelect=*
[Manufacturer]
%VER_VENDOR_NAME_STR%=DeviceList
[DeviceList]
%DCB_DESC_STR%=PRISM_DCB1, PCI\VEN_1260&DEV_3890&SUBSYS_C1041259
%DCB_DESC_STR%=PRISM_DCB1, PCI\VEN_1260&DEV_3890&SUBSYS_00001260
%DCB_DESC_STR%=PRISM_DCB1, PCI\VEN_1260&DEV_3890
[PRISM_ICB1] ; Win9x
DelReg=COMMON_AMAC_DEL.reg
AddReg=PRISM_ICB1.reg, COMMON_ICB.reg, COMMON_NDIS.reg, COMMON.reg, COMMON_PSMODE.reg, COMMON_AMAC.reg, Run.reg
;CpyFiles=PRISM_DRIVER.copy, PRISM_FWICB.copy, PRISM_APPLET.copy, PRISM_NDI.copy, PRISM_DOM.copy, CK_DLL.copy
[PRISM_ICB1.ME] ; WinMe
DelReg=COMMON_AMAC_DEL.reg
AddReg=PRISM_ICB1.reg, COMMON_ICB.reg, COMMON_NDIS.reg.ME, COMMON.reg, COMMON_PSMODE.reg, COMMON_AMAC.reg, Run.reg
;CpyFiles=PRISM_DRIVER.copy.ME, PRISM_FWICB.copy.ME, PRISM_APPLET.copy.ME, PRISM_NDI.copy.ME, PRISM_DOM.copy, CK_DLL.copy
[PRISM_ICB1.ME.ME] ; WinMe - Same as .ME (Needed for Update Driver)
DelReg=COMMON_AMAC_DEL.reg
AddReg=PRISM_ICB1.reg, COMMON_ICB.reg, COMMON_NDIS.reg.ME, COMMON.reg, COMMON_PS_MODE.reg, COMMON_AMAC.reg, Run.reg
;CpyFiles=PRISM_DRIVER.copy.ME, PRISM_FWICB.copy.ME, PRISM_APPLET.copy.ME, PRISM_NDI.copy.ME, PRISM_DOM.copy, CK_DLL.copy
[PRISM_ICB1.NT] ; Win2k
DelReg=COMMON_AMAC_DEL.reg
AddReg=PRISM_ICB1.reg, COMMON_ICB.reg, COMMON_NDIS.reg.NT, COMMON.reg, COMMON_PS_MODE_XP.reg, COMMON_AMAC.reg, RunOnce.reg
;CpyFiles=PRISM_DRIVER.copy.NT, PRISM_FWICB.copy.NT, PRISM_APPLET.copy.NT, PRISM_DOM.copy, CK_DLL.copy
BusType=5 ; PCI
Characteristics= 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[PRISM_ICB1.NT.Services]
AddService="WLCB54GT", 2, PRISM_DRIVER_ICB.Service, PRISM_DRIVER.EventLog
[PRISM_ICB1.NT.CoInstallers]
;CpyFiles=PRISM_COINSTALL.copy.NT
AddReg=PRISM_COINSTALL.reg.NT
[PRISM_ICB1.reg]
[PRISM_DCB1] ; Win9x
DelReg=COMMON_AMAC_DEL.reg
AddReg=PRISM_DCB1.reg, COMMON_ICB.reg, COMMON_NDIS.reg, COMMON.reg, COMMON_PSMODE.reg, COMMON_AMAC.reg, Run.reg
;CpyFiles=PRISM_DRIVER.copy, PRISM_FWDCB.copy, PRISM_APPLET.copy, PRISM_NDI.copy, PRISM_DOM.copy, CK_DLL.copy
[PRISM_DCB1.ME] ; WinMe
DelReg=COMMON_AMAC_DEL.reg
AddReg=PRISM_DCB1.reg, COMMON_ICB.reg, COMMON_NDIS.reg.ME, COMMON.reg, COMMON_PSMODE.reg, COMMON_AMAC.reg, Run.reg
;CpyFiles=PRISM_DRIVER.copy.ME, PRISM_FWDCB.copy.ME, PRISM_APPLET.copy.ME, PRISM_NDI.copy.ME, PRISM_DOM.copy, CK_DLL.copy
[PRISM_DCB1.ME.ME] ; WinMe - Same as .ME (Needed for Update Driver)
DelReg=COMMON_AMAC_DEL.reg
AddReg=PRISM_DCB1.reg, COMMON_ICB.reg, COMMON_NDIS.reg.ME, COMMON.reg, COMMON_PS_MODE.reg, COMMON_AMAC.reg, Run.reg
;CpyFiles=PRISM_DRIVER.copy.ME, PRISM_FWDCB.copy.ME, PRISM_APPLET.copy.ME, PRISM_NDI.copy.ME, PRISM_DOM.copy, CK_DLL.copy
[PRISM_DCB1.NT] ; Win2k
DelReg=COMMON_AMAC_DEL.reg
AddReg=PRISM_DCB1.reg, COMMON_ICB.reg, COMMON_NDIS.reg.NT, COMMON.reg, COMMON_PS_MODE_XP.reg, COMMON_AMAC.reg, RunOnce.reg
;CpyFiles=PRISM_DRIVER.copy.NT, PRISM_FWDCB.copy.NT, PRISM_APPLET.copy.NT, PRISM_DOM.copy, CK_DLL.copy
BusType=5 ; PCI
Characteristics= 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[PRISM_DCB1.NT.Services]
AddService="WLCB54GT", 2, PRISM_DRIVER_DCB.Service, PRISM_DRIVER.EventLog
[PRISM_DCB1.NT.CoInstallers]
;CpyFiles=PRISM_COINSTALL.copy.NT
AddReg=PRISM_COINSTALL.reg.NT
[PRISM_DCB1.reg]
HKR,Ndi,DeviceID,0,"PCI\VEN_&DEV_&SUBSYS__PRISM_PCI_SUBSYSID_"
HKR,,PlatformID,0,14480
HKR,,VendorDesc,0,%DCB_DESC_STR%
[PRISM_COINSTALL.reg.NT]
[PRISM_DRIVER_ICB.Service]
[PRISM_DRIVER_DCB.Service]
DisplayName=%PRISM_SERVICE_DISPLAY_DCB%
ServiceType=1 ; SERVICE_KERNEL_DRIVER
StartType=3 ; SERVICE_DEMAND_START
ErrorControl=1 ; NORMAL
ServiceBinary=%12%\cowgcb.sys
LoadOrderGroup=NDIS
[PRISM_DRIVER.EventLog]
AddReg=PRISM_DRIVER.EventLog.reg
[PRISM_DRIVER.EventLog.reg]
HKR, ,EventMessageFile ,0x00020000 ,"%%SystemRoot%%\System32\netevent.dll"
HKR, ,TypesSupported ,0x00010001 ,7
[Runonce.reg]
[Run.reg]
[COMMON_PCMCIA.reg]
[COMMON_PCI.reg]
[COMMON_USB.reg]
[COMMON_ICB.reg]
HKR,NDI ,Service ,0 ,"WLCB54GT"
HKR, ,BusType ,0 ,"5"
HKR, ,DeviceVxDs ,0 ,"cowgcb5.sys"
HKR, ,EnableIRQSharing ,1 ,01,00,00,00
HKR, ,IOBaseAddress ,1 ,02,00,00,00
HKR, ,InterruptNumber ,1 ,04,00,00,00
HKR, ,11dMode ,0 ,"0"
HKR, ,CountryCode ,0 ,"DE"
HKR, ,DomainCode ,1 ,30,00,00,00
HKR, ,Band ,0 ,"1"
[COMMON_NDIS.reg]
HKR, ,RunningWin9X ,0 ,"1"
HKR, ,DevLoader ,0 ,"*ndis"
HKR,NDI\Interfaces ,UpperRange ,0 ,"ndis3"
HKR,NDI\Interfaces ,LowerRange ,0 ,"ethernet"
HKR,NDI\Interfaces ,DefUpper ,0 ,"ndis3"
HKR,NDI\Interfaces ,DefLower ,0 ,"ethernet"
HKR,NDIS ,LogDriverName ,0 ,"PRISM"
HKR,NDIS ,MajorNdisVersion ,1 ,03
HKR,NDIS ,MinorNdisVersion ,1 ,0a
[COMMON_NDIS.reg.ME]
HKR, ,RunningWin9X ,0 ,"1"
HKR, ,DevLoader ,0 ,"*ndis"
HKR,NDI\Interfaces ,UpperRange ,0 ,"ndis3"
HKR,NDI\Interfaces ,LowerRange ,0 ,"ethernet"
HKR,NDI\Interfaces ,DefUpper ,0 ,"ndis3"
HKR,NDI\Interfaces ,DefLower ,0 ,"ethernet"
HKR,NDIS ,LogDriverName ,0 ,"PRISM"
HKR,NDIS ,MajorNdisVersion ,1 ,03
HKR,NDIS ,MinorNdisVersion ,1 ,0a
[COMMON_NDIS.reg.NT]
HKR,NDI\Interfaces ,UpperRange ,0 ,"ndis5"
HKR,NDI\Interfaces ,LowerRange ,0 ,"ethernet"
[COMMON.reg]
HKR, ,PRISMIOC ,0 ,"1"
HKR, ,SilentInstall ,0 ,"1"
HKR,NDI\params\RTSThresh,,0,2347
HKR,Ndi\params\RTSThresh,default,0,2347
HKR,NDI\params\RTSThresh,ParamDesc,0,%RTSTHRESH_STR%
HKR,NDI\params\RTSThresh,type,0,int
HKR,NDI\params\RTSThresh,flag,1,20,00,00,00
HKR,NDI\params\RTSThresh,min,0,0
HKR,NDI\params\RTSThresh,max,0,2347
HKR,NDI\params\RTSThresh,step,0,1
HKR,NDI\params\RTSThresh,optional,0,1
HKR,NDI\params\FragThresh,,0,2346
HKR,Ndi\params\FragThresh,default,0,2346
HKR,NDI\params\FragThresh,ParamDesc,0,%FRAGTHRESH_STR%
HKR,NDI\params\FragThresh,type,0,int
HKR,NDI\params\FragThresh,flag,1,20,00,00,00
HKR,NDI\params\FragThresh,min,0,256
HKR,NDI\params\FragThresh,max,0,2346
HKR,NDI\params\FragThresh,step,0,2
HKR,NDI\params\FragThresh,optional,0,1
[COMMON_AMAC_DEL.reg]
HKR,defaults,DataRates
HKR,NDI\params\DataRates
HKR,NDI\params\DataRate
HKR,DSChannel
HKR,defaults,DSChannel
HKR,NDI\params\DSChannel
[COMMON_AMAC.reg]
HKR,NDI\params\ShortRetryLimit,,0,7
HKR,NDI\params\ShortRetryLimit,default,0,7
HKR,NDI\params\ShortRetryLimit,ParamDesc,,%SHORT_RETRY_STR%
HKR,NDI\params\ShortRetryLimit,type,,int
HKR,NDI\params\ShortRetryLimit,min,0,1
HKR,NDI\params\ShortRetryLimit,max,0,255
HKR,NDI\params\ShortRetryLimit,step,0,1
HKR,NDI\params\ShortRetryLimit,optional,0,1
HKR,NDI\params\LongRetryLimit,,0,4
HKR,NDI\params\LongRetryLimit,default,0,4
HKR,NDI\params\LongRetryLimit,ParamDesc,,%LONG_RETRY_STR%
HKR,NDI\params\LongRetryLimit,type,0,int
HKR,NDI\params\LongRetryLimit,min,0,1
HKR,NDI\params\LongRetryLimit,max,0,255
HKR,NDI\params\LongRetryLimit,step,0,1
HKR,NDI\params\LongRetryLimit,optional,0,1
HKR,NDI\params\ConfigProfile,,0,1
HKR,NDI\params\ConfigProfile,default,0,1
HKR,NDI\params\ConfigProfile,ParamDesc,,%CONFIG_PROFILE%
HKR,NDI\params\ConfigProfile,type,,enum
HKR,NDI\params\ConfigProfile,flag,1,30,00,00,00
HKR,NDI\params\ConfigProfile\enum,0,,%CONFIG_PROF_B_ONLY%
HKR,NDI\params\ConfigProfile\enum,1,,%CONFIG_PROF_MIXED%
HKR,NDI\params\ConfigProfile\enum,3,,%CONFIG_PROF_G_ONLY%
HKR,NDI\params\ConfigProfile,optional,0,1
HKR,,NitroMode ,0,"1"
HKR,NDI\params\NitroMode,,0,1
HKR,NDI\params\NitroMode,default,0,1
HKR,NDI\params\NitroMode,ParamDesc,,%NITRO_MODE%
HKR,NDI\params\NitroMode,type,0,int
HKR,NDI\params\NitroMode,min,0,0
HKR,NDI\params\NitroMode,max,0,1
HKR,NDI\params\NitroMode,step,0,1
HKR,NDI\params\NitroMode,optional,0,1
HKR,,NitroTime ,0,"1000"
HKR,NDI\params\NitroTime,,0,1000
HKR,NDI\params\NitroTime,default,0,1000
HKR,NDI\params\NitroTime,ParamDesc,,%NITRO_TIME%
HKR,NDI\params\NitroTime,type,,int
HKR,NDI\params\NitroTime,min,0,0
HKR,NDI\params\NitroTime,max,0,6000
HKR,NDI\params\NitroTime,step,0,1
HKR,NDI\params\NitroTime,optional,0,1
[COMMON_PSMODE.reg]
HKR,defaults,PSMode,0,1
HKR,NDI\params\PSMode,,0,1
HKR,Ndi\params\PSMode,default,0,1
HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
HKR,NDI\params\PSMode,type,,enum
HKR,NDI\params\PSMode,flag,1,30,00,00,00
HKR,NDI\params\PSMode\enum,1,,%POWER_SAVE_OFF_STR%
HKR,NDI\params\PSMode\enum,2,,%POWER_SAVE_DYN_STR%
HKR,NDI\params\PSMode\enum,3,,%POWER_SAVE_MAX_STR%
HKR,NDI\params\PSMode,optional,0,1
[COMMON_PS_MODE_XP.reg]
HKR,defaults,PSMode,0,1
HKR,NDI\params\PSMode,,0,1
HKR,Ndi\params\PSMode,default,0,1
HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
HKR,NDI\params\PSMode,type,,enum
HKR,NDI\params\PSMode,flag,1,30,00,00,00
HKR,NDI\params\PSMode\enum,1,,%POWER_SAVE_OFF_STR%
HKR,NDI\params\PSMode\enum,2,,%POWER_SAVE_DYN_STR%
HKR,NDI\params\PSMode\enum,3,,%POWER_SAVE_MAX_STR%
HKR,NDI\params\PSMode\enum,4,,%POWER_SAVE_AUTO_DYN_STR%
HKR,NDI\params\PSMode\enum,5,,%POWER_SAVE_AUTO_MAX_STR%
HKR,NDI\params\PSMode,optional,0,1
[DestinationDirs]
DefaultDestDir=11 ; Win9x=%windir%\system Win2k=%windir%\system32
PRISM_DRIVER.copy=11 ; Win9x=%windir%\system
PRISM_DRIVER.copy.ME=11 ; Win9x=%windir%\system
PRISM_DRIVER.copy.NT=12 ; Win2k=%windir%\system32\drivers
PRISM_FWICB.copy=11 ; Win9x=%windir%\system
PRISM_FWICB.copy.ME=11 ; Win9x=%windir%\system
PRISM_FWICB.copy.NT=12 ; Win2k=%windir%\system32\drivers
PRISM_FWDCB.copy=11 ; Win9x=%windir%\system
PRISM_FWDCB.copy.ME=11 ; Win9x=%windir%\system
PRISM_FWDCB.copy.NT=12 ; Win2k=%windir%\system32\drivers
PRISM_DOM.copy=10 ; %windir% all OS
CK_DLL.copy=11
[CK_DLL.copy]
[PRISM_NDI.copy]
[PRISM_NDI.copy.ME]
[PRISM_COINSTALL.copy.NT]
[PRISM_DRIVER.copy]
cowgcb5.sys
PRISMIOC.vxd ; Win9x Ioctl interface
[PRISM_DRIVER.copy.ME]
cowgcb5.sys
PRISMIOC.vxd ; Win9x Ioctl interface
[PRISM_DRIVER.copy.NT]
cowgcb.sys
[PRISM_FWICB.copy]
[PRISM_FWICB.copy.ME]
[PRISM_FWICB.copy.NT]
[PRISM_FWDCB.copy]
[PRISM_FWDCB.copy.ME]
[PRISM_FWDCB.copy.NT]
[PRISM_APPLET.copy]
[PRISM_APPLET.copy.ME]
[PRISM_APPLET.copy.NT]
[PRISM_DOM.copy]
[SourceDisksNames]
1=%INSTALL_DISK_STR%,,,
[SourceDisksFiles] ; Win9x
cowgCFG.dll=1
checkdll.dll=1
[SourceDisksFiles.ME] ; WinMe
cowgCFG.dll=1
PRISMIOC.vxd=1
cowgcb5.sys=1
checkdll.dll=1
[SourceDisksFiles.X86] ; Win2k/Xp
cowgcb.sys=1
checkdll.dll=1
[Strings]
VER_VENDOR_STR="corega"
VER_VENDOR_NAME_STR="corega K.K."
PRISM_SERVICE_DISPLAY_DCB="corega WLCB-54GT Driver"
INSTALL_DISK_STR="corega WLCB-54GT Install Disk"
ADHOC_DEMO_STR="Adhoc Demo Mode"
SHORT_PREAM_STR="Preamble Mode"
RTSTHRESH_STR="RTS Threshold"
FRAGTHRESH_STR="Fragmentation Threshold"
AUTHENT_TYPE_STR="Authentication Algorithm"
LISTENINTERVAL_STR="Listen Interval"
POWER_SAVE_STR="Power Save Mode"
POWER_SAVE_OFF_STR="Disabled"
POWER_SAVE_DYN_STR="Dynamic"
POWER_SAVE_MAX_STR="Maximum"
POWER_SAVE_AUTO_DYN_STR="Auto Dynamic"
POWER_SAVE_AUTO_MAX_STR="Auto Maximum"
LOAD_FIRMWARE_STR="Firmware Download"
SHORT_RETRY_STR="Short Retry Limit"
LONG_RETRY_STR="Long Retry Limit"
CHANNEL_STR="Channel"
DATARATES_STR="Data Rate"
DATARATES_AUTO="Fully Automatic"
ALSR_STR="Auto Long Slot Reassociation"
CONFIG_PROFILE="Configuration Profile"
CONFIG_PROF_B_ONLY="B only"
CONFIG_PROF_MIXED="Mixed"
CONFIG_PROF_G_ONLY="G only"
NITRO_MODE="Nitro Mode"
NITRO_TIME="Nitro Time"
DCB_DESC_STR="corega WLCB-54GT"

