
[Version]
DriverVer=11/20/2001,1.0.0.9
Signature="$Chicago$"
Compatible=1
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%VER_VENDOR_STR%
[ControlFlags]
ExcludeFromSelect=*
ExcludeFromSelect=PCI\VEN_14E4&DEV_4320&SUBSYS_00131737 ;PCI
ExcludeFromSelect=PCI\VEN_14E4&DEV_4320&SUBSYS_906E182D ;PCI
ExcludeFromSelect=PCI\VEN_14E4&DEV_4320&SUBSYS_9064182D ;Cardbus
ExcludeFromSelect=PCI\VEN_14E4&DEV_4320&SUBSYS_041714E4 ;PCI
ExcludeFromSelect=PCI\VEN_14E4&DEV_4320&SUBSYS_041814E4
ExcludeFromSelect=PCI\VEN_14E4&DEV_4309
ExcludeFromSelect=PCI\VEN_14E4&DEV_4321
ExcludeFromSelect=PCI\VEN_14E4&DEV_4324
ExcludeFromSelect=PCMCIA\Broadcom-02D0-0406
ExcludeFromSelect=PCMCIA\Broadcom-802.11b_PCMCIA-02D0-0406
ExcludeFromSelect=PCI\VEN_1814&DEV_0101&SUBSYS_9010182D
[Manufacturer]
%VER_VENDOR_NAME_STR%=Adapters
[Adapters]
%PCMCIAFVNET3V.DeviceDesc%=PCMCIAFVNETRXP,PCMCIA\ATMEL-AT76C502-0FBF
%PCMCIAFVNETR5V.DeviceDesc%=PCMCIAFVNETRXP,PCMCIA\ATMEL-AT76C502AR-59BD
%PCMCIAFVNETR5V.DeviceDesc%=PCMCIAFVNETRXP,PCMCIA\Linksys-Instant_Wireless_Network_PC_Card-5CD2
%PCMCIAFVNETR5V.DeviceDesc%=PCMCIAFVNETRXP,PCMCIA\ATMEL-AT76C502AR_E-F543
%USBNET.DeviceDesc%=USBNETXP.NT, USB\VID_03eb&PID_7605
%BCM430B.DeviceDesc%=BCM43XX, PCI\VEN_14E4&DEV_4320&SUBSYS_00131737
%BCM430B.DeviceDesc%=BCM43XG, PCI\VEN_14E4&DEV_4320&SUBSYS_906E182D
%BCM430G.DeviceDesc%=BCM43XG, PCI\VEN_14E4&DEV_4320&SUBSYS_9064182D ;Cardbus
%BCM430B.DeviceDesc%=BCM43XG, PCI\VEN_14E4&DEV_4320&SUBSYS_041714E4
%BCM430G.DeviceDesc%=BCM43XG, PCI\VEN_14E4&DEV_4320&SUBSYS_041814E4
%BCM430A.DeviceDesc%=BCM43XA, PCI\VEN_14E4&DEV_4309
%BCM430A.DeviceDesc%=BCM43XA, PCI\VEN_14E4&DEV_4321
%BCM430M.DeviceDesc%=BCM43XM, PCI\VEN_14E4&DEV_4324
%BCM43pc.DeviceDesc%=BCM43PCM, PCMCIA\Broadcom-02D0-0406
%BCM43pc.DeviceDesc%=BCM43PCM, PCMCIA\Broadcom-802.11b_PCMCIA-02D0-0406
%RT2400.DeviceDesc%=RT2400.ndi, PCI\VEN_1814&DEV_0101&SUBSYS_9010182D
[PCMCIAFVNETR.Ndi.NT]
Characteristics=0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType=8 ; PCMCIA
AddReg=PCMCIAFVNETR.NT.Reg, PCMCIAFVNETR.Params
;CpyFiles=CopyFile.NT.Sys
DriverVer=4/30/2002,4.2.3.40
[PCMCIAFVNETR.Ndi.NT.Services]
AddService=PCMCIAFVNETR, 2, PCMCIAFVNETR.Service, Common.EventLog
[PCMCIAFVNETR.Ndi]
AddReg=PCMCIAFVNETR.Reg, PCMCIAFVNETR.Params
;CpyFiles=CopyFile.Sys
DriverVer=4/30/2002,4.2.3.40
[PCMCIAFVNETR.Reg]
HKR,Ndi,DeviceID,,PCMCIA\ATMEL-AT76C502-0FBF
HKR,Ndi,DeviceID,,PCMCIA\ATMEL-AT76C502AR-59BD
HKR,Ndi,CardType,,"PNP"
HKR,,DevLoader,,*ndis,*ntkern,*ndis
HKR,,DeviceVxDs,,fvnetr.sys
HKR,NDIS,MajorNdisVersion,1,05
HKR,NDIS,MinorNdisVersion,1,00
HKR,NDIS,LogDriverName,,VNETPCMCIAR
HKR,Ndi\Interfaces,DefUpper,,"ndis3"
HKR,Ndi\Interfaces,DefLower,,"ethernet"
HKR,Ndi\Interfaces,UpperRange,,"ndis3"
HKR,Ndi\Interfaces,LowerRange,,"ethernet"
HKR,Ndi,HelpText,,%Help_Text%
[PCMCIAFVNETR.Ndi.NT]
Characteristics=0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType=8 ; PCMCIA
AddReg=PCMCIAFVNETR.NT.Reg, PCMCIAFVNETRXP.Params
;CpyFiles=CopyFile.NT.Sys
DriverVer=4/30/2002,4.2.3.40
[PCMCIAFVNETR.Ndi.NT.Services]
AddService=PCMCIAFVNETR, 2, PCMCIAFVNETR.Service, Common.EventLog
[USBNET.Ndi]
AddReg=USBNET.Reg, USBNET.Params
;CpyFiles=CopyFile.Sys
[USBNET.Ndi.NT]
Characteristics=0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType=15 ; USB
AddReg=USBNET.NT.Reg, USBNET.Params
;CpyFiles=CopyFile.NT.Sys
DriverVer=12/10/2001,1.2.2.58
[USBNET.Ndi.NT.Services]
AddService=USBNET, 2, USBNET.Service, Common.EventLog
[USBNETXP.NT]
Characteristics=0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType=15 ; USB
AddReg=USBNETXP.Reg, USBNETXP.Params
;CpyFiles=CopyFile.XP.Sys
[USBNETXP.NT.Services]
AddService=USBNET_XP, 2, USBNETXP.Service, Common.EventLog
[USBNETXP.Reg]
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi, Service, 0, "USBNET_XP"
[USBNET.Service]
DisplayName=%USBNET.DisplayName%
ServiceType=1
StartType=3
ErrorControl=1
ServiceBinary=%12%\netusb.sys
LoadOrderGroup=NDIS
[USBNETXP.Service]
DisplayName=%USBNETXP.DisplayName%
ServiceType=1
StartType=3
ErrorControl=1
ServiceBinary=%12%\netusbxp.sys
LoadOrderGroup=NDIS
[USBNET.Reg]
HKR,Ndi,DeviceID,,USB\VID_03ebA&PID_7605
HKR,Ndi,CardType,,"PNP"
HKR,,DevLoader,,*ndis,*ntkern,*ndis
HKR,,DeviceVxDs,,netusb.sys
HKR,NDIS,MajorNdisVersion,1,05
HKR,NDIS,MinorNdisVersion,1,00
HKR,NDIS,LogDriverName,,netusb
HKR,Ndi\Interfaces,DefUpper,,"ndis3"
HKR,Ndi\Interfaces,DefLower,,"ethernet"
HKR,Ndi\Interfaces,UpperRange,,"ndis3"
HKR,Ndi\Interfaces,LowerRange,,"ethernet"
[USBNET.NT.Reg]
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi, Service, 0, "USBNET"
[RT2400.ndi]
AddReg=Common.reg, RT2400.ndi.reg
;CpyFiles=win9x.CopyFiles,RT2400.Apps
[RT2400.ndi.NT]
AddReg=Common.reg, RT2400.ndi.NT.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=5
;CpyFiles=NT.CopyFiles,RT2400.Apps
[RT2400.ndi.NT.Services]
AddService=RT2400, 2, RT2400.Service, common.EventLog
[RT2400.ndi.NT.CoInstallers]
;CpyFiles=RT2400CoInstallFile
AddReg=RT2400.CoInstallers_AddReg
[RT2400CoInstallFile]
[win9x.CopyFiles]
[NT.CopyFiles]
rt2400.sys,,,2
[RT2400.Apps]
[RT2400.ndi.reg]
HKR, , NTMPDriver, 0, RT2400.sys
HKR, Ndi, DeviceID, 0, "PCI\VEN_1814&DEV_0101&SUBSYS_24601814"
HKR, , RunningWin9X, 0, "1"
HKR, , DevLoader, 0, *ndis
HKR, , DeviceVxDs, 0, RT2400.sys
HKR, , EnumPropPages, 0, "netdi.dll,EnumPropPages"
HKR, NDIS, LogDriverName, 0, "RT2400"
HKR, NDIS, MajorNdisVersion,1, 03
HKR, NDIS, MinorNdisVersion,1, 0A
HKR, , BusType, 0, 5
HKR, NDI, CardType, 0, "PCI"
HKR, Ndi\Interfaces, DefUpper, 0, "ndis3"
HKR, Ndi\Interfaces, DefLower, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis3"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
[win9x.CopyFiles]
[Common.reg]
HKR, , SSID, 0, %SSID_DEF_STR%
HKR, Default, SSID, 0, %SSID_DEF_STR%
HKR, NDI\params\SSID, ParamDesc, 0, "SSID"
HKR, NDI\params\SSID, type, 0, "edit"
HKR, NDI\params\SSID, limitText, 0, "32"
HKR, NDI\params\SSID, default, 0, %SSID_DEF_STR%
HKR, , NetworkType, 0, %NETWORK_TYPE_DEF_STR%
HKR, Default, NetworkType, 0, %NETWORK_TYPE_DEF_STR%
HKR, NDI\params\NetworkType, ParamDesc, 0, "Network Type"
HKR, NDI\params\NetworkType, type, 0, "enum"
HKR, NDI\params\NetworkType, default, 0, %NETWORK_TYPE_DEF_STR%
HKR, NDI\params\NetworkType\enum, 0, 0, "802.11 Ad Hoc"
HKR, NDI\params\NetworkType\enum, 1, 0, "Infrastructure"
HKR, , Channel, 0, %CHANNEL%
HKR, Default, Channel, 0, %CHANNEL%
HKR, NDI\params\Channel, ParamDesc, 0, "Channel"
HKR, NDI\params\Channel, type, 0, "enum"
HKR, NDI\params\Channel, default, 0, %CHANNEL%
HKR, NDI\params\Channel\enum, 1, 0, "01"
HKR, NDI\params\Channel\enum, 2, 0, "02"
HKR, NDI\params\Channel\enum, 3, 0, "03"
HKR, NDI\params\Channel\enum, 4, 0, "04"
HKR, NDI\params\Channel\enum, 5, 0, "05"
HKR, NDI\params\Channel\enum, 6, 0, "06"
HKR, NDI\params\Channel\enum, 7, 0, "07"
HKR, NDI\params\Channel\enum, 8, 0, "08"
HKR, NDI\params\Channel\enum, 9, 0, "09"
HKR, NDI\params\Channel\enum, 10, 0, "10"
HKR, NDI\params\Channel\enum, 11, 0, "11"
HKR, , NetworkAddress, 0, ""
HKR, Default, NetworkAddress, 0, ""
HKR, NDI\params\NetworkAddress, ParamDesc, 0, "Local Administration MAC Network Address"
HKR, NDI\params\NetworkAddress, type, 0, "edit"
HKR, NDI\params\NetworkAddress, limitText, 0, "12"
HKR, NDI\params\NetworkAddress, default, 0, ""
HKR, , FirstRun, 0, "0"
HKR, , RaConfig, 0, "1" ;1=RaConfig , 0=ZeroConfig for MiniPCI
HKR, , CountryRegion, 0, "2"
HKR, NDI\params\CountryRegion, ParamDesc, 0, "Country Region"
HKR, NDI\params\CountryRegion, type, 0, "enum"
HKR, NDI\params\CountryRegion, default, 0, "0"
HKR, NDI\params\CountryRegion\enum, 0, 0, "FCC (Channel 1 - 11)"
HKR, NDI\params\CountryRegion\enum, 1, 0, "IC (Channel 1 - 11)"
HKR, NDI\params\CountryRegion\enum, 2, 0, "ETSI (Channel 1 - 13)"
HKR, NDI\params\CountryRegion\enum, 3, 0, "Spain (Channel 10 - 11)"
HKR, NDI\params\CountryRegion\enum, 4, 0, "France (Channel 10 - 13)"
HKR, NDI\params\CountryRegion\enum, 5, 0, "MKK (Channel 14)"
HKR, NDI\params\CountryRegion\enum, 6, 0, "MKK1 (Channel 1 - 14)"
HKR, NDI\params\CountryRegion\enum, 7, 0, "Israel (Channel 3 - 9)"
HKR, , PSMode, 0, "0"
HKR, Default, PSMode, 0, "0"
HKR, NDI\params\PSMode, ParamDesc, 0, "Power Saving Mode"
HKR, NDI\params\PSMode, type, 0, "enum"
HKR, NDI\params\PSMode, default, 0, "0"
HKR, NDI\params\PSMode\enum, 0, 0, "CAM (Constantly Awake Mode)"
HKR, NDI\params\PSMode\enum, 1, 0, "Max_PSP (Max Power Savings)"
HKR, NDI\params\PSMode\enum, 2, 0, "Fast_PSP (Power Save Mode)"
HKR, , ACPowerCam, 0, "0"
HKR, Default, ACPowerCam, 0, "0"
HKR, NDI\params\ACPowerCam, ParamDesc, 0, "CAM when AC Power"
HKR, NDI\params\ACPowerCam, type, 0, "enum"
HKR, NDI\params\ACPowerCam, default, 0, "0"
HKR, NDI\params\ACPowerCam\enum, 0, 0, "Disable"
HKR, NDI\params\ACPowerCam\enum, 1, 0, "Enable"
HKR, , AntennaTx, 0, "0"
HKR, Default, AntennaTx, 0, "0"
HKR, NDI\params\AntennaTx, ParamDesc, 0, "Antenna Tx Diversity"
HKR, NDI\params\AntennaTx, type, 0, "enum"
HKR, NDI\params\AntennaTx, default, 0, "0"
HKR, NDI\params\AntennaTx\enum, 0, 0, "Diversity"
HKR, NDI\params\AntennaTx\enum, 1, 0, "Antenna A Only"
HKR, NDI\params\AntennaTx\enum, 2, 0, "Antenna B Only"
HKR, , AntennaRx, 0, "0"
HKR, Default, AntennaRx, 0, "0"
HKR, NDI\params\AntennaRx, ParamDesc, 0, "Antenna Rx Diversity"
HKR, NDI\params\AntennaRx, type, 0, "enum"
HKR, NDI\params\AntennaRx, default, 0, "0"
HKR, NDI\params\AntennaRx\enum, 0, 0, "Diversity"
HKR, NDI\params\AntennaRx\enum, 1, 0, "Antenna A Only"
HKR, NDI\params\AntennaRx\enum, 2, 0, "Antenna B Only"
HKR, , TransRate, 0, "0"
HKR, Default, TransRate, 0, "0"
HKR, NDI\params\TransRate, ParamDesc, 0, "Transmit Rate"
HKR, NDI\params\TransRate, type, 0, "enum"
HKR, NDI\params\TransRate, default, 0, "0"
HKR, NDI\params\TransRate\enum, 0, 0, "Auto"
HKR, NDI\params\TransRate\enum, 1, 0, "11 Mb/s"
HKR, NDI\params\TransRate\enum, 2, 0, "5.5 Mb/s"
HKR, NDI\params\TransRate\enum, 3, 0, "2 Mb/s"
HKR, NDI\params\TransRate\enum, 4, 0, "1 Mb/s"
HKR, , PreambleType, 0, "2"
HKR, Default, PreambleType, 0, "2"
HKR, NDI\params\PreambleType, ParamDesc, 0, "Preamble Type"
HKR, NDI\params\PreambleType, type, 0, "enum"
HKR, Ndi\params\PreambleType, default, 0, "2"
HKR, NDI\params\PreambleType\enum,0, 0, "Long"
HKR, NDI\params\PreambleType\enum,1, 0, "Short"
HKR, NDI\params\PreambleType\enum,2, 0, "Auto"
HKR, NDI\params\PreambleType, optional, 0, "0"
HKR, , RTSThresh, 0, "2347"
HKR, Default, RTSThresh, 0, "2347"
HKR, NDI\params\RTSThresh, ParamDesc, 0, "RTS Threshold"
HKR, NDI\params\RTSThresh, type, 0, "int"
HKR, Ndi\params\RTSThresh, default, 0, "2347"
HKR, NDI\params\RTSThresh, min, 0, "0"
HKR, NDI\params\RTSThresh, max, 0, "2347"
HKR, NDI\params\RTSThresh, step, 0, "32"
HKR, NDI\params\RTSThresh, optional, 0, "0"
HKR, , FragThresh, 0, "2346"
HKR, Default, FragThresh, 0, "2346"
HKR, NDI\params\FragThresh, ParamDesc, 0, "Fragment Threshold"
HKR, NDI\params\FragThresh, type, 0, "int"
HKR, Ndi\params\FragThresh, default, 0, "2346"
HKR, NDI\params\FragThresh, min, 0, "256"
HKR, NDI\params\FragThresh, max, 0, "2346"
HKR, NDI\params\FragThresh, step, 0, "32"
HKR, NDI\params\FragThresh, optional, 0, "0"
HKR, , Radio, 0, "0"
HKR, NDI\params\Radio, ParamDesc, 0, "Radio Status"
HKR, NDI\params\Radio, type, 0, "enum"
HKR, NDI\params\Radio, default, 0, "0"
HKR, NDI\params\Radio\enum, 1, 0, "Disable"
HKR, NDI\params\Radio\enum, 0, 0, "Enable"
HKR, , AuthenType, 0, "0"
HKR, Default, AuthenType, 0, "0"
HKR, NDI\params\AuthenType, ParamDesc, 0, "Authentication Type"
HKR, NDI\params\AuthenType, type, 0, "enum"
HKR, NDI\params\AuthenType, default, 0, "0"
HKR, NDI\params\AuthenType\enum, 0, 0, "Open System"
HKR, NDI\params\AuthenType\enum, 1, 0, "Shared Key"
HKR, , Encryption, 0, "0"
HKR, Default, Encryption, 0, "0"
HKR, , WEPKeyLen, 0, "0"
HKR, Default, WEPKeyLen, 0, "0"
HKR, , WEPKeyUse, 0,"1"
HKR, Default, WEPKeyUse, 0,"1"
HKR, , WEPKey1, 0,""
HKR, Default, WEPKey1, 0,""
HKR, , WEPKey2, 0,""
HKR, Default, WEPKey2, 0,""
HKR, , WEPKey3, 0,""
HKR, Default, WEPKey3, 0,""
HKR, , WEPKey4, 0,""
HKR, Default, WEPKey4, 0,""
HKR, , CurProfile, 0,""
HKR, Default, CurProfile, 0,""
[RT2400.ndi.NT.reg]
HKR, Ndi, Service, 0, "RT2400"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
[RT2400.Service]
DisplayName=%RT2400.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_AUTO_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\RT2400.sys
LoadOrderGroup=NDIS
[common.EventLog]
AddReg=common.AddEventLog.reg
[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000,"%%SystemRoot%%\System32\netevent.dll,%%SystemRoot%%\System32\drivers\RT2400.sys"
HKR, , TypesSupported, 0x00010001, 7
[RT2400.CoInstallers_AddReg]
[USBNET.Params]
HKR, Ndi\params\PreambleType, ParamDesc, 0, "Preamble Type"
HKR, Ndi\params\PreambleType, default, 0, "0"
HKR, Ndi\params\PreambleType, type, 0, "enum"
HKR, Ndi\params\PreambleType\enum, 0, 0, "Long"
HKR, Ndi\params\PreambleType\enum, 1, 0, "Short"
HKR, Ndi\params\PreambleType\enum, 2, 0, "Auto"
HKR, , PreambleType, 0, "0"
HKR, Ndi\params\Channel, ParamDesc, 0, "Channel"
HKR, Ndi\params\Channel, default, 0, "3"
HKR, Ndi\params\Channel, type, 0, "int"
HKR, Ndi\params\Channel, min, 0, "1"
HKR, Ndi\params\Channel, max, 0, "14"
HKR, Ndi\params\Channel, step, 0, "1"
HKR, , Channel, 0, "3"
HKR, Ndi\params\Rate, ParamDesc, 0, "Rate (Mbps)"
HKR, Ndi\params\Rate, default, 0, "3"
HKR, Ndi\params\Rate, type, 0, "enum"
HKR, Ndi\params\Rate\enum, 0, 0, "1"
HKR, Ndi\params\Rate\enum, 1, 0, "2"
HKR, Ndi\params\Rate\enum, 2, 0, "5.5"
HKR, Ndi\params\Rate\enum, 3, 0, "11"
HKR, Ndi\params\Rate\enum, 4, 0, "Auto"
HKR, , Rate, 0, "3"
HKR, Ndi\params\RTS_Threshold, ParamDesc, 0, "RTS Threshold"
HKR, Ndi\params\RTS_Threshold, default, 0, "2347"
HKR, Ndi\params\RTS_Threshold, type, 0, "int"
HKR, Ndi\params\RTS_Threshold, min, 0, "0"
HKR, Ndi\params\RTS_Threshold, max, 0, "2347"
HKR, Ndi\params\RTS_Threshold, step, 0, "1"
HKR, , RTS_Threshold, 0, "2347"
HKR, Ndi\params\Frag_Threshold, ParamDesc, 0, "Fragmentation Threshold"
HKR, Ndi\params\Frag_Threshold, default, 0, "2346"
HKR, Ndi\params\Frag_Threshold, type, 0, "int"
HKR, Ndi\params\Frag_Threshold, min, 0, "256"
HKR, Ndi\params\Frag_Threshold, max, 0, "2346"
HKR, Ndi\params\Frag_Threshold, step, 0, "1"
HKR, , Frag_Threshold, 0, "2346"
HKR, Ndi\params\Operating_Mode, ParamDesc, 0, "Operating Mode"
HKR, Ndi\params\Operating_Mode, default, 0, "1"
HKR, Ndi\params\Operating_Mode, type, 0, "enum"
HKR, Ndi\params\Operating_Mode\enum, 0, 0, "Ad-Hoc"
HKR, Ndi\params\Operating_Mode\enum, 1, 0, "Infrastructure"
HKR, , Operating_Mode, 0, "1"
HKR, Ndi\params\ESSID, ParamDesc, 0, "ESSID"
HKR, Ndi\params\ESSID, default, 0, "ANY"
HKR, Ndi\params\ESSID, type, 0, "edit"
HKR, Ndi\params\ESSID, LimitText, 0, "32"
HKR, Ndi\params\ESSID, UpperCase, 0, "0"
HKR, , ESSID, 0, "ANY"
HKR, Ndi\params\AuthenticationType, ParamDesc, 0, "Authentication Type"
HKR, Ndi\params\AuthenticationType, default, 0, "0"
HKR, Ndi\params\AuthenticationType, type, 0, "enum"
HKR, Ndi\params\AuthenticationType\enum,0, 0, "Open System"
HKR, Ndi\params\AuthenticationType\enum,1, 0, "Shared Key"
HKR, Ndi\params\AuthenticationType\enum,2, 0, "Auto"
HKR, , AuthenticationType, 0, "0"
HKR, Ndi\params\WEP_Mode, ParamDesc, 0, "WEP Mode"
HKR, Ndi\params\WEP_Mode, default, 0, "0"
HKR, Ndi\params\WEP_Mode, type, 0, "enum"
HKR, Ndi\params\WEP_Mode\enum, 0, 0, "Mandatory"
HKR, Ndi\params\WEP_Mode\enum, 1, 0, "Optional"
HKR, , WEP_Mode, 0, "0"
HKR,Ndi\params\EncryptionLevel, ParamDesc, 0,"Encryption Level"
HKR,Ndi\params\EncryptionLevel, type, 0,"enum"
HKR,Ndi\params\EncryptionLevel, default, 0,"0"
HKR,Ndi\params\EncryptionLevel\enum, 0, 0,"None"
HKR,Ndi\params\EncryptionLevel\enum, 1, 0,"64-bit encryption"
HKR,Ndi\params\EncryptionLevel\enum, 2, 0,"128-bit encryption"
HKR,, EncryptionLevel, 0,"0"
HKR,Ndi\params\WEP_KEY_INDEX, ParamDesc, 0,"WEP Key to use"
HKR,Ndi\params\WEP_KEY_INDEX, type, 0,"enum"
HKR,Ndi\params\WEP_KEY_INDEX, default, 0,"0"
HKR,Ndi\params\WEP_KEY_INDEX\enum, 0, 0,"1"
HKR,Ndi\params\WEP_KEY_INDEX\enum, 1, 0,"2"
HKR,Ndi\params\WEP_KEY_INDEX\enum, 2, 0,"3"
HKR,Ndi\params\WEP_KEY_INDEX\enum, 3, 0,"4"
HKR,, WEP_KEY_INDEX, 0,"0"
HKR,Ndi\params\WEP_KEY_1, ParamDesc, 0,"WEP KEY #1"
HKR,Ndi\params\WEP_KEY_1, default, 0,"00000000000000000000000000"
HKR,Ndi\params\WEP_KEY_1, type, 0,"edit"
HKR,Ndi\params\WEP_KEY_1, LimitText, 0,"26"
HKR,Ndi\params\WEP_KEY_1, UpperCase, 0,"1"
HKR,, WEP_KEY_1, 0,"00000000000000000000000000"
HKR,Ndi\params\WEP_KEY_2, ParamDesc, 0,"WEP KEY #2"
HKR,Ndi\params\WEP_KEY_2, default, 0,"00000000000000000000000000"
HKR,Ndi\params\WEP_KEY_2, type, 0,"edit"
HKR,Ndi\params\WEP_KEY_2, LimitText, 0,"26"
HKR,Ndi\params\WEP_KEY_2, UpperCase, 0,"1"
HKR,, WEP_KEY_2, 0,"00000000000000000000000000"
HKR,Ndi\params\WEP_KEY_3, ParamDesc, 0,"WEP KEY #3"
HKR,Ndi\params\WEP_KEY_3, default, 0,"00000000000000000000000000"
HKR,Ndi\params\WEP_KEY_3, type, 0,"edit"
HKR,Ndi\params\WEP_KEY_3, LimitText, 0,"26"
HKR,Ndi\params\WEP_KEY_3, UpperCase, 0,"1"
HKR,, WEP_KEY_3, 0,"00000000000000000000000000"
HKR,Ndi\params\WEP_KEY_4, ParamDesc, 0,"WEP KEY #4"
HKR,Ndi\params\WEP_KEY_4, default, 0,"00000000000000000000000000"
HKR,Ndi\params\WEP_KEY_4, type, 0,"edit"
HKR,Ndi\params\WEP_KEY_4, LimitText, 0,"26"
HKR,Ndi\params\WEP_KEY_4, UpperCase, 0,"1"
HKR,, WEP_KEY_4, 0,"00000000000000000000000000"
[PCMCIAFVNETR.Params]
HKR, Ndi\params\Channel, ParamDesc, 0, %ChannelStr%
HKR, Ndi\params\Channel, type, 0, "int"
HKR, Ndi\params\Channel, default, 0, "3"
HKR, Ndi\params\Channel, min, 0, "1"
HKR, Ndi\params\Channel, max, 0, "14"
HKR, Ndi\params\Channel, step, 0, "1"
HKR, , Channel, 0, "3"
HKR, Ndi\params\Rate, ParamDesc, 0, %RateStr%
HKR, Ndi\params\Rate, type, 0, "enum"
HKR, Ndi\params\Rate, default, 0, "3"
HKR, Ndi\params\Rate\enum, 0, 0, %Fixed1Str%
HKR, Ndi\params\Rate\enum, 1, 0, %Fixed2Str%
HKR, Ndi\params\Rate\enum, 2, 0, %Fixed55Str%
HKR, Ndi\params\Rate\enum, 3, 0, %Fixed11Str%
HKR, Ndi\params\Rate\enum, 4, 0, %AutoStr%
HKR, , Rate, 0, "3"
HKR, Ndi\params\RTS_Threshold, ParamDesc, 0, %RTS_Str%
HKR, Ndi\params\RTS_Threshold, type, 0, "int"
HKR, Ndi\params\RTS_Threshold, default, 0, "2347"
HKR, Ndi\params\RTS_Threshold, min, 0, "0"
HKR, Ndi\params\RTS_Threshold, max, 0, "2347"
HKR, Ndi\params\RTS_Threshold, step, 0, "1"
HKR, , RTS_Threshold, 0, "2347"
HKR, Ndi\params\Frag_Threshold, ParamDesc, 0, %FragmentationStr%
HKR, Ndi\params\Frag_Threshold, type, 0, "int"
HKR, Ndi\params\Frag_Threshold, default, 0, "2346"
HKR, Ndi\params\Frag_Threshold, min, 0, "256"
HKR, Ndi\params\Frag_Threshold, max, 0, "2346"
HKR, Ndi\params\Frag_Threshold, step, 0, "1"
HKR, , Frag_Threshold, 0, "2346"
HKR, Ndi\params\Operating_Mode, ParamDesc, 0, %OperatingModeStr%
HKR, Ndi\params\Operating_Mode, type, 0, "enum"
HKR, Ndi\params\Operating_Mode, default, 0, "1"
HKR, Ndi\params\Operating_Mode\enum, 0, 0, %AdHocStr%
HKR, Ndi\params\Operating_Mode\enum, 1, 0, %InfrastructureStr%
HKR, , Operating_Mode, 0, "1"
HKR, Ndi\params\ESSID, ParamDesc, 0, %ESSID_Str%
HKR, Ndi\params\ESSID, type, 0, "edit"
HKR, Ndi\params\ESSID, default, 0, ""
HKR, Ndi\params\ESSID, LimitText, 0, "32"
HKR, Ndi\params\ESSID, UpperCase, 0, "0"
HKR, , ESSID, 0, ""
HKR,Ndi\params\WEP_KEY_INDEX, ParamDesc, 0,%WEP_Key_Str%
HKR,Ndi\params\WEP_KEY_INDEX, type, 0,"enum"
HKR,Ndi\params\WEP_KEY_INDEX, default, 0,"0"
HKR,Ndi\params\WEP_KEY_INDEX\enum, 0, 0,%Key1Str%
HKR,Ndi\params\WEP_KEY_INDEX\enum, 1, 0,%Key2Str%
HKR,Ndi\params\WEP_KEY_INDEX\enum, 2, 0,%Key3Str%
HKR,Ndi\params\WEP_KEY_INDEX\enum, 3, 0,%Key4Str%
HKR,, WEP_KEY_INDEX, 0,"0"
HKR,Ndi\params\EncryptionLevel, ParamDesc, 0,"Encryption Level"
HKR,Ndi\params\EncryptionLevel, type, 0,"enum"
HKR,Ndi\params\EncryptionLevel, default, 0,"0"
HKR,Ndi\params\EncryptionLevel\enum, 0, 0,%DisabledStr%
HKR,Ndi\params\EncryptionLevel\enum, 1, 0,%64bit%
HKR,Ndi\params\EncryptionLevel\enum, 2, 0,%128bit%
HKR,, EncryptionLevel,0,"0"
HKR,Ndi\params\WEP_KEY_1, ParamDesc, 0,%KEY1_Str%
HKR,Ndi\params\WEP_KEY_1, type, 0,"edit"
HKR,Ndi\params\WEP_KEY_1, default, 0,"0000000000"
HKR,Ndi\params\WEP_KEY_1, LimitText, 0,"10"
HKR,Ndi\params\WEP_KEY_1, UpperCase, 0,"1"
HKR,, WEP_KEY_1, 0,"0000000000"
HKR,Ndi\params\WEP_KEY_2, ParamDesc, 0,%KEY2_Str%
HKR,Ndi\params\WEP_KEY_2, type, 0,"edit"
HKR,Ndi\params\WEP_KEY_2, default, 0,"0000000000"
HKR,Ndi\params\WEP_KEY_2, LimitText, 0,"10"
HKR,Ndi\params\WEP_KEY_2, UpperCase, 0,"1"
HKR,, WEP_KEY_2, 0,"0000000000"
HKR,Ndi\params\WEP_KEY_3, ParamDesc, 0,%KEY3_Str%
HKR,Ndi\params\WEP_KEY_3, type, 0,"edit"
HKR,Ndi\params\WEP_KEY_3, default, 0,"0000000000"
HKR,Ndi\params\WEP_KEY_3, LimitText, 0,"10"
HKR,Ndi\params\WEP_KEY_3, UpperCase, 0,"1"
HKR,, WEP_KEY_3, 0,"0000000000"
HKR,Ndi\params\WEP_KEY_4, ParamDesc, 0,%KEY4_Str%
HKR,Ndi\params\WEP_KEY_4, type, 0,"edit"
HKR,Ndi\params\WEP_KEY_4, default, 0,"0000000000"
HKR,Ndi\params\WEP_KEY_4, LimitText, 0,"10"
HKR,Ndi\params\WEP_KEY_4, UpperCase, 0,"1"
HKR,, WEP_KEY_4, 0,"0000000000"
HKR,Ndi\params\WEP_Mode, ParamDesc, 0,%WEP_Mode_Str%
HKR,Ndi\params\WEP_Mode, type, 0,"enum"
HKR,Ndi\params\WEP_Mode, default, 0,"0"
HKR,Ndi\params\WEP_Mode\enum, 0, 0,%WepMandatoryStr%
HKR,Ndi\params\WEP_Mode\enum, 1, 0,%WepOptionalStr%
HKR,, WEP_Mode, 0,"0"
HKR,Ndi\params\AuthenticationType, ParamDesc, 0,%AuthTypeStr%
HKR,Ndi\params\AuthenticationType, type, 0,"enum"
HKR,Ndi\params\AuthenticationType, default, 0,"2"
HKR,Ndi\params\AuthenticationType\enum, 0, 0,%OpenSystemStr%
HKR,Ndi\params\AuthenticationType\enum, 1, 0,%SharedKeyStr%
HKR,Ndi\params\AuthenticationType\enum, 2, 0,%AutoAuthStr%
HKR,, AuthenticationType, 0,"2"
HKR,Ndi\params\PreambleType, ParamDesc, 0,%PreambleStr%
HKR,Ndi\params\PreambleType, type, 0,"enum"
HKR,Ndi\params\PreambleType, default, 0,"2"
HKR,Ndi\params\PreambleType\enum, 0, 0,%LongPreambleStr%
HKR,Ndi\params\PreambleType\enum, 1, 0,%ShortPreambleStr%
HKR,Ndi\params\PreambleType\enum, 2, 0,%AutoPreambleStr%
HKR,, PreambleType, 0,"2"
HKR,Ndi\params\PowerMgmtMode, ParamDesc, 0,%PowerMgmtStr%
HKR,Ndi\params\PowerMgmtMode, type, 0,"enum"
HKR,Ndi\params\PowerMgmtMode, default, 0,"0"
HKR,Ndi\params\PowerMgmtMode\enum, 0, 0,%ActiveStr%
HKR,Ndi\params\PowerMgmtMode\enum, 1, 0,%PSStr%
HKR,, PowerMgmtMode, 0,"0"
HKR,Ndi\params\BasicRates, ParamDesc, 0,%BasicRatesStr%
HKR,Ndi\params\BasicRates, type, 0,"enum"
HKR,Ndi\params\BasicRates, default, 0,"0"
HKR,Ndi\params\BasicRates\enum, 0, 0,%BR1Str%
HKR,Ndi\params\BasicRates\enum, 1, 0,%BR2Str%
HKR,, BasicRates, 0,"0"
HKR, Ndi\params\BeaconPeriod, ParamDesc, 0, %BeaconPeriodStr%
HKR, Ndi\params\BeaconPeriod, type, 0, "int"
HKR, Ndi\params\BeaconPeriod, default, 0, "100"
HKR, Ndi\params\BeaconPeriod, min, 0, "20"
HKR, Ndi\params\BeaconPeriod, max, 0, "1000"
HKR, Ndi\params\BeaconPeriod, step, 0, "1"
HKR, , BeaconPeriod, 0, "100"
HKR,Ndi\params\RadioOnOff, ParamDesc, 0,%RadioOnOffStr%
HKR,Ndi\params\RadioOnOff, type, 0,"enum"
HKR,Ndi\params\RadioOnOff, default, 0,"1"
HKR,Ndi\params\RadioOnOff\enum, 0, 0,%RadioOffStr%
HKR,Ndi\params\RadioOnOff\enum, 1, 0,%RadioOnStr%
HKR,, RadioOnOff, 0,"1"
[PCMCIAFVNETRXP.Params]
HKR, Ndi\params\Rate, ParamDesc, 0, %RateStr%
HKR, Ndi\params\Rate, type, 0, "enum"
HKR, Ndi\params\Rate, default, 0, "3"
HKR, Ndi\params\Rate\enum, 0, 0, %Fixed1Str%
HKR, Ndi\params\Rate\enum, 1, 0, %Fixed2Str%
HKR, Ndi\params\Rate\enum, 2, 0, %Fixed55Str%
HKR, Ndi\params\Rate\enum, 3, 0, %Fixed11Str%
HKR, Ndi\params\Rate\enum, 4, 0, %AutoStr%
HKR, , Rate, 0, "3"
HKR, Ndi\params\RTS_Threshold, ParamDesc, 0, %RTS_Str%
HKR, Ndi\params\RTS_Threshold, type, 0, "int"
HKR, Ndi\params\RTS_Threshold, default, 0, "2347"
HKR, Ndi\params\RTS_Threshold, min, 0, "0"
HKR, Ndi\params\RTS_Threshold, max, 0, "2347"
HKR, Ndi\params\RTS_Threshold, step, 0, "1"
HKR, , RTS_Threshold, 0, "2347"
HKR, Ndi\params\Frag_Threshold, ParamDesc, 0, %FragmentationStr%
HKR, Ndi\params\Frag_Threshold, type, 0, "int"
HKR, Ndi\params\Frag_Threshold, default, 0, "2346"
HKR, Ndi\params\Frag_Threshold, min, 0, "256"
HKR, Ndi\params\Frag_Threshold, max, 0, "2346"
HKR, Ndi\params\Frag_Threshold, step, 0, "1"
HKR, , Frag_Threshold, 0, "2346"
HKR,Ndi\params\PreambleType, ParamDesc, 0,%PreambleStr%
HKR,Ndi\params\PreambleType, type, 0,"enum"
HKR,Ndi\params\PreambleType, default, 0,"2"
HKR,Ndi\params\PreambleType\enum, 0, 0,%LongPreambleStr%
HKR,Ndi\params\PreambleType\enum, 1, 0,%ShortPreambleStr%
HKR,Ndi\params\PreambleType\enum, 2, 0,%AutoPreambleStr%
HKR,, PreambleType, 0,"2"
HKR,Ndi\params\RadioOnOff, ParamDesc, 0,%RadioOnOffStr%
HKR,Ndi\params\RadioOnOff, type, 0,"enum"
HKR,Ndi\params\RadioOnOff, default, 0,"1"
HKR,Ndi\params\RadioOnOff\enum, 0, 0,%RadioOffStr%
HKR,Ndi\params\RadioOnOff\enum, 1, 0,%RadioOnStr%
HKR,,
[USBNETXP.Params]
HKR, ,GTKSIOC ,0 ,"1"
HKR, Ndi\params\Rate, ParamDesc, 0, "Rate (Mbps)"
HKR, Ndi\params\Rate, default, 0, "3"
HKR, Ndi\params\Rate, type, 0, "enum"
HKR, Ndi\params\Rate\enum, 0, 0, "1"
HKR, Ndi\params\Rate\enum, 1, 0, "2"
HKR, Ndi\params\Rate\enum, 2, 0, "5.5"
HKR, Ndi\params\Rate\enum, 3, 0, "11"
HKR, Ndi\params\Rate\enum, 4, 0, "Auto"
HKR, , Rate, 0, "3"
HKR, Ndi\params\RTS_Threshold, ParamDesc, 0, "RTS Threshold"
HKR, Ndi\params\RTS_Threshold, default, 0, "2347"
HKR, Ndi\params\RTS_Threshold, type, 0, "int"
HKR, Ndi\params\RTS_Threshold, min, 0, "0"
HKR, Ndi\params\RTS_Threshold, max, 0, "2347"
HKR, Ndi\params\RTS_Threshold, step, 0, "1"
HKR, , RTS_Threshold, 0, "2347"
HKR, Ndi\params\Frag_Threshold, ParamDesc, 0, "Fragmentation Threshold"
HKR, Ndi\params\Frag_Threshold, default, 0, "2346"
HKR, Ndi\params\Frag_Threshold, type, 0, "int"
HKR, Ndi\params\Frag_Threshold, min, 0, "256"
HKR, Ndi\params\Frag_Threshold, max, 0, "2346"
HKR, Ndi\params\Frag_Threshold, step, 0, "1"
HKR, , Frag_Threshold, 0, "2346"
HKR, Ndi\params\PreambleType, ParamDesc, 0, "Preamble Type"
HKR, Ndi\params\PreambleType, default, 0, "0"
HKR, Ndi\params\PreambleType, type, 0, "enum"
HKR, Ndi\params\PreambleType\enum, 0, 0, "Long"
HKR, Ndi\params\PreambleType\enum, 1, 0, "Short"
HKR, Ndi\params\PreambleType\enum, 2, 0, "Auto"
HKR, , PreambleType, 0, "2"
HKR,Ndi\params\PowerMgmtMode, ParamDesc, 0,"802.11 Power Save"
HKR,Ndi\params\PowerMgmtMode, type, 0,"enum"
HKR,Ndi\params\PowerMgmtMode, default, 0,"0"
HKR,Ndi\params\PowerMgmtMode\enum, 0, 0,"Disabled"
HKR,Ndi\params\PowerMgmtMode\enum, 1, 0,"Enabled"
HKR,, PowerMgmtMode, 0,"0"
[CopyFile.Sys]
[PCMCIAFVNETR.NT.Reg]
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi, Service, 0, "PCMCIAFVNETR"
[PCMCIAFVNETR.Service]
DisplayName=%PCMCIAFVNETR.DisplayName%
ServiceType=1
StartType=3
ErrorControl=1
ServiceBinary=%12%\fvnetr.sys
LoadOrderGroup=NDIS
[Common.EventLog]
AddReg=Common.AddEventLog.Reg
[Common.AddEventLog.Reg]
HKR, , EventMessageFile, 0x00020000, %%SystemRoot%%\System32\netevent.dll, %%SystemRoot%%\System32\drivers\netusbxp.sys
HKR, , TypesSupported , 0x00010001, 7
[CopyFile.NT.Sys]
netusb.sys
fvnetr.sys
[BCM43XX]
AddReg=BCM43XX.win.reg, BCM43XX.win.brcm.reg, common.reg, b.options.reg, bg.options.reg
;CpyFiles=BCM43XX.sys.files
DriverVer=05/26/2003, 3.20.21.0
[BCM43PCM]
AddReg=BCM43XX.win.reg, BCM43XX.win.brcm.reg, common.reg, b.options.reg, bg.options.reg
;CpyFiles=BCM43XX.sys.files
DriverVer=05/26/2003, 3.20.21.0
[BCM43XG]
AddReg=BCM43XX.win.reg, BCM43XX.win.brcm.reg, common.reg, g.options.reg, bg.options.reg
;CpyFiles=BCM43XX.sys.files
DriverVer=05/26/2003, 3.20.21.0
[BCM43XA]
AddReg=BCM43XX.win.reg, BCM43XX.win.brcm.reg, common.reg, a.options.reg
;CpyFiles=BCM43XX.sys.files
DriverVer=05/26/2003, 3.20.21.0
[BCM43XM]
AddReg=BCM43XX.win.reg, BCM43XX.win.brcm.reg, common.reg, bag.options.reg
;CpyFiles=BCM43XX.sys.files
DriverVer=05/26/2003, 3.20.21.0
[BCM43XX.win.reg]
HKR, Ndi, DeviceID, , "PCI\VEN_14E4&DEV_4320&SUBSYS_00131737"
HKR, Ndi, DeviceID, , "PCI\VEN_14E4&DEV_4320&SUBSYS_906E182D"
HKR, Ndi, DeviceID, , "PCI\VEN_14E4&DEV_4320&SUBSYS_9064182D"
HKR, Ndi, DeviceID, , "PCI\VEN_14E4&DEV_4320&SUBSYS_041714E4"
HKR, Ndi, DeviceID, , "PCI\VEN_14E4&DEV_4320&SUBSYS_041814E4"
HKR, , EnumPropPages, 0, "netdi.dll,EnumPropPages"
HKR, NDIS, MajorNdisVersion, 1, 03
HKR, NDIS, MinorNdisVersion, 1, 0A
HKR, NDIS, LogDriverName, , "BCM43XX"
HKR, NDIS, MajorDriverVersion, 1, 1
HKR, NDIS, MinorDriverVersion, 1, 0
HKR, Ndi\Install, , , "BCM43XX.ndi.install"
HKR, Ndi\Interfaces, DefUpper, 0, "ndis3"
HKR, Ndi\Interfaces, DefLower, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis3"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
[BCM43XX.win.brcm.reg]
HKR, Ndi, HelpText, , %BCM43XX_HELP%
[BCM43XX.ndi.install]
AddReg=BCM43XX.ndi.reg
[BCM43XX.ndi.reg]
HKR, , DevLoader, 0, "*ndis"
HKR, , DeviceVxDs, 0, %DEFAULT_WIN9X_SYS%
[BCM43XX.sys.files]
[BCM43XX.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, b.options.reg, bg.options.reg
;CpyFiles=BCM43XX.files.NT
DriverVer=05/26/2003, 3.20.21.0
[BCM43PCM.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=8 ; PCMCIA bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, b.options.reg, bg.options.reg
;CpyFiles=BCM43XX.files.NT
DriverVer=05/26/2003, 3.20.21.0
[BCM43XG.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, g.options.reg, bg.options.reg
;CpyFiles=BCM43XX.files.NT
DriverVer=05/26/2003, 3.20.21.0
[BCM43XA.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, a.options.reg
;CpyFiles=BCM43XX.files.NT
DriverVer=05/26/2003, 3.20.21.0
[BCM43XM.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, bag.options.reg
;CpyFiles=BCM43XX.files.NT
DriverVer=05/26/2003, 3.20.21.0
[BCM43XX.NT.Services]
AddService=BCM43XX, 2, BCM43XX.Service, common.EventLog
[BCM43PCM.NT.Services]
AddService=BCM43XX, 2, BCM43XX.Service, common.EventLog
[BCM43XG.NT.Services]
AddService=BCM43XX, 2, BCM43XX.Service, common.EventLog
[BCM43XA.NT.Services]
AddService=BCM43XX, 2, BCM43XX.Service, common.EventLog
[BCM43XM.NT.Services]
AddService=BCM43XX, 2, BCM43XX.Service, common.EventLog
[BCM43XX.reg]
HKR, Ndi\Interfaces, UpperRange, , "ndis5"
HKR, Ndi\Interfaces, LowerRange, , "ethernet"
[BCM43XX.brcm.reg]
HKR, Ndi, HelpText, , %BCM43XX_HELP%
HKR, Ndi, Service, 0, "BCM43XX"
[BCM43XX.Service]
DisplayName=%BCM43XX.Service.DispName%
ServiceType=1 ; %SERVICE_KERNEL_DRIVER%
StartType=3 ; %SERVICE_DEMAND_START%
ErrorControl=1 ; %SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\bcmwl5.sys
LoadOrderGroup=NDIS
[common.EventLog]
AddReg=common.AddEventLog.reg
[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported, 0x00010001, 7
[BCM43XX.files.NT]
BCMWL5.SYS,,,2
[common.reg]
HKR, Ndi\params\RadioState, ParamDesc, 0, "Radio Enable/Disable"
HKR, Ndi\params\RadioState, type, 0, "enum"
HKR, Ndi\params\RadioState\enum, "1", 0, "Disabled"
HKR, Ndi\params\RadioState\enum, "0", 0, "Enabled"
HKR, Ndi\params\RadioState,default,,"0"
HKR, Ndi\params\PowerSaveMode, ParamDesc, 0, "Power Save Mode"
HKR, Ndi\params\PowerSaveMode, type, 0, "enum"
HKR, Ndi\params\PowerSaveMode\enum, "0", 0, "Disabled"
HKR, Ndi\params\PowerSaveMode\enum, "1", 0, "Enabled"
HKR, Ndi\params\PowerSaveMode,default,,"0"
HKR, Ndi\params\frag, ParamDesc, 0, "Fragmentation Threshold"
HKR, Ndi\params\frag,type,0,"dword"
HKR, Ndi\params\frag,min,,"256"
HKR, Ndi\params\frag,max,,"2346"
HKR, Ndi\params\frag,default,,"2346"
HKR, Ndi\params\rts, ParamDesc, 0, "RTS Threshold"
HKR, Ndi\params\rts,type,0,"dword"
HKR, Ndi\params\rts,min,,"0"
HKR, Ndi\params\rts,max,,"2347"
HKR, Ndi\params\rts,default,,"2347"
HKR, Ndi\params\NetworkAddress, ParamDesc, 0, "Locally Administered MAC Address"
HKR, Ndi\params\NetworkAddress, type, 0, "edit"
HKR, Ndi\params\NetworkAddress, LimitText, 0, "12"
HKR, Ndi\params\NetworkAddress, UpperCase, 0, "1"
HKR, Ndi\params\NetworkAddress, default, 0, ""
HKR, Ndi\params\NetworkAddress, optional, 0, "1"
HKR, Ndi\params\PwrOut, ParamDesc, 0, "Power Output"
HKR, Ndi\params\PwrOut, type, 0, "enum"
HKR, Ndi\params\PwrOut\enum, "100", 0, "100%"
HKR, Ndi\params\PwrOut\enum, "75", 0, "75%"
HKR, Ndi\params\PwrOut\enum, "50", 0, "50%"
HKR, Ndi\params\PwrOut\enum, "25", 0, "25%"
HKR, Ndi\params\PwrOut,default,,"100"
HKR, ,"EnableAutoConnect", 0, "0"
HKR, ,"WEP", 0, ""
HKR, ,"NetworkType", 0, "-1"
HKR, ,"SSID", 0, ""
HKR, ,"gpio0", 0, "-1"
HKR, ,"gpio1", 0, "-1"
HKR, ,"gpio2", 0, "-1"
HKR, ,"gpio3", 0, "-1"
HKR, ,"scan_channel_time", 0, "-1"
HKR, ,"scan_unassoc_time", 0, "-1"
HKR, ,"scan_home_time", 0, "-1"
HKR, ,"scan_passes", 0, "-1"
HKR, ,"BadFramePreempt", 0, "0"
HKR, ,"Interference_Mode", 0, "-1"
HKR, Ndi\params\antdiv, ParamDesc, 0, "Antenna Diversity"
HKR, Ndi\params\antdiv, type, 0, "enum"
HKR, Ndi\params\antdiv\enum, "-1", 0, "Auto"
HKR, Ndi\params\antdiv,default,,"-1"
[b.options.reg]
HKR, Ndi\params\PLCPHeader, ParamDesc, 0, "PLCP Header"
HKR, Ndi\params\PLCPHeader, type, 0, "enum"
HKR, Ndi\params\PLCPHeader\enum, "-1", 0, "Long"
HKR, Ndi\params\PLCPHeader\enum, "0", 0, "Auto (Short/Long)"
HKR, Ndi\params\PLCPHeader,default,,"0"
HKR, Ndi\params\Rate, ParamDesc, 0, "Rate"
HKR, Ndi\params\Rate, type, 0, "enum"
HKR, Ndi\params\Rate\enum, "0", 0, "Use best rate"
HKR, Ndi\params\Rate\enum, "2", 0, " 1"
HKR, Ndi\params\Rate\enum, "4", 0, " 2"
HKR, Ndi\params\Rate\enum, "11", 0, " 5.5"
HKR, Ndi\params\Rate\enum, "22", 0, "11"
HKR, Ndi\params\Rate,default,,"0"
HKR, Ndi\params\Locale, ParamDesc, 0, "Locale"
HKR, Ndi\params\Locale, type, 0, "enum"
HKR, Ndi\params\Locale\enum, "0", 0, "Worldwide"
HKR, Ndi\params\Locale\enum, "1", 0, "Thailand"
HKR, Ndi\params\Locale\enum, "2", 0, "Israel"
HKR, Ndi\params\Locale\enum, "3", 0, "Jordan"
HKR, Ndi\params\Locale\enum, "5", 0, "Japan"
HKR, Ndi\params\Locale,default,,"15"
[g.options.reg]
HKR, Ndi\params\RoamTrigger, ParamDesc, 0, "Roaming Decision"
HKR, Ndi\params\RoamTrigger, type, 0, "enum"
HKR, Ndi\params\RoamTrigger\enum, "-60", 0, "Optimize Bandwidth"
HKR, Ndi\params\RoamTrigger\enum, "-70", 0, "Default"
HKR, Ndi\params\RoamTrigger\enum, "-80", 0, "Optimize Distance"
HKR, Ndi\params\RoamTrigger,default,,"-70"
HKR, Ndi\params\PLCPHeader, ParamDesc, 0, "BSS PLCP Header"
HKR, Ndi\params\PLCPHeader, type, 0, "enum"
HKR, Ndi\params\PLCPHeader\enum, "-1", 0, "Long"
HKR, Ndi\params\PLCPHeader\enum, "0", 0, "Auto (Short/Long)"
HKR, Ndi\params\PLCPHeader,default,,"0"
HKR, Ndi\params\IBSSGMode, ParamDesc, 0, "IBSS 54g(tm) Mode"
HKR, Ndi\params\IBSSGMode, type, 0, "enum"
HKR, Ndi\params\IBSSGMode\enum, "0", 0, "802.11b Only"
HKR, Ndi\params\IBSSGMode\enum, "1", 0, "54g - LRS"
HKR, Ndi\params\IBSSGMode\enum, "2", 0, "54g - Auto"
HKR, Ndi\params\IBSSGMode\enum, "4", 0, "54g - Performance"
HKR, Ndi\params\IBSSGMode,default,,"0"
HKR, Ndi\params\IBSSGProtection, ParamDesc, 0, "IBSS 54g(tm) Protection Mode"
HKR, Ndi\params\IBSSGProtection, type, 0, "enum"
HKR, Ndi\params\IBSSGProtection\enum, "0", 0, "Disabled"
HKR, Ndi\params\IBSSGProtection\enum, "2", 0, "Auto"
HKR, Ndi\params\IBSSGProtection,default,,"2"
HKR, Ndi\params\Locale, ParamDesc, 0, "Locale"
HKR, Ndi\params\Locale, type, 0, "enum"
HKR, Ndi\params\Locale\enum, "0", 0, "Worldwide"
HKR, Ndi\params\Locale\enum, "1", 0, "Thailand"
HKR, Ndi\params\Locale\enum, "2", 0, "Israel"
HKR, Ndi\params\Locale\enum, "3", 0, "Jordan"
HKR, Ndi\params\Locale\enum, "5", 0, "Japan"
HKR, Ndi\params\Locale\enum, "6", 0, "USA"
HKR, Ndi\params\Locale,default,,"15"
HKR, Ndi\params\Rate, ParamDesc, 0, "Rate"
HKR, Ndi\params\Rate, type, 0, "enum"
HKR, Ndi\params\Rate\enum, "0", 0, "Use best rate"
HKR, Ndi\params\Rate\enum, "2", 0, " 1"
HKR, Ndi\params\Rate\enum, "4", 0, " 2"
HKR, Ndi\params\Rate\enum, "11", 0, " 5.5"
HKR, Ndi\params\Rate\enum, "12", 0, " 6"
HKR, Ndi\params\Rate\enum, "18", 0, " 9"
HKR, Ndi\params\Rate\enum, "22", 0, "11"
HKR, Ndi\params\Rate\enum, "24", 0, "12"
HKR, Ndi\params\Rate\enum, "36", 0, "18"
HKR, Ndi\params\Rate\enum, "48", 0, "24"
HKR, Ndi\params\Rate\enum, "72", 0, "36"
HKR, Ndi\params\Rate\enum, "96", 0, "48"
HKR, Ndi\params\Rate\enum, "108",0, "54"
HKR, Ndi\params\Rate,default,,"0"
[bg.options.reg]
HKR, Ndi\params\Channel, ParamDesc, 0, "IBSS Channel Number"
HKR, Ndi\params\Channel, default, 0, "11"
HKR, Ndi\params\Channel, min, 0, "1"
HKR, Ndi\params\Channel, max, 0, "14"
HKR, Ndi\params\Channel, step, 0, "1"
HKR, Ndi\params\Channel, base, 0, "10"
HKR, Ndi\params\Channel, type, 0, "int"
[a.options.reg]
HKR, Ndi\params\Locale, ParamDesc, 0, "Locale"
HKR, Ndi\params\Locale, type, 0, "enum"
HKR, Ndi\params\Locale\enum, "0", 0, "Worldwide"
HKR, Ndi\params\Locale\enum, "1", 0, "Thailand"
HKR, Ndi\params\Locale\enum, "2", 0, "Israel"
HKR, Ndi\params\Locale\enum, "3", 0, "Jordan"
HKR, Ndi\params\Locale\enum, "5", 0, "Japan"
HKR, Ndi\params\Locale\enum, "6", 0, "USA"
HKR, Ndi\params\Locale,default,,"15"
HKR, Ndi\params\Rate, ParamDesc, 0, "Rate"
HKR, Ndi\params\Rate, type, 0, "enum"
HKR, Ndi\params\Rate\enum, "0", 0, "Use best rate"
HKR, Ndi\params\Rate\enum, "12", 0, " 6"
HKR, Ndi\params\Rate\enum, "18", 0, " 9"
HKR, Ndi\params\Rate\enum, "24", 0, "12"
HKR, Ndi\params\Rate\enum, "36", 0, "18"
HKR, Ndi\params\Rate\enum, "48", 0, "24"
HKR, Ndi\params\Rate\enum, "72", 0, "36"
HKR, Ndi\params\Rate\enum, "96", 0, "48"
HKR, Ndi\params\Rate\enum, "108",0, "54"
HKR, Ndi\params\Rate,default,,"0"
HKR, Ndi\params\Channel, ParamDesc, 0, "IBSS Channel Number"
HKR, Ndi\params\Channel, type, 0, "enum"
HKR, Ndi\params\Channel\enum, "36", 0, " 36"
HKR, Ndi\params\Channel\enum, "40", 0, " 40"
HKR, Ndi\params\Channel\enum, "44", 0, " 44"
HKR, Ndi\params\Channel\enum, "48", 0, " 48"
HKR, Ndi\params\Channel\enum, "52", 0, " 52"
HKR, Ndi\params\Channel\enum, "56", 0, " 56"
HKR, Ndi\params\Channel\enum, "60", 0, " 60"
HKR, Ndi\params\Channel\enum, "64", 0, " 64"
HKR, Ndi\params\Channel\enum, "100", 0, "100"
HKR, Ndi\params\Channel\enum, "104", 0, "104"
HKR, Ndi\params\Channel\enum, "108", 0, "108"
HKR, Ndi\params\Channel\enum, "112", 0, "112"
HKR, Ndi\params\Channel\enum, "116", 0, "116"
HKR, Ndi\params\Channel\enum, "120", 0, "120"
HKR, Ndi\params\Channel\enum, "124", 0, "124"
HKR, Ndi\params\Channel\enum, "128", 0, "128"
HKR, Ndi\params\Channel\enum, "132", 0, "132"
HKR, Ndi\params\Channel\enum, "136", 0, "136"
HKR, Ndi\params\Channel\enum, "140", 0, "140"
HKR, Ndi\params\Channel\enum, "184", 0, "184"
HKR, Ndi\params\Channel\enum, "188", 0, "188"
HKR, Ndi\params\Channel\enum, "192", 0, "192"
HKR, Ndi\params\Channel\enum, "196", 0, "196"
HKR, Ndi\params\Channel\enum, "200", 0, "200"
HKR, Ndi\params\Channel\enum, "204", 0, "204"
HKR, Ndi\params\Channel\enum, "208", 0, "208"
HKR, Ndi\params\Channel\enum, "212", 0, "212"
HKR, Ndi\params\Channel\enum, "216", 0, "216"
HKR, Ndi\params\Channel, default, 0, "36"
[bag.options.reg]
HKR, Ndi\params\RoamTrigger, ParamDesc, 0, "Roaming Decision"
HKR, Ndi\params\RoamTrigger, type, 0, "enum"
HKR, Ndi\params\RoamTrigger\enum, "-60", 0, "Optimize Bandwidth"
HKR, Ndi\params\RoamTrigger\enum, "-70", 0, "Default"
HKR, Ndi\params\RoamTrigger\enum, "-80", 0, "Optimize Distance"
HKR, Ndi\params\RoamTrigger,default,,"-70"
HKR, Ndi\params\PLCPHeader, ParamDesc, 0, "BSS PLCP Header"
HKR, Ndi\params\PLCPHeader, type, 0, "enum"
HKR, Ndi\params\PLCPHeader\enum, "-1", 0, "Long"
HKR, Ndi\params\PLCPHeader\enum, "0", 0, "Auto (Short/Long)"
HKR, Ndi\params\PLCPHeader,default,,"0"
HKR, Ndi\params\band, ParamDesc, 0, "Disable Bands"
HKR, Ndi\params\band, type, 0, "enum"
HKR, Ndi\params\band\enum, "0", 0, "None"
HKR, Ndi\params\band\enum, "1", 0, "Disable 802.11g/b"
HKR, Ndi\params\band\enum, "2", 0, "Disable 802.11a"
HKR, Ndi\params\band,default,,"0"
HKR, Ndi\params\Locale, ParamDesc, 0, "Locale"
HKR, Ndi\params\Locale, type, 0, "enum"
HKR, Ndi\params\Locale\enum, "0", 0, "Worldwide"
HKR, Ndi\params\Locale\enum, "1", 0, "Thailand"
HKR, Ndi\params\Locale\enum, "2", 0, "Israel"
HKR, Ndi\params\Locale\enum, "3", 0, "Jordan"
HKR, Ndi\params\Locale\enum, "5", 0, "Japan"
HKR, Ndi\params\Locale\enum, "6", 0, "USA"
HKR, Ndi\params\Locale,default,,"15"
HKR, Ndi\params\AssocPref, ParamDesc, 0, "Association Preference"
HKR, Ndi\params\AssocPref, type, 0, "enum"
HKR, Ndi\params\AssocPref\enum, "0", 0, "None"
HKR, Ndi\params\AssocPref\enum, "1", 0, "Prefer 802.11a"
HKR, Ndi\params\AssocPref\enum, "2", 0, "Prefer 802.11g/b"
HKR, Ndi\params\AssocPref,default,,"0"
HKR, Ndi\params\RoamPref, ParamDesc, 0, "Roaming Preference"
HKR, Ndi\params\RoamPref, type, 0, "enum"
HKR, Ndi\params\RoamPref\enum, "0", 0, "None"
HKR, Ndi\params\RoamPref\enum, "1", 0, "Stay In Band"
HKR, Ndi\params\RoamPref,default,,"0"
HKR, Ndi\params\IBSSGMode, ParamDesc, 0, "IBSS 54g(tm) Mode"
HKR, Ndi\params\IBSSGMode, type, 0, "enum"
HKR, Ndi\params\IBSSGMode\enum, "0", 0, "802.11b Only"
HKR, Ndi\params\IBSSGMode\enum, "1", 0, "54g - LRS"
HKR, Ndi\params\IBSSGMode\enum, "2", 0, "54g - Auto"
HKR, Ndi\params\IBSSGMode\enum, "4", 0, "54g - Performance"
HKR, Ndi\params\IBSSGMode,default,,"2"
HKR, Ndi\params\IBSSGProtection, ParamDesc, 0, "IBSS 54g(tm) Protection Mode"
HKR, Ndi\params\IBSSGProtection, type, 0, "enum"
HKR, Ndi\params\IBSSGProtection\enum, "0", 0, "Disabled"
HKR, Ndi\params\IBSSGProtection\enum, "2", 0, "Auto"
HKR, Ndi\params\IBSSGProtection,default,,"2"
HKR, Ndi\params\Rate, ParamDesc, 0, "Rate"
HKR, Ndi\params\Rate, type, 0, "enum"
HKR, Ndi\params\Rate\enum, "0", 0, "Use best rate"
HKR, Ndi\params\Rate\enum, "2", 0, " 1"
HKR, Ndi\params\Rate\enum, "4", 0, " 2"
HKR, Ndi\params\Rate\enum, "11", 0, " 5.5"
HKR, Ndi\params\Rate\enum, "12", 0, " 6"
HKR, Ndi\params\Rate\enum, "18", 0, " 9"
HKR, Ndi\params\Rate\enum, "22", 0, "11"
HKR, Ndi\params\Rate\enum, "24", 0, "12"
HKR, Ndi\params\Rate\enum, "36", 0, "18"
HKR, Ndi\params\Rate\enum, "48", 0, "24"
HKR, Ndi\params\Rate\enum, "72", 0, "36"
HKR, Ndi\params\Rate\enum, "96", 0, "48"
HKR, Ndi\params\Rate\enum, "108",0, "54"
HKR, Ndi\params\Rate,default,,"0"
HKR, Ndi\params\Channel, ParamDesc, 0, "IBSS Channel Number"
HKR, Ndi\params\Channel, type, 0, "enum"
HKR, Ndi\params\Channel\enum, "1", 0, " 1"
HKR, Ndi\params\Channel\enum, "2", 0, " 2"
HKR, Ndi\params\Channel\enum, "3", 0, " 3"
HKR, Ndi\params\Channel\enum, "4", 0, " 4"
HKR, Ndi\params\Channel\enum, "5", 0, " 5"
HKR, Ndi\params\Channel\enum, "6", 0, " 6"
HKR, Ndi\params\Channel\enum, "7", 0, " 7"
HKR, Ndi\params\Channel\enum, "8", 0, " 8"
HKR, Ndi\params\Channel\enum, "9", 0, " 9"
HKR, Ndi\params\Channel\enum, "10", 0, " 10"
HKR, Ndi\params\Channel\enum, "11", 0, " 11"
HKR, Ndi\params\Channel\enum, "12", 0, " 12"
HKR, Ndi\params\Channel\enum, "13", 0, " 13"
HKR, Ndi\params\Channel\enum, "14", 0, " 14"
HKR, Ndi\params\Channel\enum, "36", 0, " 36"
HKR, Ndi\params\Channel\enum, "40", 0, " 40"
HKR, Ndi\params\Channel\enum, "44", 0, " 44"
HKR, Ndi\params\Channel\enum, "48", 0, " 48"
HKR, Ndi\params\Channel\enum, "52", 0, " 52"
HKR, Ndi\params\Channel\enum, "56", 0, " 56"
HKR, Ndi\params\Channel\enum, "60", 0, " 60"
HKR, Ndi\params\Channel\enum, "64", 0, " 64"
HKR, Ndi\params\Channel\enum, "100", 0, "100"
HKR, Ndi\params\Channel\enum, "104", 0, "104"
HKR, Ndi\params\Channel\enum, "108", 0, "108"
HKR, Ndi\params\Channel\enum, "112", 0, "112"
HKR, Ndi\params\Channel\enum, "116", 0, "116"
HKR, Ndi\params\Channel\enum, "120", 0, "120"
HKR, Ndi\params\Channel\enum, "124", 0, "124"
HKR, Ndi\params\Channel\enum, "128", 0, "128"
HKR, Ndi\params\Channel\enum, "132", 0, "132"
HKR, Ndi\params\Channel\enum, "136", 0, "136"
HKR, Ndi\params\Channel\enum, "140", 0, "140"
HKR, Ndi\params\Channel\enum, "184", 0, "184"
HKR, Ndi\params\Channel\enum, "188", 0, "188"
HKR, Ndi\params\Channel\enum, "192", 0, "192"
HKR, Ndi\params\Channel\enum, "196", 0, "196"
HKR, Ndi\params\Channel\enum, "200", 0, "200"
HKR, Ndi\params\Channel\enum, "204", 0, "204"
HKR, Ndi\params\Channel\enum, "208", 0, "208"
HKR, Ndi\params\Channel\enum, "212", 0, "212"
HKR, Ndi\params\Channel\enum, "216", 0, "216"
HKR, Ndi\params\Channel, default, 0, "11"
[CopyFile.XP.Sys]
fvnetrxp.sys
netusbxp.sys
[DestinationDirs]
DefaultDestDir=11
BCM43XX.sys.files=11
BCM43XX.files.NT=12
CopyFile.Sys=11
CopyFile.NT.Sys=12
CopyFile.XP.Sys=12
NT.CopyFiles=12 ; system32\drivers subdirectory on NT
win9x.CopyFiles=11 ; system32 subdirectory on win9x
RT2400.Apps=11
RT2400CoInstallFile=11
[NT.CopyFiles]
RT2400.sys ; NT Installation
[SourceDisksNames]
1=%BCM43XX.DiskName%,,
1=%DriverDisketteName%,,
1= %INSTALL_DISK_STR%,,
[SourceDisksFiles]
BCMWL5.SYS=1
netusb.sys=1
netusbxp.sys=1
fvnetr.sys=1
fvnetrxp.sys=1
RT2400.sys=1
[SourceDisksFiles.X86] ; Win2k/Xp
[Strings]
VER_VENDOR_STR="Sitecom"
VER_VENDOR_NAME_STR="Sitecom Corporation"
PCMCIAFVNET3V.DeviceDesc="IEEE 802.11b Network LAN PC Card 2.6"
PCMCIAFVNET5V.DeviceDesc="IEEE 802.11 Wireless LAN PC Card 2.6"
PCMCIAFVNETR5V.DeviceDesc="IEEE 802.11 Wireless LAN PC Card 2.6"
PCMCIAFVNETR.DisplayName="IEEE 802.11 Wireless LAN PC Card 2.6"
PCMCIAFVNETRXP.DisplayName="IEEE 802.11 Wireless LAN PC Card 2.6"
USBNET.DeviceDesc="IEEE 802.11 Wireless LAN USB 2.6"
USBNET.DisplayName="Instant Wireless USB Network Adapter ver.2.6 Driver"
USBNETXP.DisplayName="Instant Wireless USB XP Network Adapter ver.2.6 Driver"
USBFVNETR.DisplayName="Instant Wireless USB Network Adapter ver.2.6 Driver"
DriverDisketteName="ATMEL PCMCIA FastVNET-R Drivers Disk"
Help_Text="VirtualNET lets you set up easily and operate a Wireless LAN compliant with 802.11 Standard. It operates in the license free 2.4 GHz ISM band and achieves a peak data rate of 11 Mbs."
ChannelStr="Channel"
RateStr="Rate"
Fixed1Str="Fixed 1 Mbps"
Fixed2Str="Fixed 2 Mbps"
Fixed55Str="Fixed 5.5 Mbps"
Fixed11Str="Fixed 11 Mbps"
AutoStr="Auto"
RTS_Str="RTS Threshold"
FragmentationStr="Fragmentation Threshold"
OperatingModeStr="Operating Mode"
AdHocStr="Ad-Hoc"
InfrastructureStr="Infrastructure"
ESSID_Str="ESSID"
WEP_Key_Str="WEP Key To Use"
KEY1_Str="WEP Key 1"
KEY2_Str="WEP Key 2"
KEY3_Str="WEP Key 3"
KEY4_Str="WEP Key 4"
WEP_Mode_Str="WEP Mode"
Key1Str="Key 1"
Key2Str="Key 2"
Key3Str="Key 3"
Key4Str="Key 4"
DisabledStr="Disabled"
64bit="64-bit"
128bit="128-bit"
WepMandatoryStr="Mandatory"
WepOptionalStr="Optional"
AuthTypeStr="Authentication Type"
OpenSystemStr="Open System"
SharedKeyStr="Shared Key"
AutoAuthStr="Auto"
PreambleStr="Preamble Type"
LongPreambleStr="Long"
ShortPreambleStr="Short"
AutoPreambleStr="Auto"
PowerMgmtStr="Power Mgmt Mode"
ActiveStr="Active"
PSStr="Power Save"
BasicRatesStr="Basic Rates"
BR1Str="1, 2 Mbps"
BR2Str="1, 2, 5.5, 11 Mbps"
BeaconPeriodStr="Beacon Period"
V_BCM="Sitecom"
BCM430B.DeviceDesc="Sitecom Wireless Network PCI Card 54 Mbps WL-110b"
BCM430G.DeviceDesc="Sitecom Wireless Network Cardbus PC Card 54 Mbps WL-100b"
BCM430A.DeviceDesc="Sitecom 802.11a Network Adapter"
BCM430M.DeviceDesc="Sitecom 802.11 Multiband Network Adapter"
BCM43pc.DeviceDesc="Sitecom 802.11b PCMCIA Network Adapter"
BCM43XX_HELP="The Mot 802.11b Network Adapter provides wireless local area networking."
BCM43XX.Service.DispName="Mot 802.11b Network Adapter Driver"
BCM43XX.DiskName="802.11b Network Adapter Install Disk"
DEFAULT_WIN9X_SYS="BCMWL5.SYS"
ADHOC_DEMO_STR="Adhoc Demo Mode"
SHORT_PREAM_STR="Preamble Mode"
RTSTHRESH_STR="RTS Threshold"
FRAGTHRESH_STR="Fragmentation Threshold"
AUTHENT_TYPE_STR="Authentication Algorithm"
LISTENINTERVAL_STR="Listen Interval"
POWER_SAVE_STR="Power Save Mode"
POWER_LEVEL_STR="Power Save Level"
RT2400.DeviceDesc= "Sitecom Wireless PCI Adapter 11Mbps WL-016"
RT2400.Service.DispName= "Sitecom Wireless Driver"
INSTALL_DISK_STR= "Sitecom Wireless LAN Installation Disk"
SSID_DEF_STR="any"
NETWORK_TYPE_DEF_STR="1"
CHANNEL="1"

