
[Version]
Signature="$Chicago$"
Compatible=1
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%Realtek%
CatalogFile.NT=net8187b.cat ;; for WHQL certified
DriverVer=03/31/2010,5.1163.0331.2010
[Manufacturer]
%Realtek%=Realtek,NTx86
[ControlFlags]
ExcludeFromSelect=USB\VID_0BDA&PID_8197&REV_0200
[Realtek.NTamd64]
%RTL8187B.DeviceDesc%=RTL8187B.ndi, USB\VID_0BDA&PID_8197&REV_0200
%RTL8187B.DeviceDesc%=RTL8187B.ndi, USB\VID_0BDA&PID_8198&REV_0200
%RTL8187B.DeviceDesc%=RTL8187B.ndi, USB\VID_0BDA&PID_8199&REV_0200
[Realtek.NTx86]
%RTL8187B.DeviceDesc%=RTL8187B.ndi, USB\VID_0BDA&PID_8197&REV_0200
%RTL8187B.DeviceDesc%=RTL8187B.ndi, USB\VID_0BDA&PID_8198&REV_0200
%RTL8187B.DeviceDesc%=RTL8187B.ndi, USB\VID_0BDA&PID_8199&REV_0200
[Realtek]
%RTL8187B.DeviceDesc%=RTL8187B.ndi, USB\VID_0BDA&PID_8197&REV_0200
%RTL8187B.DeviceDesc%=RTL8187B.ndi, USB\VID_0BDA&PID_8198&REV_0200
%RTL8187B.DeviceDesc%=RTL8187B.ndi, USB\VID_0BDA&PID_8199&REV_0200
[RTL8187B.ndi]
DriverVer=03/29/2010,1163
AddReg=RTL8187B.win.reg, RTL8187B.common.reg, RTLWLAN.reg
;CpyFiles=RTL8187B.CopyFiles98
[RTL8187B.ndi.NT]
AddReg=RTL8187B.nt5.reg, RTL8187B.common.reg, RTLWLAN.reg
Characteristics=0x84
BusType=15
;CpyFiles=RTL8187B.CopyFiles
[RTL8187B.ndi.NT.Services]
AddService=RTL8187B, 2, RTL8187B.nt5.Service, RTL8187B.nt5.EventLog
[RTL8187B.win.reg]
HKR, Ndi, DeviceID, 0, USB\VID_0BDA&PID_8187&REV_0200
HKR,Ndi,CardType,,"PNP"
HKR, , DriverDesc, 0, "Realtek RTL8187B Wireless 802.11g 54Mbps USB 2.0 Network Adapter"
HKR, , DevLoader,,*ndis,*ntkern,*ndis
HKR, , DeviceVxDs,,RTL8187B.sys
HKR, , EnumPropPages, 0, netdi.dll, EnumPropPages
HKR,NDIS,MajorNdisVersion,1,03
HKR,NDIS,MinorNdisVersion,1,0a
HKR,NDIS,LogDriverName,,RTL8187B
HKR,Ndi\Interfaces,DefLower,,"ethernet"
HKR,Ndi\Interfaces,LowerRange,,"ethernet"
HKR,Ndi\Interfaces,DefUpper,,"ndis3"
HKR,Ndi\Interfaces,UpperRange,,"ndis3"
[RTL8187B.nt5.reg]
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5,mdcwifi,wifipro"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi, Service, 0, "RTL8187B"
[RTL8187B.nt5.Service]
DisplayName=%RTL8187B.DeviceDesc.DispName%
ServiceType=1 ; %SERVICE_KERNEL_DRIVER%
StartType=3 ; %SERRVICE_DEMAND_START%
ErrorControl=1 ; %SERRVICE_ERROR_NORMAL%
ServiceBinary=%12%\RTL8187B.sys
LoadOrderGroup=NDIS
[RTL8187B.nt5.EventLog]
AddReg=RTL8187B.nt5.AddEventLog.reg
[RTL8187B.nt5.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported , 0x00010001, 7
[RTL8187B.common.reg]
HKR,Ndi\params\QoS, ParamDesc, 0, %QOS_STR%
HKR,Ndi\params\QoS, type, 0, "enum"
HKR,Ndi\params\QoS, default, 0, "0"
HKR,Ndi\params\QoS\enum, "0", 0, %DISABLE_STR%
HKR,Ndi\params\QoS\enum, "1", 0, %ENABLE_STR%
HKR,defaults,QoS,0,"0"
HKR,,QoS,0,"0"
[RTLWLAN.reg]
HKR,,Channel,0,"10"
HKR,Ndi\params\WirelessMode, ParamDesc, 0, %WL_MODE_STR%
HKR,Ndi\params\WirelessMode, type, 0, "enum"
HKR,Ndi\params\WirelessMode, default, 0, "8"
HKR,Ndi\params\WirelessMode\enum, "2", 0, %IEEE_802_11B_STR%
HKR,Ndi\params\WirelessMode\enum, "4", 0, %IEEE_802_11BG_STR%
HKR,defaults,WirelessMode, 0, "4"
HKR,,WirelessMode, 0, "4"
HKR,Ndi\params\PSPXlinkMode, ParamDesc, 0, %PSP_XLINK_STR%
HKR,Ndi\params\PSPXlinkMode, type, 0, "enum"
HKR,Ndi\params\PSPXlinkMode, default, 0, "0"
HKR,Ndi\params\PSPXlinkMode\enum, "0", 0, %DISABLE_STR%
HKR,Ndi\params\PSPXlinkMode\enum, "1", 0, %ENABLE_STR%
HKR,defaults,PSPXlinkMode,0,"0"
HKR,,PSPXlinkMode,0,"0"
HKR,Ndi\params\Dot11dEnable, ParamDesc, 0, %DOT11_ENABLE_STR%
HKR,Ndi\params\Dot11dEnable, type, 0, "enum"
HKR,Ndi\params\Dot11dEnable, default, 0, "0"
HKR,Ndi\params\Dot11dEnable\enum, "0", 0, %DISABLE_STR%
HKR,Ndi\params\Dot11dEnable\enum, "1", 0, %ENABLE_STR%
HKR,defaults,Dot11dEnable,0,"0"
HKR,,Dot11dEnable,0,"0"
HKR,,bInactivePs,0,"1"
HKR,,DefaultKeyID,,"0"
HKR,,DefaultKey0,,""
HKR,,DefaultKey1,,""
HKR,,DefaultKey2,,""
HKR,,DefaultKey3,,""
[RTL8187B.CopyFiles]
RTL8187B.sys,,,2
[RTL8187B.CopyFiles98]
RTL8187B.sys,,,2
[DestinationDirs]
RTL8187B.CopyFiles98=11
RTL8187B.CopyFiles=12
[SourceDisksFiles]
RTL8187B.sys=1
[SourceDisksNames]
1=%DISKNAME%,,,
[Strings]
Realtek="Realtek Semiconductor Corp."
SSID_STR="SSID"
CHANNEL_STR="Channel"
NETWORK_TYPE_STR="Network Type"
LED_CONTROL_STR="LED Control"
POWER_SAVE_STR="Power Save Mode"
WIFI_IBSS_STR="IBSS Default 11b Mode"
RATE_ADAPTIVE_STR="Rate Adaptive"
QOS_STR="QoS"
WMM_APSD="WMM APSD"
CCX_RM_STR="CCX Radio Measurement"
CCX_OFF_LINE_DUR_UP_LIMIT_STR="CCX Max Off-Line Measurement (0: unlimited)"
FORCE_PRIORITY_STR="Forced Priority"
HW_PARA_STR="Init from HwParaFile"
THREE_WIRE_MODE_STR="Three Wire Programming Mode"
BOARD_TYPE_STR="Board Type"
PROTECTION_MODE_STR="Protection Mode"
TPC_STR="Transmit Power Control"
TPC_POLARITY_STR="TPC Polarity Select"
HIGH_POWER_STR="High Power Mechanism"
INIT_GAIN_STR="Initial Gain State"
CW_MAX_MIN_STR="Contention Window"
PSP_XLINK_STR="PSP XLink Mode"
CHANNEL_PLAN_STR="Channel Plan"
WL_MODE_STR="Wireless Mode"
PREAMBLE_MODE_STR="Preamble Mode"
FRAGTHRESH_STR="Fragmentation Threshold"
RTSTHRESH_STR="RTS Threshold"
DOT11_ENABLE_STR="802.11d"
DISABLE_STR="Disable"
ENABLE_STR="Enable"
CAM_STR="CAM"
MAX_PSP_STR="MAX_PSP"
FAST_PSP_STR="Fast_PSP"
AD_HOC_STR="Ad Hoc"
INFRASTRUCTURE_STR="Infrastructure"
AUTO_SELECT_STR="Auto select"
DOMAIN_FROM_EEPROM_STR="DOMAIN_FROM_EEPROM"
AUTO_STR="Auto"
LONG_PREAMBLE_STR="Long Preamble"
SHORT_PREAMBLE_STR="Short Preamble"
FCC_STR="FCC"
IC_STR="IC"
ETSI_STR="ETSI"
SPAIN_STR="Spain"
FRANCE_STR="France"
MKK_STR="MKK"
MKK1_STR="MKK1"
ISRAEL_STR="Israel"
TELEC_STR="TELEC"
IEEE_802_11A_STR="IEEE 802.11a"
IEEE_802_11B_STR="IEEE 802.11b"
IEEE_802_11BG_STR="IEEE 802.11 b/g"
DISKNAME="Realtek RTL8187B Wireless 802.11b/g 54Mbps USB 2.0 Network Adapter Driver Disk"
RTL8187B.DeviceDesc="Realtek RTL8187B Wireless 802.11b/g 54Mbps USB 2.0 Network Adapter"
RTL8187B.DeviceDesc.DispName="Realtek RTL8187B Wireless 802.11b/g 54Mbps USB 2.0 Network Adapter"

