
[Version]
Signature="$CHICAGO$"
Compatible=1
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%V_3COM%
CatalogFile=netwux96.cat
DriverVer=1/28/2003,1.0.1.14
[Manufacturer]
%V_3COM%=3COM,NTx86,NTx86.5.1
[ControlFlags]
ExcludeFromSelect.NTx86=*
[3COM]
%WLUX96.DeviceDesc%=WLUX96.Ndi,USB\VID_0506&PID_0a01&Rev_0100
[3COM.NTx86]
%WLUX96.DeviceDesc%=WLUX96.Ndi.NT,USB\VID_0506&PID_0a01&Rev_0100
[3COM.NTx86.5.1]
%WLUX96.DeviceDesc%=WLUX96.Ndi.NT.5.1,USB\VID_0506&PID_0a01&Rev_0100
[WLUX96.Ndi]
AddReg=WLUX96.9x.Reg, WLUX96.Params, Advanced.Params
;CpyFiles=CopyFile.NDIS50.Sys, WLUX96.Apps
[WLUX96.Ndi.NT]
Characteristics=0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType=15 ; USB
AddReg=WLUX96.NT.Reg, WLUX96.Params, Advanced.Params
;CpyFiles=CopyFile.NDIS50.NT.Sys, WLUX96.Apps
[WLUX96.Ndi.NT.Services]
AddService=WLUX96, 2, WLUX96.2k.Service, Common.EventLog.NDIS50
[WLUX96.Ndi.NT.CoInstallers]
;CpyFiles=WLUX96CoInstallFiles
AddReg=WLUX96.CoInstallers_AddReg
[WLUX96.Ndi.NT.5.1]
Characteristics=0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType=15 ; USB
AddReg=WLUX96.NT.Reg, WLUX96.Params
;CpyFiles=CopyFile.NDIS51.Sys, WLUX96.Apps
[WLUX96.Ndi.NT.5.1.Services]
AddService=WLUX96, 2, WLUX96.XP.Service, Common.EventLog.NDIS51
[WLUX96.Ndi.NT.5.1.CoInstallers]
;CpyFiles=WLUX96CoInstallFiles
AddReg=WLUX96.CoInstallers_AddReg
[WLUX96.Params]
HKR, Ndi\params\Rate, ParamDesc, 0, "Rate (Mbps)"
HKR, Ndi\params\Rate, default, 0, "4"
HKR, Ndi\params\Rate, type, 0, "enum"
HKR, Ndi\params\Rate\enum, 0, 0, "1"
HKR, Ndi\params\Rate\enum, 1, 0, "2"
HKR, Ndi\params\Rate\enum, 2, 0, "5.5"
HKR, Ndi\params\Rate\enum, 3, 0, "11"
HKR, Ndi\params\Rate\enum, 4, 0, "Auto"
HKR, , Rate, 0, "4"
HKR, Ndi\params\RTS_Threshold, ParamDesc, 0, "RTS Threshold"
HKR, Ndi\params\RTS_Threshold, default, 0, "2347"
HKR, Ndi\params\RTS_Threshold, type, 0, "int"
HKR, Ndi\params\RTS_Threshold, min, 0, "0"
HKR, Ndi\params\RTS_Threshold, max, 0, "2347"
HKR, Ndi\params\RTS_Threshold, step, 0, "1"
HKR, , RTS_Threshold, 0, "2347"
HKR, Ndi\params\Frag_Threshold, ParamDesc, 0, "Fragmentation Threshold"
HKR, Ndi\params\Frag_Threshold, default, 0, "2346"
HKR, Ndi\params\Frag_Threshold, type, 0, "int"
HKR, Ndi\params\Frag_Threshold, min, 0, "256"
HKR, Ndi\params\Frag_Threshold, max, 0, "2346"
HKR, Ndi\params\Frag_Threshold, step, 0, "1"
HKR, , Frag_Threshold, 0, "2346"
HKR, Ndi\params\PreambleType, ParamDesc, 0, "Preamble Type"
HKR, Ndi\params\PreambleType, default, 0, "2"
HKR, Ndi\params\PreambleType, type, 0, "enum"
HKR, Ndi\params\PreambleType\enum, 0, 0, "Long"
HKR, Ndi\params\PreambleType\enum, 1, 0, "Short"
HKR, Ndi\params\PreambleType\enum, 2, 0, "Auto"
HKR, , PreambleType, 0, "2"
HKR,Ndi\params\PowerMgmtMode, ParamDesc, 0,"802.11 Power Save"
HKR,Ndi\params\PowerMgmtMode, type, 0,"enum"
HKR,Ndi\params\PowerMgmtMode, default, 0,"0"
HKR,Ndi\params\PowerMgmtMode\enum, 0, 0,"Disabled"
HKR,Ndi\params\PowerMgmtMode\enum, 1, 0,"Enabled"
HKR,, PowerMgmtMode, 0,"0"
[Advanced.Params]
HKR, Ndi\params\Channel, ParamDesc, 0, "Channel"
HKR, Ndi\params\Channel, default, 0, "3"
HKR, Ndi\params\Channel, type, 0, "int"
HKR, Ndi\params\Channel, min, 0, "1"
HKR, Ndi\params\Channel, max, 0, "14"
HKR, Ndi\params\Channel, step, 0, "1"
HKR, , Channel, 0, "3"
HKR, Ndi\params\Operating_Mode, ParamDesc, 0, "Operating Mode"
HKR, Ndi\params\Operating_Mode, default, 0, "1"
HKR, Ndi\params\Operating_Mode, type, 0, "enum"
HKR, Ndi\params\Operating_Mode\enum, 0, 0, "Ad-Hoc"
HKR, Ndi\params\Operating_Mode\enum, 1, 0, "Infrastructure"
HKR, , Operating_Mode, 0, "1"
HKR, Ndi\params\InternationalRoaming, ParamDesc, 0, "International Roaming"
HKR, Ndi\params\InternationalRoaming, default, 0, "0"
HKR, Ndi\params\InternationalRoaming, type, 0, "enum"
HKR, Ndi\params\InternationalRoaming\enum, 0, 0, "Disabled (Reg. Domain)"
HKR, Ndi\params\InternationalRoaming\enum, 1, 0, "Enabled (Int. Roaming)"
HKR, , InternationalRoaming,0, "0"
HKR, Ndi\params\ESSID, ParamDesc, 0, "ESSID"
HKR, Ndi\params\ESSID, default, 0, ""
HKR, Ndi\params\ESSID, type, 0, "edit"
HKR, Ndi\params\ESSID, LimitText, 0, "32"
HKR, Ndi\params\ESSID, UpperCase, 0, "0"
HKR, , ESSID, 0, ""
HKR, Ndi\params\AuthenticationType, ParamDesc, 0, "Authentication Type"
HKR, Ndi\params\AuthenticationType, default, 0, "2"
HKR, Ndi\params\AuthenticationType, type, 0, "enum"
HKR, Ndi\params\AuthenticationType\enum, 0, 0, "Open System"
HKR, Ndi\params\AuthenticationType\enum, 1, 0, "Shared Key"
HKR, Ndi\params\AuthenticationType\enum, 2, 0, "Auto"
HKR, , AuthenticationType, 0, "2"
HKR, Ndi\params\WEP_Mode, ParamDesc, 0, "WEP Mode"
HKR, Ndi\params\WEP_Mode, default, 0, "0"
HKR, Ndi\params\WEP_Mode, type, 0, "enum"
HKR, Ndi\params\WEP_Mode\enum, 0, 0, "Mandatory"
HKR, Ndi\params\WEP_Mode\enum, 1, 0, "Optional"
HKR, , WEP_Mode, 0, "0"
HKR,Ndi\params\EncryptionLevel, ParamDesc, 0, "Encryption Level"
HKR,Ndi\params\EncryptionLevel, type, 0, "enum"
HKR,Ndi\params\EncryptionLevel, default, 0, "0"
HKR,Ndi\params\EncryptionLevel\enum, 0, 0, "None"
HKR,Ndi\params\EncryptionLevel\enum, 1, 0, "64-bit encryption"
HKR,Ndi\params\EncryptionLevel\enum, 2, 0, "128-bit encryption"
HKR,, EncryptionLevel, 0, "0"
HKR,Ndi\params\WEP_KEY_INDEX, ParamDesc, 0, "WEP Key to use"
HKR,Ndi\params\WEP_KEY_INDEX, type, 0, "enum"
HKR,Ndi\params\WEP_KEY_INDEX, default, 0, "0"
HKR,Ndi\params\WEP_KEY_INDEX\enum, 0, 0, "1"
HKR,Ndi\params\WEP_KEY_INDEX\enum, 1, 0, "2"
HKR,Ndi\params\WEP_KEY_INDEX\enum, 2, 0, "3"
HKR,Ndi\params\WEP_KEY_INDEX\enum, 3, 0, "4"
HKR,, WEP_KEY_INDEX, 0, "0"
HKR,Ndi\params\WEP_KEY_1, ParamDesc, 0, "WEP KEY #1"
HKR,Ndi\params\WEP_KEY_1, default, 0, "00000000000000000000000000"
HKR,Ndi\params\WEP_KEY_1, type, 0, "edit"
HKR,Ndi\params\WEP_KEY_1, LimitText, 0, "26"
HKR,Ndi\params\WEP_KEY_1, UpperCase, 0, "1"
HKR,, WEP_KEY_1, 0, "00000000000000000000000000"
HKR,Ndi\params\WEP_KEY_2, ParamDesc, 0, "WEP KEY #2"
HKR,Ndi\params\WEP_KEY_2, default, 0, "00000000000000000000000000"
HKR,Ndi\params\WEP_KEY_2, type, 0, "edit"
HKR,Ndi\params\WEP_KEY_2, LimitText, 0, "26"
HKR,Ndi\params\WEP_KEY_2, UpperCase, 0, "1"
HKR,, WEP_KEY_2, 0, "00000000000000000000000000"
HKR,Ndi\params\WEP_KEY_3, ParamDesc, 0, "WEP KEY #3"
HKR,Ndi\params\WEP_KEY_3, default, 0, "00000000000000000000000000"
HKR,Ndi\params\WEP_KEY_3, type, 0, "edit"
HKR,Ndi\params\WEP_KEY_3, LimitText, 0, "26"
HKR,Ndi\params\WEP_KEY_3, UpperCase, 0, "1"
HKR,, WEP_KEY_3, 0, "00000000000000000000000000"
HKR,Ndi\params\WEP_KEY_4, ParamDesc, 0, "WEP KEY #4"
HKR,Ndi\params\WEP_KEY_4, default, 0, "00000000000000000000000000"
HKR,Ndi\params\WEP_KEY_4, type, 0, "edit"
HKR,Ndi\params\WEP_KEY_4, LimitText, 0, "26"
HKR,Ndi\params\WEP_KEY_4, UpperCase, 0, "1"
HKR,, WEP_KEY_4, 0, "00000000000000000000000000"
HKR,Ndi\params\BasicRates, ParamDesc, 0, "Basic Rates"
HKR,Ndi\params\BasicRates, type, 0, "enum"
HKR,Ndi\params\BasicRates, default, 0, "1"
HKR,Ndi\params\BasicRates\enum, 0, 0, "1,2 Mbps"
HKR,Ndi\params\BasicRates\enum, 1, 0, "1,2,5.5,11 Mbps"
HKR,, BasicRates, 0, "1"
HKR, Ndi\params\BeaconPeriod, ParamDesc, 0, "Beacon Period"
HKR, Ndi\params\BeaconPeriod, type, 0, "int"
HKR, Ndi\params\BeaconPeriod, default, 0, "100"
HKR, Ndi\params\BeaconPeriod, min, 0, "20"
HKR, Ndi\params\BeaconPeriod, max, 0, "1000"
HKR, Ndi\params\BeaconPeriod, step, 0, "1"
HKR,, BeaconPeriod, 0, "100"
[WLUX96.9x.Reg]
HKR,Ndi,DeviceID,0,USB\VID_0506&PID_0a01&Rev_0100
HKR,Ndi,CardType,,"PNP"
HKR,, DevLoader,,*ndis,*ntkern,*ndis
HKR,, DriverDesc,0,%WLUX96.DeviceDesc%
HKR,, DeviceVxDs,,wlux96e.sys
HKR,, EnumPropPages,0,netdi.dll,EnumPropPages
HKR,NDIS,MajorNdisVersion,1,05
HKR,NDIS,MinorNdisVersion,1,00
HKR,NDIS,LogDriverName,,WLUX96E
HKR,Ndi\Interfaces,DefUpper,,"ndis3"
HKR,Ndi\Interfaces,DefLower,,"ethernet"
HKR,Ndi\Interfaces,UpperRange,,"ndis3"
HKR,Ndi\Interfaces,LowerRange,,"ethernet"
HKR,Ndi,HelpText,,%Help_Text%
[WLUX96.NT.Reg]
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi, Service, 0, "WLUX96"
[WLUX96.2k.Service]
DisplayName=%WLUX96.DisplayName%
ServiceType=1
StartType=3
ErrorControl=1
ServiceBinary=%12%\WLUX96E.SYS
LoadOrderGroup=NDIS
[Ndis50.EventLog]
AddReg=Ndis50.AddEventLog.Reg
[Ndis50.AddEventLog.Reg]
HKR, , EventMessageFile, 0x00020000, %%SystemRoot%%\System32\netevent.dll, %%SystemRoot%%\System32\drivers\wlux96e.sys
HKR, , TypesSupported , 0x00010001, 7
[WLUX96.CoInstallers_AddReg]
[WLUX96.XP.Service]
DisplayName=%WLUX96.DisplayName%
ServiceType=1
StartType=3
ErrorControl=1
ServiceBinary=%12%\WLUX96F.SYS
LoadOrderGroup=NDIS
[Ndis51.EventLog]
AddReg=Ndis51.AddEventLog.Reg
[Ndis51.AddEventLog.Reg]
HKR, , EventMessageFile, 0x00020000, %%SystemRoot%%\System32\netevent.dll, %%SystemRoot%%\System32\drivers\wlux96f.sys
HKR, , TypesSupported , 0x00010001, 7
[CopyFile.NDIS51.Sys]
wlux96f.sys,,,2
[CopyFile.NDIS50.Sys]
wlux96e.sys,,,2
[CopyFile.NDIS50.NT.Sys]
wlux96e.sys,,,2
[WLUX96.Apps]
[WLUX96CoInstallFiles]
[DestinationDirs]
DefaultDestDir=12 ; Drivers directory
CopyFile.NDIS50.Sys=11
CopyFile.NDIS50.NT.Sys=12
CopyFile.NDIS51.Sys=12
WLUX96.Apps=11 ; System directory
WLUX96CoInstallFiles=11 ; System directory
[SourceDisksNames]
50=%DriverDisketteName%,,
[SourceDisksFiles]
wlux96e.sys=50,.,wlux96e.sys,60000
wlux96f.sys=50,.,wlux96f.sys,60000
[Strings]
V_3COM="3COM"
WLUX96.DeviceDesc="3Com 3CRSHEW696 Wireless LAN USB Adapter"
WLUX96.DisplayName="3Com 3CRSHEW696 Wireless LAN USB Adapter"
DriverDisketteName="3Com 3CRSHEW696 Drivers Disk"
Help_Text="3Com 3CRSHEW696 lets you set up easily and operate a Wireless LAN compliant with 802.11 Standard. It operates in the license free 2.4 GHz ISM band and achieves a peak data rate of 11 Mbs."
