
[Version]
Signature="$Windows NT$"
Compatible=1
Provider=%V_AVM%
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
CatalogFile.NT=fwlan.cat
DriverVer=12/28/2006,2.0.6.1647
[Manufacturer]
%V_AVM%=AVM
[ControlFlags]
ExcludeFromSelect=USB\VID_057C&PID_5601
ExcludeFromSelect=USB\VID_057C&PID_6201
[AVM]
%FWLAN.DeviceDesc%=FWLAN, USB\VID_057C&PID_5601
%FWLAN.DeviceDesc2%=FWLAN, USB\VID_057C&PID_6201
[Strings]
V_AVM="AVM GmbH"
FWLAN.DeviceDesc="AVM FRITZ!WLAN USB Stick"
FWLAN.DeviceDesc2="AVM FRITZ!WLAN USB Stick v1.1"
FWLAN.Service.DispName="AVM FRITZ!WLAN"
DiskName="AVM FRITZ!WLAN Installation Disk"
StartProg="client\instwcli.exe"
StartProgReg="SOFTWARE\AVMXXX"
AVMDriverDate="12/28/2006"
[FWLAN.NT]
BusType=15
AddReg=FWLAN.ndi.reg.NT, AVM.Param.Reg, BG.Param.Reg
Characteristics=0x84
;CpyFiles=FWLAN.CopyFiles.NT
[FWLAN.NT.CoInstallers]
AddReg=FWLAN.CoInstallers.reg
;CpyFiles=FWLAN.CopyCoinst
[FWLAN.CoInstallers.reg]
HKR,,InstPath,0,"%01%"
HKR,,StartProg,0,%StartProg%
HKR,,StartProgReg,0,%StartProgReg%
HKR,AVMParams,StartSetup,0,%StartProg%
[FWLAN.CopyCoinst]
[FWLAN.ndi.reg.NT]
HKR, Ndi, Service, 0, "FWLANUSB"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
[FWLAN.NT.Services]
AddService=FWLANUSB, 2, FWLAN.Service, FWLAN.EventLog
[FWLAN.CopyFiles.NT]
fwlanusb.sys
[FWLAN.Service]
DisplayName=%FWLAN.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_DEMAND_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\fwlanusb.sys
LoadOrderGroup=NDIS
[FWLAN.EventLog]
AddReg=FWLAN.AddEventLog.reg
[FWLAN.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported, 0x00010001, 7
[BG.Param.Reg]
HKR, ,dot11SupportedRateMask,, "8"
HKR, ,dot11BasicRateMask,, "1"
HKR,NDI\params\Mode4x,ParamDesc,, "Mode4x"
HKR,NDI\params\Mode4x,type,,"enum"
HKR,NDI\params\Mode4x,default,,"1"
HKR,NDI\params\Mode4x\enum,"0",,"Off"
HKR,NDI\params\Mode4x\enum,"1",,"On"
HKR,NDI\params\dot11NetworkType,ParamDesc,, "Network Type"
HKR,NDI\params\dot11NetworkType,type,,"enum"
HKR,NDI\params\dot11NetworkType,default,,"3"
HKR,NDI\params\dot11NetworkType\enum,"1",,"11b"
HKR,NDI\params\dot11NetworkType\enum,"3",,"11b+g"
HKR, ,dot11DesiredChannel, ,1
[AVM.Param.Reg]
HKR, ,dot11DesiredBSSType,, "1"
HKR, ,DisableSsidPending,, "1"
HKR, ,dot11PowerMode,,"1"
HKR,NDI\params\dot11PowerMode,ParamDesc,,"Power Mode"
HKR,NDI\params\dot11PowerMode,type,,"enum"
HKR,NDI\params\dot11PowerMode,default,,"1"
HKR,NDI\params\dot11PowerMode\enum,"0",,"Continuous Access Mode"
HKR,NDI\params\dot11PowerMode\enum,"1",,"Maximum Power Save"
HKR, Ndi\Params\dot11FragmentationThreshold, ParamDesc, ,"Fragmentation Threshold"
HKR, Ndi\Params\dot11FragmentationThreshold, Type, , "int"
HKR, Ndi\Params\dot11FragmentationThreshold, Default, , "4096"
HKR, Ndi\Params\dot11FragmentationThreshold, Min, , "256"
HKR, Ndi\Params\dot11FragmentationThreshold, Max, , "4096"
HKR, Ndi\Params\dot11FragmentationThreshold, Step, , "1"
HKR, Ndi\Params\dot11FragmentationThreshold, Base, , "10"
HKR, Ndi\Params\dot11RTSThreshold, ParamDesc, ,"RTS Threshold"
HKR, Ndi\Params\dot11RTSThreshold, Type, , "int"
HKR, Ndi\Params\dot11RTSThreshold, Default, , "4096"
HKR, Ndi\Params\dot11RTSThreshold, Min, , "1"
HKR, Ndi\Params\dot11RTSThreshold, Max, , "4096"
HKR, Ndi\Params\dot11RTSThreshold, Step, , "1"
HKR, Ndi\Params\dot11RTSThreshold, Base, , "10"
[DestinationDirs]
DefaultDestDir=12 ; Windows\System32\Drivers
FWLAN.CopyFiles.NT=12 ; Winnt\System32\Drivers Directory ; Win2k
FWLAN.CopyCoinst=11
[SourceDisksNames]
1=%DiskName%,,
[SourceDisksFiles]
fwlanusb.sys=1
[CoinstInfo]
OriginalInfSourcePath=%01%
