
[Version]
DriverVer=Fri 02/01/2002, 1.31.00
Signature="$Chicago$"
Compatible=1
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%VER_VENDOR_STR%
MillenniumPreferred=.ME
[ControlFlags]
ExcludeFromSelect=PCMCIA\ACCTON-WN3301/Cheetah_Wireless_PCMCIA-2D13
ExcludeFromSelect=PCMCIA\ACCTON-WN3301/Cheetah_Wireless_PCMCIA-90BB
ExcludeFromSelect=PCMCIA\ACCTON-WN3301F/G_Wireless_PCMCIA-ECD6
ExcludeFromSelect=PCMCIA\Accton-AC-EW3101-FC84
ExcludeFromSelect=PCMCIA\Accton-AC-EW3101-850A
ExcludeFromSelect=PCI\VEN_1260&DEV_3873&SUBSYS_31011113
ExcludeFromSelect=PCI\VEN_1260&DEV_3873&SUBSYS_36011113
ExcludeFromSelect=PCI\VEN_1638&DEV_1100&SUBSYS_11001638
ExcludeFromSelect=USB\VID_083A&PID_3502
[Manufacturer]
%VER_VENDOR_NAME_STR%=DeviceList
[DeviceList]
%PRISM_PCMCIA1_STR%=PRISM_PCMCIA1, PCMCIA\ACCTON-WN3301/Cheetah_Wireless_PCMCIA-2D13
%PRISM_PCMCIA2_STR%=PRISM_PCMCIA2, PCMCIA\ACCTON-WN3301/Cheetah_Wireless_PCMCIA-90BB
%PRISM_PCMCIA3_STR%=PRISM_PCMCIA2, PCMCIA\ACCTON-WN3301F/G_Wireless_PCMCIA-ECD6
%PRISM_PCMCIA4_STR%=PRISM_PCMCIA3, PCMCIA\Accton-AC-EW3101-FC84
%PRISM_PCMCIA5_STR%=PRISM_PCMCIA4, PCMCIA\Accton-AC-EW3101-850A
%PRISM_PCI1_STR%=PRISM_PCI1, PCI\VEN_1260&DEV_3873&SUBSYS_31011113
%PRISM_PCI2_STR%=PRISM_PCI2, PCI\VEN_1260&DEV_3873&SUBSYS_36011113
%PRISM_PCI3_STR%=PRISM_PCI3, PCI\VEN_1638&DEV_1100&SUBSYS_11001638
%PRISM_USB1_STR%=PRISM_USB1, USB\VID_083A&PID_3502
[PRISM_PCMCIA1] ; Win9x
AddReg=PRISM_PCMCIA1.reg, COMMON_PCMCIA.reg, COMMON_NDIS.reg, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy, PRISM_APPLET.copy, PRISM_NDI.copy
[PRISM_PCMCIA1.ME] ; WinMe
AddReg=PRISM_PCMCIA1.reg, COMMON_PCMCIA.reg, COMMON_NDIS.reg.ME, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.ME, PRISM_APPLET.copy.ME, PRISM_NDI.copy.ME
[PRISM_PCMCIA1.ME.ME] ; WinMe - Same as .ME (Needed for Update Driver)
AddReg=PRISM_PCMCIA1.reg, COMMON_PCMCIA.reg, COMMON_NDIS.reg.ME, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.ME, PRISM_APPLET.copy.ME, PRISM_NDI.copy.ME
[PRISM_PCMCIA1.NT] ; Win2k
AddReg=PRISM_PCMCIA1.reg, COMMON_PCMCIA.reg, COMMON_NDIS.reg.NT, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.NT, PRISM_APPLET.copy.NT
BusType=8 ; PCMCIA
Characteristics= 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[PRISM_PCMCIA1.NT.Services]
AddService="ACTN", 2, PRISM_DRIVER.Service, PRISM_DRIVER.EventLog
[PRISM_PCMCIA1.NT.CoInstallers]
;CpyFiles=PRISM_COINSTALL.copy.NT
AddReg=PRISM_COINSTALL.reg.NT
[PRISM_PCMCIA1.reg]
HKR,Ndi ,DeviceID,0,"PCMCIA\ACCTON-WN3301/Cheetah_Wireless_PCMCIA-2D13"
[PRISM_PCMCIA2] ; Win9x
AddReg=PRISM_PCMCIA2.reg, COMMON_PCMCIA.reg, COMMON_NDIS.reg, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy, PRISM_APPLET.copy, PRISM_NDI.copy
[PRISM_PCMCIA2.ME] ; WinMe
AddReg=PRISM_PCMCIA2.reg, COMMON_PCMCIA.reg, COMMON_NDIS.reg.ME, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.ME, PRISM_APPLET.copy.ME, PRISM_NDI.copy.ME
[PRISM_PCMCIA2.ME.ME] ; WinMe - Same as .ME (Needed for Update Driver)
AddReg=PRISM_PCMCIA2.reg, COMMON_PCMCIA.reg, COMMON_NDIS.reg.ME, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.ME, PRISM_APPLET.copy.ME, PRISM_NDI.copy.ME
[PRISM_PCMCIA2.NT] ; Win2k
AddReg=PRISM_PCMCIA2.reg, COMMON_PCMCIA.reg, COMMON_NDIS.reg.NT, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.NT, PRISM_APPLET.copy.NT
BusType=8 ; PCMCIA
Characteristics= 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[PRISM_PCMCIA2.NT.Services]
AddService="ACTN", 2, PRISM_DRIVER.Service, PRISM_DRIVER.EventLog
[PRISM_PCMCIA2.NT.CoInstallers]
;CpyFiles=PRISM_COINSTALL.copy.NT
AddReg=PRISM_COINSTALL.reg.NT
[PRISM_PCMCIA2.reg]
HKR,Ndi ,DeviceID,0,"PCMCIA\ACCTON-WN3301/Cheetah_Wireless_PCMCIA-90BB"
[PRISM_PCMCIA3] ; Win9x
AddReg=PRISM_PCMCIA3.reg, COMMON_PCMCIA.reg, COMMON_NDIS.reg, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy, PRISM_APPLET.copy, PRISM_NDI.copy
[PRISM_PCMCIA3.ME] ; WinMe
AddReg=PRISM_PCMCIA3.reg, COMMON_PCMCIA.reg, COMMON_NDIS.reg.ME, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.ME, PRISM_APPLET.copy.ME, PRISM_NDI.copy.ME
[PRISM_PCMCIA3.ME.ME] ; WinMe - Same as .ME (Needed for Update Driver)
AddReg=PRISM_PCMCIA3.reg, COMMON_PCMCIA.reg, COMMON_NDIS.reg.ME, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.ME, PRISM_APPLET.copy.ME, PRISM_NDI.copy.ME
[PRISM_PCMCIA3.NT] ; Win2k
AddReg=PRISM_PCMCIA3.reg, COMMON_PCMCIA.reg, COMMON_NDIS.reg.NT, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.NT, PRISM_APPLET.copy.NT
BusType=8 ; PCMCIA
Characteristics= 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[PRISM_PCMCIA3.NT.Services]
AddService="ACTN", 2, PRISM_DRIVER.Service, PRISM_DRIVER.EventLog
[PRISM_PCMCIA3.NT.CoInstallers]
;CpyFiles=PRISM_COINSTALL.copy.NT
AddReg=PRISM_COINSTALL.reg.NT
[PRISM_PCMCIA3.reg]
HKR,Ndi ,DeviceID,0,"PCMCIA\ACCTON-WN3301F/G_Wireless_PCMCIA-ECD6"
[PRISM_PCMCIA4] ; Win9x
AddReg=PRISM_PCMCIA4.reg, COMMON_PCMCIA.reg, COMMON_NDIS.reg, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy, PRISM_APPLET.copy, PRISM_NDI.copy
[PRISM_PCMCIA4.ME] ; WinMe
AddReg=PRISM_PCMCIA4.reg, COMMON_PCMCIA.reg, COMMON_NDIS.reg.ME, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.ME, PRISM_APPLET.copy.ME, PRISM_NDI.copy.ME
[PRISM_PCMCIA4.ME.ME] ; WinMe - Same as .ME (Needed for Update Driver)
AddReg=PRISM_PCMCIA4.reg, COMMON_PCMCIA.reg, COMMON_NDIS.reg.ME, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.ME, PRISM_APPLET.copy.ME, PRISM_NDI.copy.ME
[PRISM_PCMCIA4.NT] ; Win2k
AddReg=PRISM_PCMCIA4.reg, COMMON_PCMCIA.reg, COMMON_NDIS.reg.NT, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.NT, PRISM_APPLET.copy.NT
BusType=8 ; PCMCIA
Characteristics= 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[PRISM_PCMCIA4.NT.Services]
AddService="ACTN", 2, PRISM_DRIVER.Service, PRISM_DRIVER.EventLog
[PRISM_PCMCIA4.NT.CoInstallers]
;CpyFiles=PRISM_COINSTALL.copy.NT
AddReg=PRISM_COINSTALL.reg.NT
[PRISM_PCMCIA4.reg]
HKR,Ndi ,DeviceID,0,"PCMCIA\Accton-AC-EW3101-FC84"
[PRISM_PCMCIA5] ; Win9x
AddReg=PRISM_PCMCIA5.reg, COMMON_PCMCIA.reg, COMMON_NDIS.reg, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy, PRISM_APPLET.copy, PRISM_NDI.copy
[PRISM_PCMCIA5.ME] ; WinME
AddReg=PRISM_PCMCIA5.reg, COMMON_PCMCIA.reg, COMMON_NDIS.reg.ME, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.ME, PRISM_APPLET.copy.ME, PRISM_NDI.copy.ME
[PRISM_PCMCIA5.ME.ME] ; WinME - Same as .ME (Needed for Update Driver)
AddReg=PRISM_PCMCIA5.reg, COMMON_PCMCIA.reg, COMMON_NDIS.reg.ME, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.ME, PRISM_APPLET.copy.ME, PRISM_NDI.copy.ME
[PRISM_PCMCIA5.NT] ; Win2k
AddReg=PRISM_PCMCIA5.reg, COMMON_PCMCIA.reg, COMMON_NDIS.reg.NT, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.NT, PRISM_APPLET.copy.NT
BusType=8 ; PCMCIA
Characteristics= 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[PRISM_PCMCIA5.NT.Services]
AddService="ACTN", 2, PRISM_DRIVER.Service, PRISM_DRIVER.EventLog
[PRISM_PCMCIA5.NT.CoInstallers]
;CpyFiles=PRISM_COINSTALL.copy.NT
AddReg=PRISM_COINSTALL.reg.NT
[PRISM_PCMCIA5.reg]
HKR,Ndi ,DeviceID,0,"PCMCIA\Accton-AC-EW3101-850A"
[PRISM_PCI1] ; Win9x
AddReg=PRISM_PCI1.reg, COMMON_PCI.reg, COMMON_NDIS.reg, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy, PRISM_APPLET.copy, PRISM_NDI.copy
[PRISM_PCI1.ME] ; WinMe
AddReg=PRISM_PCI1.reg, COMMON_PCI.reg, COMMON_NDIS.reg.ME, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.ME, PRISM_APPLET.copy.ME, PRISM_NDI.copy.ME
[PRISM_PCI1.ME.ME] ; WinMe - Same as .ME (Needed for Update Driver)
AddReg=PRISM_PCI1.reg, COMMON_PCI.reg, COMMON_NDIS.reg.ME, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.ME, PRISM_APPLET.copy.ME, PRISM_NDI.copy.ME
[PRISM_PCI1.NT] ; Win2k
AddReg=PRISM_PCI1.reg, COMMON_PCI.reg, COMMON_NDIS.reg.NT, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.NT, PRISM_APPLET.copy.NT
BusType=5 ; PCI
Characteristics= 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[PRISM_PCI1.NT.Services]
AddService="ACTN", 2, PRISM_DRIVER.Service, PRISM_DRIVER.EventLog
[PRISM_PCI1.NT.CoInstallers]
;CpyFiles=PRISM_COINSTALL.copy.NT
AddReg=PRISM_COINSTALL.reg.NT
[PRISM_PCI1.reg]
HKR,Ndi ,DeviceID,0,"PCI\VEN_1260&DEV_3873&SUBSYS_31011113"
[PRISM_PCI2] ; Win9x
AddReg=PRISM_PCI2.reg, COMMON_PCI.reg, COMMON_NDIS.reg, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy, PRISM_APPLET.copy, PRISM_NDI.copy
[PRISM_PCI2.ME] ; WinMe
AddReg=PRISM_PCI2.reg, COMMON_PCI.reg, COMMON_NDIS.reg.ME, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.ME, PRISM_APPLET.copy.ME, PRISM_NDI.copy.ME
[PRISM_PCI2.ME.ME] ; WinMe - Same as .ME (Needed for Update Driver)
AddReg=PRISM_PCI2.reg, COMMON_PCI.reg, COMMON_NDIS.reg.ME, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.ME, PRISM_APPLET.copy.ME, PRISM_NDI.copy.ME
[PRISM_PCI2.NT] ; Win2k
AddReg=PRISM_PCI2.reg, COMMON_PCI.reg, COMMON_NDIS.reg.NT, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.NT, PRISM_APPLET.copy.NT
BusType=5 ; PCI
Characteristics= 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[PRISM_PCI2.NT.Services]
AddService="ACTN", 2, PRISM_DRIVER.Service, PRISM_DRIVER.EventLog
[PRISM_PCI2.NT.CoInstallers]
;CpyFiles=PRISM_COINSTALL.copy.NT
AddReg=PRISM_COINSTALL.reg.NT
[PRISM_PCI2.reg]
HKR,Ndi ,DeviceID,0,"PCI\VEN_1260&DEV_3873&SUBSYS_36011113"
[PRISM_PCI3] ; Win9x
AddReg=PRISM_PCI3.reg, COMMON_PCI.reg, COMMON_NDIS.reg, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy, PRISM_APPLET.copy, PRISM_NDI.copy
[PRISM_PCI3.ME] ; WinMe
AddReg=PRISM_PCI3.reg, COMMON_PCI.reg, COMMON_NDIS.reg.ME, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.ME, PRISM_APPLET.copy.ME, PRISM_NDI.copy.ME
[PRISM_PCI3.ME.ME] ; WinMe - Same as .ME (Needed for Update Driver)
AddReg=PRISM_PCI3.reg, COMMON_PCI.reg, COMMON_NDIS.reg.ME, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.ME, PRISM_APPLET.copy.ME, PRISM_NDI.copy.ME
[PRISM_PCI3.NT] ; Win2k
AddReg=PRISM_PCI3.reg, COMMON_PCI.reg, COMMON_NDIS.reg.NT, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.NT, PRISM_APPLET.copy.NT
BusType=5 ; PCI
Characteristics= 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[PRISM_PCI3.NT.Services]
AddService="ACTN", 2, PRISM_DRIVER.Service, PRISM_DRIVER.EventLog
[PRISM_PCI3.NT.CoInstallers]
;CpyFiles=PRISM_COINSTALL.copy.NT
AddReg=PRISM_COINSTALL.reg.NT
[PRISM_PCI3.reg]
HKR,Ndi ,DeviceID,0,"PCI\VEN_1638&DEV_1100&SUBSYS_11001638"
[PRISM_USB1] ; Win9x
AddReg=PRISM_USB1.reg, COMMON_USB.reg, COMMON_NDIS.reg, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy, PRISM_APPLET.copy, PRISM_NDI.copy
[PRISM_USB1.ME] ; WinMe
AddReg=PRISM_USB1.reg, COMMON_USB.reg, COMMON_NDIS.reg.ME, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.ME, PRISM_APPLET.copy.ME, PRISM_NDI.copy.ME
[PRISM_USB1.ME.ME] ; WinMe - Same as .ME (Needed for Update Driver)
AddReg=PRISM_USB1.reg, COMMON_USB.reg, COMMON_NDIS.reg.ME, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.ME, PRISM_APPLET.copy.ME, PRISM_NDI.copy.ME
[PRISM_USB1.NT] ; Win2k
AddReg=PRISM_USB1.reg, COMMON_USB.reg, COMMON_NDIS.reg.NT, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.NT, PRISM_APPLET.copy.NT
BusType=0 ; USB
Characteristics= 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[PRISM_USB1.NT.Services]
AddService="ACTN_USB", 2, PRISM_USB_DRIVER.Service, PRISM_DRIVER.EventLog
[PRISM_USB1.NT.CoInstallers]
;CpyFiles=PRISM_COINSTALL.copy.NT
AddReg=PRISM_COINSTALL.reg.NT
[PRISM_USB1.reg]
HKR,Ndi ,DeviceID,0,"USB\VID_083A&PID_3502"
[PRISM_COINSTALL.reg.NT]
[PRISM_DRIVER.Service]
DisplayName=%PRISM_SERVICE_DISPLAY%
ServiceType=1 ; SERVICE_KERNEL_DRIVER
StartType=3 ; SERVICE_DEMAND_START
ErrorControl=1 ; NORMAL
ServiceBinary=%12%\ACTNNDS.sys
LoadOrderGroup=NDIS
[PRISM_USB_DRIVER.Service]
DisplayName=%PRISM_USB_SERVICE_DISPLAY%
ServiceType=1 ; SERVICE_KERNEL_DRIVER
StartType=3 ; SERVICE_DEMAND_START
ErrorControl=1 ; NORMAL
ServiceBinary=%12%\ACTNUSB.sys
LoadOrderGroup=NDIS
[PRISM_DRIVER.EventLog]
AddReg=PRISM_DRIVER.EventLog.reg
[PRISM_DRIVER.EventLog.reg]
HKR, ,EventMessageFile ,0x00020000 ,"%%SystemRoot%%\System32\netevent.dll"
HKR, ,TypesSupported ,0x00010001 ,7
[COMMON_PCMCIA.reg]
HKR,NDI ,Service ,0 ,"ACTN"
HKR,NDI ,CardType ,0 ,"PCMCIA"
HKR, ,BusType ,0 ,"8"
HKR, ,DeviceVxDs ,0 ,"ACTNNDS.sys"
HKR, ,EnableIRQSharing ,1 ,01,00,00,00
HKR, ,IOBaseAddress ,1 ,02,00,00,00
HKR, ,InterruptNumber ,1 ,04,00,00,00
[COMMON_PCI.reg]
HKR,NDI ,Service ,0 ,"ACTN"
HKR,NDI ,CardType ,0 ,"PCI"
HKR, ,BusType ,0 ,"5"
HKR, ,DeviceVxDs ,0 ,"ACTNNDS.sys"
HKR, ,EnableIRQSharing ,1 ,01,00,00,00
HKR, ,IOBaseAddress ,1 ,02,00,00,00
HKR, ,InterruptNumber ,1 ,04,00,00,00
[COMMON_USB.reg]
HKR,NDI ,Service ,0 ,"ACTN_USB"
HKR,NDI ,CardType ,0 ,"USB"
HKR, ,BusType ,0 ,"0"
HKR, ,DeviceVxDs ,0 ,"ACTNUSB.sys"
[COMMON_NDIS.reg]
HKR, ,RunningWin9X ,0 ,"1"
HKR, ,DevLoader ,0 ,"*ndis"
HKR, ,EnumPropPages ,0 ,"netdi.dll,EnumPropPages"
HKR,NDI ,NdiInstaller ,0 ,"ACTNCFG.dll,NdiProc"
HKR,NDI\Interfaces ,UpperRange ,0 ,"ndis3"
HKR,NDI\Interfaces ,LowerRange ,0 ,"ethernet"
HKR,NDI\Interfaces ,DefUpper ,0 ,"ndis3"
HKR,NDI\Interfaces ,DefLower ,0 ,"ethernet"
HKR,NDIS ,LogDriverName ,0 ,"ACTN"
HKR,NDIS ,MajorNdisVersion ,1 ,03
HKR,NDIS ,MinorNdisVersion ,1 ,0a
HKR,defaults,PSMode,0,1
HKR,NDI\params\PSMode,,0,1
HKR,Ndi\params\PSMode,default,0,1
HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
HKR,NDI\params\PSMode,type,,enum
HKR,NDI\params\PSMode,flag,1,30,00,00,00
HKR,NDI\params\PSMode\enum,1,,"Disable"
HKR,NDI\params\PSMode\enum,2,,"Always Enable"
HKR,NDI\params\PSMode,optional,0,1
[COMMON_NDIS.reg.ME]
HKR, ,RunningWin9X ,0 ,"1"
HKR, ,DevLoader ,0 ,"*ndis"
HKR, ,EnumPropPages ,0 ,"netdi.dll,EnumPropPages"
HKR,NDI ,NdiInstaller ,0 ,"ACTNCFG.dll,NdiProc"
HKR,NDI\Interfaces ,UpperRange ,0 ,"ndis3"
HKR,NDI\Interfaces ,LowerRange ,0 ,"ethernet"
HKR,NDI\Interfaces ,DefUpper ,0 ,"ndis3"
HKR,NDI\Interfaces ,DefLower ,0 ,"ethernet"
HKR,NDIS ,LogDriverName ,0 ,"ACTN"
HKR,NDIS ,MajorNdisVersion ,1 ,03
HKR,NDIS ,MinorNdisVersion ,1 ,0a
HKR,defaults,PSMode,0,1
HKR,NDI\params\PSMode,,0,1
HKR,Ndi\params\PSMode,default,0,1
HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
HKR,NDI\params\PSMode,type,,enum
HKR,NDI\params\PSMode,flag,1,30,00,00,00
HKR,NDI\params\PSMode\enum,1,,"Disable"
HKR,NDI\params\PSMode\enum,2,,"Always Enable"
HKR,NDI\params\PSMode,optional,0,1
[COMMON_NDIS.reg.NT]
HKR,NDI\Interfaces ,UpperRange ,0 ,"ndis5"
HKR,NDI\Interfaces ,LowerRange ,0 ,"ethernet"
HKR,defaults,PSMode,0,1
HKR,NDI\params\PSMode,,0,1
HKR,Ndi\params\PSMode,default,0,1
HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
HKR,NDI\params\PSMode,type,,enum
HKR,NDI\params\PSMode,flag,1,30,00,00,00
HKR,NDI\params\PSMode\enum,1,,"Disable"
HKR,NDI\params\PSMode\enum,2,,"Always Enable"
HKR,NDI\params\PSMode\enum,3,,"Auto Enable"
HKR,NDI\params\PSMode,optional,0,1
[COMMON.reg]
HKR, ,ACTNIOC ,0 ,"1"
HKR, ,SilentInstall ,0 ,"1"
HKR,defaults,ListenInterval,0,3
HKR,NDI\params\ListenInterval,,0,3
HKR,Ndi\params\ListenInterval,default,0,3
HKR,NDI\params\ListenInterval,ParamDesc,,%LISTENINTERVAL_STR%
HKR,NDI\params\ListenInterval,type,,int
HKR,NDI\params\ListenInterval,flag,1,30,00,00,00
HKR,NDI\params\ListenInterval,min,0,0
HKR,NDI\params\ListenInterval,max,0,77
HKR,NDI\params\ListenInterval,step,0,1
HKR,NDI\params\ListenInterval,optional,0,1
HKR,defaults,RTSThresh,0,2432
HKR,NDI\params\RTSThresh,,0,2432
HKR,Ndi\params\RTSThresh,default,0,2432
HKR,NDI\params\RTSThresh,ParamDesc,0,%RTSTHRESH_STR%
HKR,NDI\params\RTSThresh,type,0,int
HKR,NDI\params\RTSThresh,flag,1,20,00,00,00
HKR,NDI\params\RTSThresh,min,0,0
HKR,NDI\params\RTSThresh,max,0,2432
HKR,NDI\params\RTSThresh,step,0,64
HKR,NDI\params\RTSThresh,optional,0,1
HKR,defaults,FragThresh,0,2432
HKR,NDI\params\FragThresh,,0,2432
HKR,Ndi\params\FragThresh,default,0,2432
HKR,NDI\params\FragThresh,ParamDesc,0,%FRAGTHRESH_STR%
HKR,NDI\params\FragThresh,type,0,int
HKR,NDI\params\FragThresh,flag,1,20,00,00,00
HKR,NDI\params\FragThresh,min,0,256
HKR,NDI\params\FragThresh,max,0,2432
HKR,NDI\params\FragThresh,step,0,128
HKR,NDI\params\FragThresh,optional,0,1
HKR,defaults,PreambleMode,0,1
HKR,NDI\params\PreambleMode,,0,1
HKR,Ndi\params\PreambleMode,default,0,1
HKR,NDI\params\PreambleMode,ParamDesc,,%SHORT_PREAM_STR%
HKR,NDI\params\PreambleMode,type,,enum
HKR,NDI\params\PreambleMode,flag,1,30,00,00,00
HKR,NDI\params\PreambleMode\enum,1,,"Long Tx Preamble"
HKR,NDI\params\PreambleMode\enum,2,,"Short Tx Preamble"
HKR,NDI\params\PreambleMode\enum,3,,"Auto Tx Preamble"
HKR,NDI\params\PreambleMode,optional,0,1
HKR,defaults,AuthentAlg,0,65535
HKR,NDI\params\AuthentAlg,,0,65535
HKR,NDI\params\AuthentAlg,default,0,65535
HKR,NDI\params\AuthentAlg,ParamDesc,,%AUTHENT_TYPE_STR%
HKR,NDI\params\AuthentAlg,type,,enum
HKR,NDI\params\AuthentAlg,flag,1,30,00,00,00
HKR,NDI\params\AuthentAlg\enum,1,,"WECA Compliant (always use Open)"
HKR,NDI\params\AuthentAlg\enum,2,,"Must use Shared with WEP"
HKR,NDI\params\AuthentAlg\enum,65535,,"Automatic based on WEP setting"
HKR,NDI\params\AuthentAlg,optional,0,1
HKR,defaults,AdhocDemoMode,0,0
HKR,NDI\params\AdhocDemoMode,,0,0
HKR,Ndi\params\AdhocDemoMode,default,0,0
HKR,NDI\params\AdhocDemoMode,ParamDesc,,%ADHOC_DEMO_STR%
HKR,NDI\params\AdhocDemoMode,type,,enum
HKR,NDI\params\AdhocDemoMode,flag,1,30,00,00,00
HKR,NDI\params\AdhocDemoMode\enum,0,,"Disable"
HKR,NDI\params\AdhocDemoMode\enum,1,,"Enable"
HKR,NDI\params\AdhocDemoMode,optional,0,1
[DestinationDirs]
DefaultDestDir=11 ; Win9x=%windir%\system Win2k=%windir%\system32
PRISM_DRIVER.copy=11 ; Win9x=%windir%\system
PRISM_DRIVER.copy.ME=11 ; Win9x=%windir%\system
PRISM_DRIVER.copy.NT=12 ; Win2k=%windir%\system32\drivers
[PRISM_NDI.copy]
ACTNR16.dll ; Win9x NDI
ACTNCFG.dll ; Win9x NDI
[PRISM_NDI.copy.ME]
ACTNR16.dll ; Win9x NDI
ACTNCFG.dll ; Win9x NDI
[PRISM_COINSTALL.copy.NT]
[PRISM_DRIVER.copy]
ACTNNDS.sys
ACTNUSB.sys
ACTNIOC.vxd ; Win9x Ioctl interface
[PRISM_DRIVER.copy.ME]
ACTNNDS.sys
ACTNUSB.sys
ACTNIOC.vxd ; Win9x Ioctl interface
[PRISM_DRIVER.copy.NT]
ACTNNDS.sys
ACTNUSB.sys
[PRISM_APPLET.copy]
[PRISM_APPLET.copy.ME]
[PRISM_APPLET.copy.NT]
[SourceDisksNames]
1=%INSTALL_DISK_STR%,,,
[SourceDisksFiles] ; Win9x
ACTNR16.dll=1,win9x
ACTNCFG.dll=1,win9x
ACTNIOC.vxd=1,win9x
ACTNNDS.sys=1
ACTNUSB.sys=1
[SourceDisksFiles.ME] ; WinMe
ACTNNDS.sys=1
ACTNUSB.sys=1
[SourceDisksFiles.X86] ; Win2k/Xp
ACTNNDS.sys=1
ACTNUSB.sys=1
[Strings]
VER_VENDOR_STR="Accton"
VER_VENDOR_NAME_STR="Accton Corporation"
PRISM_PCMCIA1_STR="Accton WN3301 Cheetah Wireless PCMCIA_5V"
PRISM_PCMCIA2_STR="Accton WN3301 Cheetah Wireless PCMCIA"
PRISM_PCMCIA3_STR="Accton WN3301F/G Wireless PCMCIA"
PRISM_PCMCIA4_STR="Accton AC-EW3101 Wireless PCMCIA"
PRISM_PCMCIA5_STR="Accton AC-EW3101 Wireless PCMCIA (3V)"
PRISM_PCI1_STR="Accton WN3101A Mini-PCI Wireless Adapter"
PRISM_PCI2_STR="Accton WN3601A Mini-PCI Wireless/Modem Combo Adapter"
PRISM_PCI3_STR="Accton WN3201 Cheetah Wireless PCI Adapter"
PRISM_USB1_STR="Accton WN3501D Wireless USB Adapter"
PRISM_SERVICE_DISPLAY="Accton 11Mbps Wireless LAN Driver"
PRISM_USB_SERVICE_DISPLAY="Accton 11Mbps Wireless LAN USB Driver"
INSTALL_DISK_STR="Accton 11Mbps Wireless LAN Install Disk"
ADHOC_DEMO_STR="Adhoc Demo Mode"
SHORT_PREAM_STR="Preamble Mode"
RTSTHRESH_STR="RTS Threshold"
FRAGTHRESH_STR="Fragmentation Threshold"
AUTHENT_TYPE_STR="Authentication Algorithm"
LISTENINTERVAL_STR="Listen Interval"
POWER_SAVE_STR="Power Save Mode"
POWER_LEVEL_STR="Power Save Level"

