
[Version]
DriverVer=10/02/2003, 3.1.3
Signature="$Chicago$"
Compatible=1
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%VER_VENDOR_STR%
CatalogFile=PRISMNIC.cat
[ControlFlags]
ExcludeFromSelect=D-Link-DWL-650_Wireless_PC_Card_RevP-DC64
ExcludeFromSelect=VEN_1260&DEV_3873&SUBSYS_37001186
ExcludeFromSelect=VID_2001&PID_3700
ExcludeFromSelect=VID_2001&PID_3702
[Manufacturer]
%VER_VENDOR_NAME_STR%=DeviceList
[DeviceList]
%PRISM_PCMCIA_STR%=PRISM_PCMCIA, PCMCIA\D-Link-DWL-650_Wireless_PC_Card_RevP-DC64
%PCI_DESC_STR%=PRISM_PCI1, PCI\VEN_1260&DEV_3873&SUBSYS_37001186
%PRISM_USB1_STR%=PRISM_USB1, USB\VID_2001&PID_3700
%PRISM_USB2_STR%=PRISM_USB2, USB\VID_2001&PID_3702
[PRISM_PCMCIA]
AddReg=PRISM_PCMCIA.reg, COMMON_PCMCIA.reg, COMMON_NDIS.reg, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy
[PRISM_PCMCIA.NT]
AddReg=PRISM_PCMCIA.reg, COMMON_PCMCIA.reg, COMMON_NDIS.reg.NT, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.NT
BusType=8
Characteristics= 0x84
[PRISM_PCMCIA.NT.Services]
AddService= PRISM, 2, PRISM_DRIVER.Service, PRISM_DRIVER.EventLog
[PRISM_PCMCIA.reg]
HKR,Ndi ,DeviceID,0,"PCMCIA\D-Link-DWL-650_Wireless_PC_Card_RevP-DC64"
HKR, ,PlatformId,0,"32797"
HKR, ,VendorDesc,0,%PRISM_PCMCIA_STR%
HKR, ,LoadFirmware,0,"1"
[PRISM_PCI1]
AddReg=PRISM_PCI1.reg, COMMON_PCI.reg, COMMON_NDIS.reg, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy
[PRISM_PCI1.NT]
AddReg=PRISM_PCI1.reg, COMMON_PCI.reg, COMMON_NDIS.reg.NT, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.NT
BusType=5
Characteristics= 0x84
[PRISM_PCI1.NT.Services]
AddService= PRISM, 2, PRISM_DRIVER.Service, PRISM_DRIVER.EventLog
[PRISM_PCI1.reg]
HKR,Ndi ,DeviceID,0,"PCI\VEN_1260&DEV_3873&SUBSYS_37001186"
HKR, ,PlatformId,0,"32804"
HKR, ,VendorDesc,0,%PCI_DESC_STR%
HKR, ,LoadFirmware,0,"1"
[PRISM_USB1] ; Win9x
AddReg=PRISM_USB1.reg, COMMON_USB.reg, COMMON_NDIS.reg, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy
[PRISM_USB1.NT] ; Win2k
AddReg=PRISM_USB1.reg, COMMON_USB.reg, COMMON_NDIS.reg.NT, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.NT
BusType=15 ; USB
Characteristics= 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[PRISM_USB1.NT.Services]
AddService=PRISM_USB, 2, PRISM_USB_DRIVER.Service, PRISM_DRIVER.EventLog
[PRISM_USB1.reg]
HKR,Ndi ,DeviceID,0,"USB\VID_2001&PID_3700"
HKR, ,PlatformId,0,"0"
HKR, ,VendorDesc,0,%PRISM_USB1_STR%
HKR, ,LoadFirmware,0,"1"
[PRISM_USB2] ; Win9x
AddReg=PRISM_USB2.reg, COMMON_USB.reg, COMMON_NDIS.reg, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy
[PRISM_USB2.NT] ; Win2k
AddReg=PRISM_USB2.reg, COMMON_USB.reg, COMMON_NDIS.reg.NT, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.NT
BusType=15 ; USB
Characteristics= 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[PRISM_USB2.NT.Services]
AddService=PRISM_USB, 2, PRISM_USB_DRIVER.Service, PRISM_DRIVER.EventLog
[PRISM_USB2.reg]
HKR,Ndi ,DeviceID,0,"USB\VID_2001&PID_3702"
HKR, ,PlatformId,0,"0"
HKR, ,VendorDesc,0,%PRISM_USB2_STR%
HKR, ,LoadFirmware,0,"1"
[PRISM_DRIVER.Service]
DisplayName=%PRISM_SERVICE_DISPLAY%
ServiceType=1 ; SERVICE_KERNEL_DRIVER
StartType=3 ; SERVICE_DEMAND_START
ErrorControl=1 ; NORMAL
ServiceBinary=%12%\PRISMNDS.sys
LoadOrderGroup=NDIS
[PRISM_USB_DRIVER.Service]
DisplayName=%PRISM_USB_SERVICE_DISPLAY%
ServiceType=1 ; SERVICE_KERNEL_DRIVER
StartType=3 ; SERVICE_DEMAND_START
ErrorControl=1 ; NORMAL
ServiceBinary=%12%\PRISMUSB.sys
LoadOrderGroup=NDIS
[PRISM_DRIVER.EventLog]
AddReg=PRISM_DRIVER.EventLog.reg
[PRISM_DRIVER.EventLog.reg]
HKR, ,EventMessageFile ,0x00020000 ,"%%SystemRoot%%\System32\netevent.dll"
HKR, ,TypesSupported ,0x00010001 ,7
[COMMON_PCMCIA.reg]
HKR,NDI ,Service ,0 ,"PRISM"
HKR,NDI ,CardType ,0 ,"PCMCIA"
HKR, ,BusType ,0 ,"8"
HKR, ,DeviceVxDs ,0 ,"PRISMNDS.sys"
HKR, ,EnableIRQSharing ,1 ,"01","00","00","00"
HKR, ,IOBaseAddress ,1 ,"02","00","00","00"
HKR, ,InterruptNumber ,1 ,"04","00","00","00"
[COMMON_PCI.reg]
HKR,NDI ,Service ,0 ,"PRISM"
HKR,NDI ,CardType ,0 ,"PCI"
HKR, ,BusType ,0 ,"5"
HKR, ,DeviceVxDs ,0 ,"PRISMNDS.sys"
HKR, ,EnableIRQSharing ,1 ,"01","00","00","00"
HKR, ,IOBaseAddress ,1 ,"02","00","00","00"
HKR, ,InterruptNumber ,1 ,"04","00","00","00"
[COMMON_USB.reg]
HKR,NDI ,Service ,0 ,"PRISM_USB"
HKR,NDI ,CardType ,0 ,"USB"
HKR, ,BusType ,0 ,"15"
HKR, ,DeviceVxDs ,0 ,"PRISMUSB.sys"
[COMMON_NDIS.reg]
HKR, ,RunningWin9X ,0 ,"1"
HKR, ,DevLoader ,0 ,"*ndis"
HKR, ,EnumPropPages ,0 ,"netdi.dll,EnumPropPages"
HKR,NDI\Interfaces ,UpperRange ,0 ,"ndis3"
HKR,NDI\Interfaces ,LowerRange ,0 ,"ethernet"
HKR,NDI\Interfaces ,DefUpper ,0 ,"ndis3"
HKR,NDI\Interfaces ,DefLower ,0 ,"ethernet"
HKR,NDIS ,LogDriverName ,0 ,"PRISM"
HKR,NDIS ,MajorNdisVersion ,1 ,03
HKR,NDIS ,MinorNdisVersion ,1 ,0a
HKR,defaults,PSMode,0,"1"
HKR,Ndi\params\PSMode,default,0,"1"
HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
HKR,NDI\params\PSMode,type,,"enum"
HKR,NDI\params\PSMode,flag,1,"30","00","00","00"
HKR,NDI\params\PSMode\enum,1,,"Disable"
HKR,NDI\params\PSMode\enum,2,,"Always Enable"
HKR,NDI\params\PSMode,optional,0,"1"
[COMMON_NDIS.reg.NT]
HKR,NDI\Interfaces ,UpperRange ,0 ,"ndis5"
HKR,NDI\Interfaces ,LowerRange ,0 ,"ethernet"
HKR,defaults,PSMode,0,"1"
HKR,Ndi\params\PSMode,default,0,"1"
HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
HKR,NDI\params\PSMode,type,,"enum"
HKR,NDI\params\PSMode,flag,1,"30","00","00","00"
HKR,NDI\params\PSMode\enum,1,,"Disable"
HKR,NDI\params\PSMode\enum,2,,"Always Enable"
HKR,NDI\params\PSMode\enum,3,,"Auto Enable"
HKR,NDI\params\PSMode,optional,0,"1"
[COMMON.reg]
HKR, ,SilentInstall ,0 ,"1"
HKR,defaults,ListenInterval,0,"3"
HKR,Ndi\params\ListenInterval,default,0,"3"
HKR,NDI\params\ListenInterval,ParamDesc,,%LISTENINTERVAL_STR%
HKR,NDI\params\ListenInterval,type,,"int"
HKR,NDI\params\ListenInterval,flag,1,"30","00","00","00"
HKR,NDI\params\ListenInterval,min,0,"0"
HKR,NDI\params\ListenInterval,max,0,"77"
HKR,NDI\params\ListenInterval,step,0,"1"
HKR,NDI\params\ListenInterval,optional,0,"1"
HKR,defaults,RTSThresh,0,"2432"
HKR,Ndi\params\RTSThresh,default,0,"2432"
HKR,NDI\params\RTSThresh,ParamDesc,0,%RTSTHRESH_STR%
HKR,NDI\params\RTSThresh,type,0,"int"
HKR,NDI\params\RTSThresh,flag,1,"20","00","00","00"
HKR,NDI\params\RTSThresh,min,0,"0"
HKR,NDI\params\RTSThresh,max,0,"2432"
HKR,NDI\params\RTSThresh,step,0,"64"
HKR,NDI\params\RTSThresh,optional,0,"1"
HKR,defaults,FragThresh,0,"2432"
HKR,Ndi\params\FragThresh,default,0,"2432"
HKR,NDI\params\FragThresh,ParamDesc,0,%FRAGTHRESH_STR%
HKR,NDI\params\FragThresh,type,0,"int"
HKR,NDI\params\FragThresh,flag,1,"20","00","00","00"
HKR,NDI\params\FragThresh,min,0,"256"
HKR,NDI\params\FragThresh,max,0,"2432"
HKR,NDI\params\FragThresh,step,0,"128"
HKR,NDI\params\FragThresh,optional,0,"1"
HKR,defaults,PreambleMode,0,"1"
HKR,Ndi\params\PreambleMode,default,0,"1"
HKR,NDI\params\PreambleMode,ParamDesc,,%SHORT_PREAM_STR%
HKR,NDI\params\PreambleMode,type,,"enum"
HKR,NDI\params\PreambleMode,flag,1,"30","00","00","00"
HKR,NDI\params\PreambleMode\enum,1,,"Long Tx Preamble"
HKR,NDI\params\PreambleMode\enum,2,,"Short Tx Preamble"
HKR,NDI\params\PreambleMode\enum,3,,"Auto Tx Preamble"
HKR,NDI\params\PreambleMode,optional,0,"1"
HKR,defaults,AuthentAlg,0,"65535"
HKR,NDI\params\AuthentAlg,default,0,"65535"
HKR,NDI\params\AuthentAlg,ParamDesc,,%AUTHENT_TYPE_STR%
HKR,NDI\params\AuthentAlg,type,,"enum"
HKR,NDI\params\AuthentAlg,flag,1,"30","00","00","00"
HKR,NDI\params\AuthentAlg\enum,1,,"WECA Compliant (always use Open)"
HKR,NDI\params\AuthentAlg\enum,2,,"Must use Shared with WEP"
HKR,NDI\params\AuthentAlg\enum,65535,,"Automatic based on WEP setting"
HKR,NDI\params\AuthentAlg,optional,0,"1"
HKR,defaults,AdhocDemoMode,0,"0"
HKR, ,DSChannel,0,"6"
HKR,defaults,DSChannel,0,"10"
HKR,defaults,LoadFirmware,0,"1"
HKR,Ndi\params\LoadFirmware,default,0,"1"
HKR,NDI\params\LoadFirmware,ParamDesc,,%LOAD_FIRMWARE_STR%
HKR,NDI\params\LoadFirmware,type,,"enum"
HKR,NDI\params\LoadFirmware,flag,1,"30","00","00","00"
HKR,NDI\params\LoadFirmware\enum,0,,"Disable"
HKR,NDI\params\LoadFirmware\enum,1,,"Enable"
HKR,NDI\params\LoadFirmware,optional,0,"1"
HKR,defaults,PDwellTime,0,"120"
HKR,Ndi\params\PDwellTime,default,0,"120"
HKR,NDI\params\PDwellTime,ParamDesc,0,%PDWELL_STR%
HKR,NDI\params\PDwellTime,type,0,"int"
HKR,NDI\params\PDwellTime,flag,1,"20","00","00","00"
HKR,NDI\params\PDwellTime,min,0,"0"
HKR,NDI\params\PDwellTime,max,0,"1000"
HKR,NDI\params\PDwellTime,step,0,"10"
HKR,NDI\params\PDwellTime,optional,0,"1"
HKR,defaults,11dMode,0,"0"
HKR,Ndi\params\11dMode,default,0,"0"
HKR,NDI\params\11dMode,ParamDesc,,%MDC_CONTROL_STR%
HKR,NDI\params\11dMode,type,,"enum"
HKR,NDI\params\11dMode,flag,1,"30","00","00","00"
HKR,NDI\params\11dMode\enum,0,,"None"
HKR,NDI\params\11dMode\enum,1,,"Strict"
HKR,NDI\params\11dMode\enum,2,,"Flexible"
HKR,NDI\params\11dMode,optional,0,"1"
[DestinationDirs]
DefaultDestDir=11 ; Win9x=%windir%\system Win2k=%windir%\system32
PRISM_DRIVER.copy=11 ; Win9x=%windir%\system
PRISM_DRIVER.copy.NT=12 ; Win2k=%windir%\system32\drivers
[PRISM_DRIVER.copy]
PRISMNDS.sys
PRISMUSB.sys
[PRISM_DRIVER.copy.NT]
PRISMNDS.sys
PRISMUSB.sys
[SourceDisksNames]
1=%INSTALL_DISK_STR%,,,
[SourceDisksFiles] ; Win9x
PRISMNDS.sys=1
PRISMUSB.sys=1
[SourceDisksFiles.X86] ; Win2k/Xp
PRISMNDS.sys=1
PRISMUSB.sys=1
[Strings]
VER_VENDOR_STR="D-Link"
VER_VENDOR_NAME_STR="D-Link"
PRISM_PCMCIA_STR="D-Link Air DWL-650 Wireless PC Card(rev.P)"
PCI_DESC_STR="D-Link Air DWL-520 Wireless PCI Adapter(rev.E)"
PRISM_USB1_STR="D-Link Air DWL-122 Wireless USB Adapter"
PRISM_USB2_STR="D-Link Air DWL-120 Wireless USB Adapter(rev.F)"
PRISM_SERVICE_DISPLAY="D-Link Air Wireless Prism3 Adapter Driver"
PRISM_USB_SERVICE_DISPLAY="D-Link Air Wireless USB Adapter Driver"
INSTALL_DISK_STR="D-Link Air Wireless Adapter Install Disk"
ADHOC_DEMO_STR="Adhoc Demo Mode"
SHORT_PREAM_STR="Preamble Mode"
RTSTHRESH_STR="RTS Threshold"
FRAGTHRESH_STR="Fragmentation Threshold"
AUTHENT_TYPE_STR="Authentication Algorithm"
LISTENINTERVAL_STR="Listen Interval"
POWER_SAVE_STR="Power Save"
PDWELL_STR="Passive Scan Dwell Time"
LOAD_FIRMWARE_STR="Firmware Download"
MDC_CONTROL_STR="802.11D Control"
