
[Version]
CatalogFile.NT =tnet1130.cat
Signature="$Chicago$"
Compatible=1
Provider=%VER_VENDOR_STR%
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
DriverVer=04/05/2004,6.0.0.18
[Manufacturer]
%VER_VENDOR_STR%=TexasInstruments,NTx86.5.1
[ControlFlags]
ExcludeFromSelect=PCI\VEN_104C&DEV_9066&SUBSYS_003817CF
[TexasInstruments.NTx86.5.1]
%TIACX.DeviceDesc%=TIACX_CardBus.NdiXP, PCI\VEN_104C&DEV_9066&SUBSYS_003817CF
[TexasInstruments]
%TIACX.DeviceDesc%=TIACX_CardBus, PCI\VEN_104C&DEV_9066&SUBSYS_003817CF
[TIACX_CardBus.NdiXP.NT]
BusType=5
AddReg =TIACX.ndi.reg.NdiXP.NT, TI.Param.Reg, BG.Param.Reg,wxp.Private
Characteristics=0x84
;CpyFiles =TIACX.NdiXP.CopyFiles
[TIACX_CardBus.NdiXP.NT.Services]
AddService=TNET1130, 2, TIACXLNXP.Service, TIACXLNXP.EventLog
[TIACX.ndi.reg.NdiXP.NT]
HKR, Ndi, Service, 0, "TNET1130"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
[wxp.Private]
HKR, ,PrivacyMode,, "2"
HKR, ,utlPrivacyMode,, "0"
HKR, ,utlAuthenticationMode,, "0"
HKR,,DeviceVxDs,,tnet1130.sys
[TIACXLNXP.Service]
DisplayName=%TIACXLN.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_DEMAND_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\tnet1130.sys
LoadOrderGroup=NDIS
[TIACXLNXP.EventLog]
AddReg=TIACXLNXP.AddEventLog.reg
[TIACXLNXP.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported, 0x00010001, 7
[TIACX_CardBus.NT]
BusType=5
AddReg =TIACX.ndi.reg.NT, TI.Param.Reg, BG.Param.Reg,w2k.Private
Characteristics=0x84
;CpyFiles =TIACX.CopyFiles.NT
[TIACX_CardBus.NT.Services]
AddService=TNET_2K, 2, TIACXLN.Service, TIACXLN.EventLog
[TIACX.ndi.reg.NT]
HKR, Ndi, Service, 0, "TNET_2K"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
[w2k.Private]
HKR, ,PrivacyMode,, "0"
HKR, ,utlPrivacyMode,, "0"
HKR, ,utlAuthenticationMode,, "0"
HKR,,DeviceVxDs,,tnet_2K.sys
[TIACXLN.Service]
DisplayName=%TIACXLN.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_DEMAND_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\tnet_2K.sys
LoadOrderGroup=NDIS
[TIACXLN.EventLog]
AddReg=TIACXLN.AddEventLog.reg
[TIACXLN.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported, 0x00010001, 7
[TIACX_CardBus]
AddReg=TIACX.ndi.reg, TIACX_CardBus.ndi.reg, TI.Param.Reg, BG.Param.Reg, W98.Param.Reg,TIACX.Install
[TIACX_CardBus.ndi.reg]
HKR,Ndi,DeviceID,,"PCI\VEN_104C&DEV_9066&SUBSYS_003817CF"
[TIACX.ndi.reg]
HKR,,DevLoader,,*ndis
HKR,,DeviceVxDs,,tnet_9X.sys
HKR,,EnumPropPages,,"netdi.dll,EnumPropPages"
HKR, NDIS, LogDriverName, , "tnet_9X"
HKR, NDIS, MajorNdisVersion, 1, 03
HKR, NDIS, MinorNdisVersion, 1, 0A
HKR,Ndi\Interfaces,DefLower,,"ethernet"
HKR,Ndi\Interfaces,LowerRange,,"ethernet"
HKR,Ndi\Interfaces,DefUpper,,"ndis3,ndis4,ndis5"
HKR,Ndi\Interfaces,UpperRange,,"ndis3,ndis4,ndis5"
[TIACX.Install]
HKR,Ndi\Install,,,"TIACX.Copy"
HKR,Ndi\Remove,,,"TIACX.Remove"
[TIACX.Copy]
;CpyFiles=TIACX.CopyFiles
[TIACX.Remove]
;DlFiles=TIACX.CopyFiles
[W98.Param.Reg]
HKR, ,PrivacyMode,, "0"
HKR, ,utlPrivacyMode,, "0"
HKR, ,utlAuthenticationMode,, "0"
[TI.Param.Reg]
HKR, ,WLANIOC,0,"XG-350"
HKR,defaults,dot11DesiredSSID,,"ANY"
HKR,defaults,dot11PowerMode ,,"0"
HKR,defaults,dot11FragmentationThreshold,,"4096"
HKR,defaults,dot11RTSThreshold,,"4096"
HKR,defaults,Mode4x,,"1"
HKR,defaults,dot11NetworkType,,"3"
HKR, ,dot11RadioDisableSupport,, "1"
HKR, ,dot11DesiredBSSType,, "1"
HKR, ,WiFiAdhoc,, "0"
HKR, ,DisableSsidPending,, "1"
HKR,NDI\params\dot11PowerMode,ParamDesc,,"Power Mode"
HKR,NDI\params\dot11PowerMode,type,,"enum"
HKR,NDI\params\dot11PowerMode,default,,"0"
HKR,NDI\params\dot11PowerMode\enum,"0",,"Continuous Access Mode"
HKR,NDI\params\dot11PowerMode\enum,"1",,"Maximum Power Save"
HKR, Ndi\Params\dot11FragmentationThreshold, ParamDesc, ,"Fragmentation Threshold"
HKR, Ndi\Params\dot11FragmentationThreshold, Type, , "int"
HKR, Ndi\Params\dot11FragmentationThreshold, Default, , "4096"
HKR, Ndi\Params\dot11FragmentationThreshold, Min, , "256"
HKR, Ndi\Params\dot11FragmentationThreshold, Max, , "4096"
HKR, Ndi\Params\dot11FragmentationThreshold, Step, , "1"
HKR, Ndi\Params\dot11FragmentationThreshold, Base, , "10"
HKR, Ndi\Params\dot11RTSThreshold, ParamDesc, ,"RTS Threshold"
HKR, Ndi\Params\dot11RTSThreshold, Type, , "int"
HKR, Ndi\Params\dot11RTSThreshold, Default, , "4096"
HKR, Ndi\Params\dot11RTSThreshold, Min, , "0"
HKR, Ndi\Params\dot11RTSThreshold, Max, , "4096"
HKR, Ndi\Params\dot11RTSThreshold, Step, , "1"
HKR, Ndi\Params\dot11RTSThreshold, Base, , "10"
HKR,NDI\params\Mode4x,ParamDesc,,"Mode4x"
HKR,NDI\params\Mode4x,type,,"enum"
HKR,NDI\params\Mode4x,default,,"1"
HKR,NDI\params\Mode4x\enum,"0",,"Off"
HKR,NDI\params\Mode4x\enum,"1",,"On"
[BG.Param.Reg]
HKR, ,dot11SupportedRateMask,, "8"
HKR, ,dot11BasicRateMask,, "1"
HKR,NDI\params\dot11NetworkType,ParamDesc,, "Network Type"
HKR,NDI\params\dot11NetworkType,type,,"enum"
HKR,NDI\params\dot11NetworkType,default,,"3"
HKR,NDI\params\dot11NetworkType\enum,"1",,"11b"
HKR,NDI\params\dot11NetworkType\enum,"3",,"11g"
HKR, ,dot11DesiredChannel, ,1
[DestinationDirs]
DefaultDestDir=12 ; Windows\System32\Drivers
TIACX.NdiXP.CopyFiles=12 ; Winnt\System32\Drivers Directory ; WinXP
TIACX.CopyFiles=11 ; Windows\System or Winnt\System32 Directory ; Win98/ME
TIACX.CopyFiles.NT=12 ; Winnt\System32\Drivers Directory ; Win2
[TIACX.CopyFiles.NT]
tnet_2K.sys
[TIACX.CopyFiles]
tnet_9X.sys
[TIACX.NdiXP.CopyFiles]
tnet1130.sys
[SourceDisksNames]
1=%DiskName%,,
[SourceDisksFiles]
tnet_9X.sys=1
tnet_2K.sys=1
tnet1130.sys=1
[Strings]
VER_VENDOR_STR=" "
TIACX.DeviceDesc="TNET1130 802.11G WLAN Adapter"
TIACXLN.Service.DispName="TNET1130 WLAN Adapter"
WLANAdapterHelpText= "A WLAN Adapter provides high speed connection to the Internet through 802.11G technology"
DiskName="TNET1130 WLAN Installation Disk"
