
[Version]
Signature="$Windows NT$"
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%Mfg%
DriverVer=03/02/2004, 1.4.46.18 ;DATE FORMAT MM/DD/YYYY
[Manufacturer]
%Mfg%=Models
[ControlFlags]
[Models]
%wind502u.DeviceDesc%=wind502u.ndi, USB\VID_132A&PID_1502
[wind502u.ndi.NT]
AddReg=wind502u.nt5.reg, wind502u.Parameters.reg
;CpyFiles=wind502u.nt5.CopyFiles
BusType=15 ;PnpBus. (If HCT complains, refer to Errata 355)
Characteristics=0x84 ; NCF_HAS_UI + NCF_PHYSICAL
[wind502u.ndi.NT.Services]
AddService=wind502u, 2, wind502u.Service, wind502u.EventLog
[wind502u.nt5.reg]
HKR, Ndi, Service, 0, "wind502u"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
[wind502u.nt5.CopyFiles]
wind502u.sys
[DestinationDirs]
DefaultDestDir=11 ; system dir
wind502u.nt5.CopyFiles=12 ; NT: system32\drivers
[SourceDisksNames]
99=%wind502u_Disk%,"",0
[SourceDisksFiles]
wind502u.sys=99
[wind502u.Service]
DisplayName=%wind502u.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_DEMAND_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\wind502u.sys
LoadOrderGroup=NDIS
AddReg=wind502.serv_data
[wind502.serv_data]
HKR, "Parameters\0",,4, ;delete existing
HKR, "Parameters",,16, ;ensure key exists
[wind502u.EventLog]
AddReg=wind502u.AddEventLog.reg
[wind502u.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported, 0x00010001, 7
[wind502u.Parameters.reg]
HKR,,.ssid,,"NULL_SSID"
HKR,,.useEeprom,,"1"
HKR,,.probeDelay,,"5000"
HKR,,.hostNetworkInterfaceType,,"3"
HKR,,.encapsulationType,,"1"
HKR,,.authenticationMode,,"2"
HKR,,.listenInterval,,"1"
HKR,,.serviceRoutineMaintanenceInterval,,"10"
HKR,,.selectedRxAntenna,,"2"
HKR,,.selectedTxAntenna,,"0"
HKR,,.ledPolicy,,"2"
HKR,,.acceptNonErp,,"0"
HKR,,.physicalMediumMask,,"6"
HKR,,.enableScanWhileWorkInBss,,"1"
HKR,,.enableScanWhileWorkInIbss,,"1"
HKR,,.enableLastSsidUsage,,"1"
HKR,,.enableResetUponFwRequest,,"0"
HKR,,.enableSendKeepAliveNullFrames,,"1"
HKR,,.powerSaveMode,,"1"
HKR,,.isRecieveDtim,,"1"
HKR,,.AwaitPsPollResponseTimeout,,"10"
HKR,,.AwaitBeaconTimeout,,"15"
HKR,,.AwaitMulticastTimeout,,"0"
HKR,,.ReturnToNetworkBeaconInterval,,"6"
HKR,,.HostToDeviceSduNumberReturnToNetworkThreshold,,"4"
HKR,,.HostToDeviceSduNumberGoOffNetworkThreshold,,"3"
HKR,,.GoOffNetworkLowThresholdCheckPeriod,,"15"
HKR,,.TerminationConditionEvaluationInterval,,"5"
HKR,,.fragmantationThreshold,,"2347"
HKR,,.shortRetryLimit,,"8"
HKR,,.longRetryLimit,,"8"
HKR,,.cwMax,,"256"
HKR,,.cwPersistenceFactor,,"0"
HKR,,.aifs,,"1"
HKR,,.shortPreamble,,"1"
HKR,,.shortTimeSlot,,"1"
HKR,,.preBeaconWarningOffest,,"2"
HKR,,.protectionAllowed,,"1"
HKR,,.timeSlotType,,"1"
HKR,,.preambleType,,"1"
HKR,,.txPowerForOFDM,,"0"
HKR,,.txPowerForCCK,,"0"
HKR,,.txPowerDelta,,"0"
HKR,,.txPowerOverrideDefaults,,"0"
HKR,,.xoCrystal,,"0"
HKR,,.rssiSampaleNumber,,"10"
HKR,,.dtimPeriod,,"1"
HKR,,.isRecieveDtim,,"0"
HKR,,.beaconTimeToLive,,"1"
HKR,,.txRetransmissionDelta,,"0"
HKR,,.phyRateAdaptationEnabled,,"1"
HKR,,.rtsRetransmissionCountEnabled,,"0"
HKR,,.DefaultMaxPhyRate,,"108"
HKR,,.LowerRatioThreshold,,"25"
HKR,,.UpperRatioThreshold,,"40"
HKR,,.MeasurementWindow,,"50"
HKR,,.RealRateDelayInMs,,"20000"
HKR,,.WiND_Dot11A_Support_1_Mbit,,"0"
HKR,,.WiND_Dot11A_Support_2_Mbit,,"0"
HKR,,.WiND_Dot11A_Support_5_5_Mbit,,"0"
HKR,,.WiND_Dot11A_Support_6_Mbit,,"0"
HKR,,.WiND_Dot11A_Support_9_Mbit,,"0"
HKR,,.WiND_Dot11A_Support_11_Mbit,,"0"
HKR,,.WiND_Dot11A_Support_12_Mbit,,"1"
HKR,,.WiND_Dot11A_Support_18_Mbit,,"1"
HKR,,.WiND_Dot11A_Support_24_Mbit,,"1"
HKR,,.WiND_Dot11A_Support_36_Mbit,,"1"
HKR,,.WiND_Dot11A_Support_48_Mbit,,"1"
HKR,,.WiND_Dot11A_Support_54_Mbit,,"1"
HKR,,.WiND_Dot11B_Support_1_Mbit,,"1"
HKR,,.WiND_Dot11B_Support_2_Mbit,,"1"
HKR,,.WiND_Dot11B_Support_5_5_Mbit,,"1"
HKR,,.WiND_Dot11B_Support_6_Mbit,,"0"
HKR,,.WiND_Dot11B_Support_9_Mbit,,"0"
HKR,,.WiND_Dot11B_Support_11_Mbit,,"1"
HKR,,.WiND_Dot11B_Support_12_Mbit,,"0"
HKR,,.WiND_Dot11B_Support_18_Mbit,,"0"
HKR,,.WiND_Dot11B_Support_24_Mbit,,"0"
HKR,,.WiND_Dot11B_Support_36_Mbit,,"0"
HKR,,.WiND_Dot11B_Support_48_Mbit,,"0"
HKR,,.WiND_Dot11B_Support_54_Mbit,,"0"
HKR,,.WiND_Dot11G_Support_1_Mbit,,"1"
HKR,,.WiND_Dot11G_Support_2_Mbit,,"1"
HKR,,.WiND_Dot11G_Support_5_5_Mbit,,"0"
HKR,,.WiND_Dot11G_Support_6_Mbit,,"1"
HKR,,.WiND_Dot11G_Support_9_Mbit,,"0"
HKR,,.WiND_Dot11G_Support_11_Mbit,,"0"
HKR,,.WiND_Dot11G_Support_12_Mbit,,"1"
HKR,,.WiND_Dot11G_Support_18_Mbit,,"1"
HKR,,.WiND_Dot11G_Support_24_Mbit,,"1"
HKR,,.WiND_Dot11G_Support_36_Mbit,,"1"
HKR,,.WiND_Dot11G_Support_48_Mbit,,"1"
HKR,,.WiND_Dot11G_Support_54_Mbit,,"1"
HKR,,.scanGeneralActiveScanningMaxTimePerChannel,,"50"
HKR,,.scanGeneralPassiveScanningMaxTimePerChannel,,"150"
HKR,,.scanGeneralProbeRequestPeriod,,"12"
HKR,,.scanWhileWorkActiveScanningMaxTimePerChannel,,"40"
HKR,,.scanWhileWorkPassiveScanningMaxTimePerChannel,,"150"
HKR,,.scanWhileWorkMinTimeBetweenScan,,"3500"
HKR,,.countryCode,,"16"
HKR,,.PipeHostToDeviceControlSize,,"400"
HKR,,.PipeDeviceToHostControlSize,,"400"
HKR,,.PipeDeviceToHostSduSize,,"400"
HKR,,.PipeHostToDeviceSduSize0,,"400"
HKR,,.PipeHostToDeviceSduSize1,,"400"
HKR,,.PipeHostToDeviceSduSize2,,"400"
HKR,,.maxOsNetworkResources,,"564"
HKR,,.maxOsMemoryResources,,"564"
HKR,,.maxWindFrames,,"96"
HKR,,.maxWindFramesAllocatedForRx,,"48"
HKR,,.maxStations,,"30"
HKR,,.stationHashSize,,"30"
HKR,,.maxFsmEvents,,"60"
HKR,,.maxAccessPoints,,"30"
HKR,,.maxIbssBeaconGenerators,,"30"
HKR,,.maxTimers,,"30"
HKR,,.maxTxFramesToHandle,,"14"
HKR,,.maxNumberOfIoCtlEvents,,"2"
HKR,,.authenticationTimeout,,"3000"
HKR,,.associationTimeout,,"3000"
HKR,,.linkIsUpWatchdogTimeout,,"2500"
HKR,,.disconnectIndicationWatchdogTimeout,,"7500"
HKR,,.deadStation,,"10000"
HKR,,.maxConsecutiveFailedFrames,,"3"
HKR,,.bssApConnectionKeepAliveTimeout,,"15000"
HKR,,.connectToLastSsidTimeout,,"3000"
HKR,,.fwWatchdogTimeout,,"1500000"
HKR,,.D2HMaxIdlePeriodInMs,,"5000"
HKR,,.D2HAwaitPingReplyTimeoutInMs,,"5000"
HKR,,.H2DMaxIdlePeriodInMs,,"5000"
HKR,,.H2DAwaitPingReplyTimeoutInMs,,"5000"
HKR,,.triggerPeriodic,,"1"
HKR,,.triggerPeriodInInternalTicks,,"1000"
HKR,,.internalTickPeriodInMicros,,"20"
HKR,,.decayPeriod,,"5"
HKR,,.resetOnPanic,,"1"
HKR,,.useWatchDogTimer,,"1"
HKR,,.watchDogTimerValueInMicros,,"1500000"
HKR,,.statisticsPeriod,,"0"
HKR,,.driverWep,,"1"
HKR,,.currentKey,,"0"
HKR,,.algo0,,"1"
HKR,,.PlayPlainEthernet,,"0"
HKR,,.Timeout,,"10"
HKR,,.useConstantPhyRate,,"0"
HKR,,.constantPhyRate,,"108"
HKR,,.forceGShortTimeSlot,,"1"
HKR,,.forcePhysicalMediumMask,,"1"
HKR,,.outputFirmwareMessages,,"0"
HKR,,.displayFsm,,"0"
HKR,,.displayRx,,"0"
HKR,,.displayTx,,"0"
HKR,,.BufferSizeKb,,"0"
HKR,,.MinLogLevel,,"0"
HKR,,.MinTraceLevel,,"0"
HKR,,.CheckForHangPeriod,,"4"
HKR,,.PsDebugParameter1,,"0"
HKR,,.PsDebugParameter2,,"0"
HKR,,.PsDebugParameter3,,"0"
HKR,,.PsDebugParameter4,,"0"
HKR, Ndi\params\NetworkAddress, ParamDesc, 0, %ParamDesc.NetworkAddress%
HKR, Ndi\params\NetworkAddress, Type, 0, "edit"
HKR, Ndi\params\NetworkAddress, Default, 0, ""
HKR, Ndi\params\NetworkAddress, LimitText, 0, "18"
HKR, Ndi\params\NetworkAddress, UpperCase, 0, "1"
HKR, Ndi\params\NetworkAddress, Optional, 0, "1"
HKR,Ndi\Params\.countryCode, ParamDesc,0 , %ParamDesc.countryCode%
HKR,Ndi\Params\.countryCode, Type, 0, "enum"
HKR,Ndi\Params\.countryCode, Default, 0, "1"
HKR,NDI\params\.countryCode, Optional, 0, "0"
HKR,Ndi\Params\.countryCode\enum, 1 ,, "Factory Defaults"
HKR,Ndi\Params\.countryCode\enum, 16 ,, "USA (FCC)"
HKR,Ndi\Params\.countryCode\enum, 32 ,, "Canada (IC)"
HKR,Ndi\Params\.countryCode\enum, 48 ,, "Europe (ETSI)"
HKR,Ndi\Params\.countryCode\enum, 49 ,, "Spain"
HKR,Ndi\Params\.countryCode\enum, 50 ,, "France"
HKR,Ndi\Params\.countryCode\enum, 64 ,, "Japan"
HKR,,.CfgFile, 0, "wind502u.ini"
HKR,Ndi\Params\.CfgFile, ParamDesc, 0, %ParamDesc.CfgFile%
HKR,Ndi\Params\.CfgFile, Type, 0, "edit"
HKR,Ndi\Params\.CfgFile, Default, 0, "wind502u.ini"
HKR,NDI\params\.CfgFile, LimitText, 0, "80"
HKR,NDI\params\.CfgFile, Optional, 0, "1"
HKR,Ndi\Params\.rtsThreshold, ParamDesc, 0, %ParamDesc.rtsThreshold%
HKR,Ndi\Params\.rtsThreshold, Type, 0, "int"
HKR,Ndi\Params\.rtsThreshold, Default, 0, "2347"
HKR,Ndi\Params\.rtsThreshold, Min, 0, "256"
HKR,Ndi\Params\.rtsThreshold, Max, 0, "2347"
HKR,Ndi\Params\.rtsThreshold, Step, 0, "1"
HKR,Ndi\Params\.rtsThreshold, Base, 0, "10"
HKR,NDI\params\.rtsThreshold, Optional, 0, "0"
HKR,Ndi\Params\.phyMode, ParamDesc, 0, %ParamDesc.phyMode%
HKR,Ndi\Params\.phyMode, Type, 0, "enum"
HKR,Ndi\Params\.phyMode, Default, 0, "1"
HKR,NDI\params\.phyMode, Optional, 0, "0"
HKR,Ndi\Params\.phyMode\enum, 1,, "802.11b"
HKR,Ndi\Params\.phyMode\enum, 2,, "802.11g"
HKR,Ndi\Params\.channel, ParamDesc, 0, %ParamDesc.channel%
HKR,Ndi\Params\.channel, Type, 0, "int"
HKR,Ndi\Params\.channel, Default, 0, "6"
HKR,Ndi\Params\.channel, Min, 0, "1"
HKR,Ndi\Params\.channel, Max, 0, "11"
HKR,Ndi\Params\.channel, Step, 0, "1"
HKR,Ndi\Params\.channel, Base, 0, "10"
HKR,NDI\params\.channel, Optional, 0, "0"
HKR,Ndi\Params\.beaconPeriod, ParamDesc, 0, %ParamDesc.beaconPeriod%
HKR,Ndi\Params\.beaconPeriod, Type, 0, "int"
HKR,Ndi\Params\.beaconPeriod, Default, 0, "100"
HKR,Ndi\Params\.beaconPeriod, Min, 0, "20"
HKR,Ndi\Params\.beaconPeriod, Max, 0, "1000"
HKR,Ndi\Params\.beaconPeriod, Step, 0, "1"
HKR,Ndi\Params\.beaconPeriod, Base, 0, "10"
HKR,NDI\params\.beaconPeriod, Optional, 0, "0"
HKR,Ndi\Params\.scanGeneralPolicy, ParamDesc, 0, %ParamDesc.scanPolicy%
HKR,Ndi\Params\.scanGeneralPolicy, Type, 0, "enum"
HKR,Ndi\Params\.scanGeneralPolicy, Default, 0, "1"
HKR,NDI\params\.scanGeneralPolicy, Optional, 0, "0"
HKR,Ndi\Params\.scanGeneralPolicy\enum, 1,, "Active"
HKR,Ndi\Params\.scanGeneralPolicy\enum, 2,, "Passive"
HKR,Ndi\Params\.TAG, ParamDesc, 0, %ParamDesc.TAG%
HKR,Ndi\Params\.TAG, Type, 0, "edit"
HKR,NDI\params\.TAG, LimitText, 0, "80"
HKR,NDI\params\.TAG, Optional, 0, "1"

