
[Version]
Signature="$Chicago$"
Compatible=1
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%VER_VENDOR_STR%
DriverVer=06/19/2002,1.33.0.0000
[ControlFlags]
ExcludeFromSelect=PCMCIA\U.S._Robotics-IEEE_802.11b_PC-CARD-DB69
ExcludeFromSelect=PCMCIA\U.S._Robotics-IEEE_802.11b_PC-CARD-0B6C
ExcludeFromSelect=PCI\VEN_16EC&DEV_3685&SUBSYS_00E11638
ExcludeFromSelect=PCI\VEN_16EC&DEV_3685&SUBSYS_00E21638
[Manufacturer]
%VER_VENDOR_NAME_STR%=DeviceList,NTx86.5.1
[DeviceList]
%PRISM_PCMCIA1_STR%=PRISM_PCMCIA1, PCMCIA\U.S._Robotics-IEEE_802.11b_PC-CARD-DB69
%PRISM_PCMCIA2_STR%=PRISM_PCMCIA2, PCMCIA\U.S._Robotics-IEEE_802.11b_PC-CARD-0B6C
%PRISM_PCI1_STR%=PRISM_PCI1, PCI\VEN_16EC&DEV_3685&SUBSYS_00E11638
%PRISM_PCI2_STR%=PRISM_PCI2, PCI\VEN_16EC&DEV_3685&SUBSYS_00E21638
[DeviceList.NTx86.5.1]
%PRISM_PCMCIA1_STR%=PRISM_PCMCIA1_XP, PCMCIA\U.S._Robotics-IEEE_802.11b_PC-CARD-DB69
%PRISM_PCMCIA2_STR%=PRISM_PCMCIA2_XP, PCMCIA\U.S._Robotics-IEEE_802.11b_PC-CARD-0B6C
%PRISM_PCI1_STR%=PRISM_PCI1_XP, PCI\VEN_16EC&DEV_3685&SUBSYS_00E11638
%PRISM_PCI2_STR%=PRISM_PCI2_XP, PCI\VEN_16EC&DEV_3685&SUBSYS_00E21638
[PRISM_PCMCIA1] ; Win9x
AddReg=PRISM_PCMCIA1.reg, COMMON_PCMCIA.reg, COMMON_NDIS.reg, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy, PRISM_APPLET.copy, PRISM_NDI.copy
[PRISM_PCMCIA1.NT] ; Win2k
AddReg=PRISM_PCMCIA1.reg, COMMON_PCMCIA.reg, COMMON_NDIS.reg.NT, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.NT, PRISM_APPLET.copy.NT
BusType=8 ; PCMCIA
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[PRISM_PCMCIA1.NT.Services]
AddService="USR", 2, PRISM_DRIVER.Service, PRISM_DRIVER.EventLog
[PRISM_PCMCIA1.NT.CoInstallers]
;CpyFiles=PRISM_COINSTALL.copy.NT
AddReg=PRISM_COINSTALL.reg.NT
[PRISM_PCMCIA1.reg]
HKR,Ndi ,DeviceID,0,"PCMCIA\U.S._Robotics-IEEE_802.11b_PC-CARD-DB69"
[PRISM_PCMCIA2] ; Win9x
AddReg=PRISM_PCMCIA2.reg, COMMON_PCMCIA.reg, COMMON_NDIS.reg, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy, PRISM_APPLET.copy, PRISM_NDI.copy
[PRISM_PCMCIA2.NT] ; Win2k
AddReg=PRISM_PCMCIA2.reg, COMMON_PCMCIA.reg, COMMON_NDIS.reg.NT, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.NT, PRISM_APPLET.copy.NT
BusType=8 ; PCMCIA
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[PRISM_PCMCIA2.NT.Services]
AddService="USR", 2, PRISM_DRIVER.Service, PRISM_DRIVER.EventLog
[PRISM_PCMCIA2.NT.CoInstallers]
;CpyFiles=PRISM_COINSTALL.copy.NT
AddReg=PRISM_COINSTALL.reg.NT
[PRISM_PCMCIA2.reg]
HKR,Ndi ,DeviceID,0,"PCMCIA\U.S._Robotics-IEEE_802.11b_PC-CARD-0B6C"
[PRISM_PCI1] ; Win9x
AddReg=PRISM_PCI1.reg, COMMON_PCI.reg, COMMON_NDIS.reg, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy, PRISM_APPLET.copy, PRISM_NDI.copy
[PRISM_PCI1.NT] ; Win2k
AddReg=PRISM_PCI1.reg, COMMON_PCI.reg, COMMON_NDIS.reg.NT, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.NT, PRISM_APPLET.copy.NT
BusType=5 ; PCI
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[PRISM_PCI1.NT.Services]
AddService="USR", 2, PRISM_DRIVER.Service, PRISM_DRIVER.EventLog
[PRISM_PCI1.NT.CoInstallers]
;CpyFiles=PRISM_COINSTALL.copy.NT
AddReg=PRISM_COINSTALL.reg.NT
[PRISM_PCI1.reg]
HKR,Ndi ,DeviceID,0,"PCI\VEN_16EC&DEV_3685&SUBSYS_00E11638"
[PRISM_PCI2] ; Win9x
AddReg=PRISM_PCI2.reg, COMMON_PCI.reg, COMMON_NDIS.reg, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy, PRISM_APPLET.copy, PRISM_NDI.copy
[PRISM_PCI2.NT] ; Win2k
AddReg=PRISM_PCI2.reg, COMMON_PCI.reg, COMMON_NDIS.reg.NT, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.NT, PRISM_APPLET.copy.NT
BusType=5 ; PCI
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[PRISM_PCI2.NT.Services]
AddService="USR", 2, PRISM_DRIVER.Service, PRISM_DRIVER.EventLog
[PRISM_PCI2.NT.CoInstallers]
;CpyFiles=PRISM_COINSTALL.copy.NT
AddReg=PRISM_COINSTALL.reg.NT
[PRISM_PCI2.reg]
HKR,Ndi ,DeviceID,0,"PCI\VEN_16EC&DEV_3685&SUBSYS_00E21638"
[PRISM_PCMCIA1_XP] ; WinXP
AddReg=PRISM_PCMCIA1_XP.reg, COMMON_PCMCIA.reg, COMMON_NDIS.reg.NT, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.XP, PRISM_APPLET.copy.XP
BusType=8 ; PCMCIA
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[PRISM_PCMCIA1_XP.Services]
AddService="USR", 2, PRISM_DRIVER.Service, PRISM_DRIVER.EventLog
[PRISM_PCMCIA1_XP.CoInstallers]
;CpyFiles=PRISM_COINSTALL.copy.XP
AddReg=PRISM_COINSTALL.reg.XP
[PRISM_PCMCIA1_XP.reg]
HKR,Ndi ,DeviceID,0,"PCMCIA\U.S._Robotics-IEEE_802.11b_PC-CARD-DB69"
[PRISM_PCMCIA2_XP] ; WinXP
AddReg=PRISM_PCMCIA2_XP.reg, COMMON_PCMCIA.reg, COMMON_NDIS.reg.NT, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.XP, PRISM_APPLET.copy.XP
BusType=8 ; PCMCIA
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[PRISM_PCMCIA2_XP.Services]
AddService="USR", 2, PRISM_DRIVER.Service, PRISM_DRIVER.EventLog
[PRISM_PCMCIA2_XP.CoInstallers]
;CpyFiles=PRISM_COINSTALL.copy.XP
AddReg=PRISM_COINSTALL.reg.XP
[PRISM_PCMCIA2_XP.reg]
HKR,Ndi ,DeviceID,0,"PCMCIA\U.S._Robotics-IEEE_802.11b_PC-CARD-0B6C"
[PRISM_PCI1_XP] ; WinXP
AddReg=PRISM_PCI1_XP.reg, COMMON_PCI.reg, COMMON_NDIS.reg.NT, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.XP, PRISM_APPLET.copy.XP
BusType=5 ; PCI
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[PRISM_PCI1_XP.Services]
AddService="USR", 2, PRISM_DRIVER.Service, PRISM_DRIVER.EventLog
[PRISM_PCI1_XP.CoInstallers]
;CpyFiles=PRISM_COINSTALL.copy.XP
AddReg=PRISM_COINSTALL.reg.XP
[PRISM_PCI1_XP.reg]
HKR,Ndi ,DeviceID,0,"PCI\VEN_16EC&DEV_3685&SUBSYS_00E11638"
[PRISM_PCI2_XP] ; WinXP
AddReg=PRISM_PCI2_XP.reg, COMMON_PCI.reg, COMMON_NDIS.reg.NT, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.XP, PRISM_APPLET.copy.XP
BusType=5 ; PCI
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[PRISM_PCI2_XP.Services]
AddService="USR", 2, PRISM_DRIVER.Service, PRISM_DRIVER.EventLog
[PRISM_PCI2_XP.CoInstallers]
;CpyFiles=PRISM_COINSTALL.copy.XP
AddReg=PRISM_COINSTALL.reg.XP
[PRISM_PCI2_XP.reg]
HKR,Ndi ,DeviceID,0,"PCI\VEN_16EC&DEV_3685&SUBSYS_00E21638"
[PRISM_COINSTALL.reg.NT]
HKR, ,CoInstallers32 ,0x00010000 ,"USRCFG.cpl,NdiProc"
[PRISM_COINSTALL.reg.XP]
HKR, ,CoInstallers32 ,0x00010000 ,"USRCFG.cpl,NdiProc"
[PRISM_DRIVER.Service]
DisplayName=%PRISM_SERVICE_DISPLAY%
ServiceType=1 ; SERVICE_KERNEL_DRIVER
StartType=3 ; SERVICE_DEMAND_START
ErrorControl=1 ; NORMAL
ServiceBinary=%12%\USRNDS.sys
LoadOrderGroup=NDIS
[PRISM_DRIVER.EventLog]
AddReg=PRISM_DRIVER.EventLog.reg
[PRISM_DRIVER.EventLog.reg]
HKR, ,EventMessageFile ,0x00020000 ,"%%SystemRoot%%\System32\netevent.dll"
HKR, ,TypesSupported ,0x00010001 ,7
[COMMON_PCMCIA.reg]
HKR,NDI ,Service ,0 ,"USR"
HKR,NDI ,CardType ,0 ,"PCMCIA"
HKR, ,BusType ,0 ,"8"
HKR, ,DeviceVxDs ,0 ,"USRNDS.sys"
HKR, ,EnableIRQSharing ,1 ,01,00,00,00
HKR, ,IOBaseAddress ,1 ,02,00,00,00
HKR, ,InterruptNumber ,1 ,04,00,00,00
[COMMON_PCI.reg]
HKR,NDI ,Service ,0 ,"USR"
HKR,NDI ,CardType ,0 ,"PCI"
HKR, ,BusType ,0 ,"5"
HKR, ,DeviceVxDs ,0 ,"USRNDS.sys"
HKR, ,EnableIRQSharing ,1 ,01,00,00,00
HKR, ,IOBaseAddress ,1 ,02,00,00,00
HKR, ,InterruptNumber ,1 ,04,00,00,00
[COMMON_NDIS.reg]
HKR, ,RunningWin9X ,0 ,"1"
HKR, ,DevLoader ,0 ,"*ndis"
HKR, ,EnumPropPages ,0 ,"netdi.dll,EnumPropPages"
HKR,NDI ,NdiInstaller ,0 ,"USRCFG.dll,NdiProc"
HKR,NDI\Interfaces ,UpperRange ,0 ,"ndis3"
HKR,NDI\Interfaces ,LowerRange ,0 ,"ethernet"
HKR,NDI\Interfaces ,DefUpper ,0 ,"ndis3"
HKR,NDI\Interfaces ,DefLower ,0 ,"ethernet"
HKR,NDIS ,LogDriverName ,0 ,"USR"
HKR,NDIS ,MajorNdisVersion ,1 ,03
HKR,NDIS ,MinorNdisVersion ,1 ,0a
HKR,defaults,PSMode,0,1
HKR,Ndi\params\PSMode,default,0,1
HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
HKR,NDI\params\PSMode,type,,enum
HKR,NDI\params\PSMode,flag,1,30,00,00,00
HKR,NDI\params\PSMode\enum,1,,"Disable"
HKR,NDI\params\PSMode\enum,2,,"Always Enable"
[COMMON_NDIS.reg.NT]
HKR, ,EnumPropPages32 ,0 ,"USRCFG.cpl,NetPropPageProvider"
HKR,NDI\Interfaces ,UpperRange ,0 ,"ndis5"
HKR,NDI\Interfaces ,LowerRange ,0 ,"ethernet"
HKR,defaults,PSMode,0,1
HKR,Ndi\params\PSMode,default,0,1
HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
HKR,NDI\params\PSMode,type,,enum
HKR,NDI\params\PSMode,flag,1,30,00,00,00
HKR,NDI\params\PSMode\enum,1,,"Disable"
HKR,NDI\params\PSMode\enum,2,,"Always Enable"
HKR,NDI\params\PSMode\enum,3,,"Auto Enable"
[COMMON.reg]
HKR, ,USRIOC ,0 ,"1"
HKR, ,SilentInstall ,0 ,"1"
HKR,defaults,ListenInterval,0,3
HKR,Ndi\params\ListenInterval,default,0,3
HKR,NDI\params\ListenInterval,ParamDesc,,%LISTENINTERVAL_STR%
HKR,NDI\params\ListenInterval,type,,int
HKR,NDI\params\ListenInterval,flag,1,30,00,00,00
HKR,NDI\params\ListenInterval,min,0,0
HKR,NDI\params\ListenInterval,max,0,77
HKR,NDI\params\ListenInterval,step,0,1
HKR,defaults,RTSThresh,0,2432
HKR,Ndi\params\RTSThresh,default,0,2432
HKR,NDI\params\RTSThresh,ParamDesc,0,%RTSTHRESH_STR%
HKR,NDI\params\RTSThresh,type,0,int
HKR,NDI\params\RTSThresh,flag,1,20,00,00,00
HKR,NDI\params\RTSThresh,min,0,0
HKR,NDI\params\RTSThresh,max,0,2432
HKR,NDI\params\RTSThresh,step,0,64
HKR,defaults,FragThresh,0,2432
HKR,Ndi\params\FragThresh,default,0,2432
HKR,NDI\params\FragThresh,ParamDesc,0,%FRAGTHRESH_STR%
HKR,NDI\params\FragThresh,type,0,int
HKR,NDI\params\FragThresh,flag,1,20,00,00,00
HKR,NDI\params\FragThresh,min,0,256
HKR,NDI\params\FragThresh,max,0,2432
HKR,NDI\params\FragThresh,step,0,128
HKR,defaults,PreambleMode,0,3
HKR,Ndi\params\PreambleMode,default,0,3
HKR,NDI\params\PreambleMode,ParamDesc,,%SHORT_PREAM_STR%
HKR,NDI\params\PreambleMode,type,,enum
HKR,NDI\params\PreambleMode,flag,1,30,00,00,00
HKR,NDI\params\PreambleMode\enum,1,,"Long Tx Preamble"
HKR,NDI\params\PreambleMode\enum,2,,"Short Tx Preamble"
HKR,NDI\params\PreambleMode\enum,3,,"Auto Tx Preamble"
HKR,defaults,AuthentAlg,0,2
HKR,NDI\params\AuthentAlg,default,0,2
HKR,NDI\params\AuthentAlg,ParamDesc,,%AUTHENT_TYPE_STR%
HKR,NDI\params\AuthentAlg,type,,enum
HKR,NDI\params\AuthentAlg,flag,1,30,00,00,00
HKR,NDI\params\AuthentAlg\enum,1,,"Open System"
HKR,NDI\params\AuthentAlg\enum,2,,"Shared Key"
HKR,NDI\params\AuthentAlg\enum,65535,,"Automatic based on WEP setting"
HKR,defaults,AdhocDemoMode,0,0
HKR,Ndi\params\AdhocDemoMode,default,0,0
HKR,NDI\params\AdhocDemoMode,ParamDesc,,%ADHOC_DEMO_STR%
HKR,NDI\params\AdhocDemoMode,type,,enum
HKR,NDI\params\AdhocDemoMode,flag,1,30,00,00,00
HKR,NDI\params\AdhocDemoMode\enum,0,,"Disable"
HKR,NDI\params\AdhocDemoMode\enum,1,,"Enable"
[DestinationDirs]
DefaultDestDir=11 ; Win9x=%windir%\system Win2k=%windir%\system32
PRISM_DRIVER.copy=11 ; Win9x=%windir%\system
PRISM_DRIVER.copy.NT= 12 ; Win2k=%windir%\system32\drivers
PRISM_DRIVER.copy.XP= 12 ; WinXP=%windir%\system32\drivers
[PRISM_NDI.copy]
USRR16.dll ; Win9x NDI
USRCFG.dll ; Win9x NDI
[PRISM_COINSTALL.copy.NT]
USRCFG.cpl ; Win2k CoInstaller
[PRISM_COINSTALL.copy.XP]
USRCFG.cpl ; WinXP CoInstaller
[PRISM_DRIVER.copy]
USRNDS.sys,USRNDS50.sys,,
USRIOC.vxd ; Win9x Ioctl interface
[PRISM_DRIVER.copy.NT]
USRNDS.sys,USRNDS50.sys,,
[PRISM_DRIVER.copy.XP]
USRNDS.sys,USRNDS51.sys,,
[PRISM_APPLET.copy]
USRCFG.cpl
[PRISM_APPLET.copy.NT]
[PRISM_APPLET.copy.XP]
[SourceDisksNames]
1=%INSTALL_DISK_STR%,,,
[SourceDisksFiles] ; Win9x
USRR16.dll=1,win9x
USRCFG.dll=1,win9x
USRIOC.vxd=1,win9x
USRCFG.cpl=1,winnt
USRNDS50.sys=1,win2k
[SourceDisksFiles.X86];Win2k
USRCFG.cpl=1,win2k
USRNDS50.sys=1,win2k
USRNDS51.sys=1
[Strings]
VER_VENDOR_STR="U.S. Robotics Corporation"
VER_VENDOR_NAME_STR="U.S. Robotics Corporation"
PRISM_PCMCIA1_STR="U.S. Robotics Wireless Access 802.11b"
PRISM_PCMCIA2_STR="U.S. Robotics Wireless Access 802.11b 3.3V"
PRISM_PCI1_STR="U.S. Robotics Wireless Access 802.11b PCI Adapter 3.3V"
PRISM_PCI2_STR="U.S. Robotics Wireless Access 802.11b PCI Adapter 5V"
PRISM_SERVICE_DISPLAY="U.S. Robotics Wireless Access 802.11b Driver"
INSTALL_DISK_STR="U.S. Robotics Wireless Access 802.11b Install Disk"
ADHOC_DEMO_STR="Adhoc Demo Mode"
SHORT_PREAM_STR="Preamble Mode"
RTSTHRESH_STR="RTS Threshold"
FRAGTHRESH_STR="Fragmentation Threshold"
AUTHENT_TYPE_STR="Authentication Algorithm"
LISTENINTERVAL_STR="Listen Interval"
POWER_SAVE_STR="Power Save Mode"
POWER_LEVEL_STR="Power Save Level"

