
[Version]
DriverVer=06/16/2003, 1.0.17
Signature="$Chicago$"
Compatible=1
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%VER_VENDOR_STR%
MillenniumPreferred=.ME
[ControlFlags]
ExcludeFromSelect=*
[Manufacturer]
%VER_VENDOR_NAME_STR%=DeviceList
[DeviceList]
%DCB_DESC_STR%=PRISM_DCB1, PCI\VEN_1260&DEV_3890&SUBSYS_280210B8
[PRISM_DCB1] ; Win9x
DelReg=COMMON_AMAC_DEL.reg
AddReg=PRISM_DCB1.reg, COMMON_ICB.reg, COMMON_NDIS.reg, COMMON.reg, COMMON_PSMODE.reg, COMMON_AMAC.reg
;CpyFiles=PRISM_DRIVER.copy, PRISM_FWDCB.copy, PRISM_APPLET.copy, PRISM_NDI.copy, PRISM_DOM.copy
[PRISM_DCB1.ME] ; WinMe
DelReg=COMMON_AMAC_DEL.reg
AddReg=PRISM_DCB1.reg, COMMON_ICB.reg, COMMON_NDIS.reg.ME, COMMON.reg, COMMON_PSMODE.reg, COMMON_AMAC.reg
;CpyFiles=PRISM_DRIVER.copy.ME, PRISM_FWDCB.copy.ME, PRISM_APPLET.copy.ME, PRISM_DOM.copy, PRISM_NDI.copy.ME,
[PRISM_DCB1.ME.ME] ; WinMe - Same as .ME (Needed for Update Driver)
DelReg=COMMON_AMAC_DEL.reg
AddReg=PRISM_DCB1.reg, COMMON_ICB.reg, COMMON_NDIS.reg.ME, COMMON.reg, COMMON_PS_MODE.reg, COMMON_AMAC.reg
;CpyFiles=PRISM_DRIVER.copy.ME, PRISM_FWDCB.copy.ME, PRISM_APPLET.copy.ME, PRISM_DOM.copy, PRISM_NDI.copy.ME
[PRISM_DCB1.NT] ; Win2k
DelReg=COMMON_AMAC_DEL.reg
AddReg=PRISM_DCB1.reg, COMMON_ICB.reg, COMMON_NDIS.reg.NT, COMMON.reg, COMMON_PS_MODE_XP.reg, COMMON_AMAC.reg
;CpyFiles=PRISM_DRIVER.copy.NT, PRISM_FWDCB.copy.NT, PRISM_APPLET.copy.NT, PRISM_DOM.copy
BusType=5 ; PCI
Characteristics= 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[PRISM_DCB1.NT.Services]
AddService="PRISM_ICB", 2, PRISM_DRIVER_DCB.Service, PRISM_DRIVER.EventLog
[PRISM_DCB1.NT.CoInstallers]
;CpyFiles=PRISM_COINSTALL.copy.NT
AddReg=PRISM_COINSTALL.reg.NT
[PRISM_DCB1.reg]
HKR,Ndi,DeviceID,0,"PCI\VEN_1260&DEV_3890&SUBSYS_280210B8"
HKR,,PlatformID,0,14480
HKR,,VendorDesc,0,%DCB_DESC_STR%
[PRISM_COINSTALL.reg.NT]
[PRISM_DRIVER_DCB.Service]
DisplayName=%PRISM_SERVICE_DISPLAY_DCB%
ServiceType=1 ; SERVICE_KERNEL_DRIVER
StartType=3 ; SERVICE_DEMAND_START
ErrorControl=1 ; NORMAL
ServiceBinary=%12%\smc2802w.sys
LoadOrderGroup=NDIS
[PRISM_DRIVER.EventLog]
AddReg=PRISM_DRIVER.EventLog.reg
[PRISM_DRIVER.EventLog.reg]
HKR, ,EventMessageFile ,0x00020000 ,"%%SystemRoot%%\System32\netevent.dll"
HKR, ,TypesSupported ,0x00010001 ,7
[COMMON_ICB.reg]
HKR,NDI ,Service ,0 ,"smc2802_ICB"
HKR, ,BusType ,0 ,"5"
HKR, ,DeviceVxDs ,0 ,"smc2802w.sys"
HKR, ,EnableIRQSharing ,1 ,01,00,00,00
HKR, ,IOBaseAddress ,1 ,02,00,00,00
HKR, ,InterruptNumber ,1 ,04,00,00,00
[COMMON_NDIS.reg]
HKR, ,DevLoader ,0 ,"*ndis"
HKR, ,EnumPropPages ,0 ,"netdi.dll,EnumPropPages"
HKR,NDI\Interfaces ,UpperRange ,0 ,"ndis3"
HKR,NDI\Interfaces ,LowerRange ,0 ,"ethernet"
HKR,NDI\Interfaces ,DefUpper ,0 ,"ndis3"
HKR,NDI\Interfaces ,DefLower ,0 ,"ethernet"
HKR,NDIS ,LogDriverName ,0 ,"smc2802"
HKR,NDIS ,MajorNdisVersion ,1 ,03
HKR,NDIS ,MinorNdisVersion ,1 ,0a
[COMMON_NDIS.reg.ME]
HKR, ,DevLoader ,0 ,"*ndis"
HKR, ,EnumPropPages ,0 ,"netdi.dll,EnumPropPages"
HKR,NDI\Interfaces ,UpperRange ,0 ,"ndis3"
HKR,NDI\Interfaces ,LowerRange ,0 ,"ethernet"
HKR,NDI\Interfaces ,DefUpper ,0 ,"ndis3"
HKR,NDI\Interfaces ,DefLower ,0 ,"ethernet"
HKR,NDIS ,LogDriverName ,0 ,"smc2802"
HKR,NDIS ,MajorNdisVersion ,1 ,03
HKR,NDIS ,MinorNdisVersion ,1 ,0a
[COMMON_NDIS.reg.NT]
HKR,NDI\Interfaces ,UpperRange ,0 ,"ndis5"
HKR,NDI\Interfaces ,LowerRange ,0 ,"ethernet"
[COMMON.reg]
HKR, ,WLANIOC ,0 ,"XG-300"
HKR, ,Band ,0 ,"1"
HKR,,SSID,0,"ANY"
HKR,defaults,SSID,0,"ANY"
HKR,NDI\params\SSID,ParamDesc,0,%ESSID_STR%
HKR,NDI\params\SSID,default,0,"ANY"
HKR,Ndi\params\SSID,type,0,"edit"
HKR,NDI\params\SSID,limitText,0,"32"
HKR,,NetworkType,0,1
HKR,defaults,NetworkType,0,1
HKR,NDI\params\NetworkType,ParamDesc,0,%Network_Type_STR%
HKR,Ndi\params\NetworkType,default,0,"1"
HKR,NDI\params\NetworkType,type,0,"enum"
HKR,NDI\params\NetworkType\enum,0,0,"Ad Hoc"
HKR,NDI\params\NetworkType\enum,1,0,"Infrastructure"
HKR,,DSChannel,0,1
HKR,defaults,DSChannel,0,1
HKR,NDI\params\DSChannel,ParamDesc,0,%CHANNEL_STR%
HKR,Ndi\params\DSChannel,default,0,"1"
HKR,NDI\params\DSChannel,type,0,"enum"
HKR,NDI\params\DSChannel\enum,1,0,"01"
HKR,NDI\params\DSChannel\enum,2,0,"02"
HKR,NDI\params\DSChannel\enum,3,0,"03"
HKR,NDI\params\DSChannel\enum,4,0,"04"
HKR,NDI\params\DSChannel\enum,5,0,"05"
HKR,NDI\params\DSChannel\enum,6,0,"06"
HKR,NDI\params\DSChannel\enum,7,0,"07"
HKR,NDI\params\DSChannel\enum,8,0,"08"
HKR,NDI\params\DSChannel\enum,9,0,"09"
HKR,NDI\params\DSChannel\enum,10,0,"10"
HKR,NDI\params\DSChannel\enum,11,0,"11"
HKR,,TxRate,,15
HKR,defaults,TxRate,,15
HKR,NDI\params\TxRate,ParamDesc,0,%TX_RATE_STR%
HKR,NDI\params\TxRate,default,0,"15"
HKR,NDI\params\TxRate,type,0,"enum"
HKR,NDI\params\TxRate\enum,1,0,"1 Mbps"
HKR,NDI\params\TxRate\enum,2,0,"2 Mbps"
HKR,NDI\params\TxRate\enum,3,0,"1 or 2 Mbps"
HKR,NDI\params\TxRate\enum,4,0,"5.5 Mbps"
HKR,NDI\params\TxRate\enum,8,0,"11 Mbps"
HKR,NDI\params\TxRate\enum,15,0,"Fully Auto"
HKR,,WepReq,0,0
HKR,defaults,WepReq,0,0
HKR,NDI\params\WepReq,ParamDesc,0,%WEP_STR%
HKR,Ndi\params\WepReq,default,0,"0"
HKR,NDI\params\WepReq,type,0,"enum"
HKR,NDI\params\WepReq\enum,0,0,"Disable"
HKR,NDI\params\WepReq\enum,2,0,"64-bit"
HKR,NDI\params\WepReq\enum,6,0,"128-bit"
HKR,NDI\params\WepReq,optional,0,"0"
HKR,NDI\params\RTSThresh,,0,2347
HKR,Ndi\params\RTSThresh,default,0,2347
HKR,NDI\params\RTSThresh,ParamDesc,0,%RTSTHRESH_STR%
HKR,NDI\params\RTSThresh,type,0,int
HKR,NDI\params\RTSThresh,flag,1,20,00,00,00
HKR,NDI\params\RTSThresh,min,0,0
HKR,NDI\params\RTSThresh,max,0,2347
HKR,NDI\params\RTSThresh,step,0,1
HKR,NDI\params\RTSThresh,optional,0,1
HKR,NDI\params\FragThresh,,0,2346
HKR,Ndi\params\FragThresh,default,0,2346
HKR,NDI\params\FragThresh,ParamDesc,0,%FRAGTHRESH_STR%
HKR,NDI\params\FragThresh,type,0,int
HKR,NDI\params\FragThresh,flag,1,20,00,00,00
HKR,NDI\params\FragThresh,min,0,256
HKR,NDI\params\FragThresh,max,0,2346
HKR,NDI\params\FragThresh,step,0,2
HKR,NDI\params\FragThresh,optional,0,1
HKR, ,LongPreamble,0,0
HKR, defaults,LongPreamble,0,0 ;Infrasturcture
HKR, NDI\params\LongPreamble,,0,0
HKR, Ndi\params\LongPreamble,default,0,0
HKR, Ndi\params\LongPreamble,ParamDesc,0, %SHORT_PREAM_STR%
HKR, Ndi\params\LongPreamble,type,0, "enum"
HKR, Ndi\params\LongPreamble,default,0, "1"
HKR, Ndi\params\LongPreamble\enum,1,0, "Long"
HKR, Ndi\params\LongPreamble\enum,0,0, "Short"
HKR, NDI\params\LongPreamble,optional,0,1
HKR, ,11dMode,0,0
HKR, defaults,11dMode,0,0 ;Disalbed
HKR, NDI\params\11dMode,,0,0
HKR, Ndi\params\11dMode,default,0,0
HKR, Ndi\params\11dMode,ParamDesc,0, %11D_MODE%
HKR, Ndi\params\11dMode,type,0, "enum"
HKR, Ndi\params\11dMode,default,0, "0"
HKR, Ndi\params\11dMode\enum,0,0, "Disabled"
HKR, Ndi\params\11dMode\enum,1,0, "Strict"
HKR, Ndi\params\11dMode\enum,2,0, "Flexible"
HKR, NDI\params\11dMode,optional,0,1
HKR, ,NitroMode,0,1
HKR, ,NitroTime,0,0
[COMMON_AMAC_DEL.reg]
HKR,defaults,DataRates
HKR,NDI\params\DataRates
HKR,NDI\params\DataRate
HKR,DSChannel
HKR,defaults,DSChannel
HKR,NDI\params\DSChannel
[COMMON_AMAC.reg]
HKR,NDI\params\ShortRetryLimit,,0,7
HKR,NDI\params\ShortRetryLimit,default,0,7
HKR,NDI\params\ShortRetryLimit,ParamDesc,,%SHORT_RETRY_STR%
HKR,NDI\params\ShortRetryLimit,type,,int
HKR,NDI\params\ShortRetryLimit,min,0,1
HKR,NDI\params\ShortRetryLimit,max,0,255
HKR,NDI\params\ShortRetryLimit,step,0,1
HKR,NDI\params\ShortRetryLimit,optional,0,1
HKR,NDI\params\LongRetryLimit,,0,4
HKR,NDI\params\LongRetryLimit,default,0,4
HKR,NDI\params\LongRetryLimit,ParamDesc,,%LONG_RETRY_STR%
HKR,NDI\params\LongRetryLimit,type,0,int
HKR,NDI\params\LongRetryLimit,min,0,1
HKR,NDI\params\LongRetryLimit,max,0,255
HKR,NDI\params\LongRetryLimit,step,0,1
HKR,NDI\params\LongRetryLimit,optional,0,1
[COMMON_PSMODE.reg]
HKR,defaults,PSMode,0,1
HKR,NDI\params\PSMode,,0,1
HKR,Ndi\params\PSMode,default,0,1
HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
HKR,NDI\params\PSMode,type,,enum
HKR,NDI\params\PSMode,flag,1,30,00,00,00
HKR,NDI\params\PSMode\enum,1,,%POWER_SAVE_OFF_STR%
HKR,NDI\params\PSMode\enum,2,,%POWER_SAVE_DYN_STR%
HKR,NDI\params\PSMode\enum,3,,%POWER_SAVE_MAX_STR%
HKR,NDI\params\PSMode,optional,0,1
[COMMON_PS_MODE_XP.reg]
HKR,defaults,PSMode,0,1
HKR,NDI\params\PSMode,,0,1
HKR,Ndi\params\PSMode,default,0,1
HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
HKR,NDI\params\PSMode,type,,enum
HKR,NDI\params\PSMode,flag,1,30,00,00,00
HKR,NDI\params\PSMode\enum,1,,%POWER_SAVE_OFF_STR%
HKR,NDI\params\PSMode\enum,2,,%POWER_SAVE_DYN_STR%
HKR,NDI\params\PSMode\enum,3,,%POWER_SAVE_MAX_STR%
HKR,NDI\params\PSMode\enum,4,,%POWER_SAVE_AUTO_DYN_STR%
HKR,NDI\params\PSMode\enum,5,,%POWER_SAVE_AUTO_MAX_STR%
HKR,NDI\params\PSMode,optional,0,1
[DestinationDirs]
DefaultDestDir=11 ; Win9x=%windir%\system Win2k=%windir%\system32
PRISM_DRIVER.copy=11 ; Win9x=%windir%\system
PRISM_DRIVER.copy.ME=11 ; Win9x=%windir%\system
PRISM_DRIVER.copy.NT=12 ; Win2k=%windir%\system32\drivers
PRISM_FWDCB.copy=11 ; Win9x=%windir%\system
PRISM_FWDCB.copy.ME=11 ; Win9x=%windir%\system
PRISM_FWDCB.copy.NT=12 ; Win2k=%windir%\system32\drivers
PRISM_DOM.copy=10 ; %windir% all OS
[PRISM_NDI.copy]
[PRISM_NDI.copy.ME]
[PRISM_COINSTALL.copy.NT]
[PRISM_DRIVER.copy]
smc2802w.sys
[PRISM_DRIVER.copy.ME]
smc2802w.sys
[PRISM_DRIVER.copy.NT]
smc2802w.sys
[PRISM_FWDCB.copy]
[PRISM_FWDCB.copy.ME]
[PRISM_FWDCB.copy.NT]
[PRISM_APPLET.copy]
[PRISM_APPLET.copy.ME]
[PRISM_APPLET.copy.NT]
[PRISM_DOM.copy]
smc2802w.ini
[SourceDisksNames]
1=%INSTALL_DISK_STR%,,,
[SourceDisksFiles] ; Win9x
smc2802w.sys=1
smc2802w.ini=1
[SourceDisksFiles.ME] ; WinMe
smc2802w.sys=1
smc2802w.ini=1
[SourceDisksFiles.X86] ; Win2k/Xp
smc2802w.sys=1
smc2802w.ini=1
[Strings]
VER_VENDOR_STR="SMC"
VER_VENDOR_NAME_STR="SMC Networks, Inc."
PRISM_SERVICE_DISPLAY_DCB="SMC2802W 2.4GHz 54Mbps Wireless PCI Card"
INSTALL_DISK_STR="SMC Wireless LAN Install Disk"
ESSID_STR="ESSID"
NETWORK_TYPE_STR="Network Type"
CHANNEL_STR="Channel"
TX_RATE_STR="Transmit Rate"
WEP_STR="Use WEP"
ADHOC_DEMO_STR="Adhoc Demo Mode"
SHORT_PREAM_STR="Preamble Mode"
RTSTHRESH_STR="RTS Threshold"
FRAGTHRESH_STR="Fragmentation Threshold"
AUTHENT_TYPE_STR="Authentication Algorithm"
LISTENINTERVAL_STR="Listen Interval"
POWER_SAVE_STR="Power Save Mode"
POWER_SAVE_OFF_STR="Disabled"
POWER_SAVE_DYN_STR="Dynamic"
POWER_SAVE_MAX_STR="Maximum"
POWER_SAVE_AUTO_DYN_STR="Auto Dynamic"
POWER_SAVE_AUTO_MAX_STR="Auto Maximum"
LOAD_FIRMWARE_STR="Firmware Download"
SHORT_RETRY_STR="Short Retry Limit"
LONG_RETRY_STR="Long Retry Limit"
CHANNEL_STR="Channel"
DATARATES_STR="Data Rate"
DATARATES_AUTO="Fully Automatic"
ALSR_STR="Auto Long Slot Reassociation"
11D_MODE="11D Mode"
NITRO_MODE="Nitro Mode"
DCB_DESC_STR="SMC2802W 2.4GHz 54Mbps Wireless PCI Card"

