
[Version]
Signature="$Chicago$"
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%D-Link%
Compatible=1
DriverVer=01/15/2008, 1.03.00.0000
CatalogFile=Dr71WU.cat ;for WHQL certified
[ControlFlags]
ExcludeFromSelect=VID_07D1&PID_3C03
ExcludeFromSelect=VID_07D1&PID_3C04
ExcludeFromSelect=VID_07D1&PID_3C07
[Manufacturer]
%D-Link%=D-Link,NTX86, NTAMD64
[D-Link]
%D-Link.DeviceDesc%=D-Link.ndi, USB\VID_07D1&PID_3C03
%WUA1340.DeviceDesc%=WUA1340.ndi, USB\VID_07D1&PID_3C04
%DWA110.DeviceDesc%=DWA110.ndi, USB\VID_07D1&PID_3C07
[D-Link.NTX86]
%D-Link.DeviceDesc%=D-Link.ndi, USB\VID_07D1&PID_3C03
%WUA1340.DeviceDesc%=WUA1340.ndi, USB\VID_07D1&PID_3C04
%DWA110.DeviceDesc%=DWA110.ndi, USB\VID_07D1&PID_3C07
[D-Link.NTAMD64]
%D-Link.DeviceDesc%=D-Link.ndi, USB\VID_07D1&PID_3C03
%WUA1340.DeviceDesc%=WUA1340.ndi, USB\VID_07D1&PID_3C04
%DWA110.DeviceDesc%=DWA110.ndi, USB\VID_07D1&PID_3C07
[D-Link.ndi]
AddReg=DRT71W9x.ndi.reg, Common.reg, USB9X.ndi.reg
;CpyFiles=win9x.CopyFiles
[WUA1340.ndi]
AddReg=WUA13409x.ndi.reg, Common.reg, USB9X.ndi.reg
;CpyFiles=win9x.CopyFiles
[DWA110.ndi]
AddReg=DWA110.ndi.reg, Common.reg, USB9X.ndi.reg
;CpyFiles=win9x.CopyFiles
[D-Link.ndi.NT]
AddReg=Common.reg, RTUSB.ndi.NT.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=15 ;USB
;CpyFiles=NT.CopyFiles
[WUA1340.ndi.NT]
AddReg=Common.reg, RTUSB.ndi.NT.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=15 ;USB
;CpyFiles=NT.CopyFiles
[DWA110.ndi.NT]
AddReg=Common.reg, RTUSB.ndi.NT.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=15 ;USB
;CpyFiles=NT.CopyFiles
[D-Link.ndi.NT.Services]
AddService=RT73, 2, D-Link.Service, common.EventLog
[WUA1340.ndi.NT.Services]
AddService=RT73, 2, D-Link.Service, common.EventLog
[DWA110.ndi.NT.Services]
AddService=RT73, 2, D-Link.Service, common.EventLog
[D-Link.ndi.NTAMD64]
AddReg=Common.reg, RTUSB.ndi.NT.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=15 ;USB
;CpyFiles=NTAMD64.CopyFiles
[WUA1340.ndi.NTAMD64]
AddReg=Common.reg, RTUSB.ndi.NT.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=15 ;USB
;CpyFiles=NTAMD64.CopyFiles
[DWA110.ndi.NTAMD64]
AddReg=Common.reg, RTUSB.ndi.NT.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=15 ;USB
;CpyFiles=NTAMD64.CopyFiles
[D-Link.ndi.NTAMD64.Services]
AddService=RT73, 2, D-Link.Service, common.EventLog
[WUA1340.ndi.NTAMD64.Services]
AddService=RT73, 2, D-Link.Service, common.EventLog
[DWA110.ndi.NTAMD64.Services]
AddService=RT73, 2, D-Link.Service, common.EventLog
[Common.reg]
HKR, , CurProfile, 0,""
HKR, Default, CurProfile, 0,""
HKR, , Radio, 0, "0"
HKR, NDI\params\Radio, ParamDesc, 0, "Radio On/Off"
HKR, NDI\params\Radio, type, 0, "enum"
HKR, NDI\params\Radio, default, 0, "0"
HKR, NDI\params\Radio\enum, 1, 0, "Disable"
HKR, NDI\params\Radio\enum, 0, 0, "Enable"
HKR, , AutoReconnect, 0, "1"
HKR, NDI\params\AutoReconnect, ParamDesc, 0, "Auto Reconnect Mode"
HKR, NDI\params\AutoReconnect, type, 0, "enum"
HKR, NDI\params\AutoReconnect, default, 0, "1"
HKR, NDI\params\AutoReconnect\enum, 0, 0, "Disable"
HKR, NDI\params\AutoReconnect\enum, 1, 0, "Enable"
HKR, , ShowHiddenSSID, 0, "1" ; 0=disable(default), 1=enable
HKR, , OpMode, 0, "0"
HKR, , WirelessMode, 0, "3"
HKR, , TXBurst, 0, "1"
HKR, , ShortSlot, 0, "1"
HKR, , TurboRate, 0, "0"
HKR, , AdhocOfdm, 0, "0"
HKR, , AdhocOfdm, 0, "0"
HKR, NDI\params\AdhocOfdm, ParamDesc, 0, "Adhoc Wireless Mode"
HKR, NDI\params\AdhocOfdm, type, 0, "enum"
HKR, NDI\params\AdhocOfdm, default, 0, "1"
HKR, NDI\params\AdhocOfdm\enum, 0, 0, "802.11 B Only"
HKR, NDI\params\AdhocOfdm\enum, 1, 0, "802.11 B/G Mix"
HKR, NDI\params\AdhocOfdm\enum, 2, 0, "802.11 G Only"
HKR, , BGProtection, 0, "0"
HKR, NDI\params\BGProtection, ParamDesc, 0, "B/G Protection"
HKR, NDI\params\BGProtection, type, 0, "enum"
HKR, NDI\params\BGProtection, default, 0, "0"
HKR, NDI\params\BGProtection\enum, 0, 0, "Auto"
HKR, NDI\params\BGProtection\enum, 1, 0, "On"
HKR, NDI\params\BGProtection\enum, 2, 0, "Off"
HKR, , FrameAggregation,0, "1"
HKR, NDI\params\FrameAggregation, ParamDesc, 0, "Frame Aggregation"
HKR, NDI\params\FrameAggregation, type, 0, "enum"
HKR, NDI\params\FrameAggregation, default, 0, "1"
HKR, NDI\params\FrameAggregation\enum, 0, 0, "Disable"
HKR, NDI\params\FrameAggregation\enum, 1, 0, "Enable"
HKR, , IEEE80211H, 0, "0"
HKR, , AutoChannelSelect, 0, "0"
HKR, , WMMCapable, 0, "1"
HKR, NDI\params\WMMCapable, ParamDesc, 0, "WMM Capable"
HKR, NDI\params\WMMCapable, type, 0, "enum"
HKR, NDI\params\WMMCapable, default, 0, "1"
HKR, NDI\params\WMMCapable\enum, 0, 0, "Disable"
HKR, NDI\params\WMMCapable\enum, 1, 0, "Enable"
HKR, , APSDCapable, 0, "1"
HKR, NDI\params\APSDCapable, ParamDesc, 0, "APSD Capable"
HKR, NDI\params\APSDCapable, type, 0, "enum"
HKR, NDI\params\APSDCapable, default, 0, "1"
HKR, NDI\params\APSDCapable\enum, 0, 0, "Disable"
HKR, NDI\params\APSDCapable\enum, 1, 0, "Enable"
HKR, , APSDAC_BE, 0, "1"
HKR, NDI\params\APSDAC_BE, ParamDesc, 0, "AC_BE support APSD"
HKR, NDI\params\APSDAC_BE, type, 0, "enum"
HKR, NDI\params\APSDAC_BE, default, 0, "1"
HKR, NDI\params\APSDAC_BE\enum, 0, 0, "Disable"
HKR, NDI\params\APSDAC_BE\enum, 1, 0, "Enable"
HKR, , APSDAC_BK, 0, "1"
HKR, NDI\params\APSDAC_BK, ParamDesc, 0, "AC_BK support APSD"
HKR, NDI\params\APSDAC_BK, type, 0, "enum"
HKR, NDI\params\APSDAC_BK, default, 0, "1"
HKR, NDI\params\APSDAC_BK\enum, 0, 0, "Disable"
HKR, NDI\params\APSDAC_BK\enum, 1, 0, "Enable"
HKR, , APSDAC_VI, 0, "1"
HKR, NDI\params\APSDAC_VI, ParamDesc, 0, "AC_VI support APSD"
HKR, NDI\params\APSDAC_VI, type, 0, "enum"
HKR, NDI\params\APSDAC_VI, default, 0, "1"
HKR, NDI\params\APSDAC_VI\enum, 0, 0, "Disable"
HKR, NDI\params\APSDAC_VI\enum, 1, 0, "Enable"
HKR, , APSDAC_VO, 0, "1"
HKR, NDI\params\APSDAC_VO, ParamDesc, 0, "AC_VO support APSD"
HKR, NDI\params\APSDAC_VO, type, 0, "enum"
HKR, NDI\params\APSDAC_VO, default, 0, "1"
HKR, NDI\params\APSDAC_VO\enum, 0, 0, "Disable"
HKR, NDI\params\APSDAC_VO\enum, 1, 0, "Enable"
HKR, , MaxSPLength, 0, "0"
HKR, Default, MaxSPLength, 0, "0"
HKR, NDI\params\MaxSPLength, ParamDesc, 0, "Max Service Period Length"
HKR, NDI\params\MaxSPLength, type, 0, "int"
HKR, Ndi\params\MaxSPLength, default, 0, "0"
HKR, NDI\params\MaxSPLength, min, 0, "0"
HKR, NDI\params\MaxSPLength, max, 0, "3"
HKR, NDI\params\MaxSPLength, step, 0, "1"
HKR, NDI\params\MaxSPLength, optional, 0, "0"
HKR, , DLSCapable, 0, "1"
HKR, NDI\params\DLSCapable, ParamDesc, 0, "DLS Capable"
HKR, NDI\params\DLSCapable, type, 0, "enum"
HKR, NDI\params\DLSCapable, default, 0, "1"
HKR, NDI\params\DLSCapable\enum, 0, 0, "Disable"
HKR, NDI\params\DLSCapable\enum, 1, 0, "Enable"
HKR, , PSPXlink, 0, "1"
HKR, NDI\params\PSPXlink, ParamDesc, 0, "PSP Xlink Mode"
HKR, NDI\params\PSPXlink, type, 0, "enum"
HKR, NDI\params\PSPXlink, default, 0, "1"
HKR, NDI\params\PSPXlink\enum, 0, 0, "Disable"
HKR, NDI\params\PSPXlink\enum, 1, 0, "Enable"
HKR, , CCX2Control, 0x00010001, 0x00fa4600
HKR, , CCX2Control, 0x00010001, 0x00fa4600
HKR, , FstRoam, 0, "0"
HKR, NDI\params\FstRoam, ParamDesc, 0, "Aggressive Roaming Condition"
HKR, NDI\params\FstRoam, type, 0, "enum"
HKR, NDI\params\FstRoam, default, 0, "Disabled"
HKR, NDI\params\FstRoam\enum, 0, 0, "Disabled"
HKR, NDI\params\FstRoam\enum, 1, 0, "-60dbm"
HKR, NDI\params\FstRoam\enum, 2, 0, "-70dbm"
HKR, NDI\params\FstRoam\enum, 3, 0, "-80dbm"
HKR, NDI\params\FstRoam\enum, 4, 0, "-90dbm"
HKR, , VendorDesc, 0, %VENDOR_DESC_DEF_STR%
HKR, Default, VendorDesc, 0, %VENDOR_DESC_DEF_STR%
HKR, , Channel, 0, %CHANNEL%
HKR, Default, Channel, 0, %CHANNEL%
HKR, , NetworkAddress, 0, ""
HKR, Default, NetworkAddress, 0, ""
HKR, NDI\params\NetworkAddress, ParamDesc, 0, "Local Administration MAC Network Address"
HKR, NDI\params\NetworkAddress, type, 0, "edit"
HKR, NDI\params\NetworkAddress, limitText, 0, "12"
HKR, NDI\params\NetworkAddress, default, 0, ""
HKR, , PSMode, 0, "0"
HKR, Default, PSMode, 0, "0"
HKR, NDI\params\PSMode, ParamDesc, 0, "Power Saving Mode"
HKR, NDI\params\PSMode, type, 0, "enum"
HKR, NDI\params\PSMode, default, 0, "0"
HKR, NDI\params\PSMode\enum, 0, 0, "CAM (Constantly Awake Mode)"
HKR, NDI\params\PSMode\enum, 1, 0, "Max_PSP (Max Power Savings)"
HKR, NDI\params\PSMode\enum, 2, 0, "Fast_PSP (Power Save Mode)"
HKR, , ACPowerCam, 0, "0"
HKR, Default, ACPowerCam, 0, "0"
HKR, NDI\params\ACPowerCam, ParamDesc, 0, "CAM when AC Power"
HKR, NDI\params\ACPowerCam, type, 0, "enum"
HKR, NDI\params\ACPowerCam, default, 0, "0"
HKR, NDI\params\ACPowerCam\enum, 0, 0, "Disable"
HKR, NDI\params\ACPowerCam\enum, 1, 0, "Enable"
HKR, , PreambleType, 0, "0"
HKR, Default, PreambleType, 0, "0"
HKR, , RTSThresh, 0, "2347"
HKR, Default, RTSThresh, 0, "2347"
HKR, NDI\params\RTSThresh, ParamDesc, 0, "RTS Threshold"
HKR, NDI\params\RTSThresh, type, 0, "int"
HKR, Ndi\params\RTSThresh, default, 0, "2347"
HKR, NDI\params\RTSThresh, min, 0, "0"
HKR, NDI\params\RTSThresh, max, 0, "2347"
HKR, NDI\params\RTSThresh, step, 0, "32"
HKR, NDI\params\RTSThresh, optional, 0, "0"
HKR, , FragThresh, 0, "2346"
HKR, Default, FragThresh, 0, "2346"
HKR, NDI\params\FragThresh, ParamDesc, 0, "Fragment Threshold"
HKR, NDI\params\FragThresh, type, 0, "int"
HKR, Ndi\params\FragThresh, default, 0, "2346"
HKR, NDI\params\FragThresh, min, 0, "256"
HKR, NDI\params\FragThresh, max, 0, "2346"
HKR, NDI\params\FragThresh, step, 0, "32"
HKR, NDI\params\FragThresh, optional, 0, "0"
HKR, , AuthenType, 0, "0" ; Open System
HKR, Default, AuthenType, 0, "0"
HKR, , Encryption, 0, "1" ; Disable
HKR, Default, Encryption, 0, "1"
HKR, , WEPKeyLen, 0, "0"
HKR, Default, WEPKeyLen, 0, "0"
HKR, , WEPKeyUse, 0,"1"
HKR, Default, WEPKeyUse, 0,"1"
HKR, , WEPKey1, 0,""
HKR, Default, WEPKey1, 0,""
HKR, , WEPKey2, 0,""
HKR, Default, WEPKey2, 0,""
HKR, , WEPKey3, 0,""
HKR, Default, WEPKey3, 0,""
HKR, , WEPKey4, 0,""
HKR, Default, WEPKey4, 0,""
[DRT71W9x.ndi.reg]
HKR, Ndi, DeviceID, 0, "USB\VID_07D1&PID_3C03"
[WUA13409x.ndi.reg]
HKR, Ndi, DeviceID, 0, "USB\VID_07D1&PID_3C04"
[DWA110.ndi.reg]
HKR, Ndi, DeviceID, 0, "USB\VID_07D1&PID_3C07"
[USB9X.ndi.reg]
HKR, , NTMPDriver, 0, Dr71WU98.sys
HKR, , BusType, 0, 15
HKR, NDI, CardType, 0, "PNP"
HKR, , RunningWin9X, 0, "1"
HKR, , DevLoader, 0, "*ndis"
HKR, , DeviceVxDs, 0, "Dr71WU98.sys"
HKR, , EnumPropPages, 0, "netdi.dll,EnumPropPages"
HKR, Ndi\Interfaces, DefUpper, 0, "ndis3"
HKR, Ndi\Interfaces, DefLower, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis3"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, NDIS, LogDriverName, 0, "Dr71WU98"
HKR, NDIS, MajorNdisVersion, 1, 03
HKR, NDIS, MinorNdisVersion, 1, 0A
[DestinationDirs]
NT.CopyFiles=12 ; system32\drivers subdirectory on NT
win9x.CopyFiles=11 ; system32 subdirectory on win9x
NTAMD64.CopyFiles=12 ; system32\drivers
[NT.CopyFiles]
Dr71WU.sys ; NT Installation
[win9x.CopyFiles]
Dr71WU98.sys ; Win9x Installation
[NTAMD64.CopyFiles]
Dr71WU.sys ; NT Installation
[SourceDisksNames]
1=%INSTALL_DISK_STR%,,,
[SourceDisksFiles]
Dr71WU.sys=1
Dr71WU98.sys=1
[SourceDisksFiles.X86]
Dr71WU.sys=1
Dr71WU98.sys=1
[SourceDisksFiles.AMD64]
Dr71WU.sys=1
Dr71WU98.sys=1
[RTUSB.ndi.NT.reg]
HKR, Ndi, Service, 0, "rt73"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
[D-Link.Service]
DisplayName=%D-Link.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_AUTO_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\Dr71WU.sys
LoadOrderGroup=NDIS
[common.EventLog]
AddReg=common.AddEventLog.reg
[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll,%%SystemRoot%%\System32\drivers\Dr71WU.sys"
HKR, , TypesSupported, 0x00010001, 7
[strings]
Provider="D-Link"
D-Link="D-Link"
D-Link.DeviceDesc="D-Link AirPlus G DWL-G122 Wireless USB Adapter(rev.C)"
WUA1340.DeviceDesc="D-Link WUA-1340 USB Adapter"
DWA110.DeviceDesc="D-Link Wireless G DWA-110 USB Adapter"
INSTALL_DISK_STR="D-Link USB Wireless Card Installation Disk"
D-Link.Service.DispName="D-Link USB Wireless LAN Card Driver"
SSID_DEF_STR="dlink"
VENDOR_DESC_DEF_STR="D-Link USB Wireless LAN Card"
NETWORK_TYPE_DEF_STR="1"
CHANNEL="6"

