
[Version]
CatalogFile=airplus.cat
Signature="$Windows NT$"
Provider=%TI%
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
DriverVer=09/08/2003,4.15.5.1
[Manufacturer]
%TI%=D-Link
[ControlFlags]
ExcludeFromSelect=PCI\VEN_104C&DEV_8400&SUBSYS_3B001186
ExcludeFromSelect=PCI\VEN_104C&DEV_8400&SUBSYS_3B011186
[D-Link]
%AIRPLUS.DeviceDesc1%=AIRPLUS.8400, PCI\VEN_104C&DEV_8400&SUBSYS_3B001186
%AIRPLUS.DeviceDesc2%=AIRPLUS.8400, PCI\VEN_104C&DEV_8400&SUBSYS_3B011186
[TI3000P.ndi]
AddReg=AIRPLUS.ndi.reg
[AIRPLUS.8400.NT]
BusType=5
AddReg =AIRPLUS.ndi.reg.NT, TI.Param.Reg
Characteristics=0x84
;CpyFiles =AIRPLUS.8400.CopyFiles.NT, AIRPLUS.8400.BinFiles.NT
[AIRPLUS.ndi.reg.NT]
HKR, Ndi, Service, 0, "AIRPLUS"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
[AIRPLUS.8400.NT.Services]
AddService=AIRPLUS, 2, AIRPLUS.Service, AIRPLUS.EventLog
[AIRPLUS.Service]
DisplayName=%AIRPLUS.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_DEMAND_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\airplus.sys
LoadOrderGroup=NDIS
[AIRPLUS.EventLog]
AddReg=AIRPLUS.AddEventLog.reg
[AIRPLUS.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported, 0x00010001, 7
[AIRPLUS.8400.CopyFiles.NT]
AIRPLUS.sys
[AIRPLUS.8400.BinFiles.NT]
[AIRPLUS.8400]
AddReg=AIRPLUS.ndi.reg, TI.Param.Reg, AIRPLUS.8400.Install
[AIRPLUS.8400.Install]
HKR,Ndi\Install,,,"AIRPLUS.8400.Copy"
HKR,Ndi\Remove,,,"AIRPLUS.8400.Remove"
[AIRPLUS.ndi.reg]
HKR,Ndi,DeviceID,,"PCI\VEN_104C&DEV_8400"
HKR,Ndi,HelpText,0,%WLANAdapterHelpText%
HKR,,DevLoader,,*ndis
HKR,,DeviceVxDs,,airplus.sys
HKR,,EnumPropPages,,"netdi.dll,EnumPropPages"
HKR, NDIS, LogDriverName, , "AIRPLUS"
HKR, NDIS, MajorNdisVersion, 1, 03
HKR, NDIS, MinorNdisVersion, 1, 0A
HKR,Ndi\Interfaces,DefLower,,"ethernet"
HKR,Ndi\Interfaces,LowerRange,,"ethernet"
HKR,Ndi\Interfaces,DefUpper,,"ndis3,ndis4,ndis5"
HKR,Ndi\Interfaces,UpperRange,,"ndis3,ndis4,ndis5"
HKR,Ndi,InstallInf,,"AIRPLUS.INF"
[AIRPLUS.8400.Copy]
;CpyFiles=AIRPLUS.8400.CopyFiles
[AIRPLUS.8400.Remove]
;DlFiles=AIRPLUS.8400.CopyFiles
[AIRPLUS.8400.CopyFiles]
AIRPLUS.sys
[TI.Param.Reg]
HKR, ,Radio11_RxLevel,, "bc b3 a9 9a 90 89 80 79 70 68 64 61 60 55 00"
HKR, ,Radio11_LNA,, "01 01 01 01 01 01 01 01 01 01 01 01 01 01 01"
HKR, ,Radio11_RSSI,, "0a 0f 14 19 1e 23 28 2d 32 37 3c 41 46 4b c8"
HKR, ,Radio0D_RxLevel,, "4f 4a 43 3a 32 2d 56 4e 46 3e 37 2a 23 1f 19"
HKR, ,Radio0D_LNA,, "00 00 00 00 00 00 01 01 01 01 01 01 01 01 01"
HKR, ,Radio0D_RSSI,, "0a 0f 14 19 1e 23 28 2d 32 37 3c 41 46 4b 5a"
HKR, ,Radio15_RxLevel,, "4f 4a 43 3a 32 2d 56 4e 46 3e 37 2a 23 1f 19"
HKR, ,Radio15_LNA,, "00 00 00 00 00 00 01 01 01 01 01 01 01 01 01"
HKR, ,Radio15_RSSI,, "0a 0f 14 19 1e 23 28 2d 32 37 3c 41 46 4b 5a"
HKLM,System\CurrentControlSet\Services\Tcpip\Parameters, TcpWindowSize, 0x10001, 25200
HKR,,PermAddress,,"112233"
HKR, ,HardwareID, ,"ACX100"
HKR, ,NumACXRxDescriptors, ,"10"
HKR, ,NumACXTxDescriptors, ,"10"
HKR, ,LeapUserPassword, ,""
HKR, ,DriverDescription, ,"D-Link AirPlus 22 Mbps Wireless Network Adapter"
HKR,NDI\params\dot11DesiredBSSType,ParamDesc,,"Desired BSS Type"
HKR,NDI\params\dot11DesiredBSSType,type,,"enum"
HKR,NDI\params\dot11DesiredBSSType,default,,"1"
HKR,NDI\params\dot11DesiredBSSType\enum,"0",,"Ad-Hoc"
HKR,NDI\params\dot11DesiredBSSType\enum,"1",,"Infrastructure"
HKR, Ndi\Params\dot11DesiredSSID, ParamDesc, ,"Desired SSID"
HKR, Ndi\Params\dot11DesiredSSID, Type, ,"edit"
HKR, Ndi\Params\dot11DesiredSSID, LimitText, ,"32"
HKR, Ndi\Params\dot11DesiredSSID, Default,,"default"
HKR, Ndi\Params\dot11DesiredSSID, UpperCase,,"0"
HKR,NDI\params\dot11PowerMode,ParamDesc,,"Power Mode"
HKR,NDI\params\dot11PowerMode,type,,"enum"
HKR,NDI\params\dot11PowerMode,default,,"0"
HKR,NDI\params\dot11PowerMode\enum,"0",,"Continuous Access Mode"
HKR,NDI\params\dot11PowerMode\enum,"1",,"Maximum Power Save"
HKR,NDI\params\dot11PowerMode\enum,"2",,"Fast Power Save"
HKR,NDI\params\dot11DesiredTxRate,ParamDesc,, "Desired Tx Rate"
HKR,NDI\params\dot11DesiredTxRate,type,,"enum"
HKR,NDI\params\dot11DesiredTxRate,default,,"0"
HKR,NDI\params\dot11DesiredTxRate\enum,"0",,"Auto"
HKR,NDI\params\dot11DesiredTxRate\enum,"1",,"1 Mbps"
HKR,NDI\params\dot11DesiredTxRate\enum,"2",,"2 Mbps"
HKR,NDI\params\dot11DesiredTxRate\enum,"3",,"5.5 Mbps"
HKR,NDI\params\dot11DesiredTxRate\enum,"4",,"5.5 Mbps PBCC"
HKR,NDI\params\dot11DesiredTxRate\enum,"5",,"11 Mbps"
HKR,NDI\params\dot11DesiredTxRate\enum,"6",,"11 Mbps PBCC"
HKR,NDI\params\dot11DesiredTxRate\enum,"7",,"22 Mbps PBCC"
HKR,NDI\params\dot11SupportedRateMask,ParamDesc,, "Desired Supported Rate Set"
HKR,NDI\params\dot11SupportedRateMask,type,,"enum"
HKR,NDI\params\dot11SupportedRateMask,default,,"2"
HKR,NDI\params\dot11SupportedRateMask\enum,"0",,"1,2 Mbps"
HKR,NDI\params\dot11SupportedRateMask\enum,"1",,"1,2,5.5,11 Mbps"
HKR,NDI\params\dot11SupportedRateMask\enum,"2",,"1,2,5.5,11,22 Mbps"
HKR,NDI\params\dot11BasicRateMask,ParamDesc,, "Desired Basic Rate Set"
HKR,NDI\params\dot11BasicRateMask,type,,"enum"
HKR,NDI\params\dot11BasicRateMask,default,,"0"
HKR,NDI\params\dot11BasicRateMask\enum,"0",,"1,2,5.5,11 Mbps"
HKR,NDI\params\dot11BasicRateMask\enum,"1",,"1,2 Mbps"
HKR, Ndi\Params\dot11FragmentationThreshold, ParamDesc, ,"Fragmentation Threshold"
HKR, Ndi\Params\dot11FragmentationThreshold, Type, , "int"
HKR, Ndi\Params\dot11FragmentationThreshold, Default, , "4096"
HKR, Ndi\Params\dot11FragmentationThreshold, Min, , "256"
HKR, Ndi\Params\dot11FragmentationThreshold, Max, , "6000"
HKR, Ndi\Params\dot11FragmentationThreshold, Step, , "1"
HKR, Ndi\Params\dot11FragmentationThreshold, Base, , "10"
HKR, Ndi\Params\dot11RTSThreshold, ParamDesc, ,"RTS Threshold"
HKR, Ndi\Params\dot11RTSThreshold, Type, , "int"
HKR, Ndi\Params\dot11RTSThreshold, Default, , "4096"
HKR, Ndi\Params\dot11RTSThreshold, Min, , "0"
HKR, Ndi\Params\dot11RTSThreshold, Max, , "6000"
HKR, Ndi\Params\dot11RTSThreshold, Step, , "1"
HKR, Ndi\Params\dot11RTSThreshold, Base, , "10"
HKR, ,ackE4x, ,"0"
HKR,NDI\params\PrivacyMode,ParamDesc,,"Privacy Mode"
HKR,NDI\params\PrivacyMode,type,,"enum"
HKR,NDI\params\PrivacyMode,default,,"2"
HKR,NDI\params\PrivacyMode\enum,"0",,"No Privacy"
HKR,NDI\params\PrivacyMode\enum,"1",,"WEP"
HKR,NDI\params\PrivacyMode\enum,"2",,"Windows Zero Config"
HKR,NDI\params\dot11WEPStatus,ParamDesc,,"WEP Option"
HKR,NDI\params\dot11WEPStatus,type,,"enum"
HKR,NDI\params\dot11WEPStatus,default,,"1"
HKR,NDI\params\dot11WEPStatus\enum,"0",,"WEP Enabled"
HKR,NDI\params\dot11WEPStatus\enum,"1",,"WEP Disabled"
HKR,NDI\params\dot11AuthenticationMode,ParamDesc,,"Authentication Mode"
HKR,NDI\params\dot11AuthenticationMode,type,,"enum"
HKR,NDI\params\dot11AuthenticationMode,default,,"0"
HKR,NDI\params\dot11AuthenticationMode\enum,"0",,"Open Authentication"
HKR,NDI\params\dot11AuthenticationMode\enum,"1",,"Shared Authentication"
HKR,NDI\params\dot11AuthenticationMode\enum,"2",,"Auto Switch"
HKR,NDI\params\dot11ShortPreambleInvoked,ParamDesc,,"Short Preamble"
HKR,NDI\params\dot11ShortPreambleInvoked,type,,"enum"
HKR,NDI\params\dot11ShortPreambleInvoked,default,,"0"
HKR,NDI\params\dot11ShortPreambleInvoked\enum,"0",,"Off"
HKR,NDI\params\dot11ShortPreambleInvoked\enum,"1",,"On"
HKR,NDI\params\Mode4x,ParamDesc,,"Mode4x"
HKR,NDI\params\Mode4x,type,,"enum"
HKR,NDI\params\Mode4x,default,,"1"
HKR,NDI\params\Mode4x\enum,"0",,"Off"
HKR,NDI\params\Mode4x\enum,"1",,"On"
HKR,NDI\params\MixedMode,ParamDesc,,"Privacy Mixed Mode"
HKR,NDI\params\MixedMode,type,,"enum"
HKR,NDI\params\MixedMode,default,,"0"
HKR,NDI\params\MixedMode\enum,"0",,"Disabled"
HKR,NDI\params\MixedMode\enum,"1",,"Enabled"
HKR, Ndi\Params\RateFallBackRetryLimit, ParamDesc, ,"Rate FallBack Retry Limit"
HKR, Ndi\Params\RateFallBackRetryLimit, Type, , "int"
HKR, Ndi\Params\RateFallBackRetryLimit, Default, , "1"
HKR, Ndi\Params\RateFallBackRetryLimit, Min, , "0"
HKR, Ndi\Params\RateFallBackRetryLimit, Max, , "255"
HKR, Ndi\Params\RateFallBackRetryLimit, Step, , "1"
HKR, Ndi\Params\RateFallBackRetryLimit, Base, , "10"
HKR, Ndi\Params\RateFallBackThreshold, ParamDesc, ,"Rate FallBack Threshold"
HKR, Ndi\Params\RateFallBackThreshold, Type, , "int"
HKR, Ndi\Params\RateFallBackThreshold, Default, , "12"
HKR, Ndi\Params\RateFallBackThreshold, Min, , "0"
HKR, Ndi\Params\RateFallBackThreshold, Max, , "100"
HKR, Ndi\Params\RateFallBackThreshold, Step, , "1"
HKR, Ndi\Params\RateFallBackThreshold, Base, , "10"
HKR, Ndi\Params\RateStepUpThreshold, ParamDesc, ,"Rate StepUp Threshold"
HKR, Ndi\Params\RateStepUpThreshold, Type, , "int"
HKR, Ndi\Params\RateStepUpThreshold, Default, , "3"
HKR, Ndi\Params\RateStepUpThreshold, Min, , "0"
HKR, Ndi\Params\RateStepUpThreshold, Max, , "100"
HKR, Ndi\Params\RateStepUpThreshold, Step, , "1"
HKR, Ndi\Params\RateStepUpThreshold, Base, , "10"
HKR, Ndi\Params\FBShortInterval, ParamDesc, ,"FB Short Interval"
HKR, Ndi\Params\FBShortInterval, Type, , "int"
HKR, Ndi\Params\FBShortInterval, Default, , "50"
HKR, Ndi\Params\FBShortInterval, Min, , "50"
HKR, Ndi\Params\FBShortInterval, Max, , "2000"
HKR, Ndi\Params\FBShortInterval, Step, , "10"
HKR, Ndi\Params\FBShortInterval, Base, , "10"
HKR, Ndi\Params\FBLongInterval, ParamDesc, ,"FB Long Interval"
HKR, Ndi\Params\FBLongInterval, Type, , "int"
HKR, Ndi\Params\FBLongInterval, Default, , "2000"
HKR, Ndi\Params\FBLongInterval, Min, , "1000"
HKR, Ndi\Params\FBLongInterval, Max, , "10000"
HKR, Ndi\Params\FBLongInterval, Step, , "10"
HKR, Ndi\Params\FBLongInterval, Base, , "10"
HKR,NDI\params\dot11TxAntenna,ParamDesc,,"Antenna TX"
HKR,NDI\params\dot11TxAntenna,type,,"enum"
HKR,NDI\params\dot11TxAntenna,default,,"0"
HKR,NDI\params\dot11TxAntenna\enum,"0",,"Antenna 1"
HKR,NDI\params\dot11TxAntenna\enum,"1",,"Antenna 2"
HKR,NDI\params\dot11RxAntenna,ParamDesc,,"Antenna RX"
HKR,NDI\params\dot11RxAntenna,type,,"enum"
HKR,NDI\params\dot11RxAntenna,default,,"2"
HKR,NDI\params\dot11RxAntenna\enum,"0",,"Antenna 1"
HKR,NDI\params\dot11RxAntenna\enum,"1",,"Antenna 2"
HKR,NDI\params\dot11RxAntenna\enum,"2",,"Both"
HKR, Ndi\Params\dot11DesiredChannel, ParamDesc, ,"Desired Channel"
HKR, Ndi\Params\dot11DesiredChannel, Type, , "int"
HKR, Ndi\Params\dot11DesiredChannel, Default, , "6"
HKR, Ndi\Params\dot11DesiredChannel, Min, , "1"
HKR, Ndi\Params\dot11DesiredChannel, Max, , "14"
HKR, Ndi\Params\dot11DesiredChannel, Step, , "1"
HKR, Ndi\Params\dot11DesiredChannel, Base, , "10"
[DestinationDirs]
DefaultDestDir=12 ; System Directory
AIRPLUS.8400.CopyFiles=11
AIRPLUS.8400.BinFiles.NT=10,system
[SourceDisksNames]
1=%DiskName%,,
[SourceDisksFiles]
AIRPLUS.sys=1
[Strings]
TI="D-Link"
AIRPLUS.DeviceDesc1="D-Link AirPlus DWL-650+ Wireless Cardbus Adapter"
AIRPLUS.DeviceDesc2="D-Link AirPlus DWL-520+ Wireless PCI Adapter"
AIRPLUS.Service.DispName="D-Link AirPlus Wireless Adapter"
WLANAdapterHelpText="A D-Link AirPlus Wireless Adapter provides high speed connection to the Internet through 802.11b technology"
DiskName="D-Link AirPlus Wireless Adapter Installation Disk"
