
[Version]
Signature="$CHICAGO$"
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%SMC%
Compatible=1
DriverVer=05/31/2003,2.4.0.71
Catalogfile=smc11ab.cat
[Manufacturer]
%SMC%=SMC
[ControlFlags]
ExcludeFromSelect=*
[SMC]
%ATHER.DeviceDesc.2335%=ATHER_DEV_2335.ndi, PCI\VEN_168C&DEV_0012&SUBSYS_233510B8
[ATHER_DEV_2335.ndi]
AddReg=ATHER_DEV_2335.id.reg, 5211.reg, ATHER.win.reg, 5212.abg.reg
;CpyFiles=ATHER.win.CopyFiles, DEFAULTDESTDIRS
;DlFiles=ATHER.DelIniFiles
[ATHER_DEV_2335.ndi.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5
AddReg=5211.reg, ATHER.reg, 5211.reg, 5212.abg.reg
;CpyFiles=ATHER.CopyFiles.nt, DEFAULTDESTDIRS
;DlFiles=ATHER.DelIniFiles
[ATHER_DEV_2335.ndi.NT.Services]
AddService=SMC11AB, 2, ATHER.Service, common.EventLog
[ATHER_DEV_2335.id.reg]
HKR, Ndi, DeviceID, 0, "PCI\VEN_168C&DEV_0012&SUBSYS_233510B8"
[5212.abg.reg]
HKR, , NetBand, 0x00002, "7"
HKR, CustomParams\Configurations, NicType, 0x10003, 1
HKR, CustomParams\Configurations\Cfg0, NetBand, 0x10003, 7
[5211.reg]
HKR, Ndi\params\MapRegisters, ParamDesc, 0, %MapRegisters%
HKR, Ndi\params\MapRegisters, default, 0, "256"
HKR, Ndi\params\MapRegisters, min, 0, "32"
HKR, Ndi\params\MapRegisters, max, 0, "512"
HKR, Ndi\params\MapRegisters, step, 0, "8"
HKR, Ndi\params\MapRegisters, base, 0, "10"
HKR, Ndi\params\MapRegisters, type, 0, "int"
HKR, Ndi\params\NetworkAddress, ParamDesc, 0, %NetworkAddress%
HKR, Ndi\params\NetworkAddress, default, 0, ""
HKR, Ndi\params\NetworkAddress, LimitText, 0, "12"
HKR, Ndi\params\NetworkAddress, UpperCase, 0, "1"
HKR, Ndi\params\NetworkAddress, optional, 0, "1"
HKR, Ndi\params\NetworkAddress, type, 0, "edit"
HKR, Ndi\params\sleepMode, ParamDesc, 0, %sleepMode%
HKR, Ndi\params\sleepMode, Base, 0, "10"
HKR, Ndi\params\sleepMode, default, 0, "2"
HKR, Ndi\params\sleepMode, type, 0, "enum"
HKR, Ndi\params\sleepMode\enum, "0", 0, %sleepModeOff%
HKR, Ndi\params\sleepMode\enum, "2", 0, %sleepModeNormal%
HKR, Ndi\params\sleepMode\enum, "1", 0, %sleepModeMax%
HKR, Ndi\params\tpc, ParamDesc, 0, %tpc%
HKR, Ndi\params\tpc, Base, 0, "10"
HKR, Ndi\params\tpc, default, 0, "0"
HKR, Ndi\params\tpc, type, 0, "enum"
HKR, Ndi\params\tpc\enum, "0", 0, %tpc100%
HKR, Ndi\params\tpc\enum, "1", 0, %tpc50%
HKR, Ndi\params\tpc\enum, "2", 0, %tpc25%
HKR, Ndi\params\tpc\enum, "3", 0, %tpc12%
HKR, Ndi\params\tpc\enum, "4", 0, %tpcLowest%
HKR, Ndi\params\shortPreamble, ParamDesc, 0, %shortPreamble%
HKR, Ndi\params\shortPreamble, Base, 0, "10"
HKR, Ndi\params\shortPreamble, default, 0, "1"
HKR, Ndi\params\shortPreamble, type, 0, "enum"
HKR, Ndi\params\shortPreamble\enum, "1", 0, %shortPreambleEnable%
HKR, Ndi\params\shortPreamble\enum, "0", 0, %shortPreambleDisable%
HKR, Ndi\params\radioEnable, ParamDesc, 0, %radioEnable%
HKR, Ndi\params\radioEnable, Base, 0, "10"
HKR, Ndi\params\radioEnable, default, 0, "1"
HKR, Ndi\params\radioEnable, type, 0, "enum"
HKR, Ndi\params\radioEnable\enum, "1", 0, %radioEnableOn%
HKR, Ndi\params\radioEnable\enum, "0", 0, %radioEnableOff%
HKR, Ndi\params\authTypeUseOnly, ParamDesc, 0, %authTypeUseOnly%
HKR, Ndi\params\authTypeUseOnly, Base, 0, "10"
HKR, Ndi\params\authTypeUseOnly, default, 0, "0"
HKR, Ndi\params\authTypeUseOnly, type, 0, "enum"
HKR, Ndi\params\authTypeUseOnly\enum, "0", 0, %authAuto%
HKR, Ndi\params\authTypeUseOnly\enum, "1", 0, %authOpen%
HKR, Ndi\params\authTypeUseOnly\enum, "2", 0, %authShared%
HKR, , AdHocBand, 0x00002, "0"
HKR, , AwakeTimePerf, 0x00002, "200"
HKR, , beaconInterval, 0x00002, "100"
HKR, , bkScanEnable, 0x00002, "1"
HKR, , bssType, 0x00002, "1"
HKR, , ccode, 0x00002, "US"
HKR, , clist, 0x00002, ""
HKR, , defaultKey, 0x00002, "0"
HKR, , EncryptionAlg, 0x00002, "2"
HKR, , FragThreshold, 0x00002, "2346"
HKR, , HwTxRetries, 0x00002, "4"
HKR, , privacyInvoked, 0x00002, "0"
HKR, , QoS, 0x00002, "0"
HKR, , rateCtrlEnable, 0x00002, "1"
HKR, , RTSThreshold, 0x00002, "2346"
HKR, , scanType, 0x00002, "2"
HKR, , SwTxRetryScale, 0x00002, "6"
HKR, , SmeEnable, 0x00002, "1"
HKR, CustomParams\Configurations, MajorVersion, 0x10003, 2
HKR, CustomParams\Configurations, MinorVersion, 0x10003, 0
HKR, CustomParams\Configurations, SelectedConfigurationIndex, 0x10003, 0
HKR, CustomParams\Configurations, SelectedConfigurationName, 0x00002, "Default"
HKR, CustomParams\Configurations\Cfg0, AdHocBand, 0x10003, 1
HKR, CustomParams\Configurations\Cfg0, ConfigurationName, 0x00002, "Default"
HKR, CustomParams\Configurations\Cfg0, DefaultKey, 0x10003, 0
HKR, CustomParams\Configurations\Cfg0, EnableMacAddress, 0x10003, 0
HKR, CustomParams\Configurations\Cfg0, EnableSecurity, 0x10003, 0
HKR, CustomParams\Configurations\Cfg0, EncryptionAlg, 0x10003, 4
HKR, CustomParams\Configurations\Cfg0, HexEntry, 0x10003, 1
HKR, CustomParams\Configurations\Cfg0, leapEnabled, 0x10003, 0
HKR, CustomParams\Configurations\Cfg0, MacAddress, 0x00002, ""
HKR, CustomParams\Configurations\Cfg0, NetworkConnectionType, 0x10003, 1
HKR, CustomParams\Configurations\Cfg0, NetworkName, 0x00002, ""
HKR, CustomParams\Configurations\Cfg0, PowerManagement, 0x10003, 1
HKR, CustomParams\Configurations\Cfg0, Preamble, 0x10003, 1
HKR, CustomParams\Configurations\Cfg0, QoS, 0x10003, 0
HKR, CustomParams\Configurations\Cfg0, scanType, 0x10003, 2
HKR, CustomParams\Configurations\Cfg0, tpc, 0x10003, 0
[ATHER.reg]
HKR, Ndi, Service, 0, "SMC11AB"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, , aifs, 0, "2"
HKR, , cwmin, 0, "15"
[ATHER.Service]
DisplayName=%ATHER.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_DEMAND_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\smc11ab.sys
LoadOrderGroup=NDIS
[common.EventLog]
AddReg=common.AddEventLog.reg
[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported, 0x00010001, 7
[ATHER.win.reg]
HKR, , DevLoader, 0, "*ndis"
HKR, , DeviceVxDs, 0, "smc119x.sys"
HKR, , EnumPropPages, 0, "netdi.dll,EnumPropPages"
HKR, Ndi\Interfaces, DefUpper, 0, "ndis3"
HKR, Ndi\Interfaces, DefLower, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis3"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, NDIS, LogDriverName, 0, "SMC119X"
HKR, NDIS, MajorNdisVersion, 1, 03
HKR, NDIS, MinorNdisVersion, 1, 0A
HKR, , aifs, 0, "2"
HKR, , cwmin, 0, "15"
HKR, Ndi\Install, ndis3, 0, "ATHER.install"
[ATHER.win.CopyFiles]
smc119x.sys,,,2
[ATHER.CopyFiles.nt]
smc11ab.sys,,,2
[ATHER.DelIniFiles]
Athnic.ini,,,1
[SourceDisksNames]
1=%SMC_Disk%,,,
[SourceDisksFiles]
smc11ab.sys=1,, ; on distribution disk 1
[DestinationDirs]
ATHER.CopyFiles.nt=12
ATHER.win.CopyFiles=10,system32\drivers ; %SystemRoot%\system32\drivers
ATHER.DelIniFiles=10,system32\drivers ; %SystemRoot%\system32\drivers
DefaultDestDir=11
[DEFAULTDESTDIRS]
[Strings]
SMC="SMC"
authTypeUseOnly="802.11 Authentication Type"
authAuto="Auto"
authOpen="Open"
authShared="Shared"
MapRegisters="Map Registers"
NetworkAddress="Network Address"
sleepMode="Power Save Mode"
sleepModeOff="Off"
sleepModeNormal="Normal"
sleepModeMax="Maximum"
tpc="Transmit Power"
tpcLowest="Lowest"
tpc12="12.5%"
tpc25="25%"
tpc50="50%"
tpc100="100%"
shortPreamble="802.11b Preamble"
shortPreambleEnable="Long and Short"
shortPreambleDisable="Long only"
radioEnable="Radio On/Off"
radioEnableOn="On"
radioEnableOff="Off"
SMC_Disk="SMC Driver Disk 1"
ATHER.DeviceDesc.2335="SMC2335W Universal Wireless Cardbus Adapter"
ATHER.Service.DispName="SMC2335W Universal Wireless Cardbus Adapter Service"
