
[Version]
Signature="$Chicago$"
Compatible=1
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
MillenniumPreferred=.ME
Provider=%VENDOR%
DriverVer=10/09/2002, 4.3.3.57
[Manufacturer]
%VENDOR%=OEM, NTx86.5.1
[ControlFlags]
ExcludeFromSelect=OEM-11Mbps_Wireless_LAN_PC_Card_V-3(3V)-A10A, \
OEM-11Mbps_Wireless_LAN_PC_Card_V-3-DE3A
[OEM]
%PCMCIAOEM3V.DeviceDesc%=PCMCIAOEM3V.Ndi, PCMCIA\OEM-11Mbps_Wireless_LAN_PC_Card_V-3(3V)-A10A
%PCMCIAOEM5V.DeviceDesc%=PCMCIAOEM5V.Ndi, PCMCIA\OEM-11Mbps_Wireless_LAN_PC_Card_V-3-DE3A
[OEM.NTx86.5.1]
%PCMCIAOEM3V.DeviceDesc%=PCMCIAOEM3V.XPNdi, PCMCIA\OEM-11Mbps_Wireless_LAN_PC_Card_V-3(3V)-A10A
%PCMCIAOEM5V.DeviceDesc%=PCMCIAOEM5V.XPNdi, PCMCIA\OEM-11Mbps_Wireless_LAN_PC_Card_V-3-DE3A
[PCMCIAOEM3V.XPNdi.NT]
Characteristics=0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType=8 ; PCMCIA
AddReg=PCMCIAFVNETR.XP.Reg, PCMCIAFVNETR.XP.Params
;CpyFiles=CopyFile.XP.Sys
[PCMCIAOEM5V.XPNdi.NT]
Characteristics=0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType=8 ; PCMCIA
AddReg=PCMCIAFVNETR.XP.Reg, PCMCIAFVNETR.XP.Params
;CpyFiles=CopyFile.XP.Sys
[PCMCIAOEM3V4.XPNdi.NT]
Characteristics=0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType=8 ; PCMCIA
AddReg=PCMCIAFVNETR.XP.Reg, PCMCIAFVNETR.XP.Params
;CpyFiles=CopyFile.XP.Sys
[PCMCIAOEM5V4.XPNdi.NT]
Characteristics=0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType=8 ; PCMCIA
AddReg=PCMCIAFVNETR.XP.Reg, PCMCIAFVNETR.XP.Params
;CpyFiles=CopyFile.XP.Sys
[PCMCIAOEM3V.XPNdi.NT.Services]
AddService="PCMCIAFVNETR", 2, PCMCIAFVNETR.XP.Service, Common.EventLog
[PCMCIAOEM5V.XPNdi.NT.Services]
AddService="PCMCIAFVNETR", 2, PCMCIAFVNETR.XP.Service, Common.EventLog
[PCMCIAOEM3V4.XPNdi.NT.Services]
AddService="PCMCIAFVNETR", 2, PCMCIAFVNETR.XP.Service, Common.EventLog
[PCMCIAOEM5V4.XPNdi.NT.Services]
AddService="PCMCIAFVNETR", 2, PCMCIAFVNETR.XP.Service, Common.EventLog
[PCMCIAOEM3V.Ndi.NT]
Characteristics=0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType=8 ; PCMCIA
AddReg=PCMCIAFVNETR.NT.Reg, PCMCIAFVNETR.Params
;CpyFiles=CopyFile.NT.Sys
[PCMCIAOEM5V.Ndi.NT]
Characteristics=0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType=8 ; PCMCIA
AddReg=PCMCIAFVNETR.NT.Reg, PCMCIAFVNETR.Params
;CpyFiles=CopyFile.NT.Sys
[PCMCIAOEM3V4.Ndi.NT]
Characteristics=0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType=8 ; PCMCIA
AddReg=PCMCIAFVNETR.NT.Reg, PCMCIAFVNETR.Params
;CpyFiles=CopyFile.NT.Sys
[PCMCIAOEM5V4.Ndi.NT]
Characteristics=0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType=8 ; PCMCIA
AddReg=PCMCIAFVNETR.NT.Reg, PCMCIAFVNETR.Params
;CpyFiles=CopyFile.NT.Sys
[PCMCIAOEM3V.Ndi.NT.Services]
AddService="PCMCIAFVNETR", 2, PCMCIAFVNETR.Service, Common.EventLog
[PCMCIAOEM5V.Ndi.NT.Services]
AddService="PCMCIAFVNETR", 2, PCMCIAFVNETR.Service, Common.EventLog
[PCMCIAOEM3V4.Ndi.NT.Services]
AddService="PCMCIAFVNETR", 2, PCMCIAFVNETR.Service, Common.EventLog
[PCMCIAOEM5V4.Ndi.NT.Services]
AddService="PCMCIAFVNETR", 2, PCMCIAFVNETR.Service, Common.EventLog
[PCMCIAOEM3V.Ndi]
AddReg=DEVICE3V.Reg, PCMCIAFVNETR.Reg, PCMCIAFVNETR.Params
;CpyFiles= CopyFile.Sys
[PCMCIAOEM5V.Ndi]
AddReg=DEVICE5V.Reg, PCMCIAFVNETR.Reg, PCMCIAFVNETR.Params
;CpyFiles= CopyFile.Sys
[PCMCIAOEM3V4.Ndi]
AddReg=DEVICE3V4.Reg, PCMCIAFVNETR.Reg, PCMCIAFVNETR.Params
;CpyFiles= CopyFile.Sys
[PCMCIAOEM5V4.Ndi]
AddReg=DEVICE5V4.Reg, PCMCIAFVNETR.Reg, PCMCIAFVNETR.Params
;CpyFiles= CopyFile.Sys
[DEVICE3V.Reg]
HKR,Ndi,DeviceID,,PCMCIA\OEM-11Mbps_Wireless_LAN_PC_Card_V-3(3V)-A10A
[DEVICE5V.Reg]
HKR,Ndi,DeviceID,,OEM-11Mbps_Wireless_LAN_PC_Card_V-3-DE3A
[DEVICE3V4.Reg]
HKR,Ndi,DeviceID,,PCMCIA\OEM-11Mbps_Wireless_LAN_PC_Card_V-4(3V)-1BA0
[DEVICE5V4.Reg]
HKR,Ndi,DeviceID,,PCMCIA\OEM-11Mbps_Wireless_LAN_PC_Card_V-4-10F6
[PCMCIAFVNETR.Reg]
HKR,Ndi,CardType,,"PNP"
HKR,,BusType,0,"8"
HKR,,EnableIRQSharing,1,01,00,00,00
HKR,,IOBaseAddress,1,02,00,00,00
HKR,,InterruptNumber,1,04,00,00,00
HKR,,DevLoader,,*ndis,*ntkern,*ndis
HKR,,DeviceVxDs,,fvnetr.sys
HKR,NDIS,MajorNdisVersion,1,05
HKR,NDIS,MinorNdisVersion,1,00
HKR,NDIS,LogDriverName,,"fvnetr"
HKR,Ndi\Interfaces,DefUpper,,"ndis3"
HKR,Ndi\Interfaces,DefLower,,"ethernet"
HKR,Ndi\Interfaces,UpperRange,,"ndis3"
HKR,Ndi\Interfaces,LowerRange,,"ethernet"
HKR,Ndi,HelpText,,%Help_Text%
[PCMCIAOEM3V.Ndi.ME]
AddReg=DEVICE3V.ME.Reg, PCMCIAFVNETR.ME.Reg, PCMCIAFVNETR.Params
;CpyFiles= CopyFile.Sys
[PCMCIAOEM5V.Ndi.ME]
AddReg=DEVICE5V.ME.Reg, PCMCIAFVNETR.ME.Reg, PCMCIAFVNETR.Params
;CpyFiles= CopyFile.Sys
[PCMCIAOEM3V4.Ndi.ME]
AddReg=DEVICE3V4.ME.Reg, PCMCIAFVNETR.ME.Reg, PCMCIAFVNETR.Params
;CpyFiles= CopyFile.Sys
[PCMCIAOEM5V4.Ndi.ME]
AddReg=DEVICE5V4.ME.Reg, PCMCIAFVNETR.ME.Reg, PCMCIAFVNETR.Params
;CpyFiles= CopyFile.Sys
[PCMCIAOEM3V.Ndi.ME.Services]
AddService="PCMCIAFVNETR", 2, PCMCIAFVNETR.Service, Common.EventLog
[PCMCIAOEM5V.Ndi.ME.Services]
AddService="PCMCIAFVNETR", 2, PCMCIAFVNETR.Service, Common.EventLog
[PCMCIAOEM3V4.Ndi.ME.Services]
AddService="PCMCIAFVNETR", 2, PCMCIAFVNETR.Service, Common.EventLog
[PCMCIAOEM5V4.Ndi.ME.Services]
AddService="PCMCIAFVNETR", 2, PCMCIAFVNETR.Service, Common.EventLog
[DEVICE3V.ME.Reg]
HKR,Ndi,DeviceID,,PCMCIA\OEM-11Mbps_Wireless_LAN_PC_Card_V-3(3V)-A10A
[DEVICE5V.ME.Reg]
HKR,Ndi,DeviceID,,OEM-11Mbps_Wireless_LAN_PC_Card_V-3-DE3A
[DEVICE3V4.ME.Reg]
HKR,Ndi,DeviceID,,PCMCIA\OEM-11Mbps_Wireless_LAN_PC_Card_V-4(3V)-1BA0
[DEVICE5V4.ME.Reg]
HKR,Ndi,DeviceID,,PCMCIA\OEM-11Mbps_Wireless_LAN_PC_Card_V-4-10F6
[PCMCIAFVNETR.ME.Reg]
HKR,Ndi,CardType,,"PNP"
HKR,,DevLoader,,*ndis,*ntkern,*ndis
HKR,,DeviceVxDs,,fvnetr.sys
HKR,NDIS,MajorNdisVersion,1,05
HKR,NDIS,MinorNdisVersion,1,00
HKR,NDIS,LogDriverName,,"fvnetr"
HKR,Ndi\Interfaces,DefUpper,,"ndis3"
HKR,Ndi\Interfaces,DefLower,,"ethernet"
HKR,Ndi\Interfaces,UpperRange,,"ndis3"
HKR,Ndi\Interfaces,LowerRange,,"ethernet"
HKR,Ndi,HelpText,,%Help_Text%
HKR, Ndi\Install, ndis3, 0, "PCMCIAFVNETR.ndis5me"
[PCMCIAFVNETR.ndis5me]
;CpyFiles=CopyFile.Sys
[PCMCIAFVNETR.Params]
HKR, Ndi\params\Channel, ParamDesc, 0, %ChannelStr%
HKR, Ndi\params\Channel, type, 0, "int"
HKR, Ndi\params\Channel, default, 0, "3"
HKR, Ndi\params\Channel, min, 0, "1"
HKR, Ndi\params\Channel, max, 0, "14"
HKR, Ndi\params\Channel, step, 0, "1"
HKR, , Channel, 0, "3"
HKR, Ndi\params\Rate, ParamDesc, 0, %RateStr%
HKR, Ndi\params\Rate, type, 0, "enum"
HKR, Ndi\params\Rate, default, 0, "3"
HKR, Ndi\params\Rate\enum, 0, 0, %Fixed1Str%
HKR, Ndi\params\Rate\enum, 1, 0, %Fixed2Str%
HKR, Ndi\params\Rate\enum, 2, 0, %Fixed55Str%
HKR, Ndi\params\Rate\enum, 3, 0, %Fixed11Str%
HKR, Ndi\params\Rate\enum, 4, 0, %AutoStr%
HKR, , Rate, 0, "3"
HKR, Ndi\params\RTS_Threshold, ParamDesc, 0, %RTS_Str%
HKR, Ndi\params\RTS_Threshold, type, 0, "int"
HKR, Ndi\params\RTS_Threshold, default, 0, "2347"
HKR, Ndi\params\RTS_Threshold, min, 0, "0"
HKR, Ndi\params\RTS_Threshold, max, 0, "2347"
HKR, Ndi\params\RTS_Threshold, step, 0, "1"
HKR, , RTS_Threshold, 0, "2347"
HKR, Ndi\params\Frag_Threshold, ParamDesc, 0, %FragmentationStr%
HKR, Ndi\params\Frag_Threshold, type, 0, "int"
HKR, Ndi\params\Frag_Threshold, default, 0, "2346"
HKR, Ndi\params\Frag_Threshold, min, 0, "256"
HKR, Ndi\params\Frag_Threshold, max, 0, "2346"
HKR, Ndi\params\Frag_Threshold, step, 0, "1"
HKR, , Frag_Threshold, 0, "2346"
HKR, Ndi\params\Operating_Mode, ParamDesc, 0, %OperatingModeStr%
HKR, Ndi\params\Operating_Mode, type, 0, "enum"
HKR, Ndi\params\Operating_Mode, default, 0, "1"
HKR, Ndi\params\Operating_Mode\enum, 0, 0, %AdHocStr%
HKR, Ndi\params\Operating_Mode\enum, 1, 0, %InfrastructureStr%
HKR, , Operating_Mode, 0, "1"
HKR, Ndi\params\ESSID, ParamDesc, 0, %ESSID_Str%
HKR, Ndi\params\ESSID, type, 0, "edit"
HKR, Ndi\params\ESSID, default, 0, ""
HKR, Ndi\params\ESSID, LimitText, 0, "32"
HKR, Ndi\params\ESSID, UpperCase, 0, "0"
HKR, , ESSID, 0, ""
HKR,Ndi\params\WEP_KEY_INDEX, ParamDesc, 0,%WEP_Key_Str%
HKR,Ndi\params\WEP_KEY_INDEX, type, 0,"enum"
HKR,Ndi\params\WEP_KEY_INDEX, default, 0,"0"
HKR,Ndi\params\WEP_KEY_INDEX\enum, 0, 0,%Key1Str%
HKR,Ndi\params\WEP_KEY_INDEX\enum, 1, 0,%Key2Str%
HKR,Ndi\params\WEP_KEY_INDEX\enum, 2, 0,%Key3Str%
HKR,Ndi\params\WEP_KEY_INDEX\enum, 3, 0,%Key4Str%
HKR,, WEP_KEY_INDEX, 0,"0"
HKR,Ndi\params\EncryptionLevel, ParamDesc, 0,"Encryption Level"
HKR,Ndi\params\EncryptionLevel, type, 0,"enum"
HKR,Ndi\params\EncryptionLevel, default, 0,"0"
HKR,Ndi\params\EncryptionLevel\enum, 0, 0,%DisabledStr%
HKR,Ndi\params\EncryptionLevel\enum, 1, 0,%64bit%
HKR,Ndi\params\EncryptionLevel\enum, 2, 0,%128bit%
HKR,, EncryptionLevel,0,"0"
HKR,Ndi\params\WEP_KEY_1, ParamDesc, 0,%KEY1_Str%
HKR,Ndi\params\WEP_KEY_1, type, 0,"edit"
HKR,Ndi\params\WEP_KEY_1, default, 0,"0000000000"
HKR,Ndi\params\WEP_KEY_1, LimitText, 0,"10"
HKR,Ndi\params\WEP_KEY_1, UpperCase, 0,"1"
HKR,, WEP_KEY_1, 0,"0000000000"
HKR,Ndi\params\WEP_KEY_2, ParamDesc, 0,%KEY2_Str%
HKR,Ndi\params\WEP_KEY_2, type, 0,"edit"
HKR,Ndi\params\WEP_KEY_2, default, 0,"0000000000"
HKR,Ndi\params\WEP_KEY_2, LimitText, 0,"10"
HKR,Ndi\params\WEP_KEY_2, UpperCase, 0,"1"
HKR,, WEP_KEY_2, 0,"0000000000"
HKR,Ndi\params\WEP_KEY_3, ParamDesc, 0,%KEY3_Str%
HKR,Ndi\params\WEP_KEY_3, type, 0,"edit"
HKR,Ndi\params\WEP_KEY_3, default, 0,"0000000000"
HKR,Ndi\params\WEP_KEY_3, LimitText, 0,"10"
HKR,Ndi\params\WEP_KEY_3, UpperCase, 0,"1"
HKR,, WEP_KEY_3, 0,"0000000000"
HKR,Ndi\params\WEP_KEY_4, ParamDesc, 0,%KEY4_Str%
HKR,Ndi\params\WEP_KEY_4, type, 0,"edit"
HKR,Ndi\params\WEP_KEY_4, default, 0,"0000000000"
HKR,Ndi\params\WEP_KEY_4, LimitText, 0,"10"
HKR,Ndi\params\WEP_KEY_4, UpperCase, 0,"1"
HKR,, WEP_KEY_4, 0,"0000000000"
HKR,Ndi\params\WEP_Mode, ParamDesc, 0,%WEP_Mode_Str%
HKR,Ndi\params\WEP_Mode, type, 0,"enum"
HKR,Ndi\params\WEP_Mode, default, 0,"0"
HKR,Ndi\params\WEP_Mode\enum, 0, 0,%WepMandatoryStr%
HKR,Ndi\params\WEP_Mode\enum, 1, 0,%WepOptionalStr%
HKR,, WEP_Mode, 0,"0"
HKR,Ndi\params\AuthenticationType, ParamDesc, 0,%AuthTypeStr%
HKR,Ndi\params\AuthenticationType, type, 0,"enum"
HKR,Ndi\params\AuthenticationType, default, 0,"2"
HKR,Ndi\params\AuthenticationType\enum, 0, 0,%OpenSystemStr%
HKR,Ndi\params\AuthenticationType\enum, 1, 0,%SharedKeyStr%
HKR,Ndi\params\AuthenticationType\enum, 2, 0,%AutoAuthStr%
HKR,, AuthenticationType, 0,"2"
HKR,Ndi\params\PreambleType, ParamDesc, 0,%PreambleStr%
HKR,Ndi\params\PreambleType, type, 0,"enum"
HKR,Ndi\params\PreambleType, default, 0,"2"
HKR,Ndi\params\PreambleType\enum, 0, 0,%LongPreambleStr%
HKR,Ndi\params\PreambleType\enum, 1, 0,%ShortPreambleStr%
HKR,Ndi\params\PreambleType\enum, 2, 0,%AutoPreambleStr%
HKR,, PreambleType, 0,"2"
HKR,Ndi\params\PowerMgmtMode, ParamDesc, 0,%PowerMgmtStr%
HKR,Ndi\params\PowerMgmtMode, type, 0,"enum"
HKR,Ndi\params\PowerMgmtMode, default, 0,"0"
HKR,Ndi\params\PowerMgmtMode\enum, 0, 0,%ActiveStr%
HKR,Ndi\params\PowerMgmtMode\enum, 1, 0,%PSStr%
HKR,, PowerMgmtMode, 0,"0"
HKR,Ndi\params\BasicRates, ParamDesc, 0,%BasicRatesStr%
HKR,Ndi\params\BasicRates, type, 0,"enum"
HKR,Ndi\params\BasicRates, default, 0,"1"
HKR,Ndi\params\BasicRates\enum, 0, 0,%BR1Str%
HKR,Ndi\params\BasicRates\enum, 1, 0,%BR2Str%
HKR,, BasicRates, 0,"1"
HKR, Ndi\params\BeaconPeriod, ParamDesc, 0, %BeaconPeriodStr%
HKR, Ndi\params\BeaconPeriod, type, 0, "int"
HKR, Ndi\params\BeaconPeriod, default, 0, "100"
HKR, Ndi\params\BeaconPeriod, min, 0, "20"
HKR, Ndi\params\BeaconPeriod, max, 0, "1000"
HKR, Ndi\params\BeaconPeriod, step, 0, "1"
HKR, , BeaconPeriod, 0, "100"
HKR,Ndi\params\RadioOnOff, ParamDesc, 0,%RadioOnOffStr%
HKR,Ndi\params\RadioOnOff, type, 0,"enum"
HKR,Ndi\params\RadioOnOff, default, 0,"1"
HKR,Ndi\params\RadioOnOff\enum, 0, 0,%RadioOffStr%
HKR,Ndi\params\RadioOnOff\enum, 1, 0,%RadioOnStr%
HKR,, RadioOnOff, 0,"1"
[PCMCIAFVNETR.XP.Params]
HKR, Ndi\params\Rate, ParamDesc, 0, %RateStr%
HKR, Ndi\params\Rate, type, 0, "enum"
HKR, Ndi\params\Rate, default, 0, "3"
HKR, Ndi\params\Rate\enum, 0, 0, %Fixed1Str%
HKR, Ndi\params\Rate\enum, 1, 0, %Fixed2Str%
HKR, Ndi\params\Rate\enum, 2, 0, %Fixed55Str%
HKR, Ndi\params\Rate\enum, 3, 0, %Fixed11Str%
HKR, Ndi\params\Rate\enum, 4, 0, %AutoStr%
HKR, , Rate, 0, "3"
HKR, Ndi\params\RTS_Threshold, ParamDesc, 0, %RTS_Str%
HKR, Ndi\params\RTS_Threshold, type, 0, "int"
HKR, Ndi\params\RTS_Threshold, default, 0, "2347"
HKR, Ndi\params\RTS_Threshold, min, 0, "0"
HKR, Ndi\params\RTS_Threshold, max, 0, "2347"
HKR, Ndi\params\RTS_Threshold, step, 0, "1"
HKR, , RTS_Threshold, 0, "2347"
HKR, Ndi\params\Frag_Threshold, ParamDesc, 0, %FragmentationStr%
HKR, Ndi\params\Frag_Threshold, type, 0, "int"
HKR, Ndi\params\Frag_Threshold, default, 0, "2346"
HKR, Ndi\params\Frag_Threshold, min, 0, "256"
HKR, Ndi\params\Frag_Threshold, max, 0, "2346"
HKR, Ndi\params\Frag_Threshold, step, 0, "1"
HKR, , Frag_Threshold, 0, "2346"
HKR,Ndi\params\PreambleType, ParamDesc, 0,%PreambleStr%
HKR,Ndi\params\PreambleType, type, 0,"enum"
HKR,Ndi\params\PreambleType, default, 0,"2"
HKR,Ndi\params\PreambleType\enum, 0, 0,%LongPreambleStr%
HKR,Ndi\params\PreambleType\enum, 1, 0,%ShortPreambleStr%
HKR,Ndi\params\PreambleType\enum, 2, 0,%AutoPreambleStr%
HKR,, PreambleType, 0,"2"
HKR,Ndi\params\RadioOnOff, ParamDesc, 0,%RadioOnOffStr%
HKR,Ndi\params\RadioOnOff, type, 0,"enum"
HKR,Ndi\params\RadioOnOff, default, 0,"1"
HKR,Ndi\params\RadioOnOff\enum, 0, 0,%RadioOffStr%
HKR,Ndi\params\RadioOnOff\enum, 1, 0,%RadioOnStr%
HKR,, RadioOnOff, 0,"1"
[PCMCIAFVNETR.NT.Reg]
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi, Service, 0, "PCMCIAFVNETR"
[PCMCIAFVNETR.XP.Reg]
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi, Service, 0, "PCMCIAFVNETR"
[PCMCIAFVNETR.Service]
DisplayName=%PCMCIAFVNETR.DisplayName%
ServiceType=1
StartType=3
ErrorControl=1
ServiceBinary=%12%\fvnetr.sys
LoadOrderGroup=NDIS
[PCMCIAFVNETR.XP.Service]
DisplayName=%PCMCIAFVNETR.DisplayName%
ServiceType=1
StartType=3
ErrorControl=1
ServiceBinary=%12%\fvnetr.sys
LoadOrderGroup=NDIS
[Common.EventLog]
AddReg=Common.AddEventLog.Reg
[Common.AddEventLog.Reg]
HKR, , EventMessageFile, 0x00020000, %%SystemRoot%%\System32\netevent.dll
HKR, , TypesSupported , 0x00010001, 7
[CopyFile.Sys]
[CopyFile.NT.Sys]
[CopyFile.XP.Sys]
[DestinationDirs]
CopyFile.Sys=11
CopyFile.NT.Sys=12
CopyFile.XP.Sys=12
DefaultDestDir=11 ; Drivers directory
[SourceDisksNames]
1=%DriverDisketteName%,,
[SourceDisksFiles] ;;WIN98/ME/2K
fvnetr.sys= 1,,
[SourceDisksFiles.x86] ;;WINXP
fvnetrxp.sys= 1,,
[Strings]
VENDOR=" "
PCMCIAOEM3V.DeviceDesc="WLAN 11Mbps PCMCIA ADAPTER(3.3V)"
PCMCIAOEM5V.DeviceDesc="WLAN 11Mbps PCMCIA ADAPTER(5V)"
PCMCIAFVNETR.DisplayName="WLAN 11Mbps PCMCIA ADAPTER"
DriverDisketteName="WLAN 11Mbps PCMCIA ADAPTER Drivers Diskette/CD"
Help_Text="VirtualNET lets you set up easily and operate a Wireless LAN compliant with 802.11 Standard. It operates in the license free 2.4 GHz ISM band and achieves a peak data rate of 11 Mbs."
ChannelStr="Channel"
RateStr="Rate"
Fixed1Str="Fixed 1 Mbps"
Fixed2Str="Fixed 2 Mbps"
Fixed55Str="Fixed 5.5 Mbps"
Fixed11Str="Fixed 11 Mbps"
AutoStr="Auto"
RTS_Str="RTS Threshold"
FragmentationStr="Fragmentation Threshold"
OperatingModeStr="Operating Mode"
AdHocStr="Ad-Hoc"
InfrastructureStr="Infrastructure"
ESSID_Str="ESSID"
WEP_Key_Str="WEP Key To Use"
KEY1_Str="WEP Key 1"
KEY2_Str="WEP Key 2"
KEY3_Str="WEP Key 3"
KEY4_Str="WEP Key 4"
WEP_Mode_Str="WEP Mode"
Key1Str="Key 1"
Key2Str="Key 2"
Key3Str="Key 3"
Key4Str="Key 4"
DisabledStr="Disabled"
64bit="64-bit"
128bit="128-bit"
WepMandatoryStr="Mandatory"
WepOptionalStr="Optional"
AuthTypeStr="Authentication Type"
OpenSystemStr="Open System"
SharedKeyStr="Shared Key"
AutoAuthStr="Auto"
PreambleStr="Preamble Type"
LongPreambleStr="Long"
ShortPreambleStr="Short"
AutoPreambleStr="Auto"
PowerMgmtStr="Power Mgmt Mode"
ActiveStr="Active"
PSStr="Power Save"
BasicRatesStr="Basic Rates"
BR1Str="1, 2 Mbps"
BR2Str="1, 2, 5.5, 11 Mbps"
BeaconPeriodStr="Beacon Period"
RadioOnOffStr="Radio"
RadioOffStr="Off"
RadioOnStr="On"
