
[Version]
CatalogFile=vnuwl.cat
Signature="$Chicago$"
Compatible=1
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
MillenniumPreferred=.ME
Provider=%Prov%
DriverVer=07/10/2009,1.74.0.00
[Manufacturer]
%Manuf%=MANUF
[ControlFlags]
ExcludeFromSelect=USB\VID_160A&PID_3184
[MANUF]
%VT3184.DeviceDesc%=VT3184v2.ndi, USB\VID_160A&PID_3184
[VT3184v2.ndi]
Characteristics=0x84
BusType=15
DelReg=U2W.delreg, U2W.SW.delreg
AddReg=VT3184v2.reg, USBCommon.reg, U2W.reg, U2W_win9x.reg, U2W.SW.win
;CpyFiles=U2W.CopyFiles.win, U2W.SW.CopyFiles.win
[VT3184v2.ndi.ME]
Characteristics=0x84
BusType=15
DelReg=U2W.delreg, U2W.SW.delreg
AddReg=VT3184v2.reg, USBCommon.reg, U2W.reg, U2W_me.reg, U2W.SW.win
;CpyFiles=U2W.CopyFiles.ME, U2W.SW.CopyFiles.win
[VT3184v2.ndi.NT]
Characteristics=0x84
BusType=15
DelReg=U2W.delreg, U2W.SW.delreg
AddReg=VT3184v2.reg, USBCommon.reg, U2W.reg, U2W_nt.reg, U2W.SW.NT
;CpyFiles=U2W.CopyFiles.NT, U2W.SW.CopyFiles.NT
[VT3184v2.ndi.NT.Services]
AddService="VNUWL5B", 2, U2W_nt.Service, U2W.EventLog
[VT3184v2.reg]
HKR, Ndi, DeviceID, 0, "USB\VID_160A&PID_3184"
[USBCommon.reg]
HKR, , AdapterCFID, 0, "830738694"
HKR, , AdapterType, 0, "0"
HKR, , MediaType, 0, "1"
HKR, , TransmitBuffers, 0, "128"
HKR, Ndi\params\TransmitBuffers, ParamDesc, 0, %TXBuffer%
HKR, Ndi\params\TransmitBuffers, default, 0, "128"
HKR, Ndi\params\TransmitBuffers, type, 0, "int"
HKR, Ndi\params\TransmitBuffers, Min, 0, "16"
HKR, Ndi\params\TransmitBuffers, Max, 0, "128"
HKR, Ndi\params\TransmitBuffers, Step, 0, "1"
HKR, Ndi\params\TransmitBuffers, Base, 0, "10"
HKR, Ndi\params\TransmitBuffers, flag, 1, "20","00","00","00"
HKR, , ReceiveBuffers, 0, "64"
HKR, Ndi\params\ReceiveBuffers, ParamDesc, 0, %RXBuffer%
HKR, Ndi\params\ReceiveBuffers, default, 0, "64"
HKR, Ndi\params\ReceiveBuffers, type, 0, "int"
HKR, Ndi\params\ReceiveBuffers, Min, 0, "16"
HKR, Ndi\params\ReceiveBuffers, Max, 0, "128"
HKR, Ndi\params\ReceiveBuffers, Step, 0, "1"
HKR, Ndi\params\ReceiveBuffers, Base, 0, "10"
HKR, Ndi\params\ReceiveBuffers, flag, 1, "20","00","00","00"
[U2W.reg]
HKR, , ConnectionRate, 0, "12"
HKR, Ndi\params\ConnectionRate, ParamDesc, 0, %ConnectionRate%
HKR, Ndi\params\ConnectionRate, default, 0, "12"
HKR, Ndi\params\ConnectionRate, type, 0, "enum"
HKR, Ndi\params\ConnectionRate\enum, 0, 0, %1M%
HKR, Ndi\params\ConnectionRate\enum, 1, 0, %2M%
HKR, Ndi\params\ConnectionRate\enum, 2, 0, %5M%
HKR, Ndi\params\ConnectionRate\enum, 3, 0, %11M%
HKR, Ndi\params\ConnectionRate\enum, 4, 0, %6M%
HKR, Ndi\params\ConnectionRate\enum, 5, 0, %9M%
HKR, Ndi\params\ConnectionRate\enum, 6, 0, %12M%
HKR, Ndi\params\ConnectionRate\enum, 7, 0, %18M%
HKR, Ndi\params\ConnectionRate\enum, 8, 0, %24M%
HKR, Ndi\params\ConnectionRate\enum, 9, 0, %36M%
HKR, Ndi\params\ConnectionRate\enum, 10, 0, %48M%
HKR, Ndi\params\ConnectionRate\enum, 11, 0, %54M%
HKR, Ndi\params\ConnectionRate\enum, 12, 0, %autoR%
HKR, Ndi\params\ConnectionRate, flag, 1, "30","00","00","00"
HKR, Ndi\params\NetworkAddress, ParamDesc, 0, %NetAddress%
HKR, Ndi\params\NetworkAddress, Default, 0, ""
HKR, Ndi\params\NetworkAddress, type, 0, "edit"
HKR, NDI\params\NetworkAddress, LimitText, 0, "12"
HKR, NDI\params\NetworkAddress, UpperCase, 0, "1"
HKR, NDI\params\NetworkAddress, optional, 0, "1"
HKR, NDI\params\NetworkAddress, Base, 0, "16"
HKR, Ndi\params\NetworkAddress, flag, 1, "20","00","00","00"
HKR, , Channel, 0, "6"
HKR, Ndi\params\Channel, ParamDesc, 0, %Channel%
HKR, Ndi\params\Channel, default, 0, "6"
HKR, Ndi\params\Channel, type, 0, "int"
HKR, Ndi\params\Channel, min, 0, "1"
HKR, Ndi\params\Channel, max, 0, "56"
HKR, Ndi\params\Channel, step, 0, "1"
HKR, , IBSSMode, 0, "1"
HKR, Ndi\params\IBSSMode, ParamDesc, 0, %IBSSMode%
HKR, Ndi\params\IBSSMode, default, 0, "1"
HKR, Ndi\params\IBSSMode, type, 0, "enum"
HKR, Ndi\params\IBSSMode\enum, 0, 0, "%802.11G%"
HKR, Ndi\params\IBSSMode\enum, 1, 0, "%802.11B%"
HKR, , CountryRegion11BGBand, 0, "2"
HKR, Ndi\params\CountryRegion11BGBand, ParamDesc, 0, %CountryRegion11BGBand%
HKR, Ndi\params\CountryRegion11BGBand, default, 0, "2"
HKR, Ndi\params\CountryRegion11BGBand, type, 0, "enum"
HKR, Ndi\params\CountryRegion11BGBand\enum, 0, 0, "%FCC%"
HKR, Ndi\params\CountryRegion11BGBand\enum, 1, 0, "%TELEC%"
HKR, Ndi\params\CountryRegion11BGBand\enum, 2, 0, "%ETSI%"
HKR, , CountryRegion11ABand, 0, "99"
HKR, Ndi\params\CountryRegion11ABand, ParamDesc, 0, "%CountryRegion11ABand%"
HKR, Ndi\params\CountryRegion11ABand, default, 0, "99"
HKR, Ndi\params\CountryRegion11ABand, type, 0, "enum"
HKR, Ndi\params\CountryRegion11ABand\enum,0, 0, "%CH0%"
HKR, Ndi\params\CountryRegion11ABand\enum,1, 0, "%CH1%"
HKR, Ndi\params\CountryRegion11ABand\enum,2, 0, "%CH2%"
HKR, Ndi\params\CountryRegion11ABand\enum,3, 0, "%CH3%"
HKR, Ndi\params\CountryRegion11ABand\enum,4, 0, "%CH4%"
HKR, Ndi\params\CountryRegion11ABand\enum,5, 0, "%CH5%"
HKR, Ndi\params\CountryRegion11ABand\enum,6, 0, "%CH6%"
HKR, Ndi\params\CountryRegion11ABand\enum,7, 0, "%CH7%"
HKR, Ndi\params\CountryRegion11ABand\enum,8, 0, "%CH8%"
HKR, Ndi\params\CountryRegion11ABand\enum,9, 0, "%CH9%"
HKR, Ndi\params\CountryRegion11ABand\enum,10, 0, "%CH10%"
HKR, Ndi\params\CountryRegion11ABand\enum,11, 0, "%CH11%"
HKR, Ndi\params\CountryRegion11ABand\enum,12, 0, "%CH12%"
HKR, Ndi\params\CountryRegion11ABand\enum,99, 0, "%Disable%"
HKR, , PreambleType, 0, "1"
HKR, Ndi\params\PreambleType, ParamDesc, 0, %PreambleType%
HKR, Ndi\params\PreambleType, default, 0, "1"
HKR, Ndi\params\PreambleType, type, 0, "enum"
HKR, Ndi\params\PreambleType\enum, 0, 0, %Long%
HKR, Ndi\params\PreambleType\enum, 1, 0, %Short%
HKR, , OperationMode, 0, "0"
HKR, Ndi\params\OperationMode, ParamDesc, 0, %OperationMode%
HKR, Ndi\params\OperationMode, default, 0, "0"
HKR, Ndi\params\OperationMode, type, 0, "enum"
HKR, Ndi\params\OperationMode\enum, 0, 0, "%Infrastructure%"
HKR, Ndi\params\OperationMode\enum, 1, 0, "%Ad-Hoc%"
HKR, , DesiredSSID, 0, ""
HKR, NDI\params\DesiredSSID, ParamDesc, 0, %DesiredSSID%
HKR, NDI\params\DesiredSSID, default, 0, ""
HKR, NDI\params\DesiredSSID, type, 0, "edit"
HKR, NDI\params\DesiredSSID, LimitText, 0, "32"
HKR, NDI\params\DesiredSSID, optional, 0, "1"
HKR, , RTSThreshold, 0, "2347"
HKR, Ndi\params\RTSThreshold, ParamDesc, 0, %RTSThreshold%
HKR, Ndi\params\RTSThreshold, default, 0, "2347"
HKR, Ndi\params\RTSThreshold, type, 0, "int"
HKR, Ndi\params\RTSThreshold, Min, 0, "256"
HKR, Ndi\params\RTSThreshold, Max, 0, "2347"
HKR, Ndi\params\RTSThreshold, Step, 0, "1"
HKR, Ndi\params\RTSThreshold, Base, 0, "10"
HKR, Ndi\params\RTSThreshold, flag, 1, "30","00","00","00"
HKR, , FragThreshold, 0, "2346"
HKR, Ndi\params\FragThreshold, ParamDesc, 0, %FragThreshold%
HKR, Ndi\params\FragThreshold, default, 0, "2346"
HKR, Ndi\params\FragThreshold, type, 0, "int"
HKR, Ndi\params\FragThreshold, Min, 0, "256"
HKR, Ndi\params\FragThreshold, Max, 0, "2346"
HKR, Ndi\params\FragThreshold, Step, 0, "1"
HKR, Ndi\params\FragThreshold, Base, 0, "10"
HKR, Ndi\params\FragThreshold, flag, 1, "30","00","00","00"
HKR, , BeaconInterval, 0, "100"
HKR, Ndi\params\BeaconInterval, ParamDesc, 0, %BeaconInterval%
HKR, Ndi\params\BeaconInterval, default, 0, "100"
HKR, Ndi\params\BeaconInterval, type, 0, "int"
HKR, Ndi\params\BeaconInterval, Min, 0, "1"
HKR, Ndi\params\BeaconInterval, Max, 0, "1000"
HKR, Ndi\params\BeaconInterval, Step, 0, "1"
HKR, Ndi\params\BeaconInterval, Base, 0, "10"
HKR, Ndi\params\BeaconInterval, flag, 1, "30","00","00","00"
HKR, , RadioControl, 0, "0"
HKR, Ndi\params\RadioControl, ParamDesc, 0, %RadioControl%
HKR, Ndi\params\RadioControl, default, 0, "0"
HKR, Ndi\params\RadioControl, type, 0, "enum"
HKR, Ndi\params\RadioControl\enum, 0, 0, "%On%"
HKR, Ndi\params\RadioControl\enum, 1, 0, "%Off%"
HKR, , AntennaDiversity, 0, "1"
HKR, Ndi\params\AntennaDiversity, ParamDesc, 0, %AntennaDiversity%
HKR, Ndi\params\AntennaDiversity, default, 0, "1"
HKR, Ndi\params\AntennaDiversity, type, 0, "enum"
HKR, Ndi\params\AntennaDiversity\enum, 0, 0, "%Disable%"
HKR, Ndi\params\AntennaDiversity\enum, 1, 0, "%Enable%"
HKR, , SelectiveSuspend, 0, "1"
HKR, Ndi\params\SelectiveSuspend, ParamDesc, 0, %SelectiveSuspend%
HKR, Ndi\params\SelectiveSuspend, default, 0, "1"
HKR, Ndi\params\SelectiveSuspend, type, 0, "enum"
HKR, Ndi\params\SelectiveSuspend\enum, 0, 0, "%Disable%"
HKR, Ndi\params\SelectiveSuspend\enum, 1, 0, "%Enable%"
HKR, , Roaming, 0, "1"
HKR, Ndi\params\Roaming, ParamDesc, 0, %Roaming%
HKR, Ndi\params\Roaming, default, 0, "1"
HKR, Ndi\params\Roaming, type, 0, "enum"
HKR, Ndi\params\Roaming\enum, 0, 0, "%Disable%"
HKR, Ndi\params\Roaming\enum, 1, 0, "%Enable%"
HKR, , RoamingSignalStrength, 0, "-100"
HKR, Ndi\params\RoamingsignalStrength, ParamDesc, 0, %RoamingsignalStrength%
HKR, Ndi\params\RoamingsignalStrength, default, 0, "-100"
HKR, Ndi\params\RoamingsignalStrength, type, 0, "int"
HKR, Ndi\params\RoamingsignalStrength, Min, 0, "-150"
HKR, Ndi\params\RoamingsignalStrength, Max, 0, "-1"
HKR, Ndi\params\RoamingsignalStrength, Step, 0, "1"
HKR, Ndi\params\RoamingsignalStrength, Base, 0, "10"
HKR, Ndi\params\RoamingsignalStrength, flag, 1, "30","00","00","00"
HKR, , RoamingInterval, 0, "5"
HKR, Ndi\params\RoamingInterval, ParamDesc, 0, %RoamingInterval%
HKR, Ndi\params\RoamingInterval, default, 0, "5"
HKR, Ndi\params\RoamingInterval, type, 0, "int"
HKR, Ndi\params\RoamingInterval, Min, 0, "2"
HKR, Ndi\params\RoamingInterval, Max, 0, "255"
HKR, Ndi\params\RoamingInterval, Step, 0, "1"
HKR, Ndi\params\RoamingInterval, Base, 0, "10"
HKR, Ndi\params\RoamingInterval, flag, 1, "30","00","00","00"
HKR, , RoamingChannels, 0, ""
HKR, NDI\params\RoamingChannels, ParamDesc, 0, %RoamingChannels%
HKR, NDI\params\RoamingChannels, default, 0, ""
HKR, NDI\params\RoamingChannels, type, 0, "edit"
HKR, NDI\params\RoamingChannels, LimitText, 0, "32"
HKR, NDI\params\RoamingChannels, optional, 0, "1"
[U2W_win9x.reg]
HKR, Ndi\Install, ndis3, 0, "U2W.CopyFiles.win"
HKR, NDIS, MajorNdisVersion,1,03
HKR, NDIS, MinorNdisVersion,1,0A
HKR, , DevLoader, 0, "*ndis"
HKR, , DeviceVxDs, 0, "VNUWL5A.sys"
HKR, NDIS, LogDriverName, 0, "VNUWL5A"
HKR, Ndi\Interfaces, DefLower, 0, "ethernet"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi\Interfaces, DefUpper, 0, "ndis3"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis3"
[U2W_me.reg]
HKR, Ndi\Install, ndis3, 0, "U2W.CopyFiles.ME"
HKR, NDIS, MajorNdisVersion,1,05
HKR, NDIS, MinorNdisVersion,1,00
HKR, , DevLoader, 0, "*ndis"
HKR, , DeviceVxDs, 0, "VNUWL5A.sys"
HKR, NDIS, LogDriverName, 0, "VNUWL5A"
HKR, Ndi\Interfaces, DefLower, 0, "ethernet"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi\Interfaces, DefUpper, 0, "ndis5"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
[U2W_nt.reg]
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi, Service, 0, "VNUWL5B"
[U2W.CopyFiles.win]
VNUWL5A.SYS,,,2
[U2W.CopyFiles.ME]
VNUWL5A.SYS,,,2
[U2W.CopyFiles.NT]
VNUWL5B.SYS,,,2
[U2W.SW.CopyFiles.win]
vuins16.dll,,,2
[U2W.SW.CopyFiles.NT]
[U2W.SW.win]
HKLM, Software\Microsoft\Windows\CurrentVersion\Uninstall\VN_VUIns_U2W_VIA, DisplayName, 0, %VT3184.DeviceDesc%
HKLM, Software\Microsoft\Windows\CurrentVersion\Uninstall\VN_VUIns_U2W_VIA, UninstallString, 0, "Rundll.exe vuins16.dll,vuins16Ex $U2W $VIA"
HKLM, Software\VN_VUIns\U2W\VIA\DeviceIdList, 3184, 0, "0"
[U2W.SW.NT]
HKLM, Software\Microsoft\Windows\CurrentVersion\Uninstall\VN_VUIns_U2W_VIA, DisplayName, 0, %VT3184.DeviceDesc%
HKLM, Software\VN_VUIns\U2W\VIA\DeviceIdList, 3184, 0, "0"
[U2W_nt.Service]
DisplayName=%U2W.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_DEMAND_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\VNUWL5B.SYS
LoadOrderGroup=NDIS
[U2W.EventLog]
AddReg=U2W.AddEventLog.reg
[U2W.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported, 0x00010001, 7
[DestinationDirs]
DefaultDestDir=12
U2W.CopyFiles.win=11
U2W.CopyFiles.ME=11
U2W.CopyFiles.NT=12
U2W.SW.CopyFiles.win=11
U2W.SW.CopyFiles.NT=11
[SourceDisksFiles]
VNUWL.inf=1
VNUWL5A.SYS=1
VNUWL5B.SYS=1
vuins16.dll=1
[SourceDisksNames]
1=%DiskName%,,,
[U2W.delreg]
HKR,Ndi\Params\ConnectionRate
HKR,,ConnectionRate
HKR,Ndi\Params\NetworkAddress
HKR,,NetworkAddress
HKR,Ndi\Params\Channel
HKR,,Channel
HKR,Ndi\Params\IBSSMode
HKR,,IBSSMode
HKR,Ndi\Params\PreambleType
HKR,,PreambleType
HKR,Ndi\Params\OperationMode
HKR,,OperationMode
HKR,Ndi\Params\DesiredSSID
HKR,,DesiredSSID
HKR,Ndi\Params\RTSThreshold
HKR,,RTSThreshold
HKR,Ndi\Params\FragThreshold
HKR,,FragThreshold
HKR,Ndi\params\BeaconInterval
HKR,,BeaconInterval
HKR,Ndi\Params\RadioControl
HKR,,RadioControl
HKR,Ndi\Params\AntennaDiversity
HKR,,AntennaDiversity
HKR,Ndi\Params\SelectiveSuspend
HKR,,SelectiveSuspend
HKR,Ndi\Params\Roaming
HKR,,Roaming
HKR,Ndi\Params\RoamingsignalStrength
HKR,,RoamingsignalStrength
HKR,Ndi\Params\RoamingInterval
HKR,,RoamingInterval
HKR,Ndi\Params\RoamingChannels
HKR,,RoamingChannels
HKR,Ndi\Params\CountryRegion11BGBand
HKR,,CountryRegion11BGBand
HKR,Ndi\Params\CountryRegion11ABand
HKR,,CountryRegion11ABand
[U2W.SW.delreg]
HKLM, Software\Microsoft\Windows\CurrentVersion\Uninstall\VN_VUIns_U2W_VIA
HKLM, Software\VN_VUIns\U2W\VIA
[Strings]
Prov="VIA"
DiskName="VIA USB Wireless LAN source disk"
ConnectionRate="Connection Rate"
Channel="IBSS Channel"
IBSSMode="IBSS Mode"
autoR="Auto-Rate"
1M=" 1Mbps"
2M=" 2Mbps"
5M=" 5.5Mbps"
11M="11Mbps"
6M=" 6Mbps"
9M=" 9Mbps"
12M="12Mbps"
18M="18Mbps"
24M="24Mbps"
36M="36Mbps"
48M="48Mbps"
54M="54Mbps"
PreambleType="Preamble Type"
Long="Long"
Short="Short"
Disabled="Disabled"
Enabled="Enabled"
NetAddress="Network Address"
HwDefault="Hardware Default"
OperationMode="Operation Mode"
DesiredSSID="Desired SSID"
802_11_Mode="802.11 Mode"
BeaconInterval="IBSS Beacon Interval"
RadioControl="RadioControl"
RTSThreshold="RTS Threshold"
FragThreshold="Fragment Threshold"
TXBuffer="Transmit Buffers"
RXBuffer="Receive Buffers"
AntennaDiversity="Antenna Diversity"
SelectiveSuspend="SelectiveSuspend"
Roaming="Roaming"
RoamingsignalStrength="Roaming Signal Strength"
RoamingInterval="Roaming Interval"
RoamingChannels="Roaming Channels"
Manuf="VIA Networking Technologies, Inc."
VT3184.DeviceDesc="VIA Networking Technologies USB Wireless LAN Adapter"
U2W.Service.DispName="VIA Networking Technologies USB Wireless LAN Adapter Driver Service"
802.11G="802.11G"
802.11B="802.11B"
Infrastructure="Infrastructure"
Ad-Hoc="Ad-Hoc"
On="On"
Off="Off"
Disable="Disable"
Enable="Enable"
CountryRegion11ABand="802.11ARegion"
CountryRegion11BGBand= "802.11bg zone type"
FCC="FCC"
TELEC="TELEC"
ETSI="ETSI"
CH0="# 0 Ch(36 - 64,149 - 165)"
CH1="# 1 Ch(36 - 140)"
CH2="# 2 Ch(36 - 64)"
CH3="# 3 Ch(52 - 64,149 - 161)"
CH4="# 4 Ch(149 - 165)"
CH5="# 5 Ch(149 - 161)"
CH6="# 6 Ch(36 - 48)"
CH7="# 7 Ch(36 - 165)"
CH8="# 8 Ch(52 - 64)"
CH9="# 9 Ch(36 - 116,132 - 165)"
CH10="#10 Ch(36 - 48,149 - 165)"
CH11="#11 Ch(36 - 120,149 - 161)"
CH12="#12 Ch(36 - 140)"

