
[Version]
DriverVer=11/01/2001, 2.00.09 ; Updated by build scripts
Signature="$Chicago$"
Compatible=1
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%VER_VENDOR_STR%
CatalogFile=EU3NIC.cat
MillenniumPreferred=.ME
[ControlFlags]
ExcludeFromSelect=USB\VID_0967&PID_0204
[Manufacturer]
%VER_VENDOR_NAME_STR%=DeviceList
[DeviceList]
%PRISM_USB1_STR%=PRISM_USB1, USB\VID_0967&PID_0204
[PRISM_USB1.NT] ; Win2k
AddReg=PRISM_USB1.reg, COMMON_USB.reg, COMMON_NDIS.reg.NT, COMMON.reg, COMMON_AWLAN.reg
;CpyFiles=PRISM_DRIVER.copy.NT, PRISM_APPLET.copy.NT
BusType=15 ; USB
Characteristics= 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[PRISM_USB1.NT.Services]
AddService="EU3_USB", 2, PRISM_USB_DRIVER.Service, PRISM_DRIVER.EventLog
[PRISM_USB1.reg]
HKR,Ndi ,DeviceID,0,"USB\VID_0967&PID_0204"
HKR, ,PlatformId,0,"0"
HKR, ,VendorDesc,0,%USB_DESC_STR%
HKR, ,LoadFirmware,0,1
HKR, NDI\params\LoadFirmware,default,0,1
[PRISM_USB_DRIVER.Service]
DisplayName=%PRISM_USB_SERVICE_DISPLAY%
ServiceType=1 ; SERVICE_KERNEL_DRIVER
StartType=3 ; SERVICE_DEMAND_START
ErrorControl=1 ; NORMAL
ServiceBinary=%12%\EU3USB.sys
LoadOrderGroup=NDIS
[PRISM_DRIVER.EventLog]
AddReg=PRISM_DRIVER.EventLog.reg
[PRISM_DRIVER.EventLog.reg]
HKR, ,EventMessageFile ,0x00020000 ,"%%SystemRoot%%\System32\netevent.dll"
HKR, ,TypesSupported ,0x00010001 ,7
[COMMON_USB.reg]
HKR,NDI ,Service ,0 ,"EU3_USB"
HKR,NDI ,CardType ,0 ,"USB"
HKR, ,BusType ,0 ,"0"
HKR, ,DeviceVxDs ,0 ,"EU3USB.sys"
[COMMON_NDIS.reg.NT]
HKR,NDI\Interfaces ,UpperRange ,0 ,"ndis5"
HKR,NDI\Interfaces ,LowerRange ,0 ,"ethernet"
HKR,defaults,PSMode,0,1
HKR,Ndi\params\PSMode,default,0,1
HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
HKR,NDI\params\PSMode,type,,enum
HKR,NDI\params\PSMode,flag,1,30,00,00,00
HKR,NDI\params\PSMode\enum,1,,"Disable"
HKR,NDI\params\PSMode\enum,2,,"Always Enable"
HKR,NDI\params\PSMode\enum,3,,"Auto Enable"
HKR,NDI\params\PSMode,optional,0,1
[COMMON.reg]
HKR, ,EU3IOC ,0 ,"1"
HKR, ,SilentInstall ,0 ,"1"
HKR,defaults,ListenInterval,0,3
HKR,Ndi\params\ListenInterval,default,0,3
HKR,NDI\params\ListenInterval,ParamDesc,,%LISTENINTERVAL_STR%
HKR,NDI\params\ListenInterval,type,,int
HKR,NDI\params\ListenInterval,flag,1,30,00,00,00
HKR,NDI\params\ListenInterval,min,0,0
HKR,NDI\params\ListenInterval,max,0,77
HKR,NDI\params\ListenInterval,step,0,1
HKR,NDI\params\ListenInterval,optional,0,1
HKR,defaults,RTSThresh,0,2432
HKR,Ndi\params\RTSThresh,default,0,2432
HKR,NDI\params\RTSThresh,ParamDesc,0,%RTSTHRESH_STR%
HKR,NDI\params\RTSThresh,type,0,int
HKR,NDI\params\RTSThresh,flag,1,20,00,00,00
HKR,NDI\params\RTSThresh,min,0,0
HKR,NDI\params\RTSThresh,max,0,2432
HKR,NDI\params\RTSThresh,step,0,64
HKR,NDI\params\RTSThresh,optional,0,1
HKR,defaults,FragThresh,0,2432
HKR,Ndi\params\FragThresh,default,0,2432
HKR,NDI\params\FragThresh,ParamDesc,0,%FRAGTHRESH_STR%
HKR,NDI\params\FragThresh,type,0,int
HKR,NDI\params\FragThresh,flag,1,20,00,00,00
HKR,NDI\params\FragThresh,min,0,256
HKR,NDI\params\FragThresh,max,0,2432
HKR,NDI\params\FragThresh,step,0,128
HKR,NDI\params\FragThresh,optional,0,1
HKR,defaults,PreambleMode,0,1
HKR,Ndi\params\PreambleMode,default,0,1
HKR,NDI\params\PreambleMode,ParamDesc,,%SHORT_PREAM_STR%
HKR,NDI\params\PreambleMode,type,,enum
HKR,NDI\params\PreambleMode,flag,1,30,00,00,00
HKR,NDI\params\PreambleMode\enum,1,,"Long Tx Preamble"
HKR,NDI\params\PreambleMode\enum,2,,"Short Tx Preamble"
HKR,NDI\params\PreambleMode\enum,3,,"Auto Tx Preamble"
HKR,NDI\params\PreambleMode,optional,0,1
HKR,defaults,AuthentAlg,0,65535
HKR,NDI\params\AuthentAlg,default,0,65535
HKR,NDI\params\AuthentAlg,ParamDesc,,%AUTHENT_TYPE_STR%
HKR,NDI\params\AuthentAlg,type,,enum
HKR,NDI\params\AuthentAlg,flag,1,30,00,00,00
HKR,NDI\params\AuthentAlg\enum,1,,"WECA Compliant (always use Open)"
HKR,NDI\params\AuthentAlg\enum,2,,"Must use Shared with WEP"
HKR,NDI\params\AuthentAlg\enum,65535,,"Automatic based on WEP setting"
HKR,NDI\params\AuthentAlg,optional,0,1
HKR,defaults,AdhocDemoMode,0,0
HKR,Ndi\params\AdhocDemoMode,default,0,0
HKR,NDI\params\AdhocDemoMode,ParamDesc,,%ADHOC_DEMO_STR%
HKR,NDI\params\AdhocDemoMode,type,,enum
HKR,NDI\params\AdhocDemoMode,flag,1,30,00,00,00
HKR,NDI\params\AdhocDemoMode\enum,0,,"Disable"
HKR,NDI\params\AdhocDemoMode\enum,1,,"Enable"
HKR,NDI\params\AdhocDemoMode,optional,0,1
HKR,defaults,LoadFirmware,0,1
HKR,Ndi\params\LoadFirmware,default,0,1
HKR,NDI\params\LoadFirmware,ParamDesc,,%LOAD_FIRMWARE_STR%
HKR,NDI\params\LoadFirmware,type,,enum
HKR,NDI\params\LoadFirmware,flag,1,30,00,00,00
HKR,NDI\params\LoadFirmware\enum,0,,"Disable"
HKR,NDI\params\LoadFirmware\enum,1,,"Enable"
HKR,NDI\params\LoadFirmware,optional,0,1
[COMMON_AWLAN.reg]
HKR,,ProfileName,,%PROFILE1% ;0924
HKR,defaults,ProfileName,,%PROFILE1% ;0924
HKR,ProfileList\1,ProfileName,,%PROFILE1% ; 0920
HKR,ProfileList\2,ProfileName,,%PROFILE2% ; 0920
HKR,ProfileList\3,ProfileName,,%PROFILE3% ; 0920
HKR,ProfileList\4,ProfileName,,%PROFILE4% ; 0920
HKR,ProfileList\5,ProfileName,,%PROFILE5% ; 0920
HKR,,SSID,,%SSID_DEF_STR%
HKR,defaults,SSID,,%SSID_DEF_STR%
HKR,ProfileList\1,SSID,,%SSID_DEF_STR% ; 0920
HKR,ProfileList\2,SSID,,%SSID_DEF_STR% ; 0920
HKR,ProfileList\3,SSID,,%SSID_DEF_STR% ; 0920
HKR,ProfileList\4,SSID,,%SSID_DEF_STR% ; 0920
HKR,ProfileList\5,SSID,,%SSID_DEF_STR% ; 0920
HKR,NDI\params\SSID,ParamDesc,,"SSID"
HKR,NDI\params\SSID,type,,edit
HKR,NDI\params\SSID,limitText,,32
HKR,NDI\params\SSID,default,,%SSID_DEF_STR%
HKR,NDI\params\SSID,flag,1,30,00,00,00
HKR,,DSChannel,,%DSCHANNEL_DEF_STR%
HKR,defaults,DSChannel,,%DSCHANNEL_DEF_STR%
HKR,ProfileList\1,DSChannel,,%DSCHANNEL_DEF_STR% ; 0920
HKR,ProfileList\2,DSChannel,,%DSCHANNEL_DEF_STR% ; 0920
HKR,ProfileList\3,DSChannel,,%DSCHANNEL_DEF_STR% ; 0920
HKR,ProfileList\4,DSChannel,,%DSCHANNEL_DEF_STR% ; 0920
HKR,ProfileList\5,DSChannel,,%DSCHANNEL_DEF_STR% ; 0920
HKR,,NetworkType,,%NETWORK_TYPE_DEF_STR%
HKR,defaults,NetworkType,,%NETWORK_TYPE_DEF_STR%
HKR,ProfileList\1,NetworkType,,%NETWORK_TYPE_DEF_STR% ; 0920
HKR,ProfileList\2,NetworkType,,%NETWORK_TYPE_DEF_STR% ; 0920
HKR,ProfileList\3,NetworkType,,%NETWORK_TYPE_DEF_STR% ; 0920
HKR,ProfileList\4,NetworkType,,%NETWORK_TYPE_DEF_STR% ; 0920
HKR,ProfileList\5,NetworkType,,%NETWORK_TYPE_DEF_STR% ; 0920
HKR,NDI\params\NetworkType,ParamDesc,,"Network Type"
HKR,NDI\params\NetworkType,type,,enum
HKR,NDI\params\NetworkType,default,,%NETWORK_TYPE_DEF_STR%
HKR,NDI\params\NetworkType,flag,1,30,00,00,00
HKR,NDI\params\NetworkType\enum,0,,"802.11 Ad Hoc"
HKR,NDI\params\NetworkType\enum,1,,"Infrastructure"
HKR,NDI\params\NetworkType\enum,3,,"Ad Hoc"
HKR,,WepReq,0,0
HKR,defaults,WepReq,0,0
HKR,ProfileList\1,WepReq,0,0 ; 0920
HKR,ProfileList\2,WepReq,0,0 ; 0920
HKR,ProfileList\3,WepReq,0,0 ; 0920
HKR,ProfileList\4,WepReq,0,0 ; 0920
HKR,ProfileList\5,WepReq,0,0 ; 0920
HKR,NDI\params\WepReq,default,0,0
HKR,NDI\params\WepReq,ParamDesc,,%WEPREQ_STR%
HKR,NDI\params\WepReq,flag,1,30,00,00,00
HKR,NDI\params\WepReq,type,,enum
HKR,Ndi\params\WepReq,default,,0
HKR,NDI\params\WepReq\enum,0,,"Disabled"
HKR,NDI\params\WepReq\enum,2,,"64 bit"
HKR,NDI\params\WepReq\enum,6,,"128 bit"
HKR,NDI\params\WepReq,optional,0,0
HKR,,TxRate,,15
HKR,defaults,TxRate,,15
HKR,ProfileList\1,TxRate,,15 ; 0920
HKR,ProfileList\2,TxRate,,15 ; 0920
HKR,ProfileList\3,TxRate,,15 ; 0920
HKR,ProfileList\4,TxRate,,15 ; 0920
HKR,ProfileList\5,TxRate,,15 ; 0920
HKR,NDI\params\TxRate,ParamDesc,,"Transmit Rate"
HKR,NDI\params\TxRate,type,,enum
HKR,NDI\params\TxRate,default,,15
HKR,NDI\params\TxRate,flag,1,30,00,00,00
HKR,NDI\params\TxRate\enum,1,,"Fixed 1 Mb/s"
HKR,NDI\params\TxRate\enum,2,,"Fixed 2 Mb/s"
HKR,NDI\params\TxRate\enum,3,,"Auto Select 1 or 2"
HKR,NDI\params\TxRate\enum,4,,"Fixed 5.5 Mb/s"
HKR,NDI\params\TxRate\enum,8,,"Fixed 11 Mb/s"
HKR,NDI\params\TxRate\enum,15,,"Fully Auto"
HKR,,PSMode,0,1 ;12/01
HKR,defaults,PSMode,0,1 ;12/01
HKR,ProfileList\1,PSMode,0,1 ; 0920
HKR,ProfileList\2,PSMode,0,1 ; 0920
HKR,ProfileList\3,PSMode,0,1 ; 0920
HKR,ProfileList\4,PSMode,0,1 ; 0920
HKR,ProfileList\5,PSMode,0,1 ; 0920
HKR,NDI\params\PSMode,default,0,1 ;12/01
HKR,NDI\params\PSMode,ParamDesc,,"Power Save Mode"
HKR,NDI\params\PSMode,type,,enum
HKR,NDI\params\PSMode,default,,1
HKR,NDI\params\PSMode,flag,1,30,00,00,00
HKR,NDI\params\PSMode\enum,1,,"Disabled"
HKR,NDI\params\PSMode\enum,2,,"Enabled"
HKR,,EnableRadio,0,1
HKR,defaults,EnableRadio,0,1
HKR,ProfileList\1,EnableRadio,0,1
HKR,ProfileList\2,EnableRadio,0,1
HKR,ProfileList\3,EnableRadio,0,1
HKR,ProfileList\4,EnableRadio,0,1
HKR,ProfileList\5,EnableRadio,0,1
HKR,NDI\params\EnableRadio,default,0,1
HKR,NDI\params\EnableRadio,ParamDesc,,"Enable Radio"
HKR,NDI\params\EnableRadio,type,,enum
HKR,NDI\params\EnableRadio,default,,1
HKR,NDI\params\EnableRadio,flag,1,30,00,00,00
HKR,NDI\params\EnableRadio\enum,0,,"Disabled"
HKR,NDI\params\EnableRadio\enum,1,,"Enabled"
HKR,,Country,,%COUNTRY_DEF_STR% ; 0920
HKR,ProfileList\1,Country,,%COUNTRY_DEF_STR% ; 0920
HKR,ProfileList\2,Country,,%COUNTRY_DEF_STR% ; 0920
HKR,ProfileList\3,Country,,%COUNTRY_DEF_STR% ; 0920
HKR,ProfileList\4,Country,,%COUNTRY_DEF_STR% ; 0920
HKR,ProfileList\5,Country,,%COUNTRY_DEF_STR% ; 0920
HKR,ProfileList\1,DefaultKeyID,,1 ; 0920
HKR,ProfileList\2,DefaultKeyID,,1 ; 0920
HKR,ProfileList\3,DefaultKeyID,,1 ; 0920
HKR,ProfileList\4,DefaultKeyID,,1 ; 0920
HKR,ProfileList\5,DefaultKeyID,,1 ; 0920
[DestinationDirs]
DefaultDestDir=11 ; Win9x=%windir%\system Win2k=%windir%\system32
PRISM_DRIVER.copy.NT=12 ; Win2k=%windir%\system32\drivers
[PRISM_DRIVER.copy.NT]
EU3USB.sys
[PRISM_APPLET.copy.NT]
[SourceDisksNames]
1=%INSTALL_DISK_STR%,,,
[SourceDisksFiles.X86] ; Win2k/Xp
EU3USB.sys=1
[Strings]
VER_VENDOR_STR="WNC"
VER_VENDOR_NAME_STR="WNC Corporation"
PRISM_USB1_STR="WNC 802.11b USB300"
PRISM_SERVICE_DISPLAY="WNC 802.11b USB300 Driver"
PRISM_USB_SERVICE_DISPLAY="WNC 802.11b USB300 Driver"
INSTALL_DISK_STR="WNC 802.11b USB300 Install Disk"
ADHOC_DEMO_STR="Adhoc Demo Mode"
SHORT_PREAM_STR="Preamble Mode"
RTSTHRESH_STR="RTS Threshold"
FRAGTHRESH_STR="Fragmentation Threshold"
AUTHENT_TYPE_STR="Authentication Algorithm"
LISTENINTERVAL_STR="Listen Interval"
POWER_SAVE_STR="Power Save Mode"
POWER_LEVEL_STR="Power Save Level"
LOAD_FIRMWARE_STR="Firmware Download"
USB_DESC_STR="WNC 802.11b USB300"
PROFILE1="Default"
PROFILE2="Default 1"
PROFILE3="Default 2"
PROFILE4="Default 3"
PROFILE5="Default 4"
WEPREQ_STR="Use Wep"
SSID_DEF_STR="any"
NETWORK_TYPE_DEF_STR="1"
AUTHENT_TYPE_DEF_STR="2"
DSCHANNEL_DEF_STR="6"
COUNTRY_DEF_STR="USA/Canada"
