
[Version]
DriverVer=05/20/2003, 3.0.4.205
Signature="$Windows NT$"
Compatible=1
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%VER_VENDOR_STR%
CatalogFile=MN510.cat
[ControlFlags]
ExcludeFromSelect=USB\VID_045E&PID_006E
[Manufacturer]
%VER_VENDOR_NAME_STR%=DeviceList,NTx86.5.1
[DeviceList.NTx86.5.1]
%PRISM_USB1_STR%=PRISM_USB_XP1, USB\VID_045E&PID_006E
[PRISM_USB_XP1] ; WinXP
AddReg=PRISM_USB_XP1.reg, COMMON_USB_XP1.reg, COMMON.reg, COMMON_NDIS.reg.XP
;CpyFiles=PRISM_DRIVER.copy.XP
BusType=15 ; USB
Characteristics= 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[PRISM_USB_XP1.Services]
AddService="MSW_USB", 2, PRISM_USB_DRIVER_XP1.Service, PRISM_DRIVER.EventLog
[PRISM_USB_XP1.reg]
HKR,Ndi ,DeviceID,0,"USB\VID_045E&PID_006E"
HKR,,PlatformId,0,"0"
HKR,,VendorDesc,0,%PRISM_USB1_STR%
HKR,,LoadFirmware,0,1
[PRISM_USB_DRIVER_XP1.Service]
DisplayName=%PRISM_USB_SERVICE_DISPLAY%
ServiceType=1 ; SERVICE_KERNEL_DRIVER
StartType=3 ; SERVICE_DEMAND_START
ErrorControl=1 ; NORMAL
ServiceBinary=%12%\MN510-51.sys
LoadOrderGroup=NDIS
[PRISM_DRIVER.EventLog]
AddReg=PRISM_DRIVER.EventLog.reg
[PRISM_DRIVER.EventLog.reg]
HKR, ,EventMessageFile ,0x00020000 ,"%%SystemRoot%%\System32\netevent.dll"
HKR, ,TypesSupported ,0x00010001 ,7
[COMMON_USB_XP1.reg]
HKR,NDI ,Service ,0 ,"MSW_USB"
HKR,NDI ,CardType ,0 ,"USB"
HKR, ,BusType ,0 ,"0"
HKR, ,DeviceVxDs ,0 ,"MN510-51.sys"
[COMMON_NDIS.reg.XP]
HKR,NDI\Interfaces ,UpperRange ,0 ,"ndis5"
HKR,NDI\Interfaces ,LowerRange ,0 ,"ethernet"
HKR,defaults,PSMode,0,1
HKR,Ndi\params\PSMode,default,0,1
HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
HKR,NDI\params\PSMode,type,,enum
HKR,NDI\params\PSMode,flag,1,30,00,00,00
HKR,NDI\params\PSMode\enum,1,,"Disable"
HKR,NDI\params\PSMode\enum,2,,"Always Enable"
HKR,NDI\params\PSMode\enum,3,,"Auto Enable"
[COMMON.reg]
HKR, ,MSWIOC ,0 ,"1"
HKR, ,SilentInstall ,0 ,"1"
HKR, ,APDensity ,0 ,"1"
HKR, ,ListenInterval ,0 ,"3"
HKR, ,Encapsulation ,0 ,"1"
HKR, ,Esarhpssap ,0 ,""
HKR,defaults,ListenInterval,0,3
HKR,NDI\params\ListenInterval,,0,3
HKR,Ndi\params\ListenInterval,default,0,3
HKR,NDI\params\ListenInterval,ParamDesc,,%LISTENINTERVAL_STR%
HKR,NDI\params\ListenInterval,type,,int
HKR,NDI\params\ListenInterval,flag,1,30,00,00,00
HKR,NDI\params\ListenInterval,min,0,0
HKR,NDI\params\ListenInterval,max,0,77
HKR,NDI\params\ListenInterval,step,0,1
HKR,NDI\params\ListenInterval,optional,0,1
HKR,defaults,RTSThresh,0,2432
HKR,Ndi\params\RTSThresh,default,0,2432
HKR,NDI\params\RTSThresh,ParamDesc,0,%RTSTHRESH_STR%
HKR,NDI\params\RTSThresh,type,0,int
HKR,NDI\params\RTSThresh,flag,1,20,00,00,00
HKR,NDI\params\RTSThresh,min,0,0
HKR,NDI\params\RTSThresh,max,0,2432
HKR,NDI\params\RTSThresh,step,0,64
HKR,defaults,FragThresh,0,2432
HKR,Ndi\params\FragThresh,default,0,2432
HKR,NDI\params\FragThresh,ParamDesc,0,%FRAGTHRESH_STR%
HKR,NDI\params\FragThresh,type,0,int
HKR,NDI\params\FragThresh,flag,1,20,00,00,00
HKR,NDI\params\FragThresh,min,0,256
HKR,NDI\params\FragThresh,max,0,2432
HKR,NDI\params\FragThresh,step,0,128
HKR,defaults,PreambleMode,0,1
HKR,Ndi\params\PreambleMode,default,0,1
HKR,NDI\params\PreambleMode,ParamDesc,,%SHORT_PREAM_STR%
HKR,NDI\params\PreambleMode,type,,enum
HKR,NDI\params\PreambleMode,flag,1,30,00,00,00
HKR,NDI\params\PreambleMode\enum,1,,"Long Tx Preamble"
HKR,NDI\params\PreambleMode\enum,2,,"Short Tx Preamble"
HKR,NDI\params\PreambleMode\enum,3,,"Auto Tx Preamble"
HKR,defaults,DSChannel,0,6
HKR,NDI\params\DSChannel,default,0,6
HKR,NDI\params\DSChannel,ParamDesc,0,%DSCHANNEL_STR%
HKR,NDI\params\DSChannel,type,0,"enum"
HKR,NDI\params\DSChannel\enum,1,0,"1"
HKR,NDI\params\DSChannel\enum,2,0,"2"
HKR,NDI\params\DSChannel\enum,3,0,"3"
HKR,NDI\params\DSChannel\enum,4,0,"4"
HKR,NDI\params\DSChannel\enum,5,0,"5"
HKR,NDI\params\DSChannel\enum,6,0,"6"
HKR,NDI\params\DSChannel\enum,7,0,"7"
HKR,NDI\params\DSChannel\enum,8,0,"8"
HKR,NDI\params\DSChannel\enum,9,0,"9"
HKR,NDI\params\DSChannel\enum,10,0,"10"
HKR,NDI\params\DSChannel\enum,11,0,"11"
HKR,defaults,NetworkType,0,1
HKR,NDI\params\NetworkType,default,0,1
HKR,NDI\params\NetworkType,ParamDesc,0,%NETWORKTYPE_STR%
HKR,NDI\params\NetworkType,type,0,"enum"
HKR,NDI\params\NetworkType\enum,0,0,%NETWORKTYPE_P0_STR%
HKR,NDI\params\NetworkType\enum,1,0,%NETWORKTYPE_P1_STR%
HKR,defaults,SSID,0,%DEFAULT_SSID_STR%
HKR,NDI\params\SSID,default,0,%DEFAULT_SSID_STR%
HKR,NDI\params\SSID,ParamDesc,0,%SSID_STR%
HKR,NDI\params\SSID,type,0,"edit"
HKR,NDI\params\SSID,limitText,0,"32"
HKR,NDI\params\SSID,flag,1,"30","00","00","00"
HKR,defaults,TxRate,0,15
HKR,NDI\params\TxRate,default,0,15
HKR,NDI\params\TxRate,ParamDesc,0,%TXRATE_STR%
HKR,NDI\params\TxRate,type,0,"enum"
HKR,NDI\params\TxRate\enum,3,0,%TXRATE_P3_STR%
HKR,NDI\params\TxRate\enum,4,0,%TXRATE_P4_STR%
HKR,NDI\params\TxRate\enum,8,0,%TXRATE_P8_STR%
HKR,NDI\params\TxRate\enum,15,0,%TXRATE_P15_STR%
HKR,defaults,DecryptInDriver,0,1
HKR, ,DecryptInDriver, 0, "1" ;1:Enable 0:Disable
HKR,defaults,EncryptInDriver,0,1
HKR, ,EncryptInDriver, 0, "1" ;1:Enable 0:Disable
HKR,defaults,WEPFactor,0,0
HKR, ,WEPFactor, 0, "0" ;Range:0~3
HKR,defaults,AuthentAlg,,%AUTHENT_TYPE_DEF_STR%
HKR,NDI\params\AuthentAlg,ParamDesc,,%AUTHENT_TYPE_STR%
HKR,NDI\params\AuthentAlg,type,,enum
HKR,NDI\params\AuthentAlg,default,,%AUTHENT_TYPE_DEF_STR%
HKR,NDI\params\AuthentAlg,flag,1,30,00,00,00
HKR,NDI\params\AuthentAlg\enum,1,,"WECA Compliant (always use Open)"
HKR,NDI\params\AuthentAlg\enum,2,,"Must use Shared with WEP"
HKR,NDI\params\AuthentAlg\enum,65535,,"Automatic based on WEP setting"
HKR,defaults,EnableRadio,0,1
HKR,NDI\params\EnableRadio,,0,1
HKR,NDI\params\EnableRadio,default,0,1
HKR,NDI\params\EnableRadio,ParamDesc,0,%ENABLERADIO_STR%
HKR,NDI\params\EnableRadio,type,0,"enum"
HKR,NDI\params\EnableRadio\enum,0,0,%ENABLERADIO_P0_STR%
HKR,NDI\params\EnableRadio\enum,1,0,%ENABLERADIO_P1_STR%
HKR,defaults,AdhocDemoMode,0,0
HKR,NDI\params\AdhocDemoMode,,0,0
HKR,Ndi\params\AdhocDemoMode,default,0,0
HKR,NDI\params\AdhocDemoMode,ParamDesc,,%ADHOC_DEMO_STR%
HKR,NDI\params\AdhocDemoMode,type,,enum
HKR,NDI\params\AdhocDemoMode,flag,1,30,00,00,00
HKR,NDI\params\AdhocDemoMode\enum,0,,"Disable"
HKR,NDI\params\AdhocDemoMode\enum,1,,"Enable"
HKR,NDI\params\AdhocDemoMode,optional,0,1
HKR,defaults,LoadFirmware,0,1
HKR,NDI\params\LoadFirmware,,0,1
HKR,Ndi\params\LoadFirmware,default,0,1
HKR,NDI\params\LoadFirmware,ParamDesc,,%LOAD_FIRMWARE_STR%
HKR,NDI\params\LoadFirmware,type,,enum
HKR,NDI\params\LoadFirmware,flag,1,30,00,00,00
HKR,NDI\params\LoadFirmware\enum,0,,"Disable"
HKR,NDI\params\LoadFirmware\enum,1,,"Enable"
HKR,NDI\params\LoadFirmware,optional,0,1
HKR,defaults,PDwellTime,0,120
HKR,NDI\params\PDwellTime,,0,120
HKR,Ndi\params\PDwellTime,default,0,120
HKR,NDI\params\PDwellTime,ParamDesc,0,%PDWELL_STR%
HKR,NDI\params\PDwellTime,type,0,int
HKR,NDI\params\PDwellTime,flag,1,20,00,00,00
HKR,NDI\params\PDwellTime,min,0,0
HKR,NDI\params\PDwellTime,max,0,1000
HKR,NDI\params\PDwellTime,step,0,10
HKR,NDI\params\PDwellTime,optional,0,1
HKR,defaults,11dMode,0,0
HKR,NDI\params\11dMode,,0,0
HKR,Ndi\params\11dMode,default,0,0
HKR,NDI\params\11dMode,ParamDesc,,%MDC_CONTROL_STR%
HKR,NDI\params\11dMode,type,,enum
HKR,NDI\params\11dMode,flag,1,30,00,00,00
HKR,NDI\params\11dMode\enum,0,,"None"
HKR,NDI\params\11dMode\enum,1,,"Strict"
HKR,NDI\params\11dMode\enum,2,,"Flexible"
HKR,NDI\params\11dMode,optional,0,1
HKR,defaults,IBSSInDriver,0,0
HKR, ,IBSSInDriver, 0, "0" ;1:Enable 0:Disable
HKR,defaults,BeaconPeriod,0,100
HKR, ,BeaconPeriod, 0, "100" ;Range:100~1000
HKR,defaults,BasicRates,0,15
HKR, ,BasicRates, 0, "15" ;bit0:1Mbps, bit1:2Mbps, bit2:5.5Mbps bit3:11Mbps
[DestinationDirs]
DefaultDestDir=11 ; Win9x=%windir%\system Win2k=%windir%\system32 WinXP=%windir%\system32
PRISM_DRIVER.copy.XP=12 ; WinXP=%windir%\system32\drivers
[PRISM_DRIVER.copy.XP]
MN510-51.sys,MN510-51.sys,,
[SourceDisksNames]
1=%INSTALL_DISK_STR%,,,
[SourceDisksFiles]
MN510-51.sys=1
[Strings]
VER_VENDOR_STR="Microsoft(R)"
VER_VENDOR_NAME_STR="Microsoft(R) Corporation"
PRISM_USB1_STR="Microsoft Broadband Networking Wireless USB Adapter"
PRISM_USB_SERVICE_DISPLAY="Microsoft Broadband Networking Wireless USB Driver"
INSTALL_DISK_STR="Microsoft Broadband Networking Install Disk"
SHORT_PREAM_STR="Preamble Mode"
RTSTHRESH_STR="RTS Threshold"
FRAGTHRESH_STR="Fragmentation Threshold"
POWER_SAVE_STR="Power Save Mode"
DSCHANNEL_STR="Channel"
NETWORKTYPE_STR="Network Type"
NETWORKTYPE_P0_STR="Peer to Peer"
NETWORKTYPE_P1_STR="Access Point"
SSID_STR="SSID"
DEFAULT_SSID_STR="MSHOME"
TXRATE_STR="Transmit Rate"
TXRATE_P3_STR="Auto 1 or 2 Mb"
TXRATE_P4_STR="5.5 Mb"
TXRATE_P8_STR="11 Mb"
TXRATE_P15_STR="Fully Automatic"
ENABLERADIO_STR="Enable Radio"
ENABLERADIO_P0_STR="Radio Off"
ENABLERADIO_P1_STR="Radio On"
AUTHENT_TYPE_DEF_STR="65535"
AUTHENT_TYPE_STR="Authentication Algorithm"
LISTENINTERVAL_STR="Listen Interval"
ADHOC_DEMO_STR="Adhoc Demo Mode"
LOAD_FIRMWARE_STR="Firmware Download"
PDWELL_STR="Passive Scan Dwell Time"
MDC_CONTROL_STR="802.11D Control"
