
[Version]
DriverVer=01/17/2002, 1.7.37
Signature="$Chicago$"
Compatible=1
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%VER_VENDOR_STR%
MillenniumPreferred=.ME
[ControlFlags]
ExcludeFromSelect=PCMCIA\CHOICE_MICROSYSTEMS-CW10/IEEE-5F95
ExcludeFromSelect=PCMCIA\11Mbps-Wireless_LAN_PC_CARD-B706
ExcludeFromSelect=PCMCIA\INTERSIL-HFA384x/IEEE-CC3C
ExcludeFromSelect=PCMCIA\INTERSIL-PRISM2_MINI-PCI_ADAPTER-0EE7
ExcludeFromSelect=PCMCIA\INTERSIL-PRISM2_5_MINI-PCI_ADAPTER-7759
ExcludeFromSelect=PCMCIA\INTERSIL-PRISM_FREEDOM_PCMCIA_ADAPTER-40CB
ExcludeFromSelect=PCMCIA\INTERSIL-PRISM_2_5_PCMCIA_ADAPTER-F429
ExcludeFromSelect=PCMCIA\Intersil-PRISM_ISL37101P-SSF_Adapter-A56F
ExcludeFromSelect=PCI\VEN_1260&DEV_3873&SUBSYS_00001260
ExcludeFromSelect=PCI\VEN_1260&DEV_3873&SUBSYS_38731260
ExcludeFromSelect=USB\VID_2474&PID_3642
ExcludeFromSelect=USB\VID_09AA&PID_3642
[Manufacturer]
%VER_VENDOR_NAME_STR%=DeviceList
[DeviceList]
%PRISM_PCMCIA1_STR%=PRISM_PCMCIA1, PCMCIA\CHOICE_MICROSYSTEMS-CW10/IEEE-5F95
%PRISM_PCMCIA2_STR%=PRISM_PCMCIA2, PCMCIA\11Mbps-Wireless_LAN_PC_CARD-B706
%PRISM_PCMCIA3_STR%=PRISM_PCMCIA3, PCMCIA\INTERSIL-HFA384x/IEEE-CC3C
%PRISM_PCMCIA4_STR%=PRISM_PCMCIA4, PCMCIA\INTERSIL-PRISM2_MINI-PCI_ADAPTER-0EE7
%PRISM_PCMCIA5_STR%=PRISM_PCMCIA5, PCMCIA\INTERSIL-PRISM2_5_MINI-PCI_ADAPTER-7759
%PRISM_PCMCIA6_STR%=PRISM_PCMCIA6, PCMCIA\INTERSIL-PRISM_FREEDOM_PCMCIA_ADAPTER-40CB
%PRISM_PCMCIA7_STR%=PRISM_PCMCIA7, PCMCIA\INTERSIL-PRISM_2_5_PCMCIA_ADAPTER-F429
%PRISM_PCMCIA8_STR%=PRISM_PCMCIA8, PCMCIA\Intersil-PRISM_ISL37101P-SSF_Adapter-A56F
%PRISM_PCI1_STR%=PRISM_PCI1, PCI\VEN_1260&DEV_3873&SUBSYS_00001260
%PRISM_PCI2_STR%=PRISM_PCI2, PCI\VEN_1260&DEV_3873&SUBSYS_38731260
%PRISM_USB1_STR%=PRISM_USB1, USB\VID_2474&PID_3642
%PRISM_USB1_STR%=PRISM_USB1, USB\VID_09AA&PID_3642
[PRISM_PCMCIA1.NT] ; Win2k
AddReg=PRISM_PCMCIA1.reg, COMMON_PCMCIA.reg, COMMON_NDIS.reg.NT, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.NT, PRISM_APPLET.copy.NT
BusType=8 ; PCMCIA
Characteristics= 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[PRISM_PCMCIA1.NT.Services]
AddService="PRISM", 2, PRISM_DRIVER.Service, PRISM_DRIVER.EventLog
[PRISM_PCMCIA1.NT.CoInstallers]
;CpyFiles=PRISM_COINSTALL.copy.NT
AddReg=PRISM_COINSTALL.reg.NT
[PRISM_PCMCIA1.reg]
HKR,Ndi ,DeviceID,0,"PCMCIA\CHOICE_MICROSYSTEMS-CW10/IEEE-5F95"
[PRISM_PCMCIA2.NT] ; Win2k
AddReg=PRISM_PCMCIA2.reg, COMMON_PCMCIA.reg, COMMON_NDIS.reg.NT, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.NT, PRISM_APPLET.copy.NT
BusType=8 ; PCMCIA
Characteristics= 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[PRISM_PCMCIA2.NT.Services]
AddService="PRISM", 2, PRISM_DRIVER.Service, PRISM_DRIVER.EventLog
[PRISM_PCMCIA2.NT.CoInstallers]
;CpyFiles=PRISM_COINSTALL.copy.NT
AddReg=PRISM_COINSTALL.reg.NT
[PRISM_PCMCIA2.reg]
HKR,Ndi ,DeviceID,0,"PCMCIA\11Mbps-Wireless_LAN_PC_CARD-B706"
[PRISM_PCMCIA3.NT] ; Win2k
AddReg=PRISM_PCMCIA3.reg, COMMON_PCMCIA.reg, COMMON_NDIS.reg.NT, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.NT, PRISM_APPLET.copy.NT
BusType=8 ; PCMCIA
Characteristics= 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[PRISM_PCMCIA3.NT.Services]
AddService="PRISM", 2, PRISM_DRIVER.Service, PRISM_DRIVER.EventLog
[PRISM_PCMCIA3.NT.CoInstallers]
;CpyFiles=PRISM_COINSTALL.copy.NT
AddReg=PRISM_COINSTALL.reg.NT
[PRISM_PCMCIA3.reg]
HKR,Ndi ,DeviceID,0,"PCMCIA\INTERSIL-HFA384x/IEEE-CC3C"
[PRISM_PCMCIA4.NT] ; Win2k
AddReg=PRISM_PCMCIA4.reg, COMMON_PCMCIA.reg, COMMON_NDIS.reg.NT, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.NT, PRISM_APPLET.copy.NT
BusType=8 ; PCMCIA
Characteristics= 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[PRISM_PCMCIA4.NT.Services]
AddService="PRISM", 2, PRISM_DRIVER.Service, PRISM_DRIVER.EventLog
[PRISM_PCMCIA4.NT.CoInstallers]
;CpyFiles=PRISM_COINSTALL.copy.NT
AddReg=PRISM_COINSTALL.reg.NT
[PRISM_PCMCIA4.reg]
HKR,Ndi ,DeviceID,0,"PCMCIA\INTERSIL-PRISM2_MINI-PCI_ADAPTER-0EE7"
[PRISM_PCMCIA5.NT] ; Win2k
AddReg=PRISM_PCMCIA5.reg, COMMON_PCMCIA.reg, COMMON_NDIS.reg.NT, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.NT, PRISM_APPLET.copy.NT
BusType=8 ; PCMCIA
Characteristics= 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[PRISM_PCMCIA5.NT.Services]
AddService="PRISM", 2, PRISM_DRIVER.Service, PRISM_DRIVER.EventLog
[PRISM_PCMCIA5.NT.CoInstallers]
;CpyFiles=PRISM_COINSTALL.copy.NT
AddReg=PRISM_COINSTALL.reg.NT
[PRISM_PCMCIA5.reg]
HKR,Ndi ,DeviceID,0,"PCMCIA\INTERSIL-PRISM2_5_MINI-PCI_ADAPTER-7759"
[PRISM_PCMCIA6.NT] ; Win2k
AddReg=PRISM_PCMCIA6.reg, COMMON_PCMCIA.reg, COMMON_NDIS.reg.NT, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.NT, PRISM_APPLET.copy.NT
BusType=8 ; PCMCIA
Characteristics= 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[PRISM_PCMCIA6.NT.Services]
AddService="PRISM", 2, PRISM_DRIVER.Service, PRISM_DRIVER.EventLog
[PRISM_PCMCIA6.NT.CoInstallers]
;CpyFiles=PRISM_COINSTALL.copy.NT
AddReg=PRISM_COINSTALL.reg.NT
[PRISM_PCMCIA6.reg]
HKR,Ndi ,DeviceID,0,"PCMCIA\INTERSIL-PRISM_FREEDOM_PCMCIA_ADAPTER-40CB"
[PRISM_PCMCIA7.NT] ; Win2k
AddReg=PRISM_PCMCIA7.reg, COMMON_PCMCIA.reg, COMMON_NDIS.reg.NT, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.NT, PRISM_APPLET.copy.NT
BusType=8 ; PCMCIA
Characteristics= 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[PRISM_PCMCIA7.NT.Services]
AddService="PRISM", 2, PRISM_DRIVER.Service, PRISM_DRIVER.EventLog
[PRISM_PCMCIA7.NT.CoInstallers]
;CpyFiles=PRISM_COINSTALL.copy.NT
AddReg=PRISM_COINSTALL.reg.NT
[PRISM_PCMCIA7.reg]
HKR,Ndi ,DeviceID,0,"PCMCIA\INTERSIL-PRISM_2_5_PCMCIA_ADAPTER-F429"
[PRISM_PCMCIA8.NT] ; Win2k
AddReg=PRISM_PCMCIA8.reg, COMMON_PCMCIA.reg, COMMON_NDIS.reg.NT, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.NT, PRISM_APPLET.copy.NT
BusType=8 ; PCMCIA
Characteristics= 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[PRISM_PCMCIA8.NT.Services]
AddService="PRISM", 2, PRISM_DRIVER.Service, PRISM_DRIVER.EventLog
[PRISM_PCMCIA8.NT.CoInstallers]
;CpyFiles=PRISM_COINSTALL.copy.NT
AddReg=PRISM_COINSTALL.reg.NT
[PRISM_PCMCIA8.reg]
HKR,Ndi ,DeviceID,0,"PCMCIA\Intersil-PRISM_ISL37101P-SSF_Adapter-A56F"
[PRISM_PCI1.NT] ; Win2k
AddReg=PRISM_PCI1.reg, COMMON_PCI.reg, COMMON_NDIS.reg.NT, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.NT, PRISM_APPLET.copy.NT
BusType=5 ; PCI
Characteristics= 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[PRISM_PCI1.NT.Services]
AddService="PRISM", 2, PRISM_DRIVER.Service, PRISM_DRIVER.EventLog
[PRISM_PCI1.NT.CoInstallers]
;CpyFiles=PRISM_COINSTALL.copy.NT
AddReg=PRISM_COINSTALL.reg.NT
[PRISM_PCI1.reg]
HKR,Ndi ,DeviceID,0,"PCI\VEN_1260&DEV_3873&SUBSYS_00001260"
[PRISM_PCI2.NT] ; Win2k
AddReg=PRISM_PCI2.reg, COMMON_PCI.reg, COMMON_NDIS.reg.NT, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.NT, PRISM_APPLET.copy.NT
BusType=5 ; PCI
Characteristics= 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[PRISM_PCI2.NT.Services]
AddService="PRISM", 2, PRISM_DRIVER.Service, PRISM_DRIVER.EventLog
[PRISM_PCI2.NT.CoInstallers]
;CpyFiles=PRISM_COINSTALL.copy.NT
AddReg=PRISM_COINSTALL.reg.NT
[PRISM_PCI2.reg]
HKR,Ndi ,DeviceID,0,"PCI\VEN_1260&DEV_3873&SUBSYS_38731260"
[PRISM_USB1.NT] ; Win2k
AddReg=PRISM_USB1.reg, COMMON_USB.reg, COMMON_NDIS.reg.NT, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.NT, PRISM_APPLET.copy.NT
BusType=0 ; USB
Characteristics= 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[PRISM_USB1.NT.Services]
AddService="PRISM_USB", 2, PRISM_USB_DRIVER.Service, PRISM_DRIVER.EventLog
[PRISM_USB1.NT.CoInstallers]
;CpyFiles=PRISM_COINSTALL.copy.NT
AddReg=PRISM_COINSTALL.reg.NT
[PRISM_USB1.reg]
HKR,Ndi ,DeviceID,0,"USB\VID_2474&PID_3642"
[PRISM_COINSTALL.reg.NT]
[PRISM_DRIVER.Service]
DisplayName=%PRISM_SERVICE_DISPLAY%
ServiceType=1 ; SERVICE_KERNEL_DRIVER
StartType=3 ; SERVICE_DEMAND_START
ErrorControl=1 ; NORMAL
ServiceBinary=%12%\PRISMNDS.sys
LoadOrderGroup=NDIS
[PRISM_USB_DRIVER.Service]
DisplayName=%PRISM_USB_SERVICE_DISPLAY%
ServiceType=1 ; SERVICE_KERNEL_DRIVER
StartType=3 ; SERVICE_DEMAND_START
ErrorControl=1 ; NORMAL
ServiceBinary=%12%\PRISMUSB.sys
LoadOrderGroup=NDIS
[PRISM_DRIVER.EventLog]
AddReg=PRISM_DRIVER.EventLog.reg
[PRISM_DRIVER.EventLog.reg]
HKR, ,EventMessageFile ,0x00020000 ,"%%SystemRoot%%\System32\netevent.dll"
HKR, ,TypesSupported ,0x00010001 ,7
[COMMON_PCMCIA.reg]
HKR,NDI ,Service ,0 ,"PRISM"
HKR,NDI ,CardType ,0 ,"PCMCIA"
HKR, ,BusType ,0 ,"8"
HKR, ,DeviceVxDs ,0 ,"PRISMNDS.sys"
HKR, ,EnableIRQSharing ,1 ,01,00,00,00
HKR, ,IOBaseAddress ,1 ,02,00,00,00
HKR, ,InterruptNumber ,1 ,04,00,00,00
[COMMON_PCI.reg]
HKR,NDI ,Service ,0 ,"PRISM"
HKR,NDI ,CardType ,0 ,"PCI"
HKR, ,BusType ,0 ,"5"
HKR, ,DeviceVxDs ,0 ,"PRISMNDS.sys"
HKR, ,EnableIRQSharing ,1 ,01,00,00,00
HKR, ,IOBaseAddress ,1 ,02,00,00,00
HKR, ,InterruptNumber ,1 ,04,00,00,00
[COMMON_USB.reg]
HKR,NDI ,Service ,0 ,"PRISM_USB"
HKR,NDI ,CardType ,0 ,"USB"
HKR, ,BusType ,0 ,"0"
HKR, ,DeviceVxDs ,0 ,"PRISMUSB.sys"
[COMMON_NDIS.reg]
HKR, ,RunningWin9X ,0 ,"1"
HKR, ,DevLoader ,0 ,"*ndis"
HKR, ,EnumPropPages ,0 ,"netdi.dll,EnumPropPages"
HKR,NDI ,NdiInstaller ,0 ,"PRISMCFG.dll,NdiProc"
HKR,NDI\Interfaces ,UpperRange ,0 ,"ndis3"
HKR,NDI\Interfaces ,LowerRange ,0 ,"ethernet"
HKR,NDI\Interfaces ,DefUpper ,0 ,"ndis3"
HKR,NDI\Interfaces ,DefLower ,0 ,"ethernet"
HKR,NDIS ,LogDriverName ,0 ,"PRISM"
HKR,NDIS ,MajorNdisVersion ,1 ,03
HKR,NDIS ,MinorNdisVersion ,1 ,0a
HKR,defaults,PSMode,0,1
HKR,NDI\params\PSMode,,0,1
HKR,Ndi\params\PSMode,default,0,1
HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
HKR,NDI\params\PSMode,type,,enum
HKR,NDI\params\PSMode,flag,1,30,00,00,00
HKR,NDI\params\PSMode\enum,1,,"Disable"
HKR,NDI\params\PSMode\enum,2,,"Always Enable"
HKR,NDI\params\PSMode,optional,0,1
[COMMON_NDIS.reg.ME]
HKR, ,RunningWin9X ,0 ,"1"
HKR, ,DevLoader ,0 ,"*ndis"
HKR, ,EnumPropPages ,0 ,"netdi.dll,EnumPropPages"
HKR,NDI ,NdiInstaller ,0 ,"PRISMCFG.dll,NdiProc"
HKR,NDI\Interfaces ,UpperRange ,0 ,"ndis3"
HKR,NDI\Interfaces ,LowerRange ,0 ,"ethernet"
HKR,NDI\Interfaces ,DefUpper ,0 ,"ndis3"
HKR,NDI\Interfaces ,DefLower ,0 ,"ethernet"
HKR,NDIS ,LogDriverName ,0 ,"PRISM"
HKR,NDIS ,MajorNdisVersion ,1 ,03
HKR,NDIS ,MinorNdisVersion ,1 ,0a
HKR,defaults,PSMode,0,1
HKR,NDI\params\PSMode,,0,1
HKR,Ndi\params\PSMode,default,0,1
HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
HKR,NDI\params\PSMode,type,,enum
HKR,NDI\params\PSMode,flag,1,30,00,00,00
HKR,NDI\params\PSMode\enum,1,,"Disable"
HKR,NDI\params\PSMode\enum,2,,"Always Enable"
HKR,NDI\params\PSMode,optional,0,1
[COMMON_NDIS.reg.NT]
HKR,NDI\Interfaces ,UpperRange ,0 ,"ndis5"
HKR,NDI\Interfaces ,LowerRange ,0 ,"ethernet"
HKR,defaults,PSMode,0,1
HKR,NDI\params\PSMode,,0,1
HKR,Ndi\params\PSMode,default,0,1
HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
HKR,NDI\params\PSMode,type,,enum
HKR,NDI\params\PSMode,flag,1,30,00,00,00
HKR,NDI\params\PSMode\enum,1,,"Disable"
HKR,NDI\params\PSMode\enum,2,,"Always Enable"
HKR,NDI\params\PSMode\enum,3,,"Auto Enable"
HKR,NDI\params\PSMode,optional,0,1
[COMMON.reg]
HKR, ,PRISMIOC ,0 ,"1"
HKR, ,SilentInstall ,0 ,"1"
HKR,defaults,ListenInterval,0,3
HKR,NDI\params\ListenInterval,,0,3
HKR,Ndi\params\ListenInterval,default,0,3
HKR,NDI\params\ListenInterval,ParamDesc,,%LISTENINTERVAL_STR%
HKR,NDI\params\ListenInterval,type,,int
HKR,NDI\params\ListenInterval,flag,1,30,00,00,00
HKR,NDI\params\ListenInterval,min,0,0
HKR,NDI\params\ListenInterval,max,0,77
HKR,NDI\params\ListenInterval,step,0,1
HKR,NDI\params\ListenInterval,optional,0,1
HKR,defaults,RTSThresh,0,2432
HKR,NDI\params\RTSThresh,,0,2432
HKR,Ndi\params\RTSThresh,default,0,2432
HKR,NDI\params\RTSThresh,ParamDesc,0,%RTSTHRESH_STR%
HKR,NDI\params\RTSThresh,type,0,int
HKR,NDI\params\RTSThresh,flag,1,20,00,00,00
HKR,NDI\params\RTSThresh,min,0,0
HKR,NDI\params\RTSThresh,max,0,2432
HKR,NDI\params\RTSThresh,step,0,64
HKR,NDI\params\RTSThresh,optional,0,1
HKR,defaults,FragThresh,0,2432
HKR,NDI\params\FragThresh,,0,2432
HKR,Ndi\params\FragThresh,default,0,2432
HKR,NDI\params\FragThresh,ParamDesc,0,%FRAGTHRESH_STR%
HKR,NDI\params\FragThresh,type,0,int
HKR,NDI\params\FragThresh,flag,1,20,00,00,00
HKR,NDI\params\FragThresh,min,0,256
HKR,NDI\params\FragThresh,max,0,2432
HKR,NDI\params\FragThresh,step,0,128
HKR,NDI\params\FragThresh,optional,0,1
HKR,defaults,PreambleMode,0,1
HKR,NDI\params\PreambleMode,,0,1
HKR,Ndi\params\PreambleMode,default,0,1
HKR,NDI\params\PreambleMode,ParamDesc,,%SHORT_PREAM_STR%
HKR,NDI\params\PreambleMode,type,,enum
HKR,NDI\params\PreambleMode,flag,1,30,00,00,00
HKR,NDI\params\PreambleMode\enum,1,,"Long Tx Preamble"
HKR,NDI\params\PreambleMode\enum,2,,"Short Tx Preamble"
HKR,NDI\params\PreambleMode\enum,3,,"Auto Tx Preamble"
HKR,NDI\params\PreambleMode,optional,0,1
HKR,defaults,AuthentAlg,0,65535
HKR,NDI\params\AuthentAlg,,0,65535
HKR,NDI\params\AuthentAlg,default,0,65535
HKR,NDI\params\AuthentAlg,ParamDesc,,%AUTHENT_TYPE_STR%
HKR,NDI\params\AuthentAlg,type,,enum
HKR,NDI\params\AuthentAlg,flag,1,30,00,00,00
HKR,NDI\params\AuthentAlg\enum,1,,"WECA Compliant (always use Open)"
HKR,NDI\params\AuthentAlg\enum,2,,"Must use Shared with WEP"
HKR,NDI\params\AuthentAlg\enum,65535,,"Automatic based on WEP setting"
HKR,NDI\params\AuthentAlg,optional,0,1
HKR,defaults,AdhocDemoMode,0,0
HKR,NDI\params\AdhocDemoMode,,0,0
HKR,Ndi\params\AdhocDemoMode,default,0,0
HKR,NDI\params\AdhocDemoMode,ParamDesc,,%ADHOC_DEMO_STR%
HKR,NDI\params\AdhocDemoMode,type,,enum
HKR,NDI\params\AdhocDemoMode,flag,1,30,00,00,00
HKR,NDI\params\AdhocDemoMode\enum,0,,"Disable"
HKR,NDI\params\AdhocDemoMode\enum,1,,"Enable"
HKR,NDI\params\AdhocDemoMode,optional,0,1
HKLM,"Software\Microsoft\Windows\CurrentVersion\Uninstall\Intersil PRISM Wireless LAN Driver",DisplayName,,"Intersil PRISM Wireless LAN Driver"
[DestinationDirs]
DefaultDestDir=11 ; Win9x=%windir%\system Win2k=%windir%\system32
PRISM_DRIVER.copy.NT=12 ; Win2k=%windir%\system32\drivers
[PRISM_COINSTALL.copy.NT]
[PRISM_DRIVER.copy.NT]
PRISMNDS.sys,PRISMNDS.sy_,,
PRISMUSB.sys,PRISMUSB.sy_,,
[PRISM_APPLET.copy.NT]
[SourceDisksNames]
1=%INSTALL_DISK_STR%,,,
[SourceDisksFiles.X86] ; Win2k/Xp
PRISMRES.dl_=1
PRISMIOC.dl_=1
PRISMCFG.cp_=1 ;,win2k
PRISMNDS.sy_=1 ;,winxp
PRISMUSB.sy_=1 ;,winxp
PRISMSTA.ex_=1
uninstall.ex_=1
remove.ex_=1
[Strings]
VER_VENDOR_STR="Intersil"
VER_VENDOR_NAME_STR="Intersil Corporation"
PRISM_PCMCIA1_STR="Intersil PRISM Wireless LAN PC Card (5-Volt)"
PRISM_PCMCIA2_STR="11Mbps Wireless LAN PC CARD"
PRISM_PCMCIA3_STR="Intersil PRISM Wireless LAN PC Card"
PRISM_PCMCIA4_STR="Intersil PRISM Wireless LAN Mini-PCI 2.0"
PRISM_PCMCIA5_STR="Intersil PRISM Wireless LAN Mini-PCI 2.5"
PRISM_PCMCIA6_STR="Intersil PRISM Wireless LAN Freedom PC Card"
PRISM_PCMCIA7_STR="Intersil PRISM Wireless LAN PC Card 2.5"
PRISM_PCMCIA8_STR="Intersil PRISM Wireless LAN ISL37101P PC Card"
PRISM_PCI1_STR="Intersil PRISM Wireless LAN PCI Card"
PRISM_PCI2_STR="Intersil PRISM Wireless LAN PCI Card"
PRISM_USB1_STR="Intersil PRISM Wireless LAN USB Card"
PRISM_SERVICE_DISPLAY="Intersil PRISM Wireless LAN Driver"
PRISM_USB_SERVICE_DISPLAY="Intersil PRISM Wireless LAN USB Driver"
INSTALL_DISK_STR="Intersil PRISM Wireless LAN Install Disk"
ADHOC_DEMO_STR="Adhoc Demo Mode"
SHORT_PREAM_STR="Preamble Mode"
RTSTHRESH_STR="RTS Threshold"
FRAGTHRESH_STR="Fragmentation Threshold"
AUTHENT_TYPE_STR="Authentication Algorithm"
LISTENINTERVAL_STR="Listen Interval"
POWER_SAVE_STR="Power Save Mode"
POWER_LEVEL_STR="Power Save Level"

