
[Version]
DriverVer=05/08/2002, 1.07.37.1037
Signature="$Chicago$"
Compatible=1
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%VER_VENDOR_STR%
CatalogFile=NETWPX96.cat
[ControlFlags]
ExcludeFromSelect=PCMCIA\WIRELESS_LAN-11MBPS_PC_CARD-207D
ExcludeFromSelect=PCI\VEN_1260&DEV_3873&SUBSYS_000110B7
[Manufacturer]
%VER_VENDOR_NAME_STR%=DeviceList,NTx86.5.1
[DeviceList.NTx86.5.1]
%PRISM_PCMCIA7_STR%=PRISM_PCMCIA7.NT, PCMCIA\WIRELESS_LAN-11MBPS_PC_CARD-207D
%PRISM_PCI1_STR%=PRISM_PCI1.NT, PCI\VEN_1260&DEV_3873&SUBSYS_000110B7
[DeviceList]
%PRISM_PCMCIA7_STR%=PRISM_PCMCIA7, PCMCIA\WIRELESS_LAN-11MBPS_PC_CARD-207D
%PRISM_PCI1_STR%=PRISM_PCI1, PCI\VEN_1260&DEV_3873&SUBSYS_000110B7
[PRISM_PCMCIA7] ; Win9x
AddReg=PRISM_PCMCIA7.reg, COMMON_PCMCIA.reg, COMMON_NDIS.reg, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy
[PRISM_PCMCIA7.NT] ; Win2k
AddReg=PRISM_PCMCIA7.reg, COMMON_PCMCIA.reg, COMMON_NDIS.reg.NT, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.NT
BusType=8 ; PCMCIA
Characteristics= 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[PRISM_PCMCIA7.NT.Services]
AddService="PRISM", 2, PRISM_DRIVER.Service, PRISM_DRIVER.EventLog
[PRISM_PCMCIA7.reg]
HKR,Ndi ,DeviceID,0,"PCMCIA\WIRELESS_LAN-11MBPS_PC_CARD-207D"
[PRISM_PCI1] ; Win9x
AddReg=PRISM_PCI1.reg, COMMON_PCI.reg, COMMON_NDIS.reg, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy
[PRISM_PCI1.NT] ; Win2k
AddReg=PRISM_PCI1.reg, COMMON_PCI.reg, COMMON_NDIS.reg.NT, COMMON.reg
;CpyFiles=PRISM_DRIVER.copy.NT
BusType=5 ; PCI
Characteristics= 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[PRISM_PCI1.NT.Services]
AddService="PRISM", 2, PRISM_DRIVER.Service, PRISM_DRIVER.EventLog
[PRISM_PCI1.reg]
HKR,Ndi ,DeviceID,0,"PCI\VEN_1260&DEV_3873&SUBSYS_000110B7"
[PRISM_DRIVER.Service]
DisplayName=%PRISM_SERVICE_DISPLAY%
ServiceType=1 ; SERVICE_KERNEL_DRIVER
StartType=3 ; SERVICE_DEMAND_START
ErrorControl=1 ; NORMAL
ServiceBinary=%12%\PRISMNDS.sys
LoadOrderGroup=NDIS
[PRISM_DRIVER.EventLog]
AddReg=PRISM_DRIVER.EventLog.reg
[PRISM_DRIVER.EventLog.reg]
HKR, ,EventMessageFile ,0x00020000 ,"%%SystemRoot%%\System32\netevent.dll"
HKR, ,TypesSupported ,0x00010001 ,7
[COMMON_PCMCIA.reg]
HKR,NDI ,Service ,0 ,"PRISM"
HKR,NDI ,CardType ,0 ,"PCMCIA"
HKR, ,BusType ,0 ,"8"
HKR, ,DeviceVxDs ,0 ,"PRISMNDS.sys"
HKR, ,EnableIRQSharing ,1 ,01,00,00,00
HKR, ,IOBaseAddress ,1 ,02,00,00,00
HKR, ,InterruptNumber ,1 ,04,00,00,00
[COMMON_PCI.reg]
HKR,NDI ,Service ,0 ,"PRISM"
HKR,NDI ,CardType ,0 ,"PCI"
HKR, ,BusType ,0 ,"5"
HKR, ,DeviceVxDs ,0 ,"PRISMNDS.sys"
HKR, ,EnableIRQSharing ,1 ,01,00,00,00
HKR, ,IOBaseAddress ,1 ,02,00,00,00
HKR, ,InterruptNumber ,1 ,04,00,00,00
[COMMON_NDIS.reg]
HKR, ,RunningWin9X ,0 ,"1"
HKR, ,DevLoader ,0 ,"*ndis"
HKR, ,EnumPropPages ,0 ,"netdi.dll,EnumPropPages"
HKR,NDI ,NdiInstaller ,0 ,"PRISMCFG.dll,NdiProc"
HKR,NDI\Interfaces ,UpperRange ,0 ,"ndis3"
HKR,NDI\Interfaces ,LowerRange ,0 ,"ethernet"
HKR,NDI\Interfaces ,DefUpper ,0 ,"ndis3"
HKR,NDI\Interfaces ,DefLower ,0 ,"ethernet"
HKR,NDIS ,LogDriverName ,0 ,"PRISM"
HKR,NDIS ,MajorNdisVersion ,1 ,03
HKR,NDIS ,MinorNdisVersion ,1 ,0a
HKR,defaults,PSMode,0,1
HKR,NDI\params\PSMode,,0,1
HKR,Ndi\params\PSMode,default,0,1
HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
HKR,NDI\params\PSMode,type,,enum
HKR,NDI\params\PSMode,flag,1,30,00,00,00
HKR,NDI\params\PSMode\enum,1,,"Disable"
HKR,NDI\params\PSMode\enum,2,,"Always Enable"
HKR,NDI\params\PSMode,optional,0,1
[COMMON_NDIS.reg.NT]
HKR,NDI\Interfaces ,UpperRange ,0 ,"ndis5"
HKR,NDI\Interfaces ,LowerRange ,0 ,"ethernet"
HKR,defaults,PSMode,0,1
HKR,NDI\params\PSMode,,0,1
HKR,Ndi\params\PSMode,default,0,1
HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
HKR,NDI\params\PSMode,type,,enum
HKR,NDI\params\PSMode,flag,1,30,00,00,00
HKR,NDI\params\PSMode\enum,1,,"Disable"
HKR,NDI\params\PSMode\enum,2,,"Always Enable"
HKR,NDI\params\PSMode\enum,3,,"Auto Enable"
HKR,NDI\params\PSMode,optional,0,1
[COMMON.reg]
HKR, ,GTKSIOC ,0 ,"1"
HKR, ,PRISMIOC ,0 ,"1"
HKR, ,SilentInstall ,0 ,"1"
HKR,defaults,ListenInterval,0,3
HKR,NDI\params\ListenInterval,,0,3
HKR,Ndi\params\ListenInterval,default,0,3
HKR,NDI\params\ListenInterval,ParamDesc,,%LISTENINTERVAL_STR%
HKR,NDI\params\ListenInterval,type,,int
HKR,NDI\params\ListenInterval,flag,1,30,00,00,00
HKR,NDI\params\ListenInterval,min,0,0
HKR,NDI\params\ListenInterval,max,0,77
HKR,NDI\params\ListenInterval,step,0,1
HKR,NDI\params\ListenInterval,optional,0,1
HKR,defaults,RTSThresh,0,2432
HKR,NDI\params\RTSThresh,,0,2432
HKR,Ndi\params\RTSThresh,default,0,2432
HKR,NDI\params\RTSThresh,ParamDesc,0,%RTSTHRESH_STR%
HKR,NDI\params\RTSThresh,type,0,int
HKR,NDI\params\RTSThresh,flag,1,20,00,00,00
HKR,NDI\params\RTSThresh,min,0,0
HKR,NDI\params\RTSThresh,max,0,2432
HKR,NDI\params\RTSThresh,step,0,64
HKR,NDI\params\RTSThresh,optional,0,1
HKR,defaults,FragThresh,0,2432
HKR,NDI\params\FragThresh,,0,2432
HKR,Ndi\params\FragThresh,default,0,2432
HKR,NDI\params\FragThresh,ParamDesc,0,%FRAGTHRESH_STR%
HKR,NDI\params\FragThresh,type,0,int
HKR,NDI\params\FragThresh,flag,1,20,00,00,00
HKR,NDI\params\FragThresh,min,0,256
HKR,NDI\params\FragThresh,max,0,2432
HKR,NDI\params\FragThresh,step,0,128
HKR,NDI\params\FragThresh,optional,0,1
HKR,defaults,PreambleMode,0,1
HKR,NDI\params\PreambleMode,,0,1
HKR,Ndi\params\PreambleMode,default,0,1
HKR,NDI\params\PreambleMode,ParamDesc,,%SHORT_PREAM_STR%
HKR,NDI\params\PreambleMode,type,,enum
HKR,NDI\params\PreambleMode,flag,1,30,00,00,00
HKR,NDI\params\PreambleMode\enum,1,,"Long Tx Preamble"
HKR,NDI\params\PreambleMode\enum,2,,"Short Tx Preamble"
HKR,NDI\params\PreambleMode\enum,3,,"Auto Tx Preamble"
HKR,NDI\params\PreambleMode,optional,0,1
HKR,defaults,AuthentAlg,0,65535
HKR,NDI\params\AuthentAlg,,0,65535
HKR,NDI\params\AuthentAlg,default,0,65535
HKR,NDI\params\AuthentAlg,ParamDesc,,%AUTHENT_TYPE_STR%
HKR,NDI\params\AuthentAlg,type,,enum
HKR,NDI\params\AuthentAlg,flag,1,30,00,00,00
HKR,NDI\params\AuthentAlg\enum,1,,"WECA Compliant (always use Open)"
HKR,NDI\params\AuthentAlg\enum,2,,"Must use Shared with WEP"
HKR,NDI\params\AuthentAlg\enum,65535,,"Automatic based on WEP setting"
HKR,NDI\params\AuthentAlg,optional,0,1
HKR,defaults,AdhocDemoMode,0,0
HKR,NDI\params\AdhocDemoMode,,0,0
HKR,Ndi\params\AdhocDemoMode,default,0,0
HKR,NDI\params\AdhocDemoMode,ParamDesc,,%ADHOC_DEMO_STR%
HKR,NDI\params\AdhocDemoMode,type,,enum
HKR,NDI\params\AdhocDemoMode,flag,1,30,00,00,00
HKR,NDI\params\AdhocDemoMode\enum,0,,"Disable"
HKR,NDI\params\AdhocDemoMode\enum,1,,"Enable"
HKR,NDI\params\AdhocDemoMode,optional,0,1
[DestinationDirs]
DefaultDestDir=11 ; Win9x=%windir%\system Win2k=%windir%\system32
PRISM_DRIVER.copy=11 ; Win9x=%windir%\system
PRISM_DRIVER.copy.NT=12 ; Win2k=%windir%\system32\drivers
[PRISM_DRIVER.copy]
PRISMNDS.sys
[PRISM_DRIVER.copy.NT]
PRISMNDS.sys
[SourceDisksNames]
1=%INSTALL_DISK_STR%,,,
[SourceDisksFiles] ; Win9x
PRISMNDS.sys=1
[SourceDisksFiles.X86] ; Win2k/Xp
PRISMNDS.sys=1,SYS
[Strings]
VER_VENDOR_STR="3Com"
VER_VENDOR_NAME_STR="3Com Corporation"
PRISM_PCMCIA7_STR="3Com 3CRDW696 Wireless LAN PC Card"
PRISM_PCI1_STR="3Com 3CRDW696 Wireless LAN PCI Adapter"
PRISM_PCI2_STR="3Com 3CRDW696 Wireless LAN PCI Adapter"
PRISM_SERVICE_DISPLAY="3Com 3CRDW696 Wireless LAN PCI Adapter LAN Driver"
INSTALL_DISK_STR="3Com 3CRDW696 Wireless LAN PCI Adapter Install Disk"
ADHOC_DEMO_STR="Adhoc Demo Mode"
SHORT_PREAM_STR="Preamble Mode"
RTSTHRESH_STR="RTS Threshold"
FRAGTHRESH_STR="Fragmentation Threshold"
AUTHENT_TYPE_STR="Authentication Algorithm"
LISTENINTERVAL_STR="Listen Interval"
POWER_SAVE_STR="Power Save Mode"
POWER_LEVEL_STR="Power Save Level"

