
[Version]
Signature="$Chicago$"
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%Hercules%
Compatible=1
CatalogFile=netr61.cat
DriverVer=12/13/2006,2.00.03.0000
[ControlFlags]
[Manufacturer]
%Hercules%=Hercules
[Hercules]
%Hercules.DeviceDesc1%=RALINK.ndi, PCI\VEN_1814&DEV_0301&SUBSYS_00401681
%Hercules.DeviceDesc2%=RALINK.ndi, PCI\VEN_1814&DEV_0301&SUBSYS_00501681
%Hercules.DeviceDesc3%=RALINK1.ndi, PCI\VEN_1814&DEV_0201&SUBSYS_00401681
%Hercules.DeviceDesc4%=RALINK1.ndi, PCI\VEN_1814&DEV_0201&SUBSYS_00501681
%Hercules.DeviceDesc5%=RALINK.ndi, PCI\VEN_1814&DEV_0302&SUBSYS_00401681
%Hercules.DeviceDesc6%=RALINK.ndi, PCI\VEN_1814&DEV_0302&SUBSYS_00501681
[RALINK.ndi.NT]
AddReg=RT61.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=5
;CpyFiles=NT.CopyFiles
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
[RALINK1.ndi.NT]
AddReg=Common.reg, RT2500.ndi.NT.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=5
;CpyFiles=NT1.CopyFiles
[RALINK.ndi.NT.Services]
AddService=rt61x86, 2, RALINK.Service, common.EventLog
[RALINK1.ndi.NT.Services]
AddService=RT2500, 2, RALINK1.Service, common1.EventLog
[Common.reg]
HKR, , CurProfile, 0,""
HKR, Default, CurProfile, 0,""
HKR, , Radio, 0, "0"
HKR, NDI\params\Radio, ParamDesc, 0, "Radio On/Off"
HKR, NDI\params\Radio, type, 0, "enum"
HKR, NDI\params\Radio, default, 0, "0"
HKR, NDI\params\Radio\enum, 1, 0, "Disable"
HKR, NDI\params\Radio\enum, 0, 0, "Enable"
HKR, , AutoReconnect, 0, "1"
HKR, NDI\params\AutoReconnect, ParamDesc, 0, "Auto Reconnect Mode"
HKR, NDI\params\AutoReconnect, type, 0, "enum"
HKR, NDI\params\AutoReconnect, default, 0, "1"
HKR, NDI\params\AutoReconnect\enum, 0, 0, "Disable"
HKR, NDI\params\AutoReconnect\enum, 1, 0, "Enable"
HKR, , ShowHiddenSSID, 0, "0" ; 0=disable(default), 1=enable
HKR, , CountryRegion, 0, "0"
HKR, NDI\params\CountryRegion, ParamDesc, 0, "Country Region"
HKR, NDI\params\CountryRegion, type, 0, "enum"
HKR, NDI\params\CountryRegion, default, 0, "0"
HKR, NDI\params\CountryRegion\enum, 0, 0, "FCC (Channel 1 - 11)"
HKR, NDI\params\CountryRegion\enum, 1, 0, "IC (Channel 1 - 11)"
HKR, NDI\params\CountryRegion\enum, 2, 0, "ETSI (Channel 1 - 13)"
HKR, NDI\params\CountryRegion\enum, 3, 0, "Spain (Channel 10 - 11)"
HKR, NDI\params\CountryRegion\enum, 4, 0, "France (Channel 10 - 13)"
HKR, NDI\params\CountryRegion\enum, 5, 0, "MKK (Channel 14)"
HKR, NDI\params\CountryRegion\enum, 6, 0, "MKK1 (Channel 1 - 14)"
HKR, NDI\params\CountryRegion\enum, 7, 0, "Israel (Channel 3 - 9)"
HKR, , WirelessMode, 0, "0"
HKR, , TXBurst, 0, "0"
HKR, , ShortSlot, 0, "0"
HKR, , TurboRate, 0, "0"
HKR, , AdhocOfdm, 0, "0"
HKR, , BGProtection, 0, "0"
HKR, , CCX2Control, 0x00010001, 0x00fa4600
HKR, , VendorDesc, 0, %VENDOR_DESC_DEF_STR%
HKR, Default, VendorDesc, 0, %VENDOR_DESC_DEF_STR%
HKR, , SSID, 0, %SSID_DEF_STR%
HKR, Default, SSID, 0, %SSID_DEF_STR%
HKR, NDI\params\SSID, ParamDesc, 0, "SSID"
HKR, NDI\params\SSID, type, 0, "edit"
HKR, NDI\params\SSID, limitText, 0, "32"
HKR, NDI\params\SSID, default, 0, %SSID_DEF_STR%
HKR, , NetworkType, 0, %NETWORK_TYPE_DEF_STR%
HKR, Default, NetworkType, 0, %NETWORK_TYPE_DEF_STR%
HKR, NDI\params\NetworkType, ParamDesc, 0, "Network Type"
HKR, NDI\params\NetworkType, type, 0, "enum"
HKR, NDI\params\NetworkType, default, 0, %NETWORK_TYPE_DEF_STR%
HKR, NDI\params\NetworkType\enum, 0, 0, "802.11 Ad Hoc"
HKR, NDI\params\NetworkType\enum, 1, 0, "Infrastructure"
HKR, , Channel, 0, %CHANNEL%
HKR, Default, Channel, 0, %CHANNEL%
HKR, , NetworkAddress, 0, ""
HKR, Default, NetworkAddress, 0, ""
HKR, NDI\params\NetworkAddress, ParamDesc, 0, "Local Administration MAC Network Address"
HKR, NDI\params\NetworkAddress, type, 0, "edit"
HKR, NDI\params\NetworkAddress, limitText, 0, "12"
HKR, NDI\params\NetworkAddress, default, 0, ""
HKR, , PSMode, 0, "0"
HKR, Default, PSMode, 0, "0"
HKR, NDI\params\PSMode, ParamDesc, 0, "Power Saving Mode"
HKR, NDI\params\PSMode, type, 0, "enum"
HKR, NDI\params\PSMode, default, 0, "0"
HKR, NDI\params\PSMode\enum, 0, 0, "CAM (Constantly Awake Mode)"
HKR, NDI\params\PSMode\enum, 1, 0, "Max_PSP (Max Power Savings)"
HKR, NDI\params\PSMode\enum, 2, 0, "Fast_PSP (Power Save Mode)"
HKR, , ACPowerCam, 0, "0"
HKR, Default, ACPowerCam, 0, "0"
HKR, NDI\params\ACPowerCam, ParamDesc, 0, "CAM when AC Power"
HKR, NDI\params\ACPowerCam, type, 0, "enum"
HKR, NDI\params\ACPowerCam, default, 0, "0"
HKR, NDI\params\ACPowerCam\enum, 0, 0, "Disable"
HKR, NDI\params\ACPowerCam\enum, 1, 0, "Enable"
HKR, , PreambleType, 0, "0"
HKR, Default, PreambleType, 0, "0"
HKR, , TXPower, 0, "0"
HKR, Default, TXPower, 0, "0"
HKR, , RTSThresh, 0, "2347"
HKR, Default, RTSThresh, 0, "2347"
HKR, NDI\params\RTSThresh, ParamDesc, 0, "RTS Threshold"
HKR, NDI\params\RTSThresh, type, 0, "int"
HKR, Ndi\params\RTSThresh, default, 0, "2347"
HKR, NDI\params\RTSThresh, min, 0, "0"
HKR, NDI\params\RTSThresh, max, 0, "2347"
HKR, NDI\params\RTSThresh, step, 0, "32"
HKR, NDI\params\RTSThresh, optional, 0, "0"
HKR, , FragThresh, 0, "2346"
HKR, Default, FragThresh, 0, "2346"
HKR, NDI\params\FragThresh, ParamDesc, 0, "Fragment Threshold"
HKR, NDI\params\FragThresh, type, 0, "int"
HKR, Ndi\params\FragThresh, default, 0, "2346"
HKR, NDI\params\FragThresh, min, 0, "256"
HKR, NDI\params\FragThresh, max, 0, "2346"
HKR, NDI\params\FragThresh, step, 0, "32"
HKR, NDI\params\FragThresh, optional, 0, "0"
HKR, , AuthenType, 0, "0" ; Open System
HKR, Default, AuthenType, 0, "0"
HKR, , Encryption, 0, "1" ; Disable
HKR, Default, Encryption, 0, "1"
HKR, , WEPKeyLen, 0, "0"
HKR, Default, WEPKeyLen, 0, "0"
HKR, , WEPKeyUse, 0,"1"
HKR, Default, WEPKeyUse, 0,"1"
HKR, , WEPKey1, 0,""
HKR, Default, WEPKey1, 0,""
HKR, , WEPKey2, 0,""
HKR, Default, WEPKey2, 0,""
HKR, , WEPKey3, 0,""
HKR, Default, WEPKey3, 0,""
HKR, , WEPKey4, 0,""
HKR, Default, WEPKey4, 0,""
HKR, , WPAPSK, 0, ""
HKR, Default, WPAPSK, 0, ""
HKR, , Use8021X, 0, "0"
HKR, Default, Use8021X, 0, "0"
HKR, , AuthenProtocol, 0, "0"
HKR, Default, AuthenProtocol, 0, "0"
HKR, , TunnelProtocol, 0, "3"
HKR, Default, TunnelProtocol, 0, "3"
HKR, , ID, 0, ""
HKR, Default, ID, 0, ""
HKR, , Password, 0, ""
HKR, Default, Password, 0, ""
HKR, , TunnelID, 0, ""
HKR, Default, TunnelID, 0, ""
HKR, , TunnelPassword, 0, ""
HKR, Default, TunnelPassword, 0, ""
HKR, , SessionResumption, 0, "0"
HKR, Default, SessionResumption, 0, "0"
HKR, , PasswordMode, 0, "1"
HKR, Default, PasswordMode, 0, "1"
HKR, , UseClientCert, 0, "0"
HKR, Default, UseClientCert, 0, "0"
HKR, , UseServerCert, 0, "0"
HKR, Default, UseServerCert, 0, "0"
HKR, , ClientCertLen, 0, "0"
HKR, Default, ClientCertLen, 0, "0"
HKR, , ClientCertData, 0, ""
HKR, Default, ClientCertData, 0, ""
HKR, , ServerCertLen, 0, "0"
HKR, Default, ServerCertLen, 0, "0"
HKR, , ServerCertData, 0, ""
HKR, Default, ServerCertData, 0, ""
HKR, , ServerName, 0, ""
HKR, Default, ServerName, 0, ""
HKR, , NameRule, 0, "0"
HKR, Default, NameRule, 0, "0"
HKR, , IntermediateCert, 0, "0"
HKR, Default, IntermediateCert, 0, "0"
HKR, , LeapEnabled, 0, "0"
HKR, Default, LeapEnabled, 0, "0"
HKR, , LeapUserName, 0, ""
HKR, Default, LeapUserName, 0, ""
HKR, , LeapPassword, 0, ""
HKR, Default, LeapPassword, 0, ""
HKR, , RekeyInterval, 0, "60"
HKR, , RekeyMethod, 0, "0"
[PCI0201.ndi.reg]
HKR, Ndi, DeviceID, 0, "PCI\VEN_1814&DEV_0201"
[RT25009X.ndi.reg]
HKR, , NTMPDriver, 0, RT25009x.sys
HKR, , BusType, 0, 5
HKR, NDI, CardType, 0, "PCI"
HKR, , RunningWin9X, 0, "1"
HKR, , DevLoader, 0, "*ndis"
HKR, , DeviceVxDs, 0, "RT25009x.sys"
HKR, , EnumPropPages, 0, "netdi.dll,EnumPropPages"
HKR, Ndi\Interfaces, DefUpper, 0, "ndis3"
HKR, Ndi\Interfaces, DefLower, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis3"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, NDIS, LogDriverName, 0, "RT25009X"
HKR, NDIS, MajorNdisVersion, 1, 03
HKR, NDIS, MinorNdisVersion, 1, 0A
[RT61.reg]
HKR, Ndi, Service, 0, "rt61x86"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "wlan,ethernet"
HKR, Ndi\params\*ReceiveBuffers, ParamDesc, 0, "ReceiveBuffers"
HKR, Ndi\params\*ReceiveBuffers, default, 0, "64"
HKR, Ndi\params\*ReceiveBuffers, min, 0, "1"
HKR, Ndi\params\*ReceiveBuffers, max, 0, "00000128"
HKR, Ndi\params\*ReceiveBuffers, step, 0, "1"
HKR, Ndi\params\*ReceiveBuffers, Base, 0, "10"
HKR, Ndi\params\*ReceiveBuffers, type, 0, "int"
HKR, Ndi\params\*TransmitBuffers, ParamDesc, 0, "TransmitBuffers"
HKR, Ndi\params\*TransmitBuffers, default, 0, "64"
HKR, Ndi\params\*TransmitBuffers, min, 0, "1"
HKR, Ndi\params\*TransmitBuffers, max, 0, "00000064"
HKR, Ndi\params\*TransmitBuffers, step, 0, "1"
HKR, Ndi\params\*TransmitBuffers, Base, 0, "10"
HKR, Ndi\params\*TransmitBuffers, type, 0, "int"
HKR, , WirelessMode, 0, "3"
HKR, , Channel, 0, %CHANNEL%
HKR, Default, Channel, 0, %CHANNEL%
HKR, , CountryRegion, 0, "0"
HKR, NDI\params\CountryRegion, ParamDesc, 0, "Country Region 11G"
HKR, NDI\params\CountryRegion, type, 0, "enum"
HKR, NDI\params\CountryRegion, default, 0, "0"
HKR, NDI\params\CountryRegion\enum, 0, 0, "(Channel 1 - 11)"
HKR, NDI\params\CountryRegion\enum, 1, 0, "(Channel 1 - 13)"
HKR, NDI\params\CountryRegion\enum, 2, 0, "(Channel 10 - 11)"
HKR, NDI\params\CountryRegion\enum, 3, 0, "(Channel 10 - 13)"
HKR, NDI\params\CountryRegion\enum, 4, 0, "(Channel 14)"
HKR, NDI\params\CountryRegion\enum, 5, 0, "(Channel 1 - 14)"
HKR, NDI\params\CountryRegion\enum, 6, 0, "(Channel 3 - 9)"
HKR, NDI\params\CountryRegion\enum, 7, 0, "(Channel 5 - 13)"
HKR, , CountryRegionABand, 0, "0"
HKR, NDI\params\CountryRegionABand, ParamDesc, 0, "Country Region 11A"
HKR, NDI\params\CountryRegionABand, type, 0, "enum"
HKR, NDI\params\CountryRegionABand, default, 0, "0"
HKR, NDI\params\CountryRegionABand\enum,0, 0, "Ch(36 - 64,149 - 165)"
HKR, NDI\params\CountryRegionABand\enum,1, 0, "Ch(36 - 140)"
HKR, NDI\params\CountryRegionABand\enum,2, 0, "Ch(36 - 64)"
HKR, NDI\params\CountryRegionABand\enum,3, 0, "Ch(52 - 64,149 - 161)"
HKR, NDI\params\CountryRegionABand\enum,4, 0, "Ch(149 - 165)"
HKR, NDI\params\CountryRegionABand\enum,5, 0, "Ch(149 - 161)"
HKR, NDI\params\CountryRegionABand\enum,6, 0, "Ch(36 - 48)"
HKR, NDI\params\CountryRegionABand\enum,7, 0, "Ch(36 - 165)"
HKR, NDI\params\CountryRegionABand\enum,8, 0, "Ch(52 - 64)"
HKR, NDI\params\CountryRegionABand\enum,9, 0, "Ch(34 - 46)"
HKR, NDI\params\CountryRegionABand\enum,10, 0, "Ch(34 - 64)"
[DestinationDirs]
NT.CopyFiles=12 ; system32\drivers subdirectory on NT
DefaultDestDir=11
NT1.CopyFiles=12 ; system32\drivers subdirectory on NT
XP1.CopyFiles=12 ; system32\drivers subdirectory on Windows XP
win9x1.CopyFiles=11 ; system32 subdirectory on win9x
[NT.CopyFiles]
netr61.sys,,,2
[NT1.CopyFiles]
RT2500.sys ; NT Installation
[XP1.CopyFiles]
RT2500.sys ; XP Installation
[win9x1.CopyFiles]
RT25009x.sys ; Win9x Installation
[SourceDisksNames]
1=%INSTALL_DISK_STR%,,,
[SourceDisksFiles]
netr61.sys=1,,
RT2500.sys=1
RT25009x.sys=1
[RT2500.ndi.NT.reg]
HKR, Ndi, Service, 0, "RT2500"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
[RALINK.Service]
DisplayName=%RALINK.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_AUTO_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\netr61.sys
LoadOrderGroup=NDIS
[RALINK1.Service]
DisplayName=%RALINK1.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_AUTO_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\RT2500.sys
LoadOrderGroup=NDIS
[common.EventLog]
AddReg=common.AddEventLog.reg
[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported, 0x00010001, 7
[common1.EventLog]
AddReg=common1.AddEventLog.reg
[common1.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported, 0x00010001, 7
[Strings]
Hercules="Hercules"
Hercules.DeviceDesc1="Hercules Wireless G PCMCIA"
Hercules.DeviceDesc2="Hercules Wireless G PCI"
Hercules.DeviceDesc3="Hercules Wireless G PCMCIA"
Hercules.DeviceDesc4="Hercules Wireless G PCI"
Hercules.DeviceDesc5="Hercules Wireless G PCMCIA"
Hercules.DeviceDesc6="Hercules Wireless G PCI"
INSTALL_DISK_STR="Hercules WiFi Station Installation Disk"
RALINK.Service.DispName="802.11g Wireless Driver RT61"
CHANNEL="1"

