
[Version]
CatalogFile=netwg311.cat
Signature="$Windows NT$"
Provider=%TI%
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
DriverVer=06/17/2004,6.0.5.30
[Manufacturer]
%TI%=TexasInstruments,NT.5.1
[ControlFlags]
ExcludeFromSelect=PCI\VEN_104C&DEV_9066&SUBSYS_4C001385
[TexasInstruments.NT.5.1]
%TIACX.DeviceDesc%=TIACXXP, PCI\VEN_104C&DEV_9066&SUBSYS_4C001385 ; B & G
[TexasInstruments]
%TIACX.DeviceDesc%=TIACX, PCI\VEN_104C&DEV_9066&SUBSYS_4C001385 ; B & G
[TIACXXP]
BusType=5
AddReg =TIACXXP.ndi.reg.NT, TI.Param.Reg, BG.Param.Reg
Characteristics=0x84
;CpyFiles =TIACXXP.CopyFiles
[TIACXXP.ndi.reg.NT]
HKR, Ndi, Service, 0, "netwg311"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
[TIACXXP.Services]
AddService=netwg311, 2, TIACXLNXP.Service, TIACXLNXP.EventLog
[TIACXXP.CopyFiles]
netwg311.sys, netwg311_XP.sys
[TIACXAGXP]
BusType=5
AddReg =TIACXAGXP.ndi.reg.NT, TI.Param.Reg, AG.Param.Reg
Characteristics=0x84
;CpyFiles =TIACXAGXP.CopyFiles
[TIACXAGXP.ndi.reg.NT]
HKR, Ndi, Service, 0, "netwg311"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
[TIACXAGXP.Services]
AddService=netwg311, 2, TIACXLNXP.Service, TIACXLNXP.EventLog
[TIACXAGXP.CopyFiles]
netwg311.sys, netwg311_XP.sys
[TIACXLNXP.Service]
DisplayName=%TIACXLN.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_DEMAND_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\netwg311.sys
LoadOrderGroup=NDIS
[TIACXLNXP.EventLog]
AddReg=TIACXLNXP.AddEventLog.reg
[TIACXLNXP.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported, 0x00010001, 7
[WXP.Param.Reg]
HKR, ,PrivacyMode,, "0"
HKR, ,utlPrivacyMode,, "0"
HKR, ,utlAuthenticationMode,, "0"
[TIACX.NT]
BusType=5
AddReg =TIACX.ndi.reg.NT, TI.Param.Reg, BG.Param.Reg
Characteristics=0x84
;CpyFiles =TIACX.CopyFiles.NT, TIACX.BinFiles.NT
[TIACX.ndi.reg.NT]
HKR, Ndi, Service, 0, "netwg311"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
[TIACX.NT.Services]
AddService=netwg311, 2, TIACXLN.Service, TIACXLN.EventLog
[TIACX.CopyFiles.NT]
netwg311.sys, netwg311_2K.sys
[TIACX.BinFiles.NT]
[TIACXAG.NT]
BusType=5
AddReg =TIACXAG.ndi.reg.NT, TI.Param.Reg, AG.Param.Reg
Characteristics=0x84
;CpyFiles =TIACXAG.CopyFiles.NT, TIACXAG.BinFiles.NT
[TIACXAG.ndi.reg.NT]
HKR, Ndi, Service, 0, "netwg311"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
[TIACXAG.NT.Services]
AddService=netwg311, 2, TIACXLN.Service, TIACXLN.EventLog
[TIACXAG.CopyFiles.NT]
netwg311.sys, netwg311_2K.sys
[TIACXAG.BinFiles.NT]
[TIACXLN.Service]
DisplayName=%TIACXLN.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_DEMAND_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\netwg311.sys
LoadOrderGroup=NDIS
[TIACXLN.EventLog]
AddReg=TIACXLN.AddEventLog.reg
[TIACXLN.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported, 0x00010001, 7
[W2K.Param.Reg]
HKR, ,PrivacyMode,, "0"
HKR, ,utlPrivacyMode,, "0"
HKR, ,utlAuthenticationMode,, "0"
[BG.Param.Reg]
HKR, ,dot11SupportedRateMask,, "8"
HKR, ,dot11BasicRateMask,, "1"
HKR, ,dot11DesiredChannel, ,1
[AG.Param.Reg]
HKR, ,dot11SupportedRateMask,, "8"
HKR, ,dot11BasicRateMask,, "0"
HKR, ,dot11DesiredChannel, ,11
[TI.Param.Reg]
HKR, ,DisableSsidPending,, "1"
HKR,NDI\params\dot11DesiredBSSType,ParamDesc,,"Network Type"
HKR,NDI\params\dot11DesiredBSSType,type,,"enum"
HKR,NDI\params\dot11DesiredBSSType,default,,"1"
HKR,NDI\params\dot11DesiredBSSType\enum,"0",,"802.11 Ad-hoc"
HKR,NDI\params\dot11DesiredBSSType\enum,"1",,"Infrastructure"
HKR, Ndi\Params\dot11DesiredSSID, ParamDesc, ,"SSID"
HKR, Ndi\Params\dot11DesiredSSID, Type, ,"edit"
HKR, Ndi\Params\dot11DesiredSSID, LimitText, ,"32"
HKR, Ndi\Params\dot11DesiredSSID, Default,,""
HKR, Ndi\Params\dot11DesiredSSID, UpperCase,,"0"
HKR,NDI\params\dot11DesiredTxRate,ParamDesc,, "Desired Tx Rate"
HKR,NDI\params\dot11DesiredTxRate,type,,"enum"
HKR,NDI\params\dot11DesiredTxRate,default,,"0"
HKR,NDI\params\dot11DesiredTxRate\enum,"0",,"Auto"
HKR,NDI\params\dot11DesiredTxRate\enum,"1",,"1 Mbps"
HKR,NDI\params\dot11DesiredTxRate\enum,"2",,"2 Mbps"
HKR,NDI\params\dot11DesiredTxRate\enum,"3",,"5.5 Mbps"
HKR,NDI\params\dot11DesiredTxRate\enum,"4",,"6 Mbps"
HKR,NDI\params\dot11DesiredTxRate\enum,"5",,"9 Mbps"
HKR,NDI\params\dot11DesiredTxRate\enum,"6",,"11 Mbps"
HKR,NDI\params\dot11DesiredTxRate\enum,"7",,"12 Mbps"
HKR,NDI\params\dot11DesiredTxRate\enum,"8",,"18 Mbps"
HKR,NDI\params\dot11DesiredTxRate\enum,"9",,"22 Mbps"
HKR,NDI\params\dot11DesiredTxRate\enum,"10",,"24 Mbps"
HKR,NDI\params\dot11DesiredTxRate\enum,"11",,"36 Mbps"
HKR,NDI\params\dot11DesiredTxRate\enum,"12",,"48 Mbps"
HKR,NDI\params\dot11DesiredTxRate\enum,"13",,"54 Mbps"
HKR, ,Mode4x,, "0"
HKR, ,dot11DesiredBSSType,, "1"
HKR, ,dot11BasicRateMask,, "1"
HKR, ,dot11SupportedRateMask,, "8"
HKR, ,dot11AuthenticationMode,, "2"
HKR, ,FBLongInterval,, "100"
HKR, ,FBShortInterval,, "2000"
HKR, ,PrivacyMode,, "2"
HKR, ,WiFiAdhoc,, "1"
[DestinationDirs]
DefaultDestDir=12 ; Windows\System32\Drivers
TIACXXP.CopyFiles=12 ; Winnt\System32\Drivers Directory ; WinXP
TIACXAGXP.CopyFiles=12 ; Winnt\System32\Drivers Directory ; WinXP
TIACX.CopyFiles=11 ; Windows\System or Winnt\System32 Directory ; Win98/ME
TIACX.BinFiles.NT=10,system
TIACXAG.CopyFiles=11 ; Windows\System or Winnt\System32 Directory ; Win98/ME
TIACXAG.BinFiles.NT=10,system
[SourceDisksNames]
1=%DiskName%,,
[SourceDisksFiles]
netwg311_XP.sys=1
netwg311_2K.sys=1
[Strings]
TI="NETGEAR, Inc."
TIACX.DeviceDesc="NETGEAR WG311v2 802.11g Wireless PCI Adapter"
TIACXLN.Service.DispName="NETGEAR WG311v2 802.11g Wireless PCI Adapter"
WLANAdapterHelpText= "A WLAN Adapter provides high speed connection to the Internet through 802.11g technology"
DiskName="NETGEAR WG311v2 802.11g Wireless PCI Adapter Installation Disk"
