
[Version]
Signature="$Chicago$"
Compatible=1
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%WUSB11_VENDOR%
CatalogFile.NT=netrfm2k.cat
DriverVer=03/26/2004,4.10.9.430
[ControlFlags]
ExcludeFromSelect=USB\VID_066B&PID_2211
ExcludeFromSelect=USB\VID_066B&PID_2212
ExcludeFromSelect=USB\VID_066B&PID_2219
ExcludeFromSelect=USB\VID_077B&PID_2219
ExcludeFromSelect=USB\VID_09aa&PID_3642
ExcludeFromSelect=USB\VID_1915&PID_2233
[Manufacturer]
%WUSB11_VENDOR_NAME%=DeviceList, NT.5.1
[DeviceList]
%WUSB11_20.DeviceDesc%=USBFVNETA.Ndi, USB\VID_066B&PID_2211
%WUSB11_25.DeviceDesc%=PRISM_USB1, USB\VID_066B&PID_2212
%WUSB11_26A.DeviceDesc%=USBNET.Ndi, USB\VID_066B&PID_2219
%WUSB11_26.DeviceDesc%=USBNET.Ndi, USB\VID_077B&PID_2219
%WUSB11_25.DeviceDesc%=PRISM_USB1, USB\VID_09aa&PID_3642
%WUSB11_28.DeviceDesc%=USBNET28.Ndi, USB\VID_1915&PID_2233
[DeviceList.NT.5.1]
%WUSB11_28.DeviceDesc%=USBNETXP28.Ndi, USB\VID_1915&PID_2233
%WUSB11_26A.DeviceDesc%=USBNETXP26.Ndi, USB\VID_066B&PID_2219
%WUSB11_26.DeviceDesc%=USBNETXP26.Ndi, USB\VID_077B&PID_2219
%WUSB11_25.DeviceDesc%=PRISM_USB1.NT, USB\VID_09aa&PID_3642
%WUSB11_25.DeviceDesc%=PRISM_USB1.NT, USB\VID_066B&PID_2212
%WUSB11_20.DeviceDesc%=USBFVNETAXP.Ndi, USB\VID_066B&PID_2211
[USBNET28.Ndi]
AddReg=Win9x.Reg, Win9x2k.Params
;CpyFiles=CopyFile.USBNET28.Sys
DriverVer=12/5/2003,4.10.9.424
[Win9x.Reg]
HKR,Ndi,DeviceID,0,"USB\VID_1915&PID_2233"
HKR,Ndi,CardType,,"PNP"
HKR,,DevLoader,0,"*ndis"
HKR,,DeviceVxDs,0,"vnet58l.sys"
HKR,NDIS,MajorNdisVersion,1,05
HKR,NDIS,MinorNdisVersion,1,00
HKR,NDIS,LogDriverName,,USBNET28
HKR,Ndi\Interfaces,DefUpper,,"ndis3"
HKR,Ndi\Interfaces,DefLower,,"ethernet"
HKR,Ndi\Interfaces,UpperRange,,"ndis3"
HKR,Ndi\Interfaces,LowerRange,,"ethernet"
[CopyFile.USBNET28.Sys]
[USBNET28.Ndi.ME]
Characteristics=0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType=15 ; USB
AddReg=WinMe.Reg, Win9x2k.Params
;CpyFiles=CopyFile.USBNET28.Me.Sys
[DrvInst.ndi.ME.Services]
AddService=FVNETusb, 2, FVNETusbMe.Service, FVNETusb.EventLog
[WinMe.Reg]
HKR,Ndi,Service,0,FVNETusb
HKR,,DevLoader,0,*ndis
HKR,,DeviceVxDs,0,vnet58l.sys
HKR,,EnumPropPages,0,"netdi.dll,EnumPropPages"
HKR,NDIS,MajorNdisVersion,1,05
HKR,NDIS,MinorNdisVersion,1,00
HKR,NDIS,LogDriverName,,USBNET28
HKR,Ndi\Interfaces,DefUpper,0,"ndis5"
HKR,Ndi\Interfaces,DefLower,0,"ethernet"
HKR,Ndi\Interfaces,UpperRange,0,"ndis5"
HKR,Ndi\Interfaces,LowerRange,0,"ethernet"
HKR, Ndi\Install, ndis3, 0, "FVNETusb.ndis5me"
[FVNETusb.ndis5me]
;CpyFiles=CopyFile.USBNET28.Me.Sys
[CopyFile.USBNET28.Me.Sys]
[FVNETusbMe.Service]
DisplayName=%WUSB11_28.DisplayName%
ServiceType=1
StartType=3
ErrorControl=1
ServiceBinary=%11%\vnet58l.sys
LoadOrderGroup=NDIS
[USBNET28.Ndi.NTx86]
Characteristics=0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType=15 ; USB
AddReg=Win2k.Reg, Win9x2k.Params
;CpyFiles=CopyFile.USBNET28.2k.Sys
[USBNET28.Ndi.NTx86.Services]
AddService=FVNETusb, 2, FVNETusb.Service, FVNETusb.EventLog
[Win2k.Reg]
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi, Service, 0, "FVNETusb"
[USBNETXP28.Ndi.NTx86]
Characteristics=0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType=15 ; USB
AddReg=WinXP.Reg, WinXP.Params
;CpyFiles=CopyFile.USBNET28.XP.Sys
[USBNETXP28.Ndi.NTx86.Services]
AddService=FVNETusb, 2, FVNETusb.Service, FVNETusb.EventLog
[WinXP.Reg]
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi, Service, 0, "FVNETusb"
[FVNETusb.Service]
DisplayName=%WUSB11_28.DisplayName%
ServiceType=1
StartType=3
ErrorControl=1
ServiceBinary=%12%\vnet58lx.sys
LoadOrderGroup=NDIS
[FVNETusb.EventLog]
AddReg=FVNETusb.AddEventLog.Reg
[FVNETusb.AddEventLog.Reg]
HKR, , EventMessageFile, 0x00020000, %%SystemRoot%%\System32\netevent.dll
HKR, , TypesSupported , 0x00010001, 7
[USBFVNETA.Ndi]
AddReg=USBFVNETA.Reg, USBFVNETA.Params
;CpyFiles=CopyFile.USB20.Sys
[USBFVNETA.Ndi.NT]
Characteristics=0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType=15 ; USB
AddReg=USBFVNETA.NT.Reg, USBFVNETA.Params
;CpyFiles=CopyFile.USB20NT.Sys
[USBFVNETA.Ndi.NT.Services]
AddService=USBFVNETA, 2, USBFVNETA.Service, Common.EventLog
[USBFVNETAXP.Ndi]
Characteristics=0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType=15 ; USB
AddReg=USBFVNETA.NT.Reg, USBFVNETA.Params
;CpyFiles=CopyFile.USB20XP.Sys
[USBFVNETAXP.Ndi.Services]
AddService=USBFVNETAXP, 2, USBFVNETAXP.Service, Common.EventLog
[USBFVNETA.Reg]
HKR,Ndi,DeviceID,,USB\VID_077B&PID_2211
HKR,Ndi,CardType,,"PNP"
HKR,,DevLoader,0,"*ndis"
HKR,,DeviceVxDs,0,"vnetusba.sys"
HKR,NDIS,MajorNdisVersion,1,05
HKR,NDIS,MinorNdisVersion,1,00
HKR,NDIS,LogDriverName,,VNETUSBA
HKR,Ndi\Interfaces,DefUpper,,"ndis3"
HKR,Ndi\Interfaces,DefLower,,"ethernet"
HKR,Ndi\Interfaces,UpperRange,,"ndis3"
HKR,Ndi\Interfaces,LowerRange,,"ethernet"
[USBFVNETA.NT.Reg]
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi, Service, 0, "USBFVNETA"
[USBFVNETA.Service]
DisplayName=%WUSB11_20.DisplayName%
ServiceType=1
StartType=3
ErrorControl=1
ServiceBinary=%12%\vnetusba.sys
LoadOrderGroup=NDIS
[USBFVNETAXP.Service]
DisplayName=%WUSB11_20XP.DisplayName%
ServiceType=1
StartType=3
ErrorControl=1
ServiceBinary=%12%\vnetusbxp.sys
LoadOrderGroup=NDIS
[USBFVNETA.Params]
HKR, Ndi\params\PreambleType, ParamDesc, 0, "Preamble Type"
HKR, Ndi\params\PreambleType, default, 0, "0"
HKR, Ndi\params\PreambleType, type, 0, "enum"
HKR, Ndi\params\PreambleType\enum, 0, 0, "Long"
HKR, Ndi\params\PreambleType\enum, 1, 0, "Short"
HKR, Ndi\params\PreambleType\enum, 2, 0, "Auto"
HKR, , PreambleType, 0, "2"
HKR, Ndi\params\Channel, ParamDesc, 0, "Channel"
HKR, Ndi\params\Channel, default, 0, "3"
HKR, Ndi\params\Channel, type, 0, "int"
HKR, Ndi\params\Channel, min, 0, "1"
HKR, Ndi\params\Channel, max, 0, "14"
HKR, Ndi\params\Channel, step, 0, "1"
HKR, , Channel, 0, "3"
HKR, Ndi\params\Rate, ParamDesc, 0, "Rate (Mbps)"
HKR, Ndi\params\Rate, default, 0, "4"
HKR, Ndi\params\Rate, type, 0, "enum"
HKR, Ndi\params\Rate\enum, 0, 0, "1"
HKR, Ndi\params\Rate\enum, 1, 0, "2"
HKR, Ndi\params\Rate\enum, 2, 0, "5.5"
HKR, Ndi\params\Rate\enum, 3, 0, "11"
HKR, Ndi\params\Rate\enum, 4, 0, "Auto"
HKR, , Rate, 0, "4"
HKR, Ndi\params\RTS_Threshold, ParamDesc, 0, "RTS Threshold"
HKR, Ndi\params\RTS_Threshold, default, 0, "2347"
HKR, Ndi\params\RTS_Threshold, type, 0, "int"
HKR, Ndi\params\RTS_Threshold, min, 0, "0"
HKR, Ndi\params\RTS_Threshold, max, 0, "2347"
HKR, Ndi\params\RTS_Threshold, step, 0, "1"
HKR, , RTS_Threshold, 0, "2347"
HKR, Ndi\params\Frag_Threshold, ParamDesc, 0, "Fragmentation Threshold"
HKR, Ndi\params\Frag_Threshold, default, 0, "2346"
HKR, Ndi\params\Frag_Threshold, type, 0, "int"
HKR, Ndi\params\Frag_Threshold, min, 0, "256"
HKR, Ndi\params\Frag_Threshold, max, 0, "2346"
HKR, Ndi\params\Frag_Threshold, step, 0, "1"
HKR, , Frag_Threshold, 0, "2346"
HKR, Ndi\params\Operating_Mode, ParamDesc, 0, "Operating Mode"
HKR, Ndi\params\Operating_Mode, default, 0, "1"
HKR, Ndi\params\Operating_Mode, type, 0, "enum"
HKR, Ndi\params\Operating_Mode\enum, 0, 0, "Ad-Hoc"
HKR, Ndi\params\Operating_Mode\enum, 1, 0, "Infrastructure"
HKR, , Operating_Mode, 0, "1"
HKR, Ndi\params\ESSID, ParamDesc, 0, "ESSID"
HKR, Ndi\params\ESSID, default, 0, "ANY"
HKR, Ndi\params\ESSID, type, 0, "edit"
HKR, Ndi\params\ESSID, LimitText, 0, "32"
HKR, Ndi\params\ESSID, UpperCase, 0, "0"
HKR, , ESSID, 0, "ANY"
HKR, Ndi\params\AuthenticationType, ParamDesc, 0, "Authentication Type"
HKR, Ndi\params\AuthenticationType, default, 0, "0"
HKR, Ndi\params\AuthenticationType, type, 0, "enum"
HKR, Ndi\params\AuthenticationType\enum,0, 0, "Open System"
HKR, Ndi\params\AuthenticationType\enum,1, 0, "Shared Key"
HKR, Ndi\params\AuthenticationType\enum,2, 0, "Auto"
HKR, , AuthenticationType, 0, "0"
HKR, Ndi\params\WEP_Mode, ParamDesc, 0, "WEP Mode"
HKR, Ndi\params\WEP_Mode, default, 0, "0"
HKR, Ndi\params\WEP_Mode, type, 0, "enum"
HKR, Ndi\params\WEP_Mode\enum, 0, 0, "Mandatory"
HKR, Ndi\params\WEP_Mode\enum, 1, 0, "Optional"
HKR, , WEP_Mode, 0, "0"
HKR,Ndi\params\EncryptionLevel, ParamDesc, 0, "Encryption Level"
HKR,Ndi\params\EncryptionLevel, type, 0, "enum"
HKR,Ndi\params\EncryptionLevel, default, 0, "0"
HKR,Ndi\params\EncryptionLevel\enum, 0, 0, "None"
HKR,Ndi\params\EncryptionLevel\enum, 1, 0, "64-bit encryption"
HKR,Ndi\params\EncryptionLevel\enum, 2, 0, "128-bit encryption"
HKR,, EncryptionLevel, 0, "0"
HKR,Ndi\params\WEP_KEY_INDEX, ParamDesc, 0, "WEP Key to use"
HKR,Ndi\params\WEP_KEY_INDEX, type, 0, "enum"
HKR,Ndi\params\WEP_KEY_INDEX, default, 0, "0"
HKR,Ndi\params\WEP_KEY_INDEX\enum, 0, 0, "1"
HKR,Ndi\params\WEP_KEY_INDEX\enum, 1, 0, "2"
HKR,Ndi\params\WEP_KEY_INDEX\enum, 2, 0, "3"
HKR,Ndi\params\WEP_KEY_INDEX\enum, 3, 0, "4"
HKR,, WEP_KEY_INDEX, 0, "0"
HKR,Ndi\params\WEP_KEY_1, ParamDesc, 0, "WEP KEY #1"
HKR,Ndi\params\WEP_KEY_1, default, 0, "00000000000000000000000000"
HKR,Ndi\params\WEP_KEY_1, type, 0, "edit"
HKR,Ndi\params\WEP_KEY_1, LimitText, 0, "26"
HKR,Ndi\params\WEP_KEY_1, UpperCase, 0, "1"
HKR,, WEP_KEY_1, 0, "00000000000000000000000000"
HKR,Ndi\params\WEP_KEY_2, ParamDesc, 0, "WEP KEY #2"
HKR,Ndi\params\WEP_KEY_2, default, 0, "00000000000000000000000000"
HKR,Ndi\params\WEP_KEY_2, type, 0, "edit"
HKR,Ndi\params\WEP_KEY_2, LimitText, 0, "26"
HKR,Ndi\params\WEP_KEY_2, UpperCase, 0, "1"
HKR,, WEP_KEY_2, 0, "00000000000000000000000000"
HKR,Ndi\params\WEP_KEY_3, ParamDesc, 0, "WEP KEY #3"
HKR,Ndi\params\WEP_KEY_3, default, 0, "00000000000000000000000000"
HKR,Ndi\params\WEP_KEY_3, type, 0, "edit"
HKR,Ndi\params\WEP_KEY_3, LimitText, 0, "26"
HKR,Ndi\params\WEP_KEY_3, UpperCase, 0, "1"
HKR,, WEP_KEY_3, 0, "00000000000000000000000000"
HKR,Ndi\params\WEP_KEY_4, ParamDesc, 0, "WEP KEY #4"
HKR,Ndi\params\WEP_KEY_4, default, 0, "00000000000000000000000000"
HKR,Ndi\params\WEP_KEY_4, type, 0, "edit"
HKR,Ndi\params\WEP_KEY_4, LimitText, 0, "26"
HKR,Ndi\params\WEP_KEY_4, UpperCase, 0, "1"
HKR,, WEP_KEY_4, 0, "00000000000000000000000000"
[PRISM_USB1] ; Win9x
AddReg=PRISM_USB1.reg, COMMON_USB.reg, COMMON_NDIS.reg, COMMON.reg
;CpyFiles=CopyFile.USB25.sys
[PRISM_USB1.NT] ; Win2k
AddReg=PRISM_USB1.reg, COMMON_USB.reg.NT, COMMON_NDIS.reg.NT, COMMON.reg
;CpyFiles=CopyFile.USB25NT.sys
BusType=15 ; USB
Characteristics= 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[PRISM_USB1.NT.Services]
AddService=PRISM_USB, 2, PRISM_USB_DRIVER.Service, PRISM_DRIVER.EventLog
[PRISM_USB1.reg]
HKR,Ndi ,DeviceID,0,"USB\VID_066B&PID_2212"
[USBNET.Ndi]
AddReg=USBNET.Reg, Win9x2k.Params
;CpyFiles=CopyFile.USB26.Sys
[USBNET.Ndi.NT]
Characteristics=0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType=15 ; USB
AddReg=USBNET.NT.Reg, Win9x2k.Params
;CpyFiles=CopyFile.USB26NT.Sys
[USBNET.Ndi.NT.Services]
AddService=USBNET, 2, USBNET.Service, Common.EventLog
[USBNETXP26.Ndi] ; v2.6 for XP session
Characteristics=0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType=15 ; USB
AddReg=USBNET.NT.Reg, WinXP.Params
;CpyFiles=CopyFile.USB26NT.Sys
[USBNETXP26.Ndi.Services]
AddService=USBNET, 2, USBNET.Service, Common.EventLog
[PRISM_USB_DRIVER.Service]
DisplayName=%WUSB11_25.DisplayName%
ServiceType=1 ; SERVICE_KERNEL_DRIVER
StartType=3 ; SERVICE_DEMAND_START
ErrorControl=1 ; NORMAL
ServiceBinary=%12%\PRISMXP.sys
LoadOrderGroup=NDIS
[PRISM_DRIVER.EventLog]
AddReg=PRISM_DRIVER.EventLog.reg
[PRISM_DRIVER.EventLog.reg]
HKR, ,EventMessageFile ,0x00020000 ,"%%SystemRoot%%\System32\netevent.dll"
HKR, ,TypesSupported ,0x00010001 ,7
[COMMON_USB.reg]
HKR,NDI ,Service ,0 ,"PRISM_USB"
HKR,NDI ,CardType ,0 ,"USB"
HKR, ,BusType ,0 ,"15"
HKR, ,DeviceVxDs ,0 ,"PRISM9x.sys"
[COMMON_USB.reg.NT]
HKR,NDI ,Service ,0 ,"PRISM_USB"
HKR,NDI ,CardType ,0 ,"USB"
HKR, ,BusType ,0 ,"15"
HKR, ,DeviceVxDs ,0 ,"PRISMXP.sys"
[COMMON_NDIS.reg]
HKR, ,RunningWin9X ,0 ,"1"
HKR, ,DevLoader ,0 ,"*ndis"
HKR, ,EnumPropPages ,0 ,"netdi.dll,EnumPropPages"
HKR,NDI\Interfaces ,UpperRange ,0 ,"ndis3"
HKR,NDI\Interfaces ,LowerRange ,0 ,"ethernet"
HKR,NDI\Interfaces ,DefUpper ,0 ,"ndis3"
HKR,NDI\Interfaces ,DefLower ,0 ,"ethernet"
HKR,NDIS ,LogDriverName ,0 ,"PRISM"
HKR,NDIS ,MajorNdisVersion ,1 ,03
HKR,NDIS ,MinorNdisVersion ,1 ,0a
[COMMON_NDIS.reg.NT]
HKR,NDI\Interfaces ,UpperRange ,0 ,"ndis5"
HKR,NDI\Interfaces ,LowerRange ,0 ,"ethernet"
[COMMON.reg]
HKR, ,GTKSIOC ,0 ,"1"
HKR, ,SilentInstall ,0 ,"1"
HKR,defaults,ListenInterval,0,"3"
HKR,NDI\params\ListenInterval,default,0,"3"
HKR,NDI\params\ListenInterval,ParamDesc,,%LISTENINTERVAL_STR%
HKR,NDI\params\ListenInterval,type,,"int"
HKR,ListenInterval,flag,1,30,00,00,00
HKR,NDI\params\ListenInterval,min,0,"0"
HKR,NDI\params\ListenInterval,max,0,"77"
HKR,NDI\params\ListenInterval,step,0,"1"
HKR,NDI\params\ListenInterval,optional,0,"1"
HKR,defaults,RTSThresh,0,"2432"
HKR,NDI\params\RTSThresh,default,0,"2432"
HKR,NDI\params\RTSThresh,ParamDesc,0,%RTSTHRESH_STR%
HKR,NDI\params\RTSThresh,type,0,"int"
HKR,RTSThresh,flag,1,20,00,00,00
HKR,NDI\params\RTSThresh,min,0,"0"
HKR,NDI\params\RTSThresh,max,0,"2432"
HKR,NDI\params\RTSThresh,step,0,"64"
HKR,NDI\params\RTSThresh,optional,0,"1"
HKR,defaults,FragThresh,0,"2432"
HKR,NDI\params\FragThresh,default,0,"2432"
HKR,NDI\params\FragThresh,ParamDesc,0,%FRAGTHRESH_STR%
HKR,NDI\params\FragThresh,type,0,"int"
HKR,FragThresh,flag,1,20,00,00,00
HKR,NDI\params\FragThresh,min,0,"256"
HKR,NDI\params\FragThresh,max,0,"2432"
HKR,NDI\params\FragThresh,step,0,"128"
HKR,NDI\params\FragThresh,optional,0,"1"
HKR,defaults,PreambleMode,0,"1"
HKR,NDI\params\PreambleMode,default,0,"1"
HKR,NDI\params\PreambleMode,ParamDesc,,%SHORT_PREAM_STR%
HKR,NDI\params\PreambleMode,type,,"enum"
HKR,PreambleMode,flag,1,30,00,00,00
HKR,NDI\params\PreambleMode\enum,1,,"Long Tx Preamble"
HKR,NDI\params\PreambleMode\enum,2,,"Short Tx Preamble"
HKR,NDI\params\PreambleMode\enum,3,,"Auto Tx Preamble"
HKR,NDI\params\PreambleMode,optional,0,"1"
HKR,defaults,AuthentAlg,0,"65535"
HKR,NDI\params\AuthentAlg,default,0,"65535"
HKR,NDI\params\AuthentAlg,ParamDesc,,%AUTHENT_TYPE_STR%
HKR,NDI\params\AuthentAlg,type,,"enum"
HKR,AuthentAlg,flag,1,30,00,00,00
HKR,NDI\params\AuthentAlg\enum,1,,"WECA Compliant (always use Open)"
HKR,NDI\params\AuthentAlg\enum,2,,"Must use Shared with WEP"
HKR,NDI\params\AuthentAlg\enum,65535,,"Automatic based on WEP setting"
HKR,NDI\params\AuthentAlg,optional,0,"1"
HKR,defaults,AdhocDemoMode,0,"0"
HKR,Ndi\params\AdhocDemoMode,default,0,"0"
HKR,NDI\params\AdhocDemoMode,ParamDesc,,%ADHOC_DEMO_STR%
HKR,NDI\params\AdhocDemoMode,type,,"enum"
HKR,AdhocDemoMode,flag,1,30,00,00,00
HKR,NDI\params\AdhocDemoMode\enum,0,,"Disable"
HKR,NDI\params\AdhocDemoMode\enum,1,,"Enable"
HKR,NDI\params\AdhocDemoMode,optional,0,"1"
HKR,defaults,PowerSave,0,"0"
HKR,Ndi\params\PowerSave,default,0,"0"
HKR,NDI\params\PowerSave,ParamDesc,,%POWER_SAVE_STR%
HKR,NDI\params\PowerSave,type,,"enum"
HKR,PowerSave,flag,1,30,00,00,00
HKR,NDI\params\PowerSave\enum,0,,"Disable"
HKR,NDI\params\PowerSave\enum,1,,"Always Enable"
HKR,NDI\params\PowerSave\enum,2,,"Auto Enable"
HKR,NDI\params\PowerSave,optional,0,"1"
[USBNET.Reg]
HKR,Ndi,DeviceID,0,"USB\VID_077B&PID_2219"
HKR,Ndi,CardType,,"PNP"
HKR,,DevLoader,0,"*ndis"
HKR,,DeviceVxDs,0,"vnetu9xl.sys"
HKR,NDIS,MajorNdisVersion,1,05
HKR,NDIS,MinorNdisVersion,1,00
HKR,NDIS,LogDriverName,,NETUSB
HKR,Ndi\Interfaces,DefUpper,,"ndis3"
HKR,Ndi\Interfaces,DefLower,,"ethernet"
HKR,Ndi\Interfaces,UpperRange,,"ndis3"
HKR,Ndi\Interfaces,LowerRange,,"ethernet"
[USBNET.NT.Reg]
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi, Service, 0, "USBNET"
[USBNET.Params]
HKR, ,GTKSIOC ,0 ,"1"
HKR, Ndi\params\PreambleType, ParamDesc, 0, "Preamble Type"
HKR, Ndi\params\PreambleType, default, 0, "0"
HKR, Ndi\params\PreambleType, type, 0, "enum"
HKR, Ndi\params\PreambleType\enum, 0, 0, "Long"
HKR, Ndi\params\PreambleType\enum, 1, 0, "Short"
HKR, Ndi\params\PreambleType\enum, 2, 0, "Auto"
HKR, , PreambleType, 0, "2"
HKR, Ndi\params\Channel, ParamDesc, 0, "Channel"
HKR, Ndi\params\Channel, default, 0, "3"
HKR, Ndi\params\Channel, type, 0, "int"
HKR, Ndi\params\Channel, min, 0, "1"
HKR, Ndi\params\Channel, max, 0, "14"
HKR, Ndi\params\Channel, step, 0, "1"
HKR, , Channel, 0, "3"
HKR, Ndi\params\Rate, ParamDesc, 0, "Rate (Mbps)"
HKR, Ndi\params\Rate, default, 0, "4"
HKR, Ndi\params\Rate, type, 0, "enum"
HKR, Ndi\params\Rate\enum, 0, 0, "1"
HKR, Ndi\params\Rate\enum, 1, 0, "2"
HKR, Ndi\params\Rate\enum, 2, 0, "5.5"
HKR, Ndi\params\Rate\enum, 3, 0, "11"
HKR, Ndi\params\Rate\enum, 4, 0, "Auto"
HKR, , Rate, 0, "4"
HKR, Ndi\params\RTS_Threshold, ParamDesc, 0, "RTS Threshold"
HKR, Ndi\params\RTS_Threshold, default, 0, "2347"
HKR, Ndi\params\RTS_Threshold, type, 0, "int"
HKR, Ndi\params\RTS_Threshold, min, 0, "0"
HKR, Ndi\params\RTS_Threshold, max, 0, "2347"
HKR, Ndi\params\RTS_Threshold, step, 0, "1"
HKR, , RTS_Threshold, 0, "2347"
HKR, Ndi\params\Frag_Threshold, ParamDesc, 0, "Fragmentation Threshold"
HKR, Ndi\params\Frag_Threshold, default, 0, "2346"
HKR, Ndi\params\Frag_Threshold, type, 0, "int"
HKR, Ndi\params\Frag_Threshold, min, 0, "256"
HKR, Ndi\params\Frag_Threshold, max, 0, "2346"
HKR, Ndi\params\Frag_Threshold, step, 0, "1"
HKR, , Frag_Threshold, 0, "2346"
HKR, Ndi\params\Operating_Mode, ParamDesc, 0, "Operating Mode"
HKR, Ndi\params\Operating_Mode, default, 0, "1"
HKR, Ndi\params\Operating_Mode, type, 0, "enum"
HKR, Ndi\params\Operating_Mode\enum, 0, 0, "Ad-Hoc"
HKR, Ndi\params\Operating_Mode\enum, 1, 0, "Infrastructure"
HKR, , Operating_Mode, 0, "1"
HKR, Ndi\params\ESSID, ParamDesc, 0, "ESSID"
HKR, Ndi\params\ESSID, default, 0, "ANY"
HKR, Ndi\params\ESSID, type, 0, "edit"
HKR, Ndi\params\ESSID, LimitText, 0, "32"
HKR, Ndi\params\ESSID, UpperCase, 0, "0"
HKR, , ESSID, 0, "ANY"
HKR, Ndi\params\AuthenticationType, ParamDesc, 0, "Authentication Type"
HKR, Ndi\params\AuthenticationType, default, 0, "2"
HKR, Ndi\params\AuthenticationType, type, 0, "enum"
HKR, Ndi\params\AuthenticationType\enum,0, 0, "Open System"
HKR, Ndi\params\AuthenticationType\enum,1, 0, "Shared Key"
HKR, Ndi\params\AuthenticationType\enum,2, 0, "Auto"
HKR, , AuthenticationType, 0, "2"
HKR, Ndi\params\WEP_Mode, ParamDesc, 0, "WEP Mode"
HKR, Ndi\params\WEP_Mode, default, 0, "0"
HKR, Ndi\params\WEP_Mode, type, 0, "enum"
HKR, Ndi\params\WEP_Mode\enum, 0, 0, "Mandatory"
HKR, Ndi\params\WEP_Mode\enum, 1, 0, "Optional"
HKR, , WEP_Mode, 0, "0"
HKR,Ndi\params\EncryptionLevel, ParamDesc, 0, "Encryption Level"
HKR,Ndi\params\EncryptionLevel, type, 0, "enum"
HKR,Ndi\params\EncryptionLevel, default, 0, "0"
HKR,Ndi\params\EncryptionLevel\enum, 0, 0, "None"
HKR,Ndi\params\EncryptionLevel\enum, 1, 0, "64-bit encryption"
HKR,Ndi\params\EncryptionLevel\enum, 2, 0, "128-bit encryption"
HKR,, EncryptionLevel, 0, "0"
HKR,Ndi\params\WEP_KEY_INDEX, ParamDesc, 0, "WEP Key to use"
HKR,Ndi\params\WEP_KEY_INDEX, type, 0, "enum"
HKR,Ndi\params\WEP_KEY_INDEX, default, 0, "0"
HKR,Ndi\params\WEP_KEY_INDEX\enum, 0, 0, "1"
HKR,Ndi\params\WEP_KEY_INDEX\enum, 1, 0, "2"
HKR,Ndi\params\WEP_KEY_INDEX\enum, 2, 0, "3"
HKR,Ndi\params\WEP_KEY_INDEX\enum, 3, 0, "4"
HKR,, WEP_KEY_INDEX, 0, "0"
HKR,Ndi\params\WEP_KEY_1, ParamDesc, 0, "WEP KEY #1"
HKR,Ndi\params\WEP_KEY_1, default, 0, "00000000000000000000000000"
HKR,Ndi\params\WEP_KEY_1, type, 0, "edit"
HKR,Ndi\params\WEP_KEY_1, LimitText, 0, "26"
HKR,Ndi\params\WEP_KEY_1, UpperCase, 0, "1"
HKR,, WEP_KEY_1, 0, "00000000000000000000000000"
HKR,Ndi\params\WEP_KEY_2, ParamDesc, 0, "WEP KEY #2"
HKR,Ndi\params\WEP_KEY_2, default, 0, "00000000000000000000000000"
HKR,Ndi\params\WEP_KEY_2, type, 0, "edit"
HKR,Ndi\params\WEP_KEY_2, LimitText, 0, "26"
HKR,Ndi\params\WEP_KEY_2, UpperCase, 0, "1"
HKR,, WEP_KEY_2, 0, "00000000000000000000000000"
HKR,Ndi\params\WEP_KEY_3, ParamDesc, 0, "WEP KEY #3"
HKR,Ndi\params\WEP_KEY_3, default, 0, "00000000000000000000000000"
HKR,Ndi\params\WEP_KEY_3, type, 0, "edit"
HKR,Ndi\params\WEP_KEY_3, LimitText, 0, "26"
HKR,Ndi\params\WEP_KEY_3, UpperCase, 0, "1"
HKR,, WEP_KEY_3, 0, "00000000000000000000000000"
HKR,Ndi\params\WEP_KEY_4, ParamDesc, 0, "WEP KEY #4"
HKR,Ndi\params\WEP_KEY_4, default, 0, "00000000000000000000000000"
HKR,Ndi\params\WEP_KEY_4, type, 0, "edit"
HKR,Ndi\params\WEP_KEY_4, LimitText, 0, "26"
HKR,Ndi\params\WEP_KEY_4, UpperCase, 0, "1"
HKR,, WEP_KEY_4, 0, "00000000000000000000000000"
[USBNET.Service]
DisplayName=%WUSB11_26.DisplayName%
ServiceType=1
StartType=3
ErrorControl=1
ServiceBinary=%12%\vnetusbl.sys
LoadOrderGroup=NDIS
[Common.EventLog]
AddReg=Common.AddEventLog.Reg
[Common.AddEventLog.Reg]
HKR, , EventMessageFile, 0x00020000, %%SystemRoot%%\System32\netevent.dll, %%SystemRoot%%\System32\drivers\vnetusbl.sys
HKR, , TypesSupported , 0x00010001, 7
[Win9x2k.Params]
HKR, Ndi\params\PreambleType, ParamDesc, 0, "Preamble Type"
HKR, Ndi\params\PreambleType, default, 0, "2"
HKR, Ndi\params\PreambleType, type, 0, "enum"
HKR, Ndi\params\PreambleType\enum, 0, 0, "Long"
HKR, Ndi\params\PreambleType\enum, 1, 0, "Short"
HKR, Ndi\params\PreambleType\enum, 2, 0, "Auto"
HKR, , PreambleType, 0, "2"
HKR, Ndi\params\Channel, ParamDesc, 0, "Channel"
HKR, Ndi\params\Channel, default, 0, "10"
HKR, Ndi\params\Channel, type, 0, "int"
HKR, Ndi\params\Channel, min, 0, "1"
HKR, Ndi\params\Channel, max, 0, "14"
HKR, Ndi\params\Channel, step, 0, "1"
HKR, , Channel, 0, "10"
HKR, Ndi\params\Rate, ParamDesc, 0, "TX Rate (Mbps)"
HKR, Ndi\params\Rate, default, 0, "4"
HKR, Ndi\params\Rate, type, 0, "enum"
HKR, Ndi\params\Rate\enum, 0, 0, "1 Mbps"
HKR, Ndi\params\Rate\enum, 1, 0, "2 Mbps"
HKR, Ndi\params\Rate\enum, 2, 0, "5.5 Mbps"
HKR, Ndi\params\Rate\enum, 3, 0, "11 Mbps"
HKR, Ndi\params\Rate\enum, 4, 0, "Auto"
HKR, , Rate, 0, "4"
HKR, Ndi\params\RTS_Threshold, ParamDesc, 0, "RTS Threshold"
HKR, Ndi\params\RTS_Threshold, default, 0, "2347"
HKR, Ndi\params\RTS_Threshold, type, 0, "int"
HKR, Ndi\params\RTS_Threshold, min, 0, "0"
HKR, Ndi\params\RTS_Threshold, max, 0, "2347"
HKR, Ndi\params\RTS_Threshold, step, 0, "1"
HKR, , RTS_Threshold, 0, "2347"
HKR, Ndi\params\Frag_Threshold, ParamDesc, 0, "Fragmentation Threshold"
HKR, Ndi\params\Frag_Threshold, default, 0, "2346"
HKR, Ndi\params\Frag_Threshold, type, 0, "int"
HKR, Ndi\params\Frag_Threshold, min, 0, "256"
HKR, Ndi\params\Frag_Threshold, max, 0, "2346"
HKR, Ndi\params\Frag_Threshold, step, 0, "1"
HKR, , Frag_Threshold, 0, "2346"
HKR, Ndi\params\Operating_Mode, ParamDesc, 0, "Operating Mode"
HKR, Ndi\params\Operating_Mode, default, 0, "1"
HKR, Ndi\params\Operating_Mode, type, 0, "enum"
HKR, Ndi\params\Operating_Mode\enum, 0, 0, "Ad-Hoc"
HKR, Ndi\params\Operating_Mode\enum, 1, 0, "Infrastructure"
HKR, , Operating_Mode, 0, "1"
HKR, Ndi\params\InternationalRoaming, ParamDesc, 0, "International Roaming"
HKR, Ndi\params\InternationalRoaming, default, 0, "0"
HKR, Ndi\params\InternationalRoaming, type, 0, "enum"
HKR, Ndi\params\InternationalRoaming\enum, 0, 0, "Disabled (Reg. Domain)"
HKR, Ndi\params\InternationalRoaming\enum, 1, 0, "Enabled (Int. Roaming)"
HKR, , InternationalRoaming,0, "0"
HKR, Ndi\params\ESSID, ParamDesc, 0, "ESSID"
HKR, Ndi\params\ESSID, default, 0, ""
HKR, Ndi\params\ESSID, type, 0, "edit"
HKR, Ndi\params\ESSID, LimitText, 0, "32"
HKR, Ndi\params\ESSID, UpperCase, 0, "0"
HKR, , ESSID, 0, ""
HKR, Ndi\params\AuthenticationType, ParamDesc, 0, "Authentication Type"
HKR, Ndi\params\AuthenticationType, default, 0, "2"
HKR, Ndi\params\AuthenticationType, type, 0, "enum"
HKR, Ndi\params\AuthenticationType\enum, 0, 0, "Open System"
HKR, Ndi\params\AuthenticationType\enum, 1, 0, "Shared Key"
HKR, Ndi\params\AuthenticationType\enum, 2, 0, "Auto"
HKR, , AuthenticationType, 0, "2"
HKR, Ndi\params\PowerMgmtMode, ParamDesc, 0, "802.11 Power Save"
HKR, Ndi\params\PowerMgmtMode, type, 0, "enum"
HKR, Ndi\params\PowerMgmtMode, default, 0, "0"
HKR, Ndi\params\PowerMgmtMode\enum, 0, 0, "Disabled"
HKR, Ndi\params\PowerMgmtMode\enum, 1, 0, "Enabled"
HKR, , PowerMgmtMode, 0, "0"
HKR, Ndi\params\BasicRates, ParamDesc, 0, "Basic Rates"
HKR, Ndi\params\BasicRates, type, 0, "enum"
HKR, Ndi\params\BasicRates, default, 0, "1"
HKR, Ndi\params\BasicRates\enum, 0, 0, "1,2 Mbps"
HKR, Ndi\params\BasicRates\enum, 1, 0, "1,2,5.5,11 Mbps"
HKR, , BasicRates, 0, "1"
HKR, Ndi\params\BeaconPeriod, ParamDesc, 0, "Beacon Period"
HKR, Ndi\params\BeaconPeriod, type, 0, "int"
HKR, Ndi\params\BeaconPeriod, default, 0, "100"
HKR, Ndi\params\BeaconPeriod, min, 0, "20"
HKR, Ndi\params\BeaconPeriod, max, 0, "1000"
HKR, Ndi\params\BeaconPeriod, step, 0, "1"
HKR,, BeaconPeriod, 0, "100"
HKR,Ndi\params\RadioOnOff, ParamDesc, 0, "Radio On/Off"
HKR,Ndi\params\RadioOnOff, type, 0, "enum"
HKR,Ndi\params\RadioOnOff, default, 0, "1"
HKR,Ndi\params\RadioOnOff\enum, 0, 0, "OFF"
HKR,Ndi\params\RadioOnOff\enum, 1, 0, "ON"
HKR,,
[WinXP.Params]
HKR, Ndi\params\PreambleType, ParamDesc, 0, "Preamble Type"
HKR, Ndi\params\PreambleType, default, 0, "2"
HKR, Ndi\params\PreambleType, type, 0, "enum"
HKR, Ndi\params\PreambleType\enum, 0, 0, "Long"
HKR, Ndi\params\PreambleType\enum, 1, 0, "Short"
HKR, Ndi\params\PreambleType\enum, 2, 0, "Auto"
HKR, , PreambleType, 0, "2"
HKR, Ndi\params\Rate, ParamDesc, 0, "Rate (Mbps)"
HKR, Ndi\params\Rate, default, 0, "4"
HKR, Ndi\params\Rate, type, 0, "enum"
HKR, Ndi\params\Rate\enum, 0, 0, "1"
HKR, Ndi\params\Rate\enum, 1, 0, "2"
HKR, Ndi\params\Rate\enum, 2, 0, "5.5"
HKR, Ndi\params\Rate\enum, 3, 0, "11"
HKR, Ndi\params\Rate\enum, 4, 0, "Auto"
HKR, , Rate, 0, "4"
HKR, Ndi\params\RTS_Threshold, ParamDesc, 0, "RTS Threshold"
HKR, Ndi\params\RTS_Threshold, default, 0, "2347"
HKR, Ndi\params\RTS_Threshold, type, 0, "int"
HKR, Ndi\params\RTS_Threshold, min, 0, "0"
HKR, Ndi\params\RTS_Threshold, max, 0, "2347"
HKR, Ndi\params\RTS_Threshold, step, 0, "1"
HKR, , RTS_Threshold, 0, "2347"
HKR, Ndi\params\Frag_Threshold, ParamDesc, 0, "Fragmentation Threshold"
HKR, Ndi\params\Frag_Threshold, default, 0, "2346"
HKR, Ndi\params\Frag_Threshold, type, 0, "int"
HKR, Ndi\params\Frag_Threshold, min, 0, "256"
HKR, Ndi\params\Frag_Threshold, max, 0, "2346"
HKR, Ndi\params\Frag_Threshold, step, 0, "1"
HKR, , Frag_Threshold, 0, "2346"
HKR, Ndi\params\PowerMgmtMode, ParamDesc, 0, "802.11 Power Save"
HKR, Ndi\params\PowerMgmtMode, type, 0, "enum"
HKR, Ndi\params\PowerMgmtMode, default, 0, "0"
HKR, Ndi\params\PowerMgmtMode\enum, 0, 0, "Disabled"
HKR, Ndi\params\PowerMgmtMode\enum, 1, 0, "Enabled"
HKR, , PowerMgmtMode, 0, "0"
[DestinationDirs]
CopyFile.USB20.Sys=11
CopyFile.USB20NT.Sys=12
CopyFile.USB20XP.Sys=12
CopyFile.USB25.sys=11
CopyFile.USB25NT.sys=12
CopyFile.USB26.Sys=11
CopyFile.USB26NT.Sys=12
CopyFile.USBNET28.Sys=11
CopyFile.USBNET28.2k.Sys=12
CopyFile.USBNET28.XP.Sys=12
[CopyFile.USB20.Sys]
vnetusba.sys
[CopyFile.USB20NT.Sys]
vnetusba.sys
[CopyFile.USB20XP.Sys]
vnetusbxp.sys
[CopyFile.USB25.sys]
PRISM9x.sys
[CopyFile.USB25NT.sys]
PRISMXP.sys
[CopyFile.USB26.Sys]
vnetu9xl.sys
[CopyFile.USB26NT.Sys]
vnetusbl.sys
[CopyFile.USBNET28.2k.Sys]
vnet58lx.sys
[CopyFile.USBNET28.XP.Sys]
vnet58lx.sys
[SourceDisksNames]
1=%WUSB11_20DriverDisk%,,,
2=%WUSB11_25DriverDisk%,,,
3=%WUSB11_26DriverDisk%,,,
4=%WUSB11_28DriverDisk%,,,
5=%WUSB11_28DriverDisk%,,,
[SourceDisksFiles] ; Win9x
PRISM9x.sys=2
netusb.sys=3
vnetusba.sys=1
vnet58l.sys=5
vnetu9xl.sys=3
[SourceDisksFiles.X86] ; Win2k/Xp
PRISMXP.sys=2
vnet58lx.sys=4
vnet58l.sys=5
vnetusbl.sys=3
vnetusbxp.sys=1
[Strings]
WUSB11_VENDOR="Linksys"
WUSB11_VENDOR_NAME="Cisco-Linksys LLC."
WUSB11_20.DeviceDesc="Instant Wireless USB Network Adapter ver.2.0"
WUSB11_20.DisplayName="Instant Wireless USB Network Adapter ver.2.0 Driver"
WUSB11_20XP.DisplayName="Instant Wireless USB Network Adapter ver.2.0 Driver"
WUSB11_20DriverDisk="Instant Wireless USB Network Adapter ver.2.0 Drivers Disk"
WUSB11_25.DeviceDesc="Instant Wireless USB Network Adapter ver.2.5"
WUSB11_25.DisplayName="Instant Wireless USB Network Adapter ver.2.5 Driver"
WUSB11_25DriverDisk="Instant Wireless USB Network Adapter ver.2.5 Installation Disk"
WUSB11_26A.DeviceDesc="Instant Wireless USB Network Adapter ver.2.6"
WUSB11_26.DeviceDesc="Instant Wireless USB Network Adapter ver.2.6"
WUSB11_26.DisplayName="Instant Wireless USB Network Adapter ver.2.6 Driver"
WUSB11_26DriverDisk="Instant Wireless USB Network Adapter ver.2.6 Installation Disk"
WUSB11_28.DeviceDesc="Linksys Wireless-B USB Network Adapter v2.8"
WUSB11_28.DisplayName="Linksys Wireless-B USB Network Adapter v2.8 Driver"
WUSB11_28DriverDisk="Linksys Wireless-B USB Network Adapter v2.8 Installation Disk"
ADHOC_DEMO_STR="Adhoc Demo Mode"
SHORT_PREAM_STR="Preamble Mode"
RTSTHRESH_STR="RTS Threshold"
FRAGTHRESH_STR="Fragmentation Threshold"
AUTHENT_TYPE_STR="Authentication Algorithm"
LISTENINTERVAL_STR="Listen Interval"
POWER_SAVE_STR="Power Save"

