
[Version]
Signature="$Windows NT$"
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%TI%
DriverVer=08/08/2003,3.0.32.1
[Manufacturer]
%TI%=AIRPLUS
[ControlFlags]
ExcludeFromSelect=USB\VID_2001&PID_3B00
[AIRPLUS]
%acx.DeviceDesc%=acx.Ndi,USB\VID_2001&PID_3B00
[acx.Ndi]
AddReg=acx.AddReg.Ndi,acx.AddReg.Pars
;CpyFiles=acx.CopyFiles
[acx.AddReg.Ndi]
HKR,,DevLoader,,*ndis,*ntkern,*ndis
HKR,,DeviceVxDs,,tiacxusb.sys
HKR,,EnumPropPages,,"netdi.dll,EnumPropPages"
HKR,NDIS,LogDriverName,,"tiacxusb"
HKR,NDIS,MajorNdisVersion,1,05
HKR,NDIS,MinorNdisVersion,1,00
HKR,Ndi\Interfaces,DefUpper,,"ndis3,ndis4,ndis5"
HKR,Ndi\Interfaces,DefLower,,"ethernet"
HKR,Ndi\Interfaces,UpperRange,,"ndis3,ndis4,ndis5"
HKR,Ndi\Interfaces,LowerRange,,"ethernet"
HKR,NDI,CardType,,"USB"
HKR,Ndi,DeviceID,,"USB\VID_0451&PID_60c1"
[acx.Ndi.NT]
BusType=15
AddReg=acx.AddReg.Ndi.NT, acx.AddReg.Pars
Characteristics=0x84
;CpyFiles=acx.CopyFiles
[acx.Ndi.NT.Services]
Addservice=TIACXUSB, 0x00000002, acx.AddService, acx.EventLog
[acx.AddService]
DisplayName=%acx.SvcDesc%
ServiceType=1 ; SERVICE_KERNEL_DRIVER
StartType=3 ; SERVICE_DEMAND_START
ErrorControl=1 ; SERVICE_ERROR_NORMAL
ServiceBinary=%10%\System32\Drivers\tiacxusb.sys
LoadOrderGroup=NDIS
[acx.EventLog]
AddReg=acx.AddEventLog.reg
[acx.AddEventLog.reg]
HKR, ,EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, ,TypesSupported, 0x00010001, 7
[acx.AddReg.Ndi.NT]
HKR, Ndi, Service, 0, "TIACXUSB"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
[acx.AddReg.Pars]
HKR,,PermAddress,,112233
HKR, ,HardwareID, ,"ACX101"
HKR, ,dot11DesiredChannel, ,1
HKR, ,NumACXRxDescriptors, ,10
HKR, ,NumACXTxDescriptors, ,10
HKR, ,LeapUserPassword, ,""
HKR,NDI\params\dot11DesiredBSSType,ParamDesc,,"Desired BSS Type"
HKR,NDI\params\dot11DesiredBSSType,type,,"enum"
HKR,NDI\params\dot11DesiredBSSType,default,,"1"
HKR,NDI\params\dot11DesiredBSSType\enum,"0",,"Ad-Hoc"
HKR,NDI\params\dot11DesiredBSSType\enum,"1",,"Infrastructure"
HKR, Ndi\Params\dot11DesiredSSID, ParamDesc, ,"Desired SSID"
HKR, Ndi\Params\dot11DesiredSSID, Type, ,"edit"
HKR, Ndi\Params\dot11DesiredSSID, LimitText, ,"32"
HKR, Ndi\Params\dot11DesiredSSID, Default,,"default"
HKR, Ndi\Params\dot11DesiredSSID, UpperCase,,"0"
HKR,NDI\params\dot11PowerMode,ParamDesc,,"Power Mode"
HKR,NDI\params\dot11PowerMode,type,,"enum"
HKR,NDI\params\dot11PowerMode,default,,"0"
HKR,NDI\params\dot11PowerMode\enum,"0",,"Continuous Access Mode"
HKR,NDI\params\dot11PowerMode\enum,"1",,"Maximum Power Save"
HKR,NDI\params\dot11PowerMode\enum,"2",,"Fast Power Save"
HKR,NDI\params\dot11DesiredTxRate,ParamDesc,, "Desired Tx Rate"
HKR,NDI\params\dot11DesiredTxRate,type,,"enum"
HKR,NDI\params\dot11DesiredTxRate,default,,"0"
HKR,NDI\params\dot11DesiredTxRate\enum,"0",,"Auto"
HKR,NDI\params\dot11DesiredTxRate\enum,"1",,"1 Mbps"
HKR,NDI\params\dot11DesiredTxRate\enum,"2",,"2 Mbps"
HKR,NDI\params\dot11DesiredTxRate\enum,"3",,"5.5 Mbps"
HKR,NDI\params\dot11DesiredTxRate\enum,"4",,"5.5 Mbps PBCC"
HKR,NDI\params\dot11DesiredTxRate\enum,"5",,"11 Mbps"
HKR,NDI\params\dot11DesiredTxRate\enum,"6",,"11 Mbps PBCC"
HKR,NDI\params\dot11DesiredTxRate\enum,"7",,"22 Mbps PBCC"
HKR,NDI\params\dot11WEPStatus,ParamDesc,,"WEP Option"
HKR,NDI\params\dot11WEPStatus,type,,"enum"
HKR,NDI\params\dot11WEPStatus,default,,"1"
HKR,NDI\params\dot11WEPStatus\enum,"0",,"WEP Enabled"
HKR,NDI\params\dot11WEPStatus\enum,"1",,"WEP Disabled"
HKR,NDI\params\dot11AuthMode,ParamDesc,,"Authentication Mode"
HKR,NDI\params\dot11AuthMode,type,,"enum"
HKR,NDI\params\dot11AuthMode,default,,"2"
HKR,NDI\params\dot11AuthMode\enum,"0",,"Open Authentication"
HKR,NDI\params\dot11AuthMode\enum,"1",,"Shared Authentication"
HKR,NDI\params\dot11AuthMode\enum,"2",,"Auto Switch"
HKR,NDI\params\dot11ShortPreambleInvoked,ParamDesc,,"Short Preamble"
HKR,NDI\params\dot11ShortPreambleInvoked,type,,"enum"
HKR,NDI\params\dot11ShortPreambleInvoked,default,,"0"
HKR,NDI\params\dot11ShortPreambleInvoked\enum,"0",,"Off"
HKR,NDI\params\dot11ShortPreambleInvoked\enum,"1",,"On"
HKR, Ndi\Params\dot11DesiredChannel, ParamDesc, ,"Desired Channel"
HKR, Ndi\Params\dot11DesiredChannel, Type, , "int"
HKR, Ndi\Params\dot11DesiredChannel, Default, , "6"
HKR, Ndi\Params\dot11DesiredChannel, Min, , "1"
HKR, Ndi\Params\dot11DesiredChannel, Max, , "14"
HKR, Ndi\Params\dot11DesiredChannel, Step, , "1"
HKR, Ndi\Params\dot11DesiredChannel, Base, , "10"
[acx.CopyFiles]
[DestinationDirs]
acx.CopyFiles=10,System32\Drivers ; Compatible with both 9x and 2K
[SourceDisksNames]
1=%DISKID%,,
[SourceDisksFiles]
tiacxusb.sys=1
[strings]
TI="D-link"
DISKID="AIRPLUS WLAN USB Installation Disk"
acx.DeviceDesc="D-Link AirPlus DWL-120+ Wireless USB Adapter"
acx.SvcDesc="D-Link AirPlus DWL-120+ Wireless USB Adapter"
acx.Service.DispName="D-Link AirPlus DWL-120+ Wireless USB Adapter"

