
[Version]
Signature="$CHICAGO$"
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%NETGEAR%
Compatible=1
DriverVer=01/07/2005,1.0.1.1007
[Manufacturer]
%NETGEAR%=NETGEAR
[ControlFlags]
ExcludeFromSelect=\ ;for win95 and legacy support
PCI\VEN_168C&DEV_0013
[NETGEAR]
%ATHER.DeviceDesc.5523%=ATHER_DEV_5523.ndi, USB\VID_1385&PID_4250
[ATHER_DEV_5523.ndi.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=15
AddReg=5523.reg, ATHER.reg, 5523.reg, 5212.abgmp.reg
;CpyFiles=ATHER.CopyFiles.nt, DEFAULTDESTDIRS
;DlFiles=ATHER.DelIniFiles
DelReg=5523.DelReg
[ATHER_DEV_5523.ndi]
AddReg=ATHER_DEV_5523.id.reg, 5523.reg, ATHER.win.reg, 5212.abg.reg
;CpyFiles=ATHER.win.CopyFiles, DEFAULTDESTDIRS
;DlFiles=ATHER.DelIniFiles
DelReg=5523.DelReg
[ATHER_DEV_5523.ndi.NT.Services]
AddService=AR5523, 2, ATHER.Service, common.EventLog
[ATHER_DEV_5523.id.reg]
HKR, Ndi, DeviceID, 0, "USB\VID_0CF3&PID_0001"
[5212.abgmp.reg]
HKR, , NetBand, 0x00002, "28"
HKR, CustomParams\Configurations, NicType, 0x10003, 2
[5523.DelReg]
HKR,,NetBand
HKR,,ssid
HKR,,ssid2
HKR,,ssid3
HKR,,prefBssid1
HKR,,prefBssid2
HKR,,prefBssid3
HKR,,prefBssid4
[5523.reg]
HKR, Ndi\params\NetworkAddress, ParamDesc, 0, %NetworkAddress%
HKR, Ndi\params\NetworkAddress, default, 0, ""
HKR, Ndi\params\NetworkAddress, LimitText, 0, "12"
HKR, Ndi\params\NetworkAddress, UpperCase, 0, "1"
HKR, Ndi\params\NetworkAddress, optional, 0, "1"
HKR, Ndi\params\NetworkAddress, type, 0, "edit"
HKR, Ndi\params\radioEnable, ParamDesc, 0, %radioEnable%
HKR, Ndi\params\radioEnable, Base, 0, "10"
HKR, Ndi\params\radioEnable, default, 0, "1"
HKR, Ndi\params\radioEnable, type, 0, "enum"
HKR, Ndi\params\radioEnable\enum, "1", 0, %radioEnableOn%
HKR, Ndi\params\radioEnable\enum, "0", 0, %radioEnableOff%
HKR, Ndi\params\authTypeUseOnly, ParamDesc, 0, %authTypeUseOnly%
HKR, Ndi\params\authTypeUseOnly, Base, 0, "10"
HKR, Ndi\params\authTypeUseOnly, default, 0, "0"
HKR, Ndi\params\authTypeUseOnly, type, 0, "enum"
HKR, Ndi\params\authTypeUseOnly\enum, "0", 0, %authAuto%
HKR, Ndi\params\authTypeUseOnly\enum, "1", 0, %authOpen%
HKR, Ndi\params\authTypeUseOnly\enum, "2", 0, %authShared%
HKR, CustomParams\Configurations, MajorVersion, 0x10003, 2
HKR, CustomParams\Configurations, MinorVersion, 0x10003, 0
HKR, CustomParams\Configurations, SelectedConfigurationIndex, 0x10003, 0
HKR, CustomParams\Configurations, SelectedConfigurationName, 0x00002, "Default"
HKR, , ccode, 0x00002, %ccode_DEFAULT%
HKR, Ndi\params\ccode, ParamDesc, 0, %ccode_Description%
HKR, Ndi\params\ccode, Base, 0, "10"
HKR, Ndi\params\ccode, default, 0, %ccode_DEFAULT%
HKR, Ndi\params\ccode, type, 0, "enum"
HKR, Ndi\params\ccode\enum, "DZ", 0, %ccode_Africa%
HKR, Ndi\params\ccode\enum, "CN", 0, %ccode_Asia%
HKR, Ndi\params\ccode\enum, "AU", 0, %ccode_Australia%
HKR, Ndi\params\ccode\enum, "CA", 0, %ccode_Canada%
HKR, Ndi\params\ccode\enum, "GB", 0, %ccode_Europe%
HKR, Ndi\params\ccode\enum, "FR", 0, %ccode_France%
HKR, Ndi\params\ccode\enum, "IL", 0, %ccode_Israel%
HKR, Ndi\params\ccode\enum, "JP", 0, %ccode_Japan%
HKR, Ndi\params\ccode\enum, "MX", 0, %ccode_Mexico%
HKR, Ndi\params\ccode\enum, "BR", 0, %ccode_SouthAmerica%
HKR, Ndi\params\ccode\enum, "US", 0, %ccode_UnitedStates%
HKR, , SilentInstall, 0, "1"
HKR, , AdHocBand, 0x00002, "0"
HKR, , AwakeTimePerf, 0x00002, "200"
HKR, , beaconInterval, 0x00002, "100"
HKR, , bkScanEnable, 0x00002, "1"
HKR, , bssType, 0x00002, "1"
HKR, , clist, 0x00002, ""
HKR, , defaultKey, 0x00002, "0"
HKR, , EncryptionAlg, 0x00002, "2"
HKR, , FragThreshold, 0x00002, "2346"
HKR, , HwTxRetries, 0x00002, "4"
HKR, , privacyInvoked, 0x00002, "0"
HKR, , QoS, 0x00002, "0"
HKR, , RTSThreshold, 0x00002, "2346"
HKR, , scanType, 0x00002, "2"
HKR, , SwTxRetryScale, 0x00002, "6"
HKR, , SSID, 0x00002, "any"
HKR, , SmeEnable, 0x00002, "1"
HKR, , PHlength, 0x00002, "0"
HKR, CustomParams\Configurations, MajorVersion, 0x10003, 2
HKR, CustomParams\Configurations, MinorVersion, 0x10003, 0
HKR, CustomParams\Configurations, SelectedConfigurationIndex, 0x10003, 0
HKR, CustomParams\Configurations, SelectedConfigurationName, 0x00002, "Default"
HKR, CustomParams\Configurations, ConfigurationProfileName, 0x00002, "Default"
[ATHER.reg]
HKR, Ndi, Service, 0, "AR5523"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
[ATHER.Service]
DisplayName=%ATHER.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_DEMAND_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\wg11tnd5.sys
LoadOrderGroup=NDIS
[common.EventLog]
AddReg=common.AddEventLog.reg
[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported, 0x00010001, 7
[ATHER.win.reg]
HKR, , DevLoader, 0, "*ndis"
HKR, , DeviceVxDs, 0, "wg111t9x.sys"
HKR, , EnumPropPages, 0, "netdi.dll,EnumPropPages"
HKR, Ndi\Interfaces, DefUpper, 0, "ndis3"
HKR, Ndi\Interfaces, DefLower, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis3"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, NDIS, LogDriverName, 0, "wg111t9x"
HKR, NDIS, MajorNdisVersion, 1, 03
HKR, NDIS, MinorNdisVersion, 1, 0A
HKR, Ndi\Install, ndis3, 0, "ATHER.install"
[ATHER.win.CopyFiles]
wg111t9x.sys,,,2
[ATHER.CopyFiles.nt]
wg11tnd5.sys,,,2
[ATHER.DelIniFiles]
Athnic.ini,,,1
[SourceDisksNames]
1=%NETGEAR_Disk%,,,
[SourceDisksFiles]
wg111t9x.sys=1,, ; on distribution disk 1
wg11tnd5.sys=1,, ; on distribution disk 1
[DestinationDirs]
ATHER.CopyFiles.nt=12
ATHER.win.CopyFiles=10,system32\drivers ; %SystemRoot%\system32\drivers
ATHER.DelIniFiles=10,system32\drivers ; %SystemRoot%\system32\drivers
DefaultDestDir=11
[DEFAULTDESTDIRS]
[Strings]
NETGEAR="NETGEAR"
authTypeUseOnly="802.11 Authentication Type"
authAuto="Auto"
authOpen="Open"
authShared="Shared"
MapRegisters="Map Registers"
NetworkAddress="Network Address"
sleepMode="Power Save Mode"
sleepModeOff="Off"
sleepModeNormal="Normal"
sleepModeMax="Maximum"
tpc="Transmit Power"
tpcLowest="Lowest"
tpc12="12.5%"
tpc25="25%"
tpc50="50%"
tpc100="100%"
shortPreamble="802.11b Preamble"
shortPreambleEnable="Long and Short"
shortPreambleDisable="Long only"
radioEnable="Radio On/Off"
radioEnableOn="On"
radioEnableOff="Off"
NETGEAR_Disk="NETGEAR Driver Disk 1"
ATHER.Service.DispName="NETGEAR WG111T USB2.0 Wireless Card Service"
ATHER.DeviceDesc.5523="NETGEAR WG111T 108Mbps Wireless USB2.0 Adapter"
ccode_Description="Regional Domain"
ccode_Africa="Africa"
ccode_Asia="Asia"
ccode_Australia="Australia"
ccode_Canada="Canada"
ccode_Europe="Europe"
ccode_France="France"
ccode_Israel="Israel"
ccode_Mexico="Mexico"
ccode_Japan="Japan"
ccode_SouthAmerica="South America"
ccode_UnitedStates="United States"
ccode_DEFAULT="US"
TransmitRate11b="TransmitRate11b"
TransmitRate11g="TransmitRate11g"
TransmitRate_1M="1Mbps"
TransmitRate_2M="2Mbps"
TransmitRate_5M="5.5Mbps"
TransmitRate_11M="11Mbps"
TransmitRate_6M="6Mbps"
TransmitRate_9M="9Mbps"
TransmitRate_12M="12Mbps"
TransmitRate_18M="18Mbps"
TransmitRate_24M="24Mbps"
TransmitRate_36M="36Mbps"
TransmitRate_48M="48Mbps"
TransmitRate_54M="54Mbps"
RateControl="Rate Control"
RateControlEnable="Enable"
RateControlDisable="Disable"
