
[version]
Signature="$Chicago$"
CatalogFile=LSIPNDS.cat
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%Provider%
Compatible=1
MillenniumPreferred=.ME
DriverVer=07/09/2003,3.01.7.2003
[Manufacturer]
%Provider%=Linksys, NT.5.1
[ControlFlags]
ExcludeFromSelect=PCI\VEN_17FE&DEV_2120&SUBSYS_00201737
[Linksys]
%Linksys.DeviceDesc%=IPN2120.ndi, PCI\VEN_17FE&DEV_2120&SUBSYS_00201737
[Linksys.NT.5.1]
%Linksys.DeviceDesc%=IPN2120.ndi.nt51, PCI\VEN_17FE&DEV_2120&SUBSYS_00201737
[IPN2120.ndi.nt51]
Characteristics=0x84
BusType=5
AddReg=IPN2120.common.reg, IPN2120WinNT.reg
DelReg=IPN2120.common.DelReg
;CpyFiles=IPN2120WinNT51.CopyFiles
[IPN2120.ndi.nt51.Services]
AddService=IPN2120, 2, IPN2120.Service, common.EventLog
[IPN2120.ndi.NT]
Characteristics=0x84
BusType=5
AddReg=IPN2120.common.reg, IPN2120WinNT.reg
DelReg=IPN2120.common.DelReg
;CpyFiles=IPN2120WinNT.CopyFiles
[IPN2120.ndi.NT.Services]
AddService=IPN2120, 2, IPN2120.Service, common.EventLog
[IPN2120.ndi.ME]
Characteristics=0x84
BusType=5
AddReg=IPN2120.common.reg, IPN2120WinME.reg
DelReg=IPN2120.common.DelReg
;CpyFiles=IPN2120WinME.CopyFiles
[IPN2120.ndi.ME.Services]
AddService=IPN2120, 2, IPN2120.Service, common.EventLog
[IPN2120.ndi]
DriverVer=07/09/2003,3.01.07.2003
AddReg=IPN2120Win9X.id.reg, IPN2120.common.reg, IPN2120Win9X.flags.reg, IPN2120Win9X.win.reg
DelReg=IPN2120.common.DelReg
;CpyFiles=IPN2120Win9X.CopyFiles
[IPN2120.common.reg]
HKR, Ndi\params\networkaddress, ParamDesc, 0, %NetworkAddress%
HKR, Ndi\params\networkaddress, Type, 0, "edit"
HKR, Ndi\params\networkaddress, Default, 0, " "
HKR, Ndi\params\networkaddress, Optional, 0, "1"
HKR, Ndi\params\networkaddress, LimitText, 0, "12"
HKR, Ndi\params\networkaddress, UpperCase, 0, "1"
HKR, Ndi\params\Rate, ParamDesc, 0, %Rate%
HKR, Ndi\params\Rate, Type, 0, "enum"
HKR, Ndi\params\Rate, Default, 0, "15"
HKR, Ndi\params\Rate\enum, "1", 0, %Rate1M%
HKR, Ndi\params\Rate\enum, "2", 0, %Rate2M%
HKR, Ndi\params\Rate\enum, "4", 0, %Rate5_5M%
HKR, Ndi\params\Rate\enum, "8", 0, %Rate11M%
HKR, Ndi\params\Rate\enum, "15", 0, %RateAutomatic%
HKR, Ndi\params\Ssid, ParamDesc, 0, %SSID%
HKR, Ndi\params\Ssid, Type, 0, "edit"
HKR, Ndi\params\Ssid, Default, 0, ""
HKR, Ndi\params\Ssid, Optional, 0, "1"
HKR, Ndi\params\Ssid, LimitText, 0, "32"
HKR, Ndi\params\BssType, ParamDesc, 0, %BSSType%
HKR, Ndi\params\BssType, Type, 0, "enum"
HKR, Ndi\params\BssType, Default, 0, "1"
HKR, Ndi\params\BssType\enum, "1", 0, %ESS%
HKR, Ndi\params\BssType\enum, "2", 0, %IBSS%
HKR, Ndi\params\IbssChannel, ParamDesc, 0, %IBSSChannel%
HKR, Ndi\params\IbssChannel, Type, 0, "int"
HKR, Ndi\params\IbssChannel, Default, 0, "11"
HKR, Ndi\params\IbssChannel, Min, 0, "1"
HKR, Ndi\params\IbssChannel, Max, 0, "14"
HKR, Ndi\params\IbssChannel, Step, 0, "1"
HKR, Ndi\params\IbssChannel, Base, 0, "10"
HKR, Ndi\params\IbssBasicRateSet, ParamDesc, 0, %IBSSBasicRateSet%
HKR, Ndi\params\IbssBasicRateSet, Type, 0, "enum"
HKR, Ndi\params\IbssBasicRateSet, Default, 0, "15"
HKR, Ndi\params\IbssBasicRateSet\enum, "3", 0, %IBSSBasicRateSet1%
HKR, Ndi\params\IbssBasicRateSet\enum, "15", 0, %IBSSBasicRateSet2%
HKR, Ndi\params\RtsThreshold, ParamDesc, 0, %RTSThreshold%
HKR, Ndi\params\RtsThreshold, Type, 0, "int"
HKR, Ndi\params\RtsThreshold, Default, 0, "2347"
HKR, Ndi\params\RtsThreshold, Min, 0, "0"
HKR, Ndi\params\RtsThreshold, Max, 0, "00002347"
HKR, Ndi\params\RtsThreshold, Step, 0, "1"
HKR, Ndi\params\RtsThreshold, Base, 0, "10"
HKR, Ndi\params\FragThreshold, ParamDesc, 0, %FragmentationThreshold%
HKR, Ndi\params\FragThreshold, Type, 0, "int"
HKR, Ndi\params\FragThreshold, Default, 0, "2346"
HKR, Ndi\params\FragThreshold, Min, 0, "256"
HKR, Ndi\params\FragThreshold, Max, 0, "00002346"
HKR, Ndi\params\FragThreshold, Step, 0, "1"
HKR, Ndi\params\FragThreshold, Base, 0, "10"
[IPN2120.common.DelReg]
HKR,,NumRfb
HKR, Ndi\params\NumRfb
HKR,,NumTfcb
HKR, Ndi\params\NumTfcb
HKR, Ndi\params\BssType\enum, 130
HKR,,ScanType
HKR, Ndi\params\ScanType
HKR, Ndi\params\AuthType
HKR, Ndi\params\EncryptionMode
HKR, Ndi\params\WepDefaultKeyId
HKR,,WepDefaultKey
HKR, Ndi\params\WepDefaultKey
[IPN2120WinNT.reg]
HKR, Ndi, Service, 0, "IPN2120"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
[IPN2120WinME.reg]
HKR, , DevLoader, 0, "*ndis"
HKR, , DeviceVxDs, 0, "LSIPNDS.sys"
HKR, , EnumPropPages, 0, "netdi.dll,EnumPropPages"
HKR, Ndi, CardType, 0, "PCI"
HKR, Ndi, Service, 0, "IPN2120"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, NDIS, LogDriverName, 0, "IPN2120"
HKR, NDIS, MajorNdisVersion, 1, 05
HKR, NDIS, MinorNdisVersion, 1, 00
[IPN2120Win9X.id.reg]
HKR, Ndi, CardType, 0, "PCI"
HKR, Ndi, DeviceID, 0, "PCI\VEN_17FE&DEV_2120&SUBSYS_212017FE"
[IPN2120Win9X.flags.reg]
HKR, Ndi\params\IbssChannel, flag, 1, 20,00,00,00
HKR, Ndi\params\RtsThreshold, flag, 1, 20,00,00,00
HKR, Ndi\params\FragThreshold, flag, 1, 20,00,00,00
[IPN2120Win9X.win.reg]
HKR, , DriverVersion, 0, "3.01.07.2003"
HKR, , DevLoader, 0, "*ndis"
HKR, , DeviceVxDs, 0, "LSIPNDS.sys"
HKR, , EnumPropPages, 0, "netdi.dll,EnumPropPages"
HKR, Ndi\Interfaces, DefUpper, 0, "ndis3"
HKR, Ndi\Interfaces, DefLower, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis3"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, NDIS, LogDriverName, 0, "IPN2120"
HKR, NDIS, MajorNdisVersion, 1, 03
HKR, NDIS, MinorNdisVersion, 1, 0A
HKR, Ndi\Install, ndis3, 0, "IPN2120.ndis3"
[IPN2120.Service]
DisplayName=%IPN2120.Service.DispName%
ServiceType=1
StartType=3
ErrorControl=1
ServiceBinary=%12%\LSIPNDS.sys
LoadOrderGroup=NDIS
[common.EventLog]
AddReg=common.AddEventLog.reg
[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported, 0x00010001, 7
[IPN2120WinNT.CopyFiles]
LSIPNDS.sys,,,2
[IPN2120WinNT51.CopyFiles]
LSIPNDS.sys,LSIPNDSX.sys,,2
[IPN2120WinME.CopyFiles]
LSIPNDS.sys,,,2
[IPN2120Win9X.CopyFiles]
LSIPNDS.sys,,,2
[SourceDisksNames]
1=%IPN2120.SourceDiskName%,,,
[SourceDisksFiles]
LSIPNDS.sys=1,,
LSIPNDSX.sys=1,,
[DestinationDirs]
IPN2120WinNT.CopyFiles=12
IPN2120WinNT51.CopyFiles=12
IPN2120WinME.CopyFiles=11
IPN2120Win9X.CopyFiles=11
DefaultDestDir=11
[Strings]
Provider="Linksys"
Rate="Transmission Rate"
Rate1M="1 Mbps"
Rate2M="2 Mbps"
Rate5_5M="5.5 Mbps"
Rate11M="11 Mbps"
RateAutomatic="Automatic"
NetworkAddress="Network Address"
SSID="SSID"
BSSType="Network Type"
ESS="Infrastructure"
IBSS="Ad Hoc (IBSS)"
IBSSChannel="Channel to Create Ad Hoc"
IBSSBasicRateSet="Basic Rates to Create Ad Hoc"
IBSSBasicRateSet1="1 and 2 Mbps"
IBSSBasicRateSet2="1, 2, 5.5, and 11 Mbps"
RTSThreshold="RTS Threshold"
FragmentationThreshold="Fragmentation Threshold"
Linksys.DeviceDesc="Instant Wireless-B PCI Adapter"
IPN2120.Service.DispName="Instant Wireless-B PCI Adapter Driver"
IPN2120.SourceDiskName="Instant Wireless-B PCI Adapter Driver Disk"

