
[Version]
DriverVer=01/31/2003, 1.0.17
Signature="$Chicago$"
Compatible=1
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%VER_VENDOR_STR%
MillenniumPreferred=.ME
[ControlFlags]
ExcludeFromSelect=*
[Manufacturer]
%VER_VENDOR_NAME_STR%=DeviceList
[DeviceList]
%DCB_DESC_STR%=WLAN_DCB3, PCI\VEN_1260&DEV_3890&SUBSYS_001517CF
[WLAN_DCB1.NT] ; Win2k
DelReg=COMMON_AMAC_DEL.reg
AddReg=WLAN_DCB1.reg, COMMON_DCB.reg, COMMON_NDIS.reg.NT, COMMON.reg, COMMON_PS_MODE_XP.reg, COMMON_AMAC.reg
;CpyFiles=WLAN_DRIVER.copy.NT, WLAN_FWDCB.copy.NT, WLAN_DOM.copy
BusType=5 ; PCI
Characteristics= 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[WLAN_DCB1.NT.Services]
AddService="WLAN_DCB", 2, WLAN_DRIVER_DCB.Service, WLAN_DRIVER.EventLog
[WLAN_DCB1.reg]
HKR,Ndi,DeviceID,0,"PCI\VEN_1260&DEV_3890&SUBSYS_00001260"
HKR,,PlatformID,0,14480
HKR,,VendorDesc,0,%DCB_DESC_STR%
[WLAN_DCB2.NT] ; Win2k
DelReg=COMMON_AMAC_DEL.reg
AddReg=WLAN_DCB2.reg, COMMON_DCB.reg, COMMON_NDIS.reg.NT, COMMON.reg, COMMON_PS_MODE_XP.reg, COMMON_AMAC.reg
;CpyFiles=WLAN_DRIVER.copy.NT, WLAN_FWDCB.copy.NT, WLAN_DOM.copy
BusType=5 ; PCI
Characteristics= 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[WLAN_DCB2.NT.Services]
AddService="WLAN_DCB", 2, WLAN_DRIVER_DCB.Service, WLAN_DRIVER.EventLog
[WLAN_DCB2.reg]
HKR,Ndi,DeviceID,0,"PCI\VEN_1260&DEV_3890&SUBSYS_001417CF"
HKR,,PlatformID,0,14480
HKR,,VendorDesc,0,%DCB_DESC_STR%
[WLAN_DCB3.NT] ; Win2k
DelReg=COMMON_AMAC_DEL.reg
AddReg=WLAN_DCB3.reg, COMMON_DCB.reg, COMMON_NDIS.reg.NT, COMMON.reg, COMMON_PS_MODE_XP.reg, COMMON_AMAC.reg
;CpyFiles=WLAN_DRIVER.copy.NT, WLAN_FWDCB.copy.NT, WLAN_DOM.copy
BusType=5 ; PCI
Characteristics= 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[WLAN_DCB3.NT.Services]
AddService="WLAN_DCB", 2, WLAN_DRIVER_DCB.Service, WLAN_DRIVER.EventLog
[WLAN_DCB3.reg]
HKR,Ndi,DeviceID,0,"PCI\VEN_1260&DEV_3890&SUBSYS_001517CF"
HKR,,PlatformID,0,14480
HKR,,VendorDesc,0,%DCB_DESC_STR%
[WLAN_DCB4.NT] ; Win2k
DelReg=COMMON_AMAC_DEL.reg
AddReg=WLAN_DCB4.reg, COMMON_DCB.reg, COMMON_NDIS.reg.NT, COMMON.reg, COMMON_PS_MODE_XP.reg, COMMON_AMAC.reg
;CpyFiles=WLAN_DRIVER.copy.NT, WLAN_FWDCB.copy.NT, WLAN_DOM.copy
BusType=5 ; PCI
Characteristics= 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[WLAN_DCB4.NT.Services]
AddService="WLAN_DCB", 2, WLAN_DRIVER_DCB.Service, WLAN_DRIVER.EventLog
[WLAN_DCB4.reg]
HKR,Ndi,DeviceID,0,"PCI\VEN_1260&DEV_3890&SUBSYS_002017CF"
HKR,,PlatformID,0,14480
HKR,,VendorDesc,0,%DCB_DESC_STR%
[WLAN_DRIVER_DCB.Service]
DisplayName=%WLAN_SERVICE_DISPLAY_DCB%
ServiceType=1 ; SERVICE_KERNEL_DRIVER
StartType=3 ; SERVICE_DEMAND_START
ErrorControl=1 ; NORMAL
ServiceBinary=%12%\WLANDCB.sys
LoadOrderGroup=NDIS
[WLAN_DRIVER.EventLog]
AddReg=WLAN_DRIVER.EventLog.reg
[WLAN_DRIVER.EventLog.reg]
HKR, ,EventMessageFile ,0x00020000 ,"%%SystemRoot%%\System32\netevent.dll"
HKR, ,TypesSupported ,0x00010001 ,7
[COMMON_DCB.reg]
HKR,NDI ,Service ,0 ,"WLAN_DCB"
HKR, ,BusType ,0 ,"5"
HKR, ,DeviceVxDs ,0 ,"WLANDCB.sys"
HKR, ,EnableIRQSharing ,1 ,01,00,00,00
HKR, ,IOBaseAddress ,1 ,02,00,00,00
HKR, ,InterruptNumber ,1 ,04,00,00,00
[COMMON_NDIS.reg.NT]
HKR,NDI\Interfaces ,UpperRange ,0 ,"ndis5"
HKR,NDI\Interfaces ,LowerRange ,0 ,"ethernet"
[COMMON.reg]
HKR, ,WLANIOC ,0 ,"XG-300"
HKR, ,Band ,0 ,"1"
HKR, ,RegulatorDomain ,0 ,"48"
HKR, ,SilentInstall ,0 ,"1"
HKR, ,RTSThresh,0,2347
HKR, defaults,RTSThresh,0,2347
HKR,Ndi\params\RTSThresh,default,0,2347
HKR,NDI\params\RTSThresh,ParamDesc,0,%RTSTHRESH_STR%
HKR,NDI\params\RTSThresh,type,0,int
HKR,NDI\params\RTSThresh,flag,1,20,00,00,00
HKR,NDI\params\RTSThresh,min,0,0
HKR,NDI\params\RTSThresh,max,0,2347
HKR,NDI\params\RTSThresh,step,0,1
HKR,NDI\params\RTSThresh,optional,0,1
HKR, ,FragThresh,0,2346
HKR,defaults,FragThresh,0,2346
HKR,Ndi\params\FragThresh,default,0,2346
HKR,NDI\params\FragThresh,ParamDesc,0,%FRAGTHRESH_STR%
HKR,NDI\params\FragThresh,type,0,int
HKR,NDI\params\FragThresh,flag,1,20,00,00,00
HKR,NDI\params\FragThresh,min,0,256
HKR,NDI\params\FragThresh,max,0,2346
HKR,NDI\params\FragThresh,step,0,2
HKR,NDI\params\FragThresh,optional,0,1
HKR, ,SSID,0,"ANY"
HKR, defaults,SSID,0,"ANY" ;Default value is "any"
HKR, Ndi\params\SSID,default, 0, "ANY"
HKR, Ndi\params\SSID,ParamDesc,0, %ESSID_Str%
HKR, Ndi\params\SSID,type,0, "edit"
HKR, Ndi\params\SSID,default,0, "ANY"
HKR, Ndi\params\SSID,LimitText,0, "32"
HKR, Ndi\params\SSID,UpperCase,0, "0"
HKR, NDI\params\SSID,optional,0,1
HKR, ,NetworkType,0,1
HKR, defaults,NetworkType,0,1 ;Infrasturcture
HKR, Ndi\params\NetworkType,default,0,1
HKR, Ndi\params\NetworkType,ParamDesc,0, %NET_WORK_TYPE%
HKR, Ndi\params\NetworkType,type,0, "enum"
HKR, Ndi\params\NetworkType,default,0, "1"
HKR, Ndi\params\NetworkType\enum,1,0, "Infrastructure"
HKR, Ndi\params\NetworkType\enum,0,0, "802.11 AdHoc"
HKR, NDI\params\NetworkType,optional,0,1
HKR, ,LongPreamble,0,0
HKR, defaults,LongPreamble,0,0 ;Infrasturcture
HKR, Ndi\params\LongPreamble,default,0,0
HKR, Ndi\params\LongPreamble,ParamDesc,0, %SHORT_PREAM_STR%
HKR, Ndi\params\LongPreamble,type,0, "enum"
HKR, Ndi\params\LongPreamble,default,0, "1"
HKR, Ndi\params\LongPreamble\enum,1,0, "Long"
HKR, Ndi\params\LongPreamble\enum,0,0, "Short"
HKR, NDI\params\LongPreamble,optional,0,1
HKR, ,11dMode,0,0
HKR, defaults,11dMode,0,0 ;Disalbed
HKR, Ndi\params\11dMode,default,0,0
HKR, Ndi\params\11dMode,ParamDesc,0, %11D_MODE%
HKR, Ndi\params\11dMode,type,0, "enum"
HKR, Ndi\params\11dMode,default,0, "0"
HKR, Ndi\params\11dMode\enum,0,0, "Disabled"
HKR, Ndi\params\11dMode\enum,1,0, "Strict"
HKR, Ndi\params\11dMode\enum,2,0, "Flexible"
HKR, NDI\params\11dMode,optional,0,1
HKR, ,NitroMode,0,1
HKR,defaults,NitroMode,0,1
HKR,NDI\params\NitroMode,default,0,1
HKR,NDI\params\NitroMode,ParamDesc,,%NITRO_MODE%
HKR,NDI\params\NitroMode,type,0,int
HKR,NDI\params\NitroMode,min,0,0
HKR,NDI\params\NitroMode,max,0,1
HKR,NDI\params\NitroMode,step,0,1
HKR,NDI\params\NitroMode,optional,0,1
HKR, ,NitroTime,0,650
HKR,defaults,NitroTime,0,650
HKR,NDI\params\NitroTime,default,0,650
HKR,NDI\params\NitroTime,ParamDesc,,"NitroTime"
HKR,NDI\params\NitroTime,type,0,int
HKR,NDI\params\NitroTime,min,0,0
HKR,NDI\params\NitroTime,max,0,5000
HKR,NDI\params\NitroTime,step,0,10
HKR,NDI\params\NitroTime,optional,0,1
[COMMON_AMAC_DEL.reg]
HKR,defaults,DataRates
HKR,NDI\params\DataRates
HKR,NDI\params\DataRate
HKR,DSChannel
HKR,defaults,DSChannel
HKR,NDI\params\DSChannel
[COMMON_AMAC.reg]
HKR, ,ShortRetryLimit,0,7
HKR,defaults,ShortRetryLimit,0,7
HKR,NDI\params\ShortRetryLimit,default,0,7
HKR,NDI\params\ShortRetryLimit,ParamDesc,,%SHORT_RETRY_STR%
HKR,NDI\params\ShortRetryLimit,type,,int
HKR,NDI\params\ShortRetryLimit,min,0,1
HKR,NDI\params\ShortRetryLimit,max,0,255
HKR,NDI\params\ShortRetryLimit,step,0,1
HKR,NDI\params\ShortRetryLimit,optional,0,1
HKR, ,LongRetryLimit,0,4
HKR,defaults,LongRetryLimit,0,4
HKR,NDI\params\LongRetryLimit,default,0,4
HKR,NDI\params\LongRetryLimit,ParamDesc,,%LONG_RETRY_STR%
HKR,NDI\params\LongRetryLimit,type,0,int
HKR,NDI\params\LongRetryLimit,min,0,1
HKR,NDI\params\LongRetryLimit,max,0,255
HKR,NDI\params\LongRetryLimit,step,0,1
HKR,NDI\params\LongRetryLimit,optional,0,1
[COMMON_PS_MODE_XP.reg]
HKR,,PSMode,0,1
HKR,defaults,PSMode,0,1
HKR,Ndi\params\PSMode,default,0,1
HKR,NDI\params\PSMode,ParamDesc,,%POWER_SAVE_STR%
HKR,NDI\params\PSMode,type,,enum
HKR,NDI\params\PSMode,flag,1,30,00,00,00
HKR,NDI\params\PSMode\enum,1,,%POWER_SAVE_OFF_STR%
HKR,NDI\params\PSMode\enum,2,,%POWER_SAVE_DYN_STR%
HKR,NDI\params\PSMode\enum,3,,%POWER_SAVE_MAX_STR%
HKR,NDI\params\PSMode\enum,4,,%POWER_SAVE_AUTO_DYN_STR%
HKR,NDI\params\PSMode\enum,5,,%POWER_SAVE_AUTO_MAX_STR%
HKR,NDI\params\PSMode,optional,0,1
[DestinationDirs]
DefaultDestDir=11 ; Win9x=%windir%\system Win2k=%windir%\system32
WLAN_DRIVER.copy.NT=12 ; Win2k=%windir%\system32\drivers
WLAN_FWDCB.copy.NT=12 ; Win2k=%windir%\system32\drivers
WLAN_DOM.copy=10 ; %windir% all OS
[WLAN_DRIVER.copy.NT]
WLANDCB.sys
[WLAN_FWDCB.copy.NT]
[WLAN_DOM.copy]
WLANDOM.ini
[SourceDisksNames]
1=%INSTALL_DISK_STR%,,,
[SourceDisksFiles.X86] ; Win2k/Xp
WLANDCB.sys=1
WLANDOM.ini=1
[Strings]
VER_VENDOR_STR=""
VER_VENDOR_NAME_STR=""
WLAN_SERVICE_DISPLAY_DCB="IEEE 802.11g Wireless LAN Driver"
INSTALL_DISK_STR="IEEE 802.11g Wireless LAN Install Disk"
ADHOC_DEMO_STR="Adhoc Demo Mode"
SHORT_PREAM_STR="Preamble Mode"
RTSTHRESH_STR="RTS Threshold"
FRAGTHRESH_STR="Fragmentation Threshold"
AUTHENT_TYPE_STR="Authentication Algorithm"
LISTENINTERVAL_STR="Listen Interval"
POWER_SAVE_STR="Power Save Mode"
POWER_SAVE_OFF_STR="Disabled"
POWER_SAVE_DYN_STR="Dynamic"
POWER_SAVE_MAX_STR="Maximum"
POWER_SAVE_AUTO_DYN_STR="Auto Dynamic"
POWER_SAVE_AUTO_MAX_STR="Auto Maximum"
LOAD_FIRMWARE_STR="Firmware Download"
SHORT_RETRY_STR="Short Retry Limit"
LONG_RETRY_STR="Long Retry Limit"
CHANNEL_STR="Channel"
DATARATES_STR="Data Rate"
DATARATES_AUTO="Fully Automatic"
ALSR_STR="Auto Long Slot Reassociation"
11D_MODE="11D Mode"
NITRO_MODE="Nitro Mode"
ESSID_Str="ssid"
NET_WORK_TYPE="Network Type"
DCB_DESC_STR="IEEE 802.11g Wireless LAN Adapter"

