
[Version]
Signature="$CHICAGO$"
Compatible=1
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
DriverVer=06/04/2003,1.0.1.33
Provider=%PROVIDER_NAME%
CatalogFile=WL50ND5.CAT
[Manufacturer]
%COMPANY_NAME%=Device
[ControlFlags]
ExcludeFromSelect=PCI\VEN_168C&DEV_0007&SUBSYS_25008086, \
PCI\VEN_168C&DEV_0007&SUBSYS_25018086
[Device]
%NIC1%=Install_NIC1,PCI\VEN_168C&DEV_0007&SUBSYS_25008086 ; WCB5000
%NIC2%=Install_NIC2,PCI\VEN_168C&DEV_0007&SUBSYS_25018086 ; WM3A5000
[Install_NIC1] ; WCB5000
AddReg=reg_w9x_NIC1id, reg_w9x_NIC, reg_w9x_NDIS, reg_common_NIC
;CpyFiles=Intel_copyfiles_9xSystem, Intel_copyfiles_9xNdiInst
[Install_NIC1.NT]
AddReg=reg_w2k_NIC1id, reg_w2k_NDIS, reg_w2k_NIC, reg_common_NIC
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI
;CpyFiles=Intel_copyfiles_w2kDriver
[Install_NIC1.NT.CoInstallers]
AddReg=reg_w2k_CoInstaller
;CpyFiles=Intel_copyfiles_coinstaller
[Install_NIC1.NT.Services]
AddService=WL50ND5, 2, NIC_Service, common_EventLog
[Install_NIC2] ; WM3A5000
AddReg=reg_w9x_NIC2id, reg_w9x_NIC, reg_w9x_NDIS, reg_common_NIC
;CpyFiles=Intel_copyfiles_9xSystem, Intel_copyfiles_9xNdiInst
[Install_NIC2.NT]
AddReg=reg_w2k_NIC2id, reg_w2k_NDIS, reg_w2k_NIC, reg_common_NIC
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI
;CpyFiles=Intel_copyfiles_w2kDriver
[Install_NIC2.NT.CoInstallers]
AddReg=reg_w2k_CoInstaller
;CpyFiles=Intel_copyfiles_coinstaller
[Install_NIC2.NT.Services]
AddService=WL50ND5, 2, NIC_Service, common_EventLog
[reg_w9x_NIC1id] ; WCB5000
HKR,Ndi,DeviceID, ,"PCI\VEN_168C&DEV_0007"
HKR,,AdapterModel, 0,%NIC1_AdapterModel%
HKR,,CardType, ,"1"
[reg_w9x_NIC2id] ; WM3A5000
HKR,Ndi,DeviceID, 0,"PCI\VEN_168C&DEV_0007"
HKR,,AdapterModel, 0,%NIC2_AdapterModel%
HKR,,CardType, ,"2"
[reg_w9x_NIC]
HKR,,aifs, 0x00002,"2"
HKR,,AwakeTimePerf, 0x00002,"6000"
HKR,,beaconInterval, 0x00002,"100"
HKR,,bkScanEnable, 0x00002,"1"
HKR,,bssType, 0x00002,"1"
HKR,,CLSGUID, 0x00002,%INTEL_GUID%
HKR,,cwmin, 0x00002,"15"
HKR,,defaultKey, 0x00002,"1"
HKR,,eepRD, 0x00010003,0
HKR,,FragThreshold, 0x00002,"2346"
HKR,,InitialInstall, 0x00002,"TRUE"
HKR,,InitFile, 0x00002,%InitFile%
HKR,,key0, 0x00002,""
HKR,,key1, 0x00002,""
HKR,,key2, 0x00002,""
HKR,,key3, 0x00002,""
HKR,,keyLength0, 0x00002,"0"
HKR,,keyLength1, 0x00002,"0"
HKR,,keyLength2, 0x00002,"0"
HKR,,keyLength3, 0x00002,"0"
HKR,,NetworkAddress, 0x00002," "
HKR,,privacyInvoked, 0x00002,"0"
HKR,,Provider, 0x00002,"Intel"
HKR,,rateCtrlEnable, 0x00002,"1"
HKR,,RTSThreshold, 0x00002,"2346"
HKR,,SleepMode, 0x00002,"2"
HKR,,SleepTimePerf, 0x00002,"100"
HKR,,SmeEnable, 0x00002,"1"
HKR,,ssid, 0x00002,""
HKR,,tpc, 0x00002,"0"
HKR,,TransmitRate, 0x00002,"5"
HKR,,TurboEnable, 0x00002,"0"
HKR,,uniqKey, 0x00002,""
HKR,,uniqKeyLength, 0x00002,"0"
HKR,,promiscuousEnable, 0x00002,"0"
HKR,,StealthEnable, 0x00002,"1" ;; Stealth Enable
HKR, CustomParams\Configurations, MajorVersion, 0x10003, 1
HKR, CustomParams\Configurations, MinorVersion, 0x10003, 0
HKR, CustomParams\Configurations, SelectedConfigurationIndex, 0x10003, 0
HKR, CustomParams\Configurations, SelectedConfigurationName, 0x00002, "Default"
HKR, CustomParams\Configurations\Cfg0,ConfigurationName, 0x00002, "Default"
HKR, CustomParams\Configurations\Cfg0,DefaultKey, 0x10003, 0
HKR, CustomParams\Configurations\Cfg0,EnableMacAddress, 0x10003, 0
HKR, CustomParams\Configurations\Cfg0,EnableSecurity, 0x10003, 0
HKR, CustomParams\Configurations\Cfg0,EnableTurbo, 0x10003, 0
HKR, CustomParams\Configurations\Cfg0,MacAddress, 0x00002, ""
HKR, CustomParams\Configurations\Cfg0,NetworkConnectionType, 0x10003, 1
HKR, CustomParams\Configurations\Cfg0,NetworkName, 0x00002, ""
HKR, CustomParams\Configurations\Cfg0,PowerManagement, 0x10003, 1
HKR, CustomParams\Configurations\Cfg0,RateCtrlEnable, 0x10003, 1
HKR, CustomParams\Configurations\Cfg0,TransmitRateIndex, 0x10003, 5
HKR, CustomParams\Configurations\Cfg0,SharedKey1, 0x00002, ""
HKR, CustomParams\Configurations\Cfg0,SharedKey2, 0x00002, ""
HKR, CustomParams\Configurations\Cfg0,SharedKey3, 0x00002, ""
HKR, CustomParams\Configurations\Cfg0,SharedKey4, 0x00002, ""
HKR, CustomParams\Configurations\Cfg0,SharedKey1Length, 0x10003, 40
HKR, CustomParams\Configurations\Cfg0,SharedKey2Length, 0x10003, 40
HKR, CustomParams\Configurations\Cfg0,SharedKey3Length, 0x10003, 40
HKR, CustomParams\Configurations\Cfg0,SharedKey4Length, 0x10003, 40
HKR, CustomParams\Configurations\Cfg0,UniqueKey, 0x00002, ""
HKR, CustomParams\Configurations\Cfg0,UniqueKeyLength, 0x10003, 40
[reg_common_NIC]
HKR, Ndi\params\MapRegisters, ParamDesc, 0, %MapRegisters%
HKR, Ndi\params\MapRegisters, default, 0x00002, "256"
HKR, Ndi\params\MapRegisters, min, 0, "32"
HKR, Ndi\params\MapRegisters, max, 0, "512"
HKR, Ndi\params\MapRegisters, step, 0, "8"
HKR, Ndi\params\MapRegisters, base, 0, "10"
HKR, Ndi\params\MapRegisters, type, 0, "int"
HKR, , clist, 0x00002, ""
HKR, , HwTxRetries, 0, "5"
HKR, , SwTxRetryScale, 0, "2"
HKR, Ndi\params\QoS, ParamDesc, 0, %QoS%
HKR, Ndi\params\QoS, Base, 0, "10"
HKR, Ndi\params\QoS, default, 0x00002, "0"
HKR, Ndi\params\QoS, type, 0, "enum"
HKR, Ndi\params\QoS\enum, "1", 0, "Enabled"
HKR, Ndi\params\QoS\enum, "0", 0, "Disabled"
HKR, Ndi\params\radioEnable, ParamDesc, 0, %radioEnable%
HKR, Ndi\params\radioEnable, Base, 0, "10"
HKR, Ndi\params\radioEnable, default, 0x00002, "1"
HKR, Ndi\params\radioEnable, type, 0, "enum"
HKR, Ndi\params\radioEnable\enum, "1", 0, "Enabled"
HKR, Ndi\params\radioEnable\enum, "0", 0, "Disabled"
[reg_w2k_NIC1id] ; WCB5000
HKR,,AdapterModel, 0,%NIC1_AdapterModel%
HKR,,CardType, 0x00010001,1
[reg_w2k_NIC2id] ; WM3A5000
HKR,,AdapterModel, 0,%NIC2_AdapterModel%
HKR,,CardType, 0x00010001,2
[reg_w2k_NIC]
HKR,,aifs, 0x00002, "2"
HKR,,AwakeTimePerf, 0x00002, "6000"
HKR,,beaconInterval, 0x00002, "100"
HKR,,bkScanEnable, 0x00002, "1"
HKR,,bssType, 0x00002, "1"
HKR,,CLSGUID, 0x00002, %INTEL_GUID%
HKR,,cwmin, 0x00002, "15"
HKR,,defaultKey, 0x00002, "1"
HKR,,eepRD, 0x00010003, 0
HKR,,FragThreshold, 0x00002, "2346"
HKR,,InitialInstall, 0x00002, "TRUE"
HKR,,InitFile, 0x00002, %InitFile%
HKR,,key0, 0x00002, ""
HKR,,key1, 0x00002, ""
HKR,,key2, 0x00002, ""
HKR,,key3, 0x00002, ""
HKR,,keyLength0, 0x00002, "0"
HKR,,keyLength1, 0x00002, "0"
HKR,,keyLength2, 0x00002, "0"
HKR,,keyLength3, 0x00002, "0"
HKR,,NetworkAddress, 0x00002, " "
HKR,,privacyInvoked, 0x00002, "0"
HKR,,Provider, 0x00002, "Intel"
HKR,,rateCtrlEnable, 0x00002, "1"
HKR,,RTSThreshold, 0x00002, "2346"
HKR,,SleepMode, 0x00002, "2"
HKR,,SleepTimePerf, 0x00002, "100"
HKR,,SmeEnable, 0x00002, "1"
HKR,,ssid, 0x00002, ""
HKR,,tpc, 0x00002, "0" ;; highest power
HKR,,TransmitRate, 0x00002, "5" ;; 36 Mbps
HKR,,TurboEnable, 0x00002, "0"
HKR,,uniqKey, 0x00002, ""
HKR,,uniqKeyLength, 0x00002, "0"
HKR,,promiscuousEnable, 0x00002, "0"
HKR,,StealthEnable, 0x00002, "1" ;; Stealth enable
HKR, CustomParams\Configurations, MajorVersion, 0x00010003, 1
HKR, CustomParams\Configurations, MinorVersion, 0x00010003, 0
HKR, CustomParams\Configurations, SelectedConfigurationIndex, 0x00010003, 0
HKR, CustomParams\Configurations, SelectedConfigurationName, 0x00002, "Default"
HKR, CustomParams\Configurations\Cfg0, ConfigurationName, 0x00002, "Default"
HKR, CustomParams\Configurations\Cfg0, DefaultKey, 0x00010003, 0
HKR, CustomParams\Configurations\Cfg0, EnableMacAddress, 0x00010003, 0
HKR, CustomParams\Configurations\Cfg0, EnableSecurity, 0x00010003, 0
HKR, CustomParams\Configurations\Cfg0, EnableTurbo, 0x00010003, 0
HKR, CustomParams\Configurations\Cfg0, MacAddress, 0x00002, ""
HKR, CustomParams\Configurations\Cfg0, NetworkConnectionType, 0x00010003, 1
HKR, CustomParams\Configurations\Cfg0, NetworkName, 0x00002, ""
HKR, CustomParams\Configurations\Cfg0, PowerManagement, 0x00010003, 1
HKR, CustomParams\Configurations\Cfg0, RateCtrlEnable, 0x00010003, 1
HKR, CustomParams\Configurations\Cfg0, TransmitRateIndex, 0x00010003, 5
HKR, CustomParams\Configurations\Cfg0, SharedKey1, 0x00002, ""
HKR, CustomParams\Configurations\Cfg0, SharedKey2, 0x00002, ""
HKR, CustomParams\Configurations\Cfg0, SharedKey3, 0x00002, ""
HKR, CustomParams\Configurations\Cfg0, SharedKey4, 0x00002, ""
HKR, CustomParams\Configurations\Cfg0, SharedKey1Length, 0x00010003, 40
HKR, CustomParams\Configurations\Cfg0, SharedKey2Length, 0x00010003, 40
HKR, CustomParams\Configurations\Cfg0, SharedKey3Length, 0x00010003, 40
HKR, CustomParams\Configurations\Cfg0, SharedKey4Length, 0x00010003, 40
HKR, CustomParams\Configurations\Cfg0, UniqueKey, 0x00002, ""
HKR, CustomParams\Configurations\Cfg0, UniqueKeyLength, 0x00010003, 40
[reg_w2k_NDIS]
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi, Service, 0, "WL50ND5"
[reg_w2k_CoInstaller]
[NIC_Service]
DisplayName=%NIC_Service_DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_DEMAND_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\wl50nd5.sys
LoadOrderGroup=NDIS
[common_EventLog]
AddReg=common_AddEventLog_reg
[common_AddEventLog_reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported, 0x00010001, 7
[reg_w9x_NDIS]
HKR,Ndi,NdiInstaller,,"wl5ndi.dll,Sparks11aNdiProc"
HKR,,DevLoader,,*ndis
HKR,,DeviceVxDs,,"wl50nd5.sys"
HKR,,EnumPropPages,,"netdi.dll,EnumPropPages"
HKR,NDIS,LogDriverName,,"wl50nd5"
HKR,NDIS,MajorNdisVersion,1,03
HKR,NDIS,MinorNdisVersion,1,0A
HKR,Ndi\Interfaces,DefUpper,,"ndis3"
HKR,Ndi\Interfaces,DefLower,,"ethernet"
HKR,Ndi\Interfaces,UpperRange,,"ndis3"
HKR,Ndi\Interfaces,LowerRange,,"ethernet"
HKR,Ndi\Install,,,"Intel_copyfiles_9xSystem"
[Intel_copyfiles_w2kDriver]
wl50nd5.sys,,,2
[Intel_copyfiles_coinstaller]
[Intel_copyfiles_9xSystem]
wl50nd5.sys,,,2
[Intel_copyfiles_9xNdiInst]
wl5ndi.dll
dm95.exe
[SourceDisksNames]
1=%SOURCEDISK1%,,
[SourceDisksFiles]
wl50nd5.sys=1,,
wl5ndi.dll=1,,
dm95.exe=1,,
[DestinationDirs]
DefaultDestDir =11 ; Windows\System
Intel_copyfiles_w2kDriver =12 ; Windows\System32\Drivers
Intel_copyfiles_coinstaller =11 ; Windows\System32
Intel_copyfiles_9xSystem =11 ; Windows\System
Intel_copyfiles_9xNdiInst =11 ; Windows\System
[Strings]
PROVIDER_NAME="Intel"
COMPANY_NAME="Intel"
NIC1="Intel(R) PRO/Wireless 5000 LAN Cardbus Adapter"
NIC2="Intel(R) PRO/Wireless 5000 LAN 3A Mini PCI Adapter"
NIC1_AdapterModel="PRO/Wireless 5000 LAN Cardbus Adapter"
NIC2_AdapterModel="PRO/Wireless 5000 LAN 3A Mini PCI Adapter"
NIC_Service_DispName="Intel(R) PRO/Wireless 5000 LAN Adapter Driver"
SOURCEDISK1="Intel(R) PRO/Wireless 5000 LAN Adapter Installation Disk"
INTEL_GUID="{F93AC681-94E1-4b32-B053-A163558CE1B9}"
InitFile="wl50nic.ini"
MapRegisters="Map Registers"
Qos="QoS (802.11e)"
radioEnable="Radio Enable"
