
[version]
Signature="$Windows NT$" ; Combined Win9x/Win2k inf
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%V_BCM%
Compatible=1
DriverVer=03/22/2010, 5.60.350.6
CatalogFile =BCM43XX.CAT
CatalogFile.NTamd64=BCM43XX64.CAT
[Manufacturer]
%V_BCM%=BROADCOM, NTx86.6.0, NTamd64.6.0, NTx86.6.1, NTamd64.6.1
[ControlFlags]
ExcludeFromSelect=*
[BROADCOM.NTamd64.6.1]
%BCM430G_DeviceDesc%=BCM43XG_NT61, PCI\VEN_14E4&DEV_4320&SUBSYS_00E70E11&REV_03
%BCM430G_DeviceDesc%=BCM43XGT_NT61, PCI\VEN_14E4&DEV_4320&SUBSYS_12F4103C&REV_03
%BCM430G_DeviceDesc%=BCM43XG1_NT61, PCI\VEN_14E4&DEV_4320&SUBSYS_12F8103C&REV_03
%BCM430G_DeviceDesc%=BCM43XG2_NT61, PCI\VEN_14E4&DEV_4320&SUBSYS_12FA103C&REV_03
%BCM430G_DeviceDesc%=BCM43XG3_NT61, PCI\VEN_14E4&DEV_4320&SUBSYS_12FB103C&REV_03
%BCM430M_DeviceDesc%=BCM43XM1_NT61, PCI\VEN_14E4&DEV_4324&SUBSYS_12F9103C&REV_03
%BCM430M_DeviceDesc%=BCM43XM2_NT61, PCI\VEN_14E4&DEV_4324&SUBSYS_12FC103C&REV_03
%BCM430G_DeviceDesc%=BCM43XG1_NT61, PCI\VEN_14E4&DEV_4318&SUBSYS_1355103C
%BCM430G_DeviceDesc%=BCM43XG2_NT61, PCI\VEN_14E4&DEV_4318&SUBSYS_1356103C
%BCM430G_DeviceDesc%=BCM43XG3_NT61, PCI\VEN_14E4&DEV_4318&SUBSYS_1357103C
%BCM430M_DeviceDesc%=BCM43XM1_NT61, PCI\VEN_14E4&DEV_4319&SUBSYS_1358103C
%BCM430M_DeviceDesc%=BCM43XM2_NT61, PCI\VEN_14E4&DEV_4319&SUBSYS_1359103C
%BCM430M_DeviceDesc%=BCM43XM3_NT61, PCI\VEN_14E4&DEV_4319&SUBSYS_135A103C
%BCM430G_DeviceDesc%=BCM43XG11_NT61, PCI\VEN_14E4&DEV_4311&SUBSYS_1363103C
%BCM430G_DeviceDesc%=BCM43XG12_NT61, PCI\VEN_14E4&DEV_4311&SUBSYS_1364103C
%BCM430G_DeviceDesc%=BCM43XG13_NT61, PCI\VEN_14E4&DEV_4311&SUBSYS_1365103C
%BCM430M_DeviceDesc%=BCM43XM11_NT61, PCI\VEN_14E4&DEV_4312&SUBSYS_1360103C
%BCM430M_DeviceDesc%=BCM43XM12_NT61, PCI\VEN_14E4&DEV_4312&SUBSYS_1361103C
%BCM430M_DeviceDesc%=BCM43XM13_NT61, PCI\VEN_14E4&DEV_4312&SUBSYS_1362103C
%BCM430M_DeviceDesc%=BCM43XM14_NT61, PCI\VEN_14E4&DEV_4312&SUBSYS_135F103C
%BCM430G_DeviceDesc%=BCM43XG11_NT61, PCI\VEN_14E4&DEV_4311&SUBSYS_1374103C
%BCM430G_DeviceDesc%=BCM43XG12_NT61, PCI\VEN_14E4&DEV_4311&SUBSYS_1375103C
%BCM430G_DeviceDesc%=BCM43XG13_NT61, PCI\VEN_14E4&DEV_4311&SUBSYS_1376103C
%BCM430G_DeviceDesc%=BCM43XG14_NT61, PCI\VEN_14E4&DEV_4311&SUBSYS_1377103C
%BCM430M_DeviceDesc%=BCM43XM11_NT61, PCI\VEN_14E4&DEV_4312&SUBSYS_1370103C
%BCM430M_DeviceDesc%=BCM43XM12_NT61, PCI\VEN_14E4&DEV_4312&SUBSYS_1371103C
%BCM430M_DeviceDesc%=BCM43XM13_NT61, PCI\VEN_14E4&DEV_4312&SUBSYS_1372103C
%BCM430M_DeviceDesc%=BCM43XM14_NT61, PCI\VEN_14E4&DEV_4312&SUBSYS_1373103C
%BCM430NM_DeviceDesc%=BCM43XNM11_NT61, PCI\VEN_14E4&DEV_4328&SUBSYS_1366103C
%BCM430NM_DeviceDesc%=BCM43XNM12_NT61, PCI\VEN_14E4&DEV_4328&SUBSYS_1367103C
%BCM430NM_DeviceDesc%=BCM43XNM13_NT61, PCI\VEN_14E4&DEV_4328&SUBSYS_1368103C
%BCM430NM_DeviceDesc%=BCM43XNM14_NT61, PCI\VEN_14E4&DEV_4328&SUBSYS_1369103C
%BCM430G_DeviceDesc%=BCM43XG11_NT61, PCI\VEN_14E4&DEV_4315&SUBSYS_137C103C
%BCM430G_DeviceDesc%=BCM43XG12_NT61, PCI\VEN_14E4&DEV_4315&SUBSYS_137D103C
%BCM430G_DeviceDesc%=BCM43XG11_NT61, PCI\VEN_14E4&DEV_4315&SUBSYS_1507103C
%BCM430G_DeviceDesc%=BCM43XG12_NT61, PCI\VEN_14E4&DEV_4315&SUBSYS_1508103C
%BCM430G_DeviceDesc%=BCM43XG11_NT61, PCI\VEN_14E4&DEV_4315&SUBSYS_365E103C
%BCM430G_DeviceDesc%=BCM43XG12_NT61, PCI\VEN_14E4&DEV_4315&SUBSYS_365F103C
%BCM4322NM_DeviceDesc%=BCM43XNM21_NT61, PCI\VEN_14E4&DEV_432B&SUBSYS_137F103C
%BCM4322NM_DeviceDesc%=BCM43XNM22_NT61, PCI\VEN_14E4&DEV_432B&SUBSYS_1380103C
%BCM4322NM_DeviceDesc%=BCM43XNM21_NT61, PCI\VEN_14E4&DEV_432B&SUBSYS_1509103C
%BCM4322NM_DeviceDesc%=BCM43XNM22_NT61, PCI\VEN_14E4&DEV_432B&SUBSYS_1510103C
%BCM43224NM_DeviceDesc%=BCM43XNM21_NT61, PCI\VEN_14E4&DEV_4353&SUBSYS_1509103C
%BCM43224NM_DeviceDesc%=BCM43XNM22_NT61, PCI\VEN_14E4&DEV_4353&SUBSYS_1510103C
%BCM4313NG_DeviceDesc%=BCM43XNG2022_NT61, PCI\VEN_14E4&DEV_4727&SUBSYS_145C103C
%BCM4313NG_DeviceDesc%=BCM43XNG2022_NT61, PCI\VEN_14E4&DEV_4727&SUBSYS_1483103C
%BCM43225NG_DeviceDesc%=BCM43XNG22_NT61, PCI\VEN_14E4&DEV_4357&SUBSYS_145E103C
[BROADCOM.NTx86.6.1]
%BCM430G_DeviceDesc%=BCM43XG_NT61, PCI\VEN_14E4&DEV_4320&SUBSYS_00E70E11&REV_03
%BCM430G_DeviceDesc%=BCM43XGT_NT61, PCI\VEN_14E4&DEV_4320&SUBSYS_12F4103C&REV_03
%BCM430G_DeviceDesc%=BCM43XG1_NT61, PCI\VEN_14E4&DEV_4320&SUBSYS_12F8103C&REV_03
%BCM430G_DeviceDesc%=BCM43XG2_NT61, PCI\VEN_14E4&DEV_4320&SUBSYS_12FA103C&REV_03
%BCM430G_DeviceDesc%=BCM43XG3_NT61, PCI\VEN_14E4&DEV_4320&SUBSYS_12FB103C&REV_03
%BCM430M_DeviceDesc%=BCM43XM1_NT61, PCI\VEN_14E4&DEV_4324&SUBSYS_12F9103C&REV_03
%BCM430M_DeviceDesc%=BCM43XM2_NT61, PCI\VEN_14E4&DEV_4324&SUBSYS_12FC103C&REV_03
%BCM430G_DeviceDesc%=BCM43XG1_NT61, PCI\VEN_14E4&DEV_4318&SUBSYS_1355103C
%BCM430G_DeviceDesc%=BCM43XG2_NT61, PCI\VEN_14E4&DEV_4318&SUBSYS_1356103C
%BCM430G_DeviceDesc%=BCM43XG3_NT61, PCI\VEN_14E4&DEV_4318&SUBSYS_1357103C
%BCM430M_DeviceDesc%=BCM43XM1_NT61, PCI\VEN_14E4&DEV_4319&SUBSYS_1358103C
%BCM430M_DeviceDesc%=BCM43XM2_NT61, PCI\VEN_14E4&DEV_4319&SUBSYS_1359103C
%BCM430M_DeviceDesc%=BCM43XM3_NT61, PCI\VEN_14E4&DEV_4319&SUBSYS_135A103C
%BCM430G_DeviceDesc%=BCM43XG11_NT61, PCI\VEN_14E4&DEV_4311&SUBSYS_1363103C
%BCM430G_DeviceDesc%=BCM43XG12_NT61, PCI\VEN_14E4&DEV_4311&SUBSYS_1364103C
%BCM430G_DeviceDesc%=BCM43XG13_NT61, PCI\VEN_14E4&DEV_4311&SUBSYS_1365103C
%BCM430M_DeviceDesc%=BCM43XM11_NT61, PCI\VEN_14E4&DEV_4312&SUBSYS_1360103C
%BCM430M_DeviceDesc%=BCM43XM12_NT61, PCI\VEN_14E4&DEV_4312&SUBSYS_1361103C
%BCM430M_DeviceDesc%=BCM43XM13_NT61, PCI\VEN_14E4&DEV_4312&SUBSYS_1362103C
%BCM430M_DeviceDesc%=BCM43XM14_NT61, PCI\VEN_14E4&DEV_4312&SUBSYS_135F103C
%BCM430G_DeviceDesc%=BCM43XG11_NT61, PCI\VEN_14E4&DEV_4311&SUBSYS_1374103C
%BCM430G_DeviceDesc%=BCM43XG12_NT61, PCI\VEN_14E4&DEV_4311&SUBSYS_1375103C
%BCM430G_DeviceDesc%=BCM43XG13_NT61, PCI\VEN_14E4&DEV_4311&SUBSYS_1376103C
%BCM430G_DeviceDesc%=BCM43XG14_NT61, PCI\VEN_14E4&DEV_4311&SUBSYS_1377103C
%BCM430M_DeviceDesc%=BCM43XM11_NT61, PCI\VEN_14E4&DEV_4312&SUBSYS_1370103C
%BCM430M_DeviceDesc%=BCM43XM12_NT61, PCI\VEN_14E4&DEV_4312&SUBSYS_1371103C
%BCM430M_DeviceDesc%=BCM43XM13_NT61, PCI\VEN_14E4&DEV_4312&SUBSYS_1372103C
%BCM430M_DeviceDesc%=BCM43XM14_NT61, PCI\VEN_14E4&DEV_4312&SUBSYS_1373103C
%BCM430NM_DeviceDesc%=BCM43XNM11_NT61, PCI\VEN_14E4&DEV_4328&SUBSYS_1366103C
%BCM430NM_DeviceDesc%=BCM43XNM12_NT61, PCI\VEN_14E4&DEV_4328&SUBSYS_1367103C
%BCM430NM_DeviceDesc%=BCM43XNM13_NT61, PCI\VEN_14E4&DEV_4328&SUBSYS_1368103C
%BCM430NM_DeviceDesc%=BCM43XNM14_NT61, PCI\VEN_14E4&DEV_4328&SUBSYS_1369103C
%BCM430G_DeviceDesc%=BCM43XG11_NT61, PCI\VEN_14E4&DEV_4315&SUBSYS_137C103C
%BCM430G_DeviceDesc%=BCM43XG12_NT61, PCI\VEN_14E4&DEV_4315&SUBSYS_137D103C
%BCM430G_DeviceDesc%=BCM43XG11_NT61, PCI\VEN_14E4&DEV_4315&SUBSYS_1507103C
%BCM430G_DeviceDesc%=BCM43XG12_NT61, PCI\VEN_14E4&DEV_4315&SUBSYS_1508103C
%BCM430G_DeviceDesc%=BCM43XG11_NT61, PCI\VEN_14E4&DEV_4315&SUBSYS_365E103C
%BCM430G_DeviceDesc%=BCM43XG12_NT61, PCI\VEN_14E4&DEV_4315&SUBSYS_365F103C
%BCM4322NM_DeviceDesc%=BCM43XNM21_NT61, PCI\VEN_14E4&DEV_432B&SUBSYS_137F103C
%BCM4322NM_DeviceDesc%=BCM43XNM22_NT61, PCI\VEN_14E4&DEV_432B&SUBSYS_1380103C
%BCM4322NM_DeviceDesc%=BCM43XNM21_NT61, PCI\VEN_14E4&DEV_432B&SUBSYS_1509103C
%BCM4322NM_DeviceDesc%=BCM43XNM22_NT61, PCI\VEN_14E4&DEV_432B&SUBSYS_1510103C
%BCM43224NM_DeviceDesc%=BCM43XNM21_NT61, PCI\VEN_14E4&DEV_4353&SUBSYS_1509103C
%BCM43224NM_DeviceDesc%=BCM43XNM22_NT61, PCI\VEN_14E4&DEV_4353&SUBSYS_1510103C
%BCM4313NG_DeviceDesc%=BCM43XNG2022_NT61, PCI\VEN_14E4&DEV_4727&SUBSYS_145C103C
%BCM4313NG_DeviceDesc%=BCM43XNG2022_NT61, PCI\VEN_14E4&DEV_4727&SUBSYS_1483103C
%BCM43225NG_DeviceDesc%=BCM43XNG22_NT61, PCI\VEN_14E4&DEV_4357&SUBSYS_145E103C
[BROADCOM.NTamd64.6.0]
%BCM430G_DeviceDesc%=BCM43XG_NT60, PCI\VEN_14E4&DEV_4320&SUBSYS_00E70E11&REV_03
%BCM430G_DeviceDesc%=BCM43XGT_NT60, PCI\VEN_14E4&DEV_4320&SUBSYS_12F4103C&REV_03
%BCM430G_DeviceDesc%=BCM43XG1_NT60, PCI\VEN_14E4&DEV_4320&SUBSYS_12F8103C&REV_03
%BCM430G_DeviceDesc%=BCM43XG2_NT60, PCI\VEN_14E4&DEV_4320&SUBSYS_12FA103C&REV_03
%BCM430G_DeviceDesc%=BCM43XG3_NT60, PCI\VEN_14E4&DEV_4320&SUBSYS_12FB103C&REV_03
%BCM430M_DeviceDesc%=BCM43XM1_NT60, PCI\VEN_14E4&DEV_4324&SUBSYS_12F9103C&REV_03
%BCM430M_DeviceDesc%=BCM43XM2_NT60, PCI\VEN_14E4&DEV_4324&SUBSYS_12FC103C&REV_03
%BCM430G_DeviceDesc%=BCM43XG1_NT60, PCI\VEN_14E4&DEV_4318&SUBSYS_1355103C
%BCM430G_DeviceDesc%=BCM43XG2_NT60, PCI\VEN_14E4&DEV_4318&SUBSYS_1356103C
%BCM430G_DeviceDesc%=BCM43XG3_NT60, PCI\VEN_14E4&DEV_4318&SUBSYS_1357103C
%BCM430M_DeviceDesc%=BCM43XM1_NT60, PCI\VEN_14E4&DEV_4319&SUBSYS_1358103C
%BCM430M_DeviceDesc%=BCM43XM2_NT60, PCI\VEN_14E4&DEV_4319&SUBSYS_1359103C
%BCM430M_DeviceDesc%=BCM43XM3_NT60, PCI\VEN_14E4&DEV_4319&SUBSYS_135A103C
%BCM430G_DeviceDesc%=BCM43XG11_NT60, PCI\VEN_14E4&DEV_4311&SUBSYS_1363103C
%BCM430G_DeviceDesc%=BCM43XG12_NT60, PCI\VEN_14E4&DEV_4311&SUBSYS_1364103C
%BCM430G_DeviceDesc%=BCM43XG13_NT60, PCI\VEN_14E4&DEV_4311&SUBSYS_1365103C
%BCM430M_DeviceDesc%=BCM43XM11_NT60, PCI\VEN_14E4&DEV_4312&SUBSYS_1360103C
%BCM430M_DeviceDesc%=BCM43XM12_NT60, PCI\VEN_14E4&DEV_4312&SUBSYS_1361103C
%BCM430M_DeviceDesc%=BCM43XM13_NT60, PCI\VEN_14E4&DEV_4312&SUBSYS_1362103C
%BCM430M_DeviceDesc%=BCM43XM14_NT60, PCI\VEN_14E4&DEV_4312&SUBSYS_135F103C
%BCM430G_DeviceDesc%=BCM43XG11_NT60, PCI\VEN_14E4&DEV_4311&SUBSYS_1374103C
%BCM430G_DeviceDesc%=BCM43XG12_NT60, PCI\VEN_14E4&DEV_4311&SUBSYS_1375103C
%BCM430G_DeviceDesc%=BCM43XG13_NT60, PCI\VEN_14E4&DEV_4311&SUBSYS_1376103C
%BCM430G_DeviceDesc%=BCM43XG14_NT60, PCI\VEN_14E4&DEV_4311&SUBSYS_1377103C
%BCM430M_DeviceDesc%=BCM43XM11_NT60, PCI\VEN_14E4&DEV_4312&SUBSYS_1370103C
%BCM430M_DeviceDesc%=BCM43XM12_NT60, PCI\VEN_14E4&DEV_4312&SUBSYS_1371103C
%BCM430M_DeviceDesc%=BCM43XM13_NT60, PCI\VEN_14E4&DEV_4312&SUBSYS_1372103C
%BCM430M_DeviceDesc%=BCM43XM14_NT60, PCI\VEN_14E4&DEV_4312&SUBSYS_1373103C
%BCM430NM_DeviceDesc%=BCM43XNM11_NT60, PCI\VEN_14E4&DEV_4328&SUBSYS_1366103C
%BCM430NM_DeviceDesc%=BCM43XNM12_NT60, PCI\VEN_14E4&DEV_4328&SUBSYS_1367103C
%BCM430NM_DeviceDesc%=BCM43XNM13_NT60, PCI\VEN_14E4&DEV_4328&SUBSYS_1368103C
%BCM430NM_DeviceDesc%=BCM43XNM14_NT60, PCI\VEN_14E4&DEV_4328&SUBSYS_1369103C
%BCM430G_DeviceDesc%=BCM43XG11_NT60, PCI\VEN_14E4&DEV_4315&SUBSYS_137C103C
%BCM430G_DeviceDesc%=BCM43XG12_NT60, PCI\VEN_14E4&DEV_4315&SUBSYS_137D103C
%BCM430G_DeviceDesc%=BCM43XG11_NT60, PCI\VEN_14E4&DEV_4315&SUBSYS_1507103C
%BCM430G_DeviceDesc%=BCM43XG12_NT60, PCI\VEN_14E4&DEV_4315&SUBSYS_1508103C
%BCM430G_DeviceDesc%=BCM43XG11_NT60, PCI\VEN_14E4&DEV_4315&SUBSYS_365E103C
%BCM430G_DeviceDesc%=BCM43XG12_NT60, PCI\VEN_14E4&DEV_4315&SUBSYS_365F103C
%BCM4322NM_DeviceDesc%=BCM43XNM21_NT60, PCI\VEN_14E4&DEV_432B&SUBSYS_137F103C
%BCM4322NM_DeviceDesc%=BCM43XNM22_NT60, PCI\VEN_14E4&DEV_432B&SUBSYS_1380103C
%BCM4322NM_DeviceDesc%=BCM43XNM21_NT60, PCI\VEN_14E4&DEV_432B&SUBSYS_1509103C
%BCM4322NM_DeviceDesc%=BCM43XNM22_NT60, PCI\VEN_14E4&DEV_432B&SUBSYS_1510103C
%BCM43224NM_DeviceDesc%=BCM43XNM21_NT60, PCI\VEN_14E4&DEV_4353&SUBSYS_1509103C
%BCM43224NM_DeviceDesc%=BCM43XNM22_NT60, PCI\VEN_14E4&DEV_4353&SUBSYS_1510103C
%BCM4313NG_DeviceDesc%=BCM43XNG2022_NT60, PCI\VEN_14E4&DEV_4727&SUBSYS_145C103C
%BCM4313NG_DeviceDesc%=BCM43XNG2022_NT60, PCI\VEN_14E4&DEV_4727&SUBSYS_1483103C
%BCM43225NG_DeviceDesc%=BCM43XNG22_NT60, PCI\VEN_14E4&DEV_4357&SUBSYS_145E103C
[BROADCOM.NTx86.6.0]
%BCM430G_DeviceDesc%=BCM43XG_NT60, PCI\VEN_14E4&DEV_4320&SUBSYS_00E70E11&REV_03
%BCM430G_DeviceDesc%=BCM43XGT_NT60, PCI\VEN_14E4&DEV_4320&SUBSYS_12F4103C&REV_03
%BCM430G_DeviceDesc%=BCM43XG1_NT60, PCI\VEN_14E4&DEV_4320&SUBSYS_12F8103C&REV_03
%BCM430G_DeviceDesc%=BCM43XG2_NT60, PCI\VEN_14E4&DEV_4320&SUBSYS_12FA103C&REV_03
%BCM430G_DeviceDesc%=BCM43XG3_NT60, PCI\VEN_14E4&DEV_4320&SUBSYS_12FB103C&REV_03
%BCM430M_DeviceDesc%=BCM43XM1_NT60, PCI\VEN_14E4&DEV_4324&SUBSYS_12F9103C&REV_03
%BCM430M_DeviceDesc%=BCM43XM2_NT60, PCI\VEN_14E4&DEV_4324&SUBSYS_12FC103C&REV_03
%BCM430G_DeviceDesc%=BCM43XG1_NT60, PCI\VEN_14E4&DEV_4318&SUBSYS_1355103C
%BCM430G_DeviceDesc%=BCM43XG2_NT60, PCI\VEN_14E4&DEV_4318&SUBSYS_1356103C
%BCM430G_DeviceDesc%=BCM43XG3_NT60, PCI\VEN_14E4&DEV_4318&SUBSYS_1357103C
%BCM430M_DeviceDesc%=BCM43XM1_NT60, PCI\VEN_14E4&DEV_4319&SUBSYS_1358103C
%BCM430M_DeviceDesc%=BCM43XM2_NT60, PCI\VEN_14E4&DEV_4319&SUBSYS_1359103C
%BCM430M_DeviceDesc%=BCM43XM3_NT60, PCI\VEN_14E4&DEV_4319&SUBSYS_135A103C
%BCM430G_DeviceDesc%=BCM43XG11_NT60, PCI\VEN_14E4&DEV_4311&SUBSYS_1363103C
%BCM430G_DeviceDesc%=BCM43XG12_NT60, PCI\VEN_14E4&DEV_4311&SUBSYS_1364103C
%BCM430G_DeviceDesc%=BCM43XG13_NT60, PCI\VEN_14E4&DEV_4311&SUBSYS_1365103C
%BCM430M_DeviceDesc%=BCM43XM11_NT60, PCI\VEN_14E4&DEV_4312&SUBSYS_1360103C
%BCM430M_DeviceDesc%=BCM43XM12_NT60, PCI\VEN_14E4&DEV_4312&SUBSYS_1361103C
%BCM430M_DeviceDesc%=BCM43XM13_NT60, PCI\VEN_14E4&DEV_4312&SUBSYS_1362103C
%BCM430M_DeviceDesc%=BCM43XM14_NT60, PCI\VEN_14E4&DEV_4312&SUBSYS_135F103C
%BCM430G_DeviceDesc%=BCM43XG11_NT60, PCI\VEN_14E4&DEV_4311&SUBSYS_1374103C
%BCM430G_DeviceDesc%=BCM43XG12_NT60, PCI\VEN_14E4&DEV_4311&SUBSYS_1375103C
%BCM430G_DeviceDesc%=BCM43XG13_NT60, PCI\VEN_14E4&DEV_4311&SUBSYS_1376103C
%BCM430G_DeviceDesc%=BCM43XG14_NT60, PCI\VEN_14E4&DEV_4311&SUBSYS_1377103C
%BCM430M_DeviceDesc%=BCM43XM11_NT60, PCI\VEN_14E4&DEV_4312&SUBSYS_1370103C
%BCM430M_DeviceDesc%=BCM43XM12_NT60, PCI\VEN_14E4&DEV_4312&SUBSYS_1371103C
%BCM430M_DeviceDesc%=BCM43XM13_NT60, PCI\VEN_14E4&DEV_4312&SUBSYS_1372103C
%BCM430M_DeviceDesc%=BCM43XM14_NT60, PCI\VEN_14E4&DEV_4312&SUBSYS_1373103C
%BCM430NM_DeviceDesc%=BCM43XNM11_NT60, PCI\VEN_14E4&DEV_4328&SUBSYS_1366103C
%BCM430NM_DeviceDesc%=BCM43XNM12_NT60, PCI\VEN_14E4&DEV_4328&SUBSYS_1367103C
%BCM430NM_DeviceDesc%=BCM43XNM13_NT60, PCI\VEN_14E4&DEV_4328&SUBSYS_1368103C
%BCM430NM_DeviceDesc%=BCM43XNM14_NT60, PCI\VEN_14E4&DEV_4328&SUBSYS_1369103C
%BCM430G_DeviceDesc%=BCM43XG11_NT60, PCI\VEN_14E4&DEV_4315&SUBSYS_137C103C
%BCM430G_DeviceDesc%=BCM43XG12_NT60, PCI\VEN_14E4&DEV_4315&SUBSYS_137D103C
%BCM430G_DeviceDesc%=BCM43XG11_NT60, PCI\VEN_14E4&DEV_4315&SUBSYS_1507103C
%BCM430G_DeviceDesc%=BCM43XG12_NT60, PCI\VEN_14E4&DEV_4315&SUBSYS_1508103C
%BCM430G_DeviceDesc%=BCM43XG11_NT60, PCI\VEN_14E4&DEV_4315&SUBSYS_365E103C
%BCM430G_DeviceDesc%=BCM43XG12_NT60, PCI\VEN_14E4&DEV_4315&SUBSYS_365F103C
%BCM4322NM_DeviceDesc%=BCM43XNM21_NT60, PCI\VEN_14E4&DEV_432B&SUBSYS_137F103C
%BCM4322NM_DeviceDesc%=BCM43XNM22_NT60, PCI\VEN_14E4&DEV_432B&SUBSYS_1380103C
%BCM4322NM_DeviceDesc%=BCM43XNM21_NT60, PCI\VEN_14E4&DEV_432B&SUBSYS_1509103C
%BCM4322NM_DeviceDesc%=BCM43XNM22_NT60, PCI\VEN_14E4&DEV_432B&SUBSYS_1510103C
%BCM43224NM_DeviceDesc%=BCM43XNM21_NT60, PCI\VEN_14E4&DEV_4353&SUBSYS_1509103C
%BCM43224NM_DeviceDesc%=BCM43XNM22_NT60, PCI\VEN_14E4&DEV_4353&SUBSYS_1510103C
%BCM4313NG_DeviceDesc%=BCM43XNG2022_NT60, PCI\VEN_14E4&DEV_4727&SUBSYS_145C103C
%BCM4313NG_DeviceDesc%=BCM43XNG2022_NT60, PCI\VEN_14E4&DEV_4727&SUBSYS_1483103C
%BCM43225NG_DeviceDesc%=BCM43XNG22_NT60, PCI\VEN_14E4&DEV_4357&SUBSYS_145E103C
[BROADCOM.NTamd64]
%BCM430G_DeviceDesc%=BCM43XG, PCI\VEN_14E4&DEV_4320&SUBSYS_00E70E11&REV_03
%BCM430G_DeviceDesc%=BCM43XGT, PCI\VEN_14E4&DEV_4320&SUBSYS_12F4103C&REV_03
%BCM430G_DeviceDesc%=BCM43XG1, PCI\VEN_14E4&DEV_4320&SUBSYS_12F8103C&REV_03
%BCM430G_DeviceDesc%=BCM43XG2, PCI\VEN_14E4&DEV_4320&SUBSYS_12FA103C&REV_03
%BCM430G_DeviceDesc%=BCM43XG3, PCI\VEN_14E4&DEV_4320&SUBSYS_12FB103C&REV_03
%BCM430M_DeviceDesc%=BCM43XM1, PCI\VEN_14E4&DEV_4324&SUBSYS_12F9103C&REV_03
%BCM430M_DeviceDesc%=BCM43XM2, PCI\VEN_14E4&DEV_4324&SUBSYS_12FC103C&REV_03
%BCM430G_DeviceDesc%=BCM43XG1, PCI\VEN_14E4&DEV_4318&SUBSYS_1355103C
%BCM430G_DeviceDesc%=BCM43XG2, PCI\VEN_14E4&DEV_4318&SUBSYS_1356103C
%BCM430G_DeviceDesc%=BCM43XG3, PCI\VEN_14E4&DEV_4318&SUBSYS_1357103C
%BCM430M_DeviceDesc%=BCM43XM1, PCI\VEN_14E4&DEV_4319&SUBSYS_1358103C
%BCM430M_DeviceDesc%=BCM43XM2, PCI\VEN_14E4&DEV_4319&SUBSYS_1359103C
%BCM430M_DeviceDesc%=BCM43XM3, PCI\VEN_14E4&DEV_4319&SUBSYS_135A103C
%BCM430G_DeviceDesc%=BCM43XG11, PCI\VEN_14E4&DEV_4311&SUBSYS_1363103C
%BCM430G_DeviceDesc%=BCM43XG12, PCI\VEN_14E4&DEV_4311&SUBSYS_1364103C
%BCM430G_DeviceDesc%=BCM43XG13, PCI\VEN_14E4&DEV_4311&SUBSYS_1365103C
%BCM430M_DeviceDesc%=BCM43XM11, PCI\VEN_14E4&DEV_4312&SUBSYS_1360103C
%BCM430M_DeviceDesc%=BCM43XM12, PCI\VEN_14E4&DEV_4312&SUBSYS_1361103C
%BCM430M_DeviceDesc%=BCM43XM13, PCI\VEN_14E4&DEV_4312&SUBSYS_1362103C
%BCM430M_DeviceDesc%=BCM43XM14, PCI\VEN_14E4&DEV_4312&SUBSYS_135F103C
%BCM430G_DeviceDesc%=BCM43XG11, PCI\VEN_14E4&DEV_4311&SUBSYS_1374103C
%BCM430G_DeviceDesc%=BCM43XG12, PCI\VEN_14E4&DEV_4311&SUBSYS_1375103C
%BCM430G_DeviceDesc%=BCM43XG13, PCI\VEN_14E4&DEV_4311&SUBSYS_1376103C
%BCM430G_DeviceDesc%=BCM43XG14, PCI\VEN_14E4&DEV_4311&SUBSYS_1377103C
%BCM430M_DeviceDesc%=BCM43XM11, PCI\VEN_14E4&DEV_4312&SUBSYS_1370103C
%BCM430M_DeviceDesc%=BCM43XM12, PCI\VEN_14E4&DEV_4312&SUBSYS_1371103C
%BCM430M_DeviceDesc%=BCM43XM13, PCI\VEN_14E4&DEV_4312&SUBSYS_1372103C
%BCM430M_DeviceDesc%=BCM43XM14, PCI\VEN_14E4&DEV_4312&SUBSYS_1373103C
%BCM430NM_DeviceDesc%=BCM43XNM11, PCI\VEN_14E4&DEV_4328&SUBSYS_1366103C
%BCM430NM_DeviceDesc%=BCM43XNM12, PCI\VEN_14E4&DEV_4328&SUBSYS_1367103C
%BCM430NM_DeviceDesc%=BCM43XNM13, PCI\VEN_14E4&DEV_4328&SUBSYS_1368103C
%BCM430NM_DeviceDesc%=BCM43XNM14, PCI\VEN_14E4&DEV_4328&SUBSYS_1369103C
%BCM430G_DeviceDesc%=BCM43XG11, PCI\VEN_14E4&DEV_4315&SUBSYS_137C103C
%BCM430G_DeviceDesc%=BCM43XG12, PCI\VEN_14E4&DEV_4315&SUBSYS_137D103C
%BCM430G_DeviceDesc%=BCM43XG11, PCI\VEN_14E4&DEV_4315&SUBSYS_1507103C
%BCM430G_DeviceDesc%=BCM43XG12, PCI\VEN_14E4&DEV_4315&SUBSYS_1508103C
%BCM430G_DeviceDesc%=BCM43XG11, PCI\VEN_14E4&DEV_4315&SUBSYS_365E103C
%BCM430G_DeviceDesc%=BCM43XG12, PCI\VEN_14E4&DEV_4315&SUBSYS_365F103C
%BCM4322NM_DeviceDesc%=BCM43XNM21, PCI\VEN_14E4&DEV_432B&SUBSYS_137F103C
%BCM4322NM_DeviceDesc%=BCM43XNM22, PCI\VEN_14E4&DEV_432B&SUBSYS_1380103C
%BCM4322NM_DeviceDesc%=BCM43XNM21, PCI\VEN_14E4&DEV_432B&SUBSYS_1509103C
%BCM4322NM_DeviceDesc%=BCM43XNM22, PCI\VEN_14E4&DEV_432B&SUBSYS_1510103C
%BCM43224NM_DeviceDesc%=BCM43XNM21, PCI\VEN_14E4&DEV_4353&SUBSYS_1509103C
%BCM43224NM_DeviceDesc%=BCM43XNM22, PCI\VEN_14E4&DEV_4353&SUBSYS_1510103C
%BCM4313NG_DeviceDesc%=BCM43XNG2022, PCI\VEN_14E4&DEV_4727&SUBSYS_145C103C
%BCM4313NG_DeviceDesc%=BCM43XNG2022, PCI\VEN_14E4&DEV_4727&SUBSYS_1483103C
%BCM43225NG_DeviceDesc%=BCM43XNG22, PCI\VEN_14E4&DEV_4357&SUBSYS_145E103C
[BROADCOM]
%BCM430G_DeviceDesc%=BCM43XG, PCI\VEN_14E4&DEV_4320&SUBSYS_00E70E11&REV_03
%BCM430G_DeviceDesc%=BCM43XGT, PCI\VEN_14E4&DEV_4320&SUBSYS_12F4103C&REV_03
%BCM430G_DeviceDesc%=BCM43XG1, PCI\VEN_14E4&DEV_4320&SUBSYS_12F8103C&REV_03
%BCM430G_DeviceDesc%=BCM43XG2, PCI\VEN_14E4&DEV_4320&SUBSYS_12FA103C&REV_03
%BCM430G_DeviceDesc%=BCM43XG3, PCI\VEN_14E4&DEV_4320&SUBSYS_12FB103C&REV_03
%BCM430M_DeviceDesc%=BCM43XM1, PCI\VEN_14E4&DEV_4324&SUBSYS_12F9103C&REV_03
%BCM430M_DeviceDesc%=BCM43XM2, PCI\VEN_14E4&DEV_4324&SUBSYS_12FC103C&REV_03
%BCM430G_DeviceDesc%=BCM43XG1, PCI\VEN_14E4&DEV_4318&SUBSYS_1355103C
%BCM430G_DeviceDesc%=BCM43XG2, PCI\VEN_14E4&DEV_4318&SUBSYS_1356103C
%BCM430G_DeviceDesc%=BCM43XG3, PCI\VEN_14E4&DEV_4318&SUBSYS_1357103C
%BCM430M_DeviceDesc%=BCM43XM1, PCI\VEN_14E4&DEV_4319&SUBSYS_1358103C
%BCM430M_DeviceDesc%=BCM43XM2, PCI\VEN_14E4&DEV_4319&SUBSYS_1359103C
%BCM430M_DeviceDesc%=BCM43XM3, PCI\VEN_14E4&DEV_4319&SUBSYS_135A103C
%BCM430G_DeviceDesc%=BCM43XG11, PCI\VEN_14E4&DEV_4311&SUBSYS_1363103C
%BCM430G_DeviceDesc%=BCM43XG12, PCI\VEN_14E4&DEV_4311&SUBSYS_1364103C
%BCM430G_DeviceDesc%=BCM43XG13, PCI\VEN_14E4&DEV_4311&SUBSYS_1365103C
%BCM430M_DeviceDesc%=BCM43XM11, PCI\VEN_14E4&DEV_4312&SUBSYS_1360103C
%BCM430M_DeviceDesc%=BCM43XM12, PCI\VEN_14E4&DEV_4312&SUBSYS_1361103C
%BCM430M_DeviceDesc%=BCM43XM13, PCI\VEN_14E4&DEV_4312&SUBSYS_1362103C
%BCM430M_DeviceDesc%=BCM43XM14, PCI\VEN_14E4&DEV_4312&SUBSYS_135F103C
%BCM430G_DeviceDesc%=BCM43XG11, PCI\VEN_14E4&DEV_4311&SUBSYS_1374103C
%BCM430G_DeviceDesc%=BCM43XG12, PCI\VEN_14E4&DEV_4311&SUBSYS_1375103C
%BCM430G_DeviceDesc%=BCM43XG13, PCI\VEN_14E4&DEV_4311&SUBSYS_1376103C
%BCM430G_DeviceDesc%=BCM43XG14, PCI\VEN_14E4&DEV_4311&SUBSYS_1377103C
%BCM430M_DeviceDesc%=BCM43XM11, PCI\VEN_14E4&DEV_4312&SUBSYS_1370103C
%BCM430M_DeviceDesc%=BCM43XM12, PCI\VEN_14E4&DEV_4312&SUBSYS_1371103C
%BCM430M_DeviceDesc%=BCM43XM13, PCI\VEN_14E4&DEV_4312&SUBSYS_1372103C
%BCM430M_DeviceDesc%=BCM43XM14, PCI\VEN_14E4&DEV_4312&SUBSYS_1373103C
%BCM430NM_DeviceDesc%=BCM43XNM11, PCI\VEN_14E4&DEV_4328&SUBSYS_1366103C
%BCM430NM_DeviceDesc%=BCM43XNM12, PCI\VEN_14E4&DEV_4328&SUBSYS_1367103C
%BCM430NM_DeviceDesc%=BCM43XNM13, PCI\VEN_14E4&DEV_4328&SUBSYS_1368103C
%BCM430NM_DeviceDesc%=BCM43XNM14, PCI\VEN_14E4&DEV_4328&SUBSYS_1369103C
%BCM430G_DeviceDesc%=BCM43XG11, PCI\VEN_14E4&DEV_4315&SUBSYS_137C103C
%BCM430G_DeviceDesc%=BCM43XG12, PCI\VEN_14E4&DEV_4315&SUBSYS_137D103C
%BCM430G_DeviceDesc%=BCM43XG11, PCI\VEN_14E4&DEV_4315&SUBSYS_1507103C
%BCM430G_DeviceDesc%=BCM43XG12, PCI\VEN_14E4&DEV_4315&SUBSYS_1508103C
%BCM430G_DeviceDesc%=BCM43XG11, PCI\VEN_14E4&DEV_4315&SUBSYS_365E103C
%BCM430G_DeviceDesc%=BCM43XG12, PCI\VEN_14E4&DEV_4315&SUBSYS_365F103C
%BCM4322NM_DeviceDesc%=BCM43XNM21, PCI\VEN_14E4&DEV_432B&SUBSYS_137F103C
%BCM4322NM_DeviceDesc%=BCM43XNM22, PCI\VEN_14E4&DEV_432B&SUBSYS_1380103C
%BCM4322NM_DeviceDesc%=BCM43XNM21, PCI\VEN_14E4&DEV_432B&SUBSYS_1509103C
%BCM4322NM_DeviceDesc%=BCM43XNM22, PCI\VEN_14E4&DEV_432B&SUBSYS_1510103C
%BCM43224NM_DeviceDesc%=BCM43XNM21, PCI\VEN_14E4&DEV_4353&SUBSYS_1509103C
%BCM43224NM_DeviceDesc%=BCM43XNM22, PCI\VEN_14E4&DEV_4353&SUBSYS_1510103C
%BCM4313NG_DeviceDesc%=BCM43XNG2022, PCI\VEN_14E4&DEV_4727&SUBSYS_145C103C
%BCM4313NG_DeviceDesc%=BCM43XNG2022, PCI\VEN_14E4&DEV_4727&SUBSYS_1483103C
%BCM43225NG_DeviceDesc%=BCM43XNG22, PCI\VEN_14E4&DEV_4357&SUBSYS_145E103C
[BCM43XG_NT61.NTamd64]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bg0.reg, bg.loc.reg, g.reg, cc.reg, cc_fixed.reg, gpiotype1.reg, BCMIHV.reg.NTamd64
DelReg=common.delreg, common.vista.delreg, rate.delreg
;CpyFiles=BCM43XX_NT60.files.NTamd64, BCMIHV.files.NTamd64
RegisterDlls=BCMIHVUI.regsrv.NTamd64
[BCM43XGT_NT61.NTamd64]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bg0.reg, bg.loc.reg, g.reg, gt.reg, cc.reg, cc_fixed.reg, gpiotype1.reg, BCMIHV.reg.NTamd64
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTamd64, BCMIHV.files.NTamd64
RegisterDlls=BCMIHVUI.regsrv.NTamd64
[BCM43XG1_NT61.NTamd64]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bg0.reg, bg1.reg, g.reg, us.reg, gpiotype1.reg, BCMIHV.reg.NTamd64
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTamd64, BCMIHV.files.NTamd64
RegisterDlls=BCMIHVUI.regsrv.NTamd64
[BCM43XG11_NT61.NTamd64]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bg0.reg, bg1.reg, g.reg, us.reg, gpiotype2.reg, BCMIHV.reg.NTamd64
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTamd64, BCMIHV.files.NTamd64
RegisterDlls=BCMIHVUI.regsrv.NTamd64
[BCM43XG2_NT61.NTamd64]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bg0.reg, bg.loc.reg, g.reg, cc.reg, cc_row.reg, gpiotype1.reg, BCMIHV.reg.NTamd64
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTamd64, BCMIHV.files.NTamd64
RegisterDlls=BCMIHVUI.regsrv.NTamd64
[BCM43XG12_NT61.NTamd64]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bg0.reg, bg.loc.reg, g.reg, cc.reg, cc_row.reg, gpiotype2.reg, BCMIHV.reg.NTamd64
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTamd64, BCMIHV.files.NTamd64
RegisterDlls=BCMIHVUI.regsrv.NTamd64
[BCM43XG3_NT61.NTamd64]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bg0.reg, bg3.reg, g.reg, jp.reg, gpiotype1.reg, BCMIHV.reg.NTamd64
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTamd64, BCMIHV.files.NTamd64
RegisterDlls=BCMIHVUI.regsrv.NTamd64
[BCM43XG13_NT61.NTamd64]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bg0.reg, bg3.reg, g.reg, jp.reg, gpiotype2.reg, BCMIHV.reg.NTamd64
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTamd64, BCMIHV.files.NTamd64
RegisterDlls=BCMIHVUI.regsrv.NTamd64
[BCM43XG14_NT61.NTamd64]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bg0.reg, bg3.reg, g.reg, il.reg, gpiotype2.reg, BCMIHV.reg.NTamd64
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTamd64, BCMIHV.files.NTamd64
RegisterDlls=BCMIHVUI.regsrv.NTamd64
[BCM43XM1_NT61.NTamd64]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bag.reg, hiband.reg, chans.thru64.reg, enabled.11h.reg, us.reg, gpiotype1.reg, BCMIHV.reg.NTamd64
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTamd64, BCMIHV.files.NTamd64
RegisterDlls=BCMIHVUI.regsrv.NTamd64
[BCM43XM11_NT61.NTamd64]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bag.reg, hiband.reg, chans.thru64.reg, enabled.11h.reg, us.reg, gpiotype2.reg, BCMIHV.reg.NTamd64
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTamd64, BCMIHV.files.NTamd64
RegisterDlls=BCMIHVUI.regsrv.NTamd64
[BCM43XNM11_NT61.NTamd64]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bagn.reg, hiband.reg, chans.thru64.reg, enabled.11h.reg, us.reg, gpiotype2.reg, BCMIHV.reg.NTamd64
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTamd64, BCMIHV.files.NTamd64
RegisterDlls=BCMIHVUI.regsrv.NTamd64
[BCM43XM2_NT61.NTamd64]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bag.reg, hiband.reg, chans.thru64.reg, chans.a.row.reg, chans.thru13.reg, enabled.11h.reg, cc.reg, cc_row.reg, gpiotype1.reg, BCMIHV.reg.NTamd64
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTamd64, BCMIHV.files.NTamd64
RegisterDlls=BCMIHVUI.regsrv.NTamd64
[BCM43XM12_NT61.NTamd64]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bag.reg, hiband.reg, chans.thru64.reg, chans.a.row.reg, chans.thru13.reg, enabled.11h.reg, cc.reg, cc_row.reg, gpiotype2.reg, BCMIHV.reg.NTamd64
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTamd64, BCMIHV.files.NTamd64
RegisterDlls=BCMIHVUI.regsrv.NTamd64
[BCM43XNM12_NT61.NTamd64]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bagn.reg, hiband.reg, chans.thru64.reg, chans.a.row.reg, chans.thru13.reg, enabled.11h.reg, cc.reg, cc_row.reg, gpiotype2.reg, BCMIHV.reg.NTamd64
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTamd64, BCMIHV.files.NTamd64
RegisterDlls=BCMIHVUI.regsrv.NTamd64
[BCM43XM3_NT61.NTamd64]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bag.reg, chans.a.jp.reg, chans.thru14.reg, enabled.11h.reg, jp.reg, gpiotype1.reg, BCMIHV.reg.NTamd64
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTamd64, BCMIHV.files.NTamd64
RegisterDlls=BCMIHVUI.regsrv.NTamd64
[BCM43XM13_NT61.NTamd64]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bag.reg, chans.a.jp.reg, chans.thru14.reg, enabled.11h.reg, jp.reg, gpiotype2.reg, BCMIHV.reg.NTamd64
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTamd64, BCMIHV.files.NTamd64
RegisterDlls=BCMIHVUI.regsrv.NTamd64
[BCM43XNM13_NT61.NTamd64]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bagn.reg, chans.a.jp.reg, chans.thru14.reg, enabled.11h.reg, jp.reg, gpiotype2.reg, BCMIHV.reg.NTamd64
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTamd64, BCMIHV.files.NTamd64
RegisterDlls=BCMIHVUI.regsrv.NTamd64
[BCM43XM14_NT61.NTamd64]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bag.reg, chans.thru64.reg, chans.thru13.reg, enabled.11h.reg, il.reg, gpiotype2.reg, BCMIHV.reg.NTamd64
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTamd64, BCMIHV.files.NTamd64
RegisterDlls=BCMIHVUI.regsrv.NTamd64
[BCM43XNM14_NT61.NTamd64]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bagn.reg, chans.thru64.reg, chans.thru13.reg, enabled.11h.reg, il.reg, gpiotype2.reg, BCMIHV.reg.NTamd64
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTamd64, BCMIHV.files.NTamd64
RegisterDlls=BCMIHVUI.regsrv.NTamd64
[BCM43XNM21_NT61.NTamd64]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bagn.reg, hiband.reg, chans.thru64.reg, enabled.11h.reg, us.reg, gpiotype2.reg, BCMIHV.reg.NTamd64
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTamd64, BCMIHV.files.NTamd64
RegisterDlls=BCMIHVUI.regsrv.NTamd64
[BCM43XNM22_NT61.NTamd64]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bagn.reg, hiband.reg, chans.thru64.reg, chans.a.row.reg, chans.thru13.reg, enabled.11h.reg, cc.reg, cc_row.reg, gpiotype2.reg, BCMIHV.reg.NTamd64
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTamd64, BCMIHV.files.NTamd64
RegisterDlls=BCMIHVUI.regsrv.NTamd64
[BCM43XNG2022_NT61.NTamd64]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, gn20.reg, chans.thru13.reg, us.reg, gpiotype2.reg, BCMIHV.reg.NTamd64
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTamd64, BCMIHV.files.NTamd64
RegisterDlls=BCMIHVUI.regsrv.NTamd64
[BCM43XNG22_NT61.NTamd64]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, gn.reg, chans.thru13.reg, us.reg, gpiotype2.reg, BCMIHV.reg.NTamd64
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTamd64, BCMIHV.files.NTamd64
RegisterDlls=BCMIHVUI.regsrv.NTamd64
[BCM43XX_NT61.NTamd64.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTamd64, common.EventLog
[BCM43XG_NT61.NTamd64.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTamd64, common.EventLog
[BCM43XGT_NT61.NTamd64.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTamd64, common.EventLog
[BCM43XG1_NT61.NTamd64.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTamd64, common.EventLog
[BCM43XG2_NT61.NTamd64.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTamd64, common.EventLog
[BCM43XG3_NT61.NTamd64.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTamd64, common.EventLog
[BCM43XM1_NT61.NTamd64.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTamd64, common.EventLog
[BCM43XM2_NT61.NTamd64.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTamd64, common.EventLog
[BCM43XM3_NT61.NTamd64.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTamd64, common.EventLog
[BCM43XG11_NT61.NTamd64.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTamd64, common.EventLog
[BCM43XG12_NT61.NTamd64.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTamd64, common.EventLog
[BCM43XG13_NT61.NTamd64.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTamd64, common.EventLog
[BCM43XG14_NT61.NTamd64.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTamd64, common.EventLog
[BCM43XM11_NT61.NTamd64.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTamd64, common.EventLog
[BCM43XM12_NT61.NTamd64.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTamd64, common.EventLog
[BCM43XM13_NT61.NTamd64.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTamd64, common.EventLog
[BCM43XM14_NT61.NTamd64.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTamd64, common.EventLog
[BCM43XNM11_NT61.NTamd64.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTamd64, common.EventLog
[BCM43XNM12_NT61.NTamd64.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTamd64, common.EventLog
[BCM43XNM13_NT61.NTamd64.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTamd64, common.EventLog
[BCM43XNM14_NT61.NTamd64.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTamd64, common.EventLog
[BCM43XNM21_NT61.NTamd64.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTamd64, common.EventLog
[BCM43XNM22_NT61.NTamd64.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTamd64, common.EventLog
[BCM43XNG22_NT61.NTamd64.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTamd64, common.EventLog
[BCM43XNG2022_NT61.NTamd64.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTamd64, common.EventLog
[BCM43XX_NT61.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XG_NT61.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XGT_NT61.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XG1_NT61.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XG2_NT61.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XG3_NT61.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XM1_NT61.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XM2_NT61.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XM3_NT61.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XG11_NT61.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XG12_NT61.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XG13_NT61.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XG14_NT61.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XM11_NT61.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XM12_NT61.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XM13_NT61.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XM14_NT61.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XNM11_NT61.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XNM12_NT61.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XNM13_NT61.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XNM14_NT61.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XNM21_NT61.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XNM22_NT61.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XNG22_NT61.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XNG2022_NT61.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XX_NT61.NTamd64.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration
[BCM43XG_NT61.NTamd64.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration
[BCM43XGT_NT61.NTamd64.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration
[BCM43XG1_NT61.NTamd64.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration
[BCM43XG2_NT61.NTamd64.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration
[BCM43XG3_NT61.NTamd64.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration
[BCM43XM1_NT61.NTamd64.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration
[BCM43XM2_NT61.NTamd64.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration
[BCM43XM3_NT61.NTamd64.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration
[BCM43XG11_NT61.NTamd64.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration
[BCM43XG12_NT61.NTamd64.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration
[BCM43XG13_NT61.NTamd64.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration
[BCM43XG14_NT61.NTamd64.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration
[BCM43XM11_NT61.NTamd64.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration
[BCM43XM12_NT61.NTamd64.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration
[BCM43XM13_NT61.NTamd64.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration
[BCM43XM14_NT61.NTamd64.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration
[BCM43XNM11_NT61.NTamd64.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration
[BCM43XNM12_NT61.NTamd64.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration
[BCM43XNM13_NT61.NTamd64.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration
[BCM43XNM14_NT61.NTamd64.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration
[BCM43XNM21_NT61.NTamd64.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration
[BCM43XNM22_NT61.NTamd64.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration
[BCM43XNG22_NT61.NTamd64.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration
[BCM43XNG2022_NT61.NTamd64.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration
[BCM43XG_NT61.NTx86]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bg0.reg, bg.loc.reg, g.reg, cc.reg, cc_fixed.reg, gpiotype1.reg, BCMIHV.reg.NTx86
DelReg=common.delreg, common.vista.delreg, rate.delreg
;CpyFiles=BCM43XX_NT60.files.NTx86, BCMIHV.files.NTx86
RegisterDlls=BCMIHVUI.regsrv.NTx86
[BCM43XGT_NT61.NTx86]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bg0.reg, bg.loc.reg, g.reg, gt.reg, cc.reg, cc_fixed.reg, gpiotype1.reg, BCMIHV.reg.NTx86
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTx86, BCMIHV.files.NTx86
RegisterDlls=BCMIHVUI.regsrv.NTx86
[BCM43XG1_NT61.NTx86]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bg0.reg, bg1.reg, g.reg, us.reg, gpiotype1.reg, BCMIHV.reg.NTx86
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTx86, BCMIHV.files.NTx86
RegisterDlls=BCMIHVUI.regsrv.NTx86
[BCM43XG11_NT61.NTx86]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bg0.reg, bg1.reg, g.reg, us.reg, gpiotype2.reg, BCMIHV.reg.NTx86
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTx86, BCMIHV.files.NTx86
RegisterDlls=BCMIHVUI.regsrv.NTx86
[BCM43XG2_NT61.NTx86]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bg0.reg, bg.loc.reg, g.reg, cc.reg, cc_row.reg, gpiotype1.reg, BCMIHV.reg.NTx86
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTx86, BCMIHV.files.NTx86
RegisterDlls=BCMIHVUI.regsrv.NTx86
[BCM43XG12_NT61.NTx86]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bg0.reg, bg.loc.reg, g.reg, cc.reg, cc_row.reg, gpiotype2.reg, BCMIHV.reg.NTx86
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTx86, BCMIHV.files.NTx86
RegisterDlls=BCMIHVUI.regsrv.NTx86
[BCM43XG3_NT61.NTx86]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bg0.reg, bg3.reg, g.reg, jp.reg, gpiotype1.reg, BCMIHV.reg.NTx86
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTx86, BCMIHV.files.NTx86
RegisterDlls=BCMIHVUI.regsrv.NTx86
[BCM43XG13_NT61.NTx86]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bg0.reg, bg3.reg, g.reg, jp.reg, gpiotype2.reg, BCMIHV.reg.NTx86
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTx86, BCMIHV.files.NTx86
RegisterDlls=BCMIHVUI.regsrv.NTx86
[BCM43XG14_NT61.NTx86]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bg0.reg, bg3.reg, g.reg, il.reg, gpiotype2.reg, BCMIHV.reg.NTx86
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTx86, BCMIHV.files.NTx86
RegisterDlls=BCMIHVUI.regsrv.NTx86
[BCM43XM1_NT61.NTx86]
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bag.reg, hiband.reg, chans.thru64.reg, enabled.11h.reg, us.reg, gpiotype1.reg, BCMIHV.reg.NTx86
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTx86, BCMIHV.files.NTx86
RegisterDlls=BCMIHVUI.regsrv.NTx86
[BCM43XM11_NT61.NTx86]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bag.reg, hiband.reg, chans.thru64.reg, enabled.11h.reg, us.reg, gpiotype2.reg, BCMIHV.reg.NTx86
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTx86, BCMIHV.files.NTx86
RegisterDlls=BCMIHVUI.regsrv.NTx86
[BCM43XNM11_NT61.NTx86]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bagn.reg, hiband.reg, chans.thru64.reg, enabled.11h.reg, us.reg, gpiotype2.reg, BCMIHV.reg.NTx86
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTx86, BCMIHV.files.NTx86
RegisterDlls=BCMIHVUI.regsrv.NTx86
[BCM43XM2_NT61.NTx86]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bag.reg, hiband.reg, chans.thru64.reg, chans.a.row.reg, chans.thru13.reg, enabled.11h.reg, cc.reg, cc_row.reg, gpiotype1.reg, BCMIHV.reg.NTx86
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTx86, BCMIHV.files.NTx86
RegisterDlls=BCMIHVUI.regsrv.NTx86
[BCM43XM12_NT61.NTx86]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bag.reg, hiband.reg, chans.thru64.reg, chans.a.row.reg, chans.thru13.reg, enabled.11h.reg, cc.reg, cc_row.reg, gpiotype2.reg, BCMIHV.reg.NTx86
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTx86, BCMIHV.files.NTx86
RegisterDlls=BCMIHVUI.regsrv.NTx86
[BCM43XNM12_NT61.NTx86]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bagn.reg, hiband.reg, chans.thru64.reg, chans.a.row.reg, chans.thru13.reg, enabled.11h.reg, cc.reg, cc_row.reg, gpiotype2.reg, BCMIHV.reg.NTx86
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTx86, BCMIHV.files.NTx86
RegisterDlls=BCMIHVUI.regsrv.NTx86
[BCM43XM3_NT61.NTx86]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bag.reg, chans.a.jp.reg, chans.thru14.reg, enabled.11h.reg, jp.reg, gpiotype1.reg, BCMIHV.reg.NTx86
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTx86, BCMIHV.files.NTx86
RegisterDlls=BCMIHVUI.regsrv.NTx86
[BCM43XM13_NT61.NTx86]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bag.reg, chans.a.jp.reg, chans.thru14.reg, enabled.11h.reg, jp.reg, gpiotype2.reg, BCMIHV.reg.NTx86
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTx86, BCMIHV.files.NTx86
RegisterDlls=BCMIHVUI.regsrv.NTx86
[BCM43XNM13_NT61.NTx86]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bagn.reg, chans.a.jp.reg, chans.thru14.reg, enabled.11h.reg, jp.reg, gpiotype2.reg, BCMIHV.reg.NTx86
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTx86, BCMIHV.files.NTx86
RegisterDlls=BCMIHVUI.regsrv.NTx86
[BCM43XM14_NT61.NTx86]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bag.reg, chans.thru64.reg, chans.thru13.reg, enabled.11h.reg, il.reg, gpiotype2.reg, BCMIHV.reg.NTx86
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTx86, BCMIHV.files.NTx86
RegisterDlls=BCMIHVUI.regsrv.NTx86
[BCM43XNM14_NT61.NTx86]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bagn.reg, chans.thru64.reg, chans.thru13.reg, enabled.11h.reg, il.reg, gpiotype2.reg, BCMIHV.reg.NTx86
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTx86, BCMIHV.files.NTx86
RegisterDlls=BCMIHVUI.regsrv.NTx86
[BCM43XNM21_NT61.NTx86]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bagn.reg, hiband.reg, chans.thru64.reg, enabled.11h.reg, us.reg, gpiotype2.reg, BCMIHV.reg.NTx86
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTx86, BCMIHV.files.NTx86
RegisterDlls=BCMIHVUI.regsrv.NTx86
[BCM43XNM22_NT61.NTx86]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bagn.reg, hiband.reg, chans.thru64.reg, chans.a.row.reg, chans.thru13.reg, enabled.11h.reg, cc.reg, cc_row.reg, gpiotype2.reg, BCMIHV.reg.NTx86
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTx86, BCMIHV.files.NTx86
RegisterDlls=BCMIHVUI.regsrv.NTx86
[BCM43XNG2022_NT61.NTx86]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, gn20.reg, chans.thru13.reg, us.reg, gpiotype2.reg, BCMIHV.reg.NTx86
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTx86, BCMIHV.files.NTx86
RegisterDlls=BCMIHVUI.regsrv.NTx86
[BCM43XNG22_NT61.NTx86]
Include=netvwifibus.inf
Needs=VWiFiBus.CopyFiles
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT61.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, gn.reg, chans.thru13.reg, us.reg, gpiotype2.reg, BCMIHV.reg.NTx86
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTx86, BCMIHV.files.NTx86
RegisterDlls=BCMIHVUI.regsrv.NTx86
[BCM43XX_NT61.NTx86.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog
[BCM43XG_NT61.NTx86.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog
[BCM43XGT_NT61.NTx86.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog
[BCM43XG1_NT61.NTx86.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog
[BCM43XG2_NT61.NTx86.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog
[BCM43XG3_NT61.NTx86.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog
[BCM43XM1_NT61.NTx86.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog
[BCM43XM2_NT61.NTx86.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog
[BCM43XM3_NT61.NTx86.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog
[BCM43XG11_NT61.NTx86.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog
[BCM43XG12_NT61.NTx86.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog
[BCM43XG13_NT61.NTx86.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog
[BCM43XG14_NT61.NTx86.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog
[BCM43XM11_NT61.NTx86.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog
[BCM43XM12_NT61.NTx86.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog
[BCM43XM13_NT61.NTx86.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog
[BCM43XM14_NT61.NTx86.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog
[BCM43XNM11_NT61.NTx86.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog
[BCM43XNM12_NT61.NTx86.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog
[BCM43XNM13_NT61.NTx86.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog
[BCM43XNM14_NT61.NTx86.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog
[BCM43XNM21_NT61.NTx86.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog
[BCM43XNM22_NT61.NTx86.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog
[BCM43XNG22_NT61.NTx86.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog
[BCM43XNG2022_NT61.NTx86.Services]
Include=netvwifibus.inf
Needs=VWiFiBus.Services
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog
[BCM43XX_NT61.NTx86.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XG_NT61.NTx86.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XGT_NT61.NTx86.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XG1_NT61.NTx86.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XG2_NT61.NTx86.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XG3_NT61.NTx86.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XM1_NT61.NTx86.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XM2_NT61.NTx86.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XM3_NT61.NTx86.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XG11_NT61.NTx86.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XG12_NT61.NTx86.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XG13_NT61.NTx86.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XG14_NT61.NTx86.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XM11_NT61.NTx86.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XM12_NT61.NTx86.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XM13_NT61.NTx86.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XM14_NT61.NTx86.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XNM11_NT61.NTx86.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XNM12_NT61.NTx86.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XNM13_NT61.NTx86.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XNM14_NT61.NTx86.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XNM21_NT61.NTx86.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XNM22_NT61.NTx86.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XNG22_NT61.NTx86.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XNG2022_NT61.NTx86.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XX_NT61.NTx86.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration
[BCM43XG_NT61.NTx86.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration
[BCM43XGT_NT61.NTx86.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration
[BCM43XG1_NT61.NTx86.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration
[BCM43XG2_NT61.NTx86.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration
[BCM43XG3_NT61.NTx86.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration
[BCM43XM1_NT61.NTx86.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration
[BCM43XM2_NT61.NTx86.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration
[BCM43XM3_NT61.NTx86.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration
[BCM43XG11_NT61.NTx86.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration
[BCM43XG12_NT61.NTx86.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration
[BCM43XG13_NT61.NTx86.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration
[BCM43XG14_NT61.NTx86.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration
[BCM43XM11_NT61.NTx86.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration
[BCM43XM12_NT61.NTx86.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration
[BCM43XM13_NT61.NTx86.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration
[BCM43XM14_NT61.NTx86.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration
[BCM43XNM11_NT61.NTx86.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration
[BCM43XNM12_NT61.NTx86.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration
[BCM43XNM13_NT61.NTx86.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration
[BCM43XNM14_NT61.NTx86.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration
[BCM43XNM21_NT61.NTx86.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration
[BCM43XNM22_NT61.NTx86.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration
[BCM43XNG22_NT61.NTx86.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration
[BCM43XNG2022_NT61.NTx86.HW]
Include=netvwifibus.inf
Needs=VWiFiBus.PnPFilterRegistration
[BCM43XG_NT60.NTamd64]
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT60.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bg0.reg, bg.loc.reg, g.reg, cc.reg, cc_fixed.reg, gpiotype1.reg, BCMIHV.reg.NTamd64
DelReg=common.delreg, common.vista.delreg, rate.delreg
;CpyFiles=BCM43XX_NT60.files.NTamd64, BCMIHV.files.NTamd64
RegisterDlls=BCMIHVUI.regsrv.NTamd64
[BCM43XGT_NT60.NTamd64]
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT60.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bg0.reg, bg.loc.reg, g.reg, gt.reg, cc.reg, cc_fixed.reg, gpiotype1.reg, BCMIHV.reg.NTamd64
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTamd64, BCMIHV.files.NTamd64
RegisterDlls=BCMIHVUI.regsrv.NTamd64
[BCM43XG1_NT60.NTamd64]
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT60.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bg0.reg, bg1.reg, g.reg, us.reg, gpiotype1.reg, BCMIHV.reg.NTamd64
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTamd64, BCMIHV.files.NTamd64
RegisterDlls=BCMIHVUI.regsrv.NTamd64
[BCM43XG11_NT60.NTamd64]
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT60.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bg0.reg, bg1.reg, g.reg, us.reg, gpiotype2.reg, BCMIHV.reg.NTamd64
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTamd64, BCMIHV.files.NTamd64
RegisterDlls=BCMIHVUI.regsrv.NTamd64
[BCM43XG2_NT60.NTamd64]
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT60.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bg0.reg, bg.loc.reg, g.reg, cc.reg, cc_row.reg, gpiotype1.reg, BCMIHV.reg.NTamd64
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTamd64, BCMIHV.files.NTamd64
RegisterDlls=BCMIHVUI.regsrv.NTamd64
[BCM43XG12_NT60.NTamd64]
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT60.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bg0.reg, bg.loc.reg, g.reg, cc.reg, cc_row.reg, gpiotype2.reg, BCMIHV.reg.NTamd64
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTamd64, BCMIHV.files.NTamd64
RegisterDlls=BCMIHVUI.regsrv.NTamd64
[BCM43XG3_NT60.NTamd64]
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT60.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bg0.reg, bg3.reg, g.reg, jp.reg, gpiotype1.reg, BCMIHV.reg.NTamd64
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTamd64, BCMIHV.files.NTamd64
RegisterDlls=BCMIHVUI.regsrv.NTamd64
[BCM43XG13_NT60.NTamd64]
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT60.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bg0.reg, bg3.reg, g.reg, jp.reg, gpiotype2.reg, BCMIHV.reg.NTamd64
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTamd64, BCMIHV.files.NTamd64
RegisterDlls=BCMIHVUI.regsrv.NTamd64
[BCM43XG14_NT60.NTamd64]
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT60.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bg0.reg, bg3.reg, g.reg, il.reg, gpiotype2.reg, BCMIHV.reg.NTamd64
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTamd64, BCMIHV.files.NTamd64
RegisterDlls=BCMIHVUI.regsrv.NTamd64
[BCM43XM1_NT60.NTamd64]
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT60.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bag.reg, hiband.reg, chans.thru64.reg, enabled.11h.reg, us.reg, gpiotype1.reg, BCMIHV.reg.NTamd64
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTamd64, BCMIHV.files.NTamd64
RegisterDlls=BCMIHVUI.regsrv.NTamd64
[BCM43XM11_NT60.NTamd64]
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT60.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bag.reg, hiband.reg, chans.thru64.reg, enabled.11h.reg, us.reg, gpiotype2.reg, BCMIHV.reg.NTamd64
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTamd64, BCMIHV.files.NTamd64
RegisterDlls=BCMIHVUI.regsrv.NTamd64
[BCM43XNM11_NT60.NTamd64]
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT60.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bagn.reg, hiband.reg, chans.thru64.reg, enabled.11h.reg, us.reg, gpiotype2.reg, BCMIHV.reg.NTamd64
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTamd64, BCMIHV.files.NTamd64
RegisterDlls=BCMIHVUI.regsrv.NTamd64
[BCM43XM2_NT60.NTamd64]
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT60.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bag.reg, hiband.reg, chans.thru64.reg, chans.a.row.reg, chans.thru13.reg, enabled.11h.reg, cc.reg, cc_row.reg, gpiotype1.reg, BCMIHV.reg.NTamd64
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTamd64, BCMIHV.files.NTamd64
RegisterDlls=BCMIHVUI.regsrv.NTamd64
[BCM43XM12_NT60.NTamd64]
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT60.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bag.reg, hiband.reg, chans.thru64.reg, chans.a.row.reg, chans.thru13.reg, enabled.11h.reg, cc.reg, cc_row.reg, gpiotype2.reg, BCMIHV.reg.NTamd64
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTamd64, BCMIHV.files.NTamd64
RegisterDlls=BCMIHVUI.regsrv.NTamd64
[BCM43XNM12_NT60.NTamd64]
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT60.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bagn.reg, hiband.reg, chans.thru64.reg, chans.a.row.reg, chans.thru13.reg, enabled.11h.reg, cc.reg, cc_row.reg, gpiotype2.reg, BCMIHV.reg.NTamd64
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTamd64, BCMIHV.files.NTamd64
RegisterDlls=BCMIHVUI.regsrv.NTamd64
[BCM43XM3_NT60.NTamd64]
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT60.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bag.reg, chans.a.jp.reg, chans.thru14.reg, enabled.11h.reg, jp.reg, gpiotype1.reg, BCMIHV.reg.NTamd64
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTamd64, BCMIHV.files.NTamd64
RegisterDlls=BCMIHVUI.regsrv.NTamd64
[BCM43XM13_NT60.NTamd64]
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT60.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bag.reg, chans.a.jp.reg, chans.thru14.reg, enabled.11h.reg, jp.reg, gpiotype2.reg, BCMIHV.reg.NTamd64
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTamd64, BCMIHV.files.NTamd64
RegisterDlls=BCMIHVUI.regsrv.NTamd64
[BCM43XNM13_NT60.NTamd64]
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT60.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bagn.reg, chans.a.jp.reg, chans.thru14.reg, enabled.11h.reg, jp.reg, gpiotype2.reg, BCMIHV.reg.NTamd64
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTamd64, BCMIHV.files.NTamd64
RegisterDlls=BCMIHVUI.regsrv.NTamd64
[BCM43XM14_NT60.NTamd64]
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT60.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bag.reg, chans.thru64.reg, chans.thru13.reg, enabled.11h.reg, il.reg, gpiotype2.reg, BCMIHV.reg.NTamd64
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTamd64, BCMIHV.files.NTamd64
RegisterDlls=BCMIHVUI.regsrv.NTamd64
[BCM43XNM14_NT60.NTamd64]
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT60.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bagn.reg, chans.thru64.reg, chans.thru13.reg, enabled.11h.reg, il.reg, gpiotype2.reg, BCMIHV.reg.NTamd64
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTamd64, BCMIHV.files.NTamd64
RegisterDlls=BCMIHVUI.regsrv.NTamd64
[BCM43XNM21_NT60.NTamd64]
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT60.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bagn.reg, hiband.reg, chans.thru64.reg, enabled.11h.reg, us.reg, gpiotype2.reg, BCMIHV.reg.NTamd64
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTamd64, BCMIHV.files.NTamd64
RegisterDlls=BCMIHVUI.regsrv.NTamd64
[BCM43XNM22_NT60.NTamd64]
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT60.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bagn.reg, hiband.reg, chans.thru64.reg, chans.a.row.reg, chans.thru13.reg, enabled.11h.reg, cc.reg, cc_row.reg, gpiotype2.reg, BCMIHV.reg.NTamd64
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTamd64, BCMIHV.files.NTamd64
RegisterDlls=BCMIHVUI.regsrv.NTamd64
[BCM43XNG2022_NT60.NTamd64]
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT60.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, gn20.reg, chans.thru13.reg, us.reg, gpiotype2.reg, BCMIHV.reg.NTamd64
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTamd64, BCMIHV.files.NTamd64
RegisterDlls=BCMIHVUI.regsrv.NTamd64
[BCM43XNG22_NT60.NTamd64]
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT60.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, gn.reg, chans.thru13.reg, us.reg, gpiotype2.reg, BCMIHV.reg.NTamd64
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTamd64, BCMIHV.files.NTamd64
RegisterDlls=BCMIHVUI.regsrv.NTamd64
[BCM43XX_NT60.NTamd64.Services]
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTamd64, common.EventLog
[BCM43XG_NT60.NTamd64.Services]
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTamd64, common.EventLog
[BCM43XGT_NT60.NTamd64.Services]
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTamd64, common.EventLog
[BCM43XG1_NT60.NTamd64.Services]
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTamd64, common.EventLog
[BCM43XG2_NT60.NTamd64.Services]
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTamd64, common.EventLog
[BCM43XG3_NT60.NTamd64.Services]
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTamd64, common.EventLog
[BCM43XM1_NT60.NTamd64.Services]
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTamd64, common.EventLog
[BCM43XM2_NT60.NTamd64.Services]
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTamd64, common.EventLog
[BCM43XM3_NT60.NTamd64.Services]
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTamd64, common.EventLog
[BCM43XG11_NT60.NTamd64.Services]
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTamd64, common.EventLog
[BCM43XG12_NT60.NTamd64.Services]
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTamd64, common.EventLog
[BCM43XG13_NT60.NTamd64.Services]
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTamd64, common.EventLog
[BCM43XG14_NT60.NTamd64.Services]
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTamd64, common.EventLog
[BCM43XM11_NT60.NTamd64.Services]
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTamd64, common.EventLog
[BCM43XM12_NT60.NTamd64.Services]
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTamd64, common.EventLog
[BCM43XM13_NT60.NTamd64.Services]
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTamd64, common.EventLog
[BCM43XM14_NT60.NTamd64.Services]
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTamd64, common.EventLog
[BCM43XNM11_NT60.NTamd64.Services]
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTamd64, common.EventLog
[BCM43XNM12_NT60.NTamd64.Services]
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTamd64, common.EventLog
[BCM43XNM13_NT60.NTamd64.Services]
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTamd64, common.EventLog
[BCM43XNM14_NT60.NTamd64.Services]
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTamd64, common.EventLog
[BCM43XNM21_NT60.NTamd64.Services]
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTamd64, common.EventLog
[BCM43XNM22_NT60.NTamd64.Services]
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTamd64, common.EventLog
[BCM43XNG22_NT60.NTamd64.Services]
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTamd64, common.EventLog
[BCM43XNG2022_NT60.NTamd64.Services]
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTamd64, common.EventLog
[BCM43XX_NT60.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XG_NT60.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XGT_NT60.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XG1_NT60.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XG2_NT60.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XG3_NT60.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XM1_NT60.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XM2_NT60.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XM3_NT60.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XG11_NT60.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XG12_NT60.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XG13_NT60.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XG14_NT60.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XM11_NT60.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XM12_NT60.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XM13_NT60.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XM14_NT60.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XNM11_NT60.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XNM12_NT60.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XNM13_NT60.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XNM14_NT60.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XNM21_NT60.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XNM22_NT60.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XNG22_NT60.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XNG2022_NT60.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XG_NT60.NTx86]
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT60.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bg0.reg, bg.loc.reg, g.reg, cc.reg, cc_fixed.reg, gpiotype1.reg, BCMIHV.reg.NTx86
DelReg=common.delreg, common.vista.delreg, rate.delreg
;CpyFiles=BCM43XX_NT60.files.NTx86, BCMIHV.files.NTx86
RegisterDlls=BCMIHVUI.regsrv.NTx86
[BCM43XGT_NT60.NTx86]
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT60.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bg0.reg, bg.loc.reg, g.reg, gt.reg, cc.reg, cc_fixed.reg, gpiotype1.reg, BCMIHV.reg.NTx86
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTx86, BCMIHV.files.NTx86
RegisterDlls=BCMIHVUI.regsrv.NTx86
[BCM43XG1_NT60.NTx86]
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT60.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bg0.reg, bg1.reg, g.reg, us.reg, gpiotype1.reg, BCMIHV.reg.NTx86
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTx86, BCMIHV.files.NTx86
RegisterDlls=BCMIHVUI.regsrv.NTx86
[BCM43XG11_NT60.NTx86]
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT60.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bg0.reg, bg1.reg, g.reg, us.reg, gpiotype2.reg, BCMIHV.reg.NTx86
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTx86, BCMIHV.files.NTx86
RegisterDlls=BCMIHVUI.regsrv.NTx86
[BCM43XG2_NT60.NTx86]
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT60.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bg0.reg, bg.loc.reg, g.reg, cc.reg, cc_row.reg, gpiotype1.reg, BCMIHV.reg.NTx86
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTx86, BCMIHV.files.NTx86
RegisterDlls=BCMIHVUI.regsrv.NTx86
[BCM43XG12_NT60.NTx86]
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT60.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bg0.reg, bg.loc.reg, g.reg, cc.reg, cc_row.reg, gpiotype2.reg, BCMIHV.reg.NTx86
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTx86, BCMIHV.files.NTx86
RegisterDlls=BCMIHVUI.regsrv.NTx86
[BCM43XG3_NT60.NTx86]
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT60.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bg0.reg, bg3.reg, g.reg, jp.reg, gpiotype1.reg, BCMIHV.reg.NTx86
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTx86, BCMIHV.files.NTx86
RegisterDlls=BCMIHVUI.regsrv.NTx86
[BCM43XG13_NT60.NTx86]
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT60.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bg0.reg, bg3.reg, g.reg, jp.reg, gpiotype2.reg, BCMIHV.reg.NTx86
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTx86, BCMIHV.files.NTx86
RegisterDlls=BCMIHVUI.regsrv.NTx86
[BCM43XG14_NT60.NTx86]
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT60.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bg0.reg, bg3.reg, g.reg, il.reg, gpiotype2.reg, BCMIHV.reg.NTx86
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTx86, BCMIHV.files.NTx86
RegisterDlls=BCMIHVUI.regsrv.NTx86
[BCM43XM1_NT60.NTx86]
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT60.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bag.reg, hiband.reg, chans.thru64.reg, enabled.11h.reg, us.reg, gpiotype1.reg, BCMIHV.reg.NTx86
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTx86, BCMIHV.files.NTx86
RegisterDlls=BCMIHVUI.regsrv.NTx86
[BCM43XM11_NT60.NTx86]
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT60.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bag.reg, hiband.reg, chans.thru64.reg, enabled.11h.reg, us.reg, gpiotype2.reg, BCMIHV.reg.NTx86
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTx86, BCMIHV.files.NTx86
RegisterDlls=BCMIHVUI.regsrv.NTx86
[BCM43XNM11_NT60.NTx86]
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT60.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bagn.reg, hiband.reg, chans.thru64.reg, enabled.11h.reg, us.reg, gpiotype2.reg, BCMIHV.reg.NTx86
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTx86, BCMIHV.files.NTx86
RegisterDlls=BCMIHVUI.regsrv.NTx86
[BCM43XM2_NT60.NTx86]
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT60.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bag.reg, hiband.reg, chans.thru64.reg, chans.a.row.reg, chans.thru13.reg, enabled.11h.reg, cc.reg, cc_row.reg, gpiotype1.reg, BCMIHV.reg.NTx86
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTx86, BCMIHV.files.NTx86
RegisterDlls=BCMIHVUI.regsrv.NTx86
[BCM43XM12_NT60.NTx86]
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT60.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bag.reg, hiband.reg, chans.thru64.reg, chans.a.row.reg, chans.thru13.reg, enabled.11h.reg, cc.reg, cc_row.reg, gpiotype2.reg, BCMIHV.reg.NTx86
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTx86, BCMIHV.files.NTx86
RegisterDlls=BCMIHVUI.regsrv.NTx86
[BCM43XNM12_NT60.NTx86]
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT60.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bagn.reg, hiband.reg, chans.thru64.reg, chans.a.row.reg, chans.thru13.reg, enabled.11h.reg, cc.reg, cc_row.reg, gpiotype2.reg, BCMIHV.reg.NTx86
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTx86, BCMIHV.files.NTx86
RegisterDlls=BCMIHVUI.regsrv.NTx86
[BCM43XM3_NT60.NTx86]
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT60.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bag.reg, chans.a.jp.reg, chans.thru14.reg, enabled.11h.reg, jp.reg, gpiotype1.reg, BCMIHV.reg.NTx86
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTx86, BCMIHV.files.NTx86
RegisterDlls=BCMIHVUI.regsrv.NTx86
[BCM43XM13_NT60.NTx86]
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT60.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bag.reg, chans.a.jp.reg, chans.thru14.reg, enabled.11h.reg, jp.reg, gpiotype2.reg, BCMIHV.reg.NTx86
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTx86, BCMIHV.files.NTx86
RegisterDlls=BCMIHVUI.regsrv.NTx86
[BCM43XNM13_NT60.NTx86]
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT60.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bagn.reg, chans.a.jp.reg, chans.thru14.reg, enabled.11h.reg, jp.reg, gpiotype2.reg, BCMIHV.reg.NTx86
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTx86, BCMIHV.files.NTx86
RegisterDlls=BCMIHVUI.regsrv.NTx86
[BCM43XM14_NT60.NTx86]
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT60.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bag.reg, chans.thru64.reg, chans.thru13.reg, enabled.11h.reg, il.reg, gpiotype2.reg, BCMIHV.reg.NTx86
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTx86, BCMIHV.files.NTx86
RegisterDlls=BCMIHVUI.regsrv.NTx86
[BCM43XNM14_NT60.NTx86]
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT60.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bagn.reg, chans.thru64.reg, chans.thru13.reg, enabled.11h.reg, il.reg, gpiotype2.reg, BCMIHV.reg.NTx86
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTx86, BCMIHV.files.NTx86
RegisterDlls=BCMIHVUI.regsrv.NTx86
[BCM43XNM21_NT60.NTx86]
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT60.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bagn.reg, hiband.reg, chans.thru64.reg, enabled.11h.reg, us.reg, gpiotype2.reg, BCMIHV.reg.NTx86
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTx86, BCMIHV.files.NTx86
RegisterDlls=BCMIHVUI.regsrv.NTx86
[BCM43XNM22_NT60.NTx86]
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT60.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, bagn.reg, hiband.reg, chans.thru64.reg, chans.a.row.reg, chans.thru13.reg, enabled.11h.reg, cc.reg, cc_row.reg, gpiotype2.reg, BCMIHV.reg.NTx86
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTx86, BCMIHV.files.NTx86
RegisterDlls=BCMIHVUI.regsrv.NTx86
[BCM43XNG2022_NT60.NTx86]
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT60.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, gn20.reg, chans.thru13.reg, us.reg, gpiotype2.reg, BCMIHV.reg.NTx86
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTx86, BCMIHV.files.NTx86
RegisterDlls=BCMIHVUI.regsrv.NTx86
[BCM43XNG22_NT60.NTx86]
*IfType=71 ; IF_TYPE_IEEE80211
*MediaType=16 ; NdisMediumNative802_11
*PhysicalMediaType=9 ; NdisPhysicalMediumNative802_11
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX_NT60.reg, BCM43XX.brcm.reg, common.reg, common.vista.reg, gn.reg, chans.thru13.reg, us.reg, gpiotype2.reg, BCMIHV.reg.NTx86
DelReg=common.delreg, common.vista.delreg
;CpyFiles=BCM43XX_NT60.files.NTx86, BCMIHV.files.NTx86
RegisterDlls=BCMIHVUI.regsrv.NTx86
[BCM43XX_NT60.NTx86.Services]
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog
[BCM43XG_NT60.NTx86.Services]
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog
[BCM43XGT_NT60.NTx86.Services]
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog
[BCM43XG1_NT60.NTx86.Services]
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog
[BCM43XG2_NT60.NTx86.Services]
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog
[BCM43XG3_NT60.NTx86.Services]
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog
[BCM43XM1_NT60.NTx86.Services]
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog
[BCM43XM2_NT60.NTx86.Services]
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog
[BCM43XM3_NT60.NTx86.Services]
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog
[BCM43XG11_NT60.NTx86.Services]
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog
[BCM43XG12_NT60.NTx86.Services]
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog
[BCM43XG13_NT60.NTx86.Services]
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog
[BCM43XG14_NT60.NTx86.Services]
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog
[BCM43XM11_NT60.NTx86.Services]
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog
[BCM43XM12_NT60.NTx86.Services]
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog
[BCM43XM13_NT60.NTx86.Services]
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog
[BCM43XM14_NT60.NTx86.Services]
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog
[BCM43XNM11_NT60.NTx86.Services]
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog
[BCM43XNM12_NT60.NTx86.Services]
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog
[BCM43XNM13_NT60.NTx86.Services]
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog
[BCM43XNM14_NT60.NTx86.Services]
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog
[BCM43XNM21_NT60.NTx86.Services]
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog
[BCM43XNM22_NT60.NTx86.Services]
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog
[BCM43XNG22_NT60.NTx86.Services]
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog
[BCM43XNG2022_NT60.NTx86.Services]
AddService=BCM43XX, 2, BCM43XX_NT60.Service.NTx86, common.EventLog
[BCM43XX_NT60.NTx86.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XG_NT60.NTx86.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XGT_NT60.NTx86.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XG1_NT60.NTx86.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XG2_NT60.NTx86.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XG3_NT60.NTx86.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XM1_NT60.NTx86.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XM2_NT60.NTx86.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XM3_NT60.NTx86.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XG11_NT60.NTx86.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XG12_NT60.NTx86.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XG13_NT60.NTx86.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XG14_NT60.NTx86.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XM11_NT60.NTx86.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XM12_NT60.NTx86.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XM13_NT60.NTx86.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XM14_NT60.NTx86.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XNM11_NT60.NTx86.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XNM12_NT60.NTx86.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XNM13_NT60.NTx86.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XNM14_NT60.NTx86.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XNM21_NT60.NTx86.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XNM22_NT60.NTx86.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XNG22_NT60.NTx86.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XNG2022_NT60.NTx86.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XG.NTamd64]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, common.prevista.reg, bg0.reg, bg.loc.reg, g.reg, cc.reg, cc_fixed.reg, gpiotype1.reg
DelReg=common.delreg, rate.delreg
;CpyFiles=BCM43XX.files.NTamd64
[BCM43XGT.NTamd64]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, common.prevista.reg, bg0.reg, bg.loc.reg, g.reg, gt.reg, cc.reg, cc_fixed.reg, gpiotype1.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.files.NTamd64
[BCM43XG1.NTamd64]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, common.prevista.reg, bg0.reg, bg1.reg, g.reg, us.reg, gpiotype1.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.files.NTamd64
[BCM43XG11.NTamd64]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, common.prevista.reg, bg0.reg, bg1.reg, g.reg, us.reg, gpiotype2.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.files.NTamd64
[BCM43XG2.NTamd64]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, common.prevista.reg, bg0.reg, bg.loc.reg, g.reg, cc.reg, cc_row.reg, gpiotype1.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.files.NTamd64
[BCM43XG12.NTamd64]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, common.prevista.reg, bg0.reg, bg.loc.reg, g.reg, cc.reg, cc_row.reg, gpiotype2.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.files.NTamd64
[BCM43XG3.NTamd64]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, common.prevista.reg, bg0.reg, bg3.reg, g.reg, jp.reg, gpiotype1.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.files.NTamd64
[BCM43XG13.NTamd64]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, common.prevista.reg, bg0.reg, bg3.reg, g.reg, jp.reg, gpiotype2.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.files.NTamd64
[BCM43XG14.NTamd64]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, common.prevista.reg, bg0.reg, bg3.reg, g.reg, il.reg, gpiotype2.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.files.NTamd64
[BCM43XM1.NTamd64]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, common.prevista.reg, bag.reg, hiband.reg, chans.thru64.reg, enabled.11h.reg, us.reg, gpiotype1.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.files.NTamd64
[BCM43XM11.NTamd64]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, common.prevista.reg, bag.reg, hiband.reg, chans.thru64.reg, enabled.11h.reg, us.reg, gpiotype2.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.files.NTamd64
[BCM43XNM11.NTamd64]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, common.prevista.reg, bagn.reg, hiband.reg, chans.thru64.reg, enabled.11h.reg, us.reg, gpiotype2.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.files.NTamd64
[BCM43XM2.NTamd64]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, common.prevista.reg, bag.reg, hiband.reg, chans.thru64.reg, chans.a.row.reg, chans.thru13.reg, enabled.11h.reg, cc.reg, cc_row.reg, gpiotype1.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.files.NTamd64
[BCM43XM12.NTamd64]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, common.prevista.reg, bag.reg, hiband.reg, chans.thru64.reg, chans.a.row.reg, chans.thru13.reg, enabled.11h.reg, cc.reg, cc_row.reg, gpiotype2.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.files.NTamd64
[BCM43XNM12.NTamd64]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, common.prevista.reg, bagn.reg, hiband.reg, chans.thru64.reg, chans.a.row.reg, chans.thru13.reg, enabled.11h.reg, cc.reg, cc_row.reg, gpiotype2.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.files.NTamd64
[BCM43XM3.NTamd64]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, common.prevista.reg, bag.reg, chans.a.jp.reg, chans.thru14.reg, enabled.11h.reg, jp.reg, gpiotype1.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.files.NTamd64
[BCM43XM13.NTamd64]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, common.prevista.reg, bag.reg, chans.a.jp.reg, chans.thru14.reg, enabled.11h.reg, jp.reg, gpiotype2.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.files.NTamd64
[BCM43XNM13.NTamd64]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, common.prevista.reg, bagn.reg, chans.a.jp.reg, chans.thru14.reg, enabled.11h.reg, jp.reg, gpiotype2.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.files.NTamd64
[BCM43XM14.NTamd64]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, common.prevista.reg, bag.reg, chans.thru64.reg, chans.thru13.reg, enabled.11h.reg, il.reg, gpiotype2.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.files.NTamd64
[BCM43XNM14.NTamd64]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, common.prevista.reg, bagn.reg, chans.thru64.reg, chans.thru13.reg, enabled.11h.reg, il.reg, gpiotype2.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.files.NTamd64
[BCM43XNM21.NTamd64]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, common.prevista.reg, bagn.reg, hiband.reg, chans.thru64.reg, enabled.11h.reg, us.reg, gpiotype2.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.files.NTamd64
[BCM43XNM22.NTamd64]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, common.prevista.reg, bagn.reg, hiband.reg, chans.thru64.reg, chans.a.row.reg, chans.thru13.reg, enabled.11h.reg, cc.reg, cc_row.reg, gpiotype2.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.files.NTamd64
[BCM43XNG2022.NTamd64]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, common.prevista.reg, gn20.reg, us.reg, chans.thru13.reg, gpiotype2.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.files.NTamd64
[BCM43XNG22.NTamd64]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, common.prevista.reg, gn.reg, us.reg, chans.thru13.reg, gpiotype2.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.files.NTamd64
[BCM43XG.NTamd64.Services]
AddService=BCM43XX, 2, BCM43XX.Service.NTamd64, common.EventLog
[BCM43XGT.NTamd64.Services]
AddService=BCM43XX, 2, BCM43XX.Service.NTamd64, common.EventLog
[BCM43XG1.NTamd64.Services]
AddService=BCM43XX, 2, BCM43XX.Service.NTamd64, common.EventLog
[BCM43XG2.NTamd64.Services]
AddService=BCM43XX, 2, BCM43XX.Service.NTamd64, common.EventLog
[BCM43XG3.NTamd64.Services]
AddService=BCM43XX, 2, BCM43XX.Service.NTamd64, common.EventLog
[BCM43XM1.NTamd64.Services]
AddService=BCM43XX, 2, BCM43XX.Service.NTamd64, common.EventLog
[BCM43XM2.NTamd64.Services]
AddService=BCM43XX, 2, BCM43XX.Service.NTamd64, common.EventLog
[BCM43XM3.NTamd64.Services]
AddService=BCM43XX, 2, BCM43XX.Service.NTamd64, common.EventLog
[BCM43XG11.NTamd64.Services]
AddService=BCM43XX, 2, BCM43XX.Service.NTamd64, common.EventLog
[BCM43XG12.NTamd64.Services]
AddService=BCM43XX, 2, BCM43XX.Service.NTamd64, common.EventLog
[BCM43XG13.NTamd64.Services]
AddService=BCM43XX, 2, BCM43XX.Service.NTamd64, common.EventLog
[BCM43XG14.NTamd64.Services]
AddService=BCM43XX, 2, BCM43XX.Service.NTamd64, common.EventLog
[BCM43XM11.NTamd64.Services]
AddService=BCM43XX, 2, BCM43XX.Service.NTamd64, common.EventLog
[BCM43XM12.NTamd64.Services]
AddService=BCM43XX, 2, BCM43XX.Service.NTamd64, common.EventLog
[BCM43XM13.NTamd64.Services]
AddService=BCM43XX, 2, BCM43XX.Service.NTamd64, common.EventLog
[BCM43XM14.NTamd64.Services]
AddService=BCM43XX, 2, BCM43XX.Service.NTamd64, common.EventLog
[BCM43XNM11.NTamd64.Services]
AddService=BCM43XX, 2, BCM43XX.Service.NTamd64, common.EventLog
[BCM43XNM12.NTamd64.Services]
AddService=BCM43XX, 2, BCM43XX.Service.NTamd64, common.EventLog
[BCM43XNM13.NTamd64.Services]
AddService=BCM43XX, 2, BCM43XX.Service.NTamd64, common.EventLog
[BCM43XNM14.NTamd64.Services]
AddService=BCM43XX, 2, BCM43XX.Service.NTamd64, common.EventLog
[BCM43XNM21.NTamd64.Services]
AddService=BCM43XX, 2, BCM43XX.Service.NTamd64, common.EventLog
[BCM43XNM22.NTamd64.Services]
AddService=BCM43XX, 2, BCM43XX.Service.NTamd64, common.EventLog
[BCM43XNG22.NTamd64.Services]
AddService=BCM43XX, 2, BCM43XX.Service.NTamd64, common.EventLog
[BCM43XNG2022.NTamd64.Services]
AddService=BCM43XX, 2, BCM43XX.Service.NTamd64, common.EventLog
[BCM43XG.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XGT.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XG1.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XG2.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XG3.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XM1.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XM2.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XM3.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XG11.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XG12.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XG13.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XG14.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XM11.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XM12.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XM13.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XM14.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XNM11.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XNM12.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XNM13.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XNM14.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XNM21.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XNM22.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XNG22.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XNG2022.NTamd64.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTamd64
AddReg=CoInstallers.AddReg
[BCM43XG.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, common.prevista.reg, bg0.reg, bg.loc.reg, g.reg, cc.reg, cc_fixed.reg, gpiotype1.reg
DelReg=common.delreg, rate.delreg
;CpyFiles=BCM43XX.files.NT
[BCM43XGT.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, common.prevista.reg, bg0.reg, bg.loc.reg, g.reg, gt.reg, cc.reg, cc_fixed.reg, gpiotype1.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.files.NT
[BCM43XG1.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, common.prevista.reg, bg0.reg, bg1.reg, g.reg, us.reg, gpiotype1.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.files.NT
[BCM43XG11.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, common.prevista.reg, bg0.reg, bg1.reg, g.reg, us.reg, gpiotype2.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.files.NT
[BCM43XG2.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, common.prevista.reg, bg0.reg, bg.loc.reg, g.reg, cc.reg, cc_row.reg, gpiotype1.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.files.NT
[BCM43XG12.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, common.prevista.reg, bg0.reg, bg.loc.reg, g.reg, cc.reg, cc_row.reg, gpiotype2.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.files.NT
[BCM43XG3.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, common.prevista.reg, bg0.reg, bg3.reg, g.reg, jp.reg, gpiotype1.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.files.NT
[BCM43XG13.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, common.prevista.reg, bg0.reg, bg3.reg, g.reg, jp.reg, gpiotype2.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.files.NT
[BCM43XG14.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, common.prevista.reg, bg0.reg, bg3.reg, g.reg, il.reg, gpiotype2.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.files.NT
[BCM43XM1.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, common.prevista.reg, bag.reg, hiband.reg, chans.thru64.reg, enabled.11h.reg, us.reg, gpiotype1.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.files.NT
[BCM43XM11.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, common.prevista.reg, bag.reg, hiband.reg, chans.thru64.reg, enabled.11h.reg, us.reg, gpiotype2.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.files.NT
[BCM43XNM11.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, common.prevista.reg, bagn.reg, hiband.reg, chans.thru64.reg, enabled.11h.reg, us.reg, gpiotype2.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.files.NT
[BCM43XM2.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, common.prevista.reg, bag.reg, hiband.reg, chans.thru64.reg, chans.a.row.reg, chans.thru13.reg, enabled.11h.reg, cc.reg, cc_row.reg, gpiotype1.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.files.NT
[BCM43XM12.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, common.prevista.reg, bag.reg, hiband.reg, chans.thru64.reg, chans.a.row.reg, chans.thru13.reg, enabled.11h.reg, cc.reg, cc_row.reg, gpiotype2.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.files.NT
[BCM43XNM12.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, common.prevista.reg, bagn.reg, hiband.reg, chans.thru64.reg, chans.a.row.reg, chans.thru13.reg, enabled.11h.reg, cc.reg, cc_row.reg, gpiotype2.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.files.NT
[BCM43XM3.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, common.prevista.reg, bag.reg, chans.a.jp.reg, chans.thru14.reg, enabled.11h.reg, jp.reg, gpiotype1.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.files.NT
[BCM43XM13.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, common.prevista.reg, bag.reg, chans.a.jp.reg, chans.thru14.reg, enabled.11h.reg, jp.reg, gpiotype2.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.files.NT
[BCM43XNM13.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, common.prevista.reg, bagn.reg, chans.a.jp.reg, chans.thru14.reg, enabled.11h.reg, jp.reg, gpiotype2.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.files.NT
[BCM43XM14.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, common.prevista.reg, bag.reg, chans.thru64.reg, chans.thru13.reg, enabled.11h.reg, il.reg, gpiotype2.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.files.NT
[BCM43XNM14.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, common.prevista.reg, bagn.reg, chans.thru64.reg, chans.thru13.reg, enabled.11h.reg, il.reg, gpiotype2.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.files.NT
[BCM43XNM21.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, common.prevista.reg, bagn.reg, hiband.reg, chans.thru64.reg, enabled.11h.reg, us.reg, gpiotype2.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.files.NT
[BCM43XNM22.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, common.prevista.reg, bagn.reg, hiband.reg, chans.thru64.reg, chans.a.row.reg, chans.thru13.reg, enabled.11h.reg, cc.reg, cc_row.reg, gpiotype2.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.files.NT
[BCM43XNG2022.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, common.prevista.reg, gn20.reg, us.reg, chans.thru13.reg, gpiotype2.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.files.NT
[BCM43XNG22.NT]
Characteristics=0x84 ; NCF_PHYSICAL | NCF_HAS_UI
BusType=5 ; PCI bus
AddReg=BCM43XX.reg, BCM43XX.brcm.reg, common.reg, common.prevista.reg, gn.reg, us.reg, chans.thru13.reg, gpiotype2.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.files.NT
[BCM43XG.NT.Services]
AddService=BCM43XX, 2, BCM43XX.Service.NT, common.EventLog
[BCM43XGT.NT.Services]
AddService=BCM43XX, 2, BCM43XX.Service.NT, common.EventLog
[BCM43XG1.NT.Services]
AddService=BCM43XX, 2, BCM43XX.Service.NT, common.EventLog
[BCM43XG2.NT.Services]
AddService=BCM43XX, 2, BCM43XX.Service.NT, common.EventLog
[BCM43XG3.NT.Services]
AddService=BCM43XX, 2, BCM43XX.Service.NT, common.EventLog
[BCM43XM1.NT.Services]
AddService=BCM43XX, 2, BCM43XX.Service.NT, common.EventLog
[BCM43XM2.NT.Services]
AddService=BCM43XX, 2, BCM43XX.Service.NT, common.EventLog
[BCM43XM3.NT.Services]
AddService=BCM43XX, 2, BCM43XX.Service.NT, common.EventLog
[BCM43XG11.NT.Services]
AddService=BCM43XX, 2, BCM43XX.Service.NT, common.EventLog
[BCM43XG12.NT.Services]
AddService=BCM43XX, 2, BCM43XX.Service.NT, common.EventLog
[BCM43XG13.NT.Services]
AddService=BCM43XX, 2, BCM43XX.Service.NT, common.EventLog
[BCM43XG14.NT.Services]
AddService=BCM43XX, 2, BCM43XX.Service.NT, common.EventLog
[BCM43XM11.NT.Services]
AddService=BCM43XX, 2, BCM43XX.Service.NT, common.EventLog
[BCM43XM12.NT.Services]
AddService=BCM43XX, 2, BCM43XX.Service.NT, common.EventLog
[BCM43XM13.NT.Services]
AddService=BCM43XX, 2, BCM43XX.Service.NT, common.EventLog
[BCM43XM14.NT.Services]
AddService=BCM43XX, 2, BCM43XX.Service.NT, common.EventLog
[BCM43XNM11.NT.Services]
AddService=BCM43XX, 2, BCM43XX.Service.NT, common.EventLog
[BCM43XNM12.NT.Services]
AddService=BCM43XX, 2, BCM43XX.Service.NT, common.EventLog
[BCM43XNM13.NT.Services]
AddService=BCM43XX, 2, BCM43XX.Service.NT, common.EventLog
[BCM43XNM14.NT.Services]
AddService=BCM43XX, 2, BCM43XX.Service.NT, common.EventLog
[BCM43XNM21.NT.Services]
AddService=BCM43XX, 2, BCM43XX.Service.NT, common.EventLog
[BCM43XNM22.NT.Services]
AddService=BCM43XX, 2, BCM43XX.Service.NT, common.EventLog
[BCM43XNG22.NT.Services]
AddService=BCM43XX, 2, BCM43XX.Service.NT, common.EventLog
[BCM43XNG2022.NT.Services]
AddService=BCM43XX, 2, BCM43XX.Service.NT, common.EventLog
[BCM43XG.NT.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XGT.NT.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XG1.NT.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XG2.NT.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XG3.NT.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XM1.NT.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XM2.NT.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XM3.NT.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XG11.NT.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XG12.NT.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XG13.NT.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XG14.NT.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XM11.NT.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XM12.NT.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XM13.NT.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XM14.NT.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XNM11.NT.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XNM12.NT.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XNM13.NT.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XNM14.NT.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XNM21.NT.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XNM22.NT.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XNG22.NT.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XNG2022.NT.CoInstallers]
;CpyFiles=CoInstall.CopyFiles.NTx86
AddReg=CoInstallers.AddReg
[BCM43XX_NT61.reg]
HKR, Ndi\Interfaces, UpperRange, , "ndis5"
HKR, Ndi\Interfaces, LowerRange, , "ethernet,wlan,vwifi"
[BCM43XX_NT60.reg]
HKR, Ndi\Interfaces, UpperRange, , "ndis5"
HKR, Ndi\Interfaces, LowerRange, , "ethernet,wlan"
[BCM43XX.reg]
HKR, Ndi\Interfaces, UpperRange, , "ndis5"
HKR, Ndi\Interfaces, LowerRange, , "ethernet"
[BCM43XX.brcm.reg]
HKR, Ndi, HelpText, , %BCM43XX_HELP%
HKR, Ndi, Service, 0, "BCM43XX"
[common.EventLog]
AddReg=common.AddEventLog.reg
[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported, 0x00010001, 7
[BCM43XG]
AddReg=BCM43XX.win.reg, BCM43XX.hlp.reg, common.reg, common.prevista.reg, bg0.reg, bg.loc.reg, g.reg, cc.reg, cc_fixed.reg, gpiotype1.reg
DelReg=common.delreg, rate.delreg
;CpyFiles=BCM43XX.sys.files
[BCM43XGT]
AddReg=BCM43XX.win.reg, BCM43XX.hlp.reg, common.reg, common.prevista.reg, bg0.reg, bg.loc.reg, g.reg, gt.reg, cc.reg, cc_fixed.reg, gpiotype1.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.sys.files
[BCM43XG1]
AddReg=BCM43XX.win.reg, BCM43XX.hlp.reg, common.reg, common.prevista.reg, bg0.reg, bg1.reg, g.reg, us.reg, gpiotype1.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.sys.files
[BCM43XG11]
AddReg=BCM43XX.win.reg, BCM43XX.hlp.reg, common.reg, common.prevista.reg, bg0.reg, bg1.reg, g.reg, us.reg, gpiotype2.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.sys.files
[BCM43XG2]
AddReg=BCM43XX.win.reg, BCM43XX.hlp.reg, common.reg, common.prevista.reg, bg0.reg, bg.loc.reg, g.reg, cc.reg, cc_row.reg, gpiotype1.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.sys.files
[BCM43XG12]
AddReg=BCM43XX.win.reg, BCM43XX.hlp.reg, common.reg, common.prevista.reg, bg0.reg, bg.loc.reg, g.reg, cc.reg, cc_row.reg, gpiotype2.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.sys.files
[BCM43XG3]
AddReg=BCM43XX.win.reg, BCM43XX.hlp.reg, common.reg, common.prevista.reg, bg0.reg, bg3.reg, g.reg, jp.reg, gpiotype1.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.sys.files
[BCM43XG13]
AddReg=BCM43XX.win.reg, BCM43XX.hlp.reg, common.reg, common.prevista.reg, bg0.reg, bg3.reg, g.reg, jp.reg, gpiotype2.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.sys.files
[BCM43XG14]
AddReg=BCM43XX.win.reg, BCM43XX.hlp.reg, common.reg, common.prevista.reg, bg0.reg, bg3.reg, g.reg, il.reg, gpiotype2.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.sys.files
[BCM43XM1]
AddReg=BCM43XX.win.reg, BCM43XX.hlp.reg, common.reg, common.prevista.reg, bag.reg, hiband.reg, chans.thru64.reg, enabled.11h.reg, us.reg, gpiotype1.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.sys.files
[BCM43XM11]
AddReg=BCM43XX.win.reg, BCM43XX.hlp.reg, common.reg, common.prevista.reg, bag.reg, hiband.reg, chans.thru64.reg, enabled.11h.reg, us.reg, gpiotype2.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.sys.files
[BCM43XNM11]
AddReg=BCM43XX.win.reg, BCM43XX.hlp.reg, common.reg, common.prevista.reg, bagn.reg, hiband.reg, chans.thru64.reg, enabled.11h.reg, us.reg, gpiotype2.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.sys.files
[BCM43XM2]
AddReg=BCM43XX.win.reg, BCM43XX.hlp.reg, common.reg, common.prevista.reg, bag.reg, hiband.reg, chans.thru64.reg, chans.a.row.reg, chans.thru13.reg, enabled.11h.reg, cc.reg, cc_row.reg, gpiotype1.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.sys.files
[BCM43XM12]
AddReg=BCM43XX.win.reg, BCM43XX.hlp.reg, common.reg, common.prevista.reg, bag.reg, hiband.reg, chans.thru64.reg, chans.a.row.reg, chans.thru13.reg, enabled.11h.reg, cc.reg, cc_row.reg, gpiotype2.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.sys.files
[BCM43XNM12]
AddReg=BCM43XX.win.reg, BCM43XX.hlp.reg, common.reg, common.prevista.reg, bagn.reg, hiband.reg, chans.thru64.reg, chans.a.row.reg, chans.thru13.reg, enabled.11h.reg, cc.reg, cc_row.reg, gpiotype2.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.sys.files
[BCM43XM3]
AddReg=BCM43XX.win.reg, BCM43XX.hlp.reg, common.reg, common.prevista.reg, bag.reg, chans.a.jp.reg, chans.thru14.reg, enabled.11h.reg, jp.reg, gpiotype1.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.sys.files
[BCM43XM13]
AddReg=BCM43XX.win.reg, BCM43XX.hlp.reg, common.reg, common.prevista.reg, bag.reg, chans.a.jp.reg, chans.thru14.reg, enabled.11h.reg, jp.reg, gpiotype2.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.sys.files
[BCM43XNM13]
AddReg=BCM43XX.win.reg, BCM43XX.hlp.reg, common.reg, common.prevista.reg, bagn.reg, chans.a.jp.reg, chans.thru14.reg, enabled.11h.reg, jp.reg, gpiotype2.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.sys.files
[BCM43XM14]
AddReg=BCM43XX.win.reg, BCM43XX.hlp.reg, common.reg, common.prevista.reg, bag.reg, chans.thru64.reg, chans.thru13.reg, enabled.11h.reg, il.reg, gpiotype2.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.sys.files
[BCM43XNM14]
AddReg=BCM43XX.win.reg, BCM43XX.hlp.reg, common.reg, common.prevista.reg, bagn.reg, chans.thru64.reg, chans.thru13.reg, enabled.11h.reg, il.reg, gpiotype2.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.sys.files
[BCM43XNM21]
AddReg=BCM43XX.win.reg, BCM43XX.hlp.reg, common.reg, common.prevista.reg, bagn.reg, hiband.reg, chans.thru64.reg, enabled.11h.reg, us.reg, gpiotype2.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.sys.files
[BCM43XNM22]
AddReg=BCM43XX.win.reg, BCM43XX.hlp.reg, common.reg, common.prevista.reg, bagn.reg, hiband.reg, chans.thru64.reg, chans.a.row.reg, chans.thru13.reg, enabled.11h.reg, cc.reg, cc_row.reg, gpiotype2.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.sys.files
[BCM43XNG2022]
AddReg=BCM43XX.win.reg, BCM43XX.hlp.reg, common.reg, common.prevista.reg, gn20.reg, us.reg, chans.thru13.reg, gpiotype2.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.sys.files
[BCM43XNG22]
AddReg=BCM43XX.win.reg, BCM43XX.hlp.reg, common.reg, common.prevista.reg, gn.reg, us.reg, chans.thru13.reg, gpiotype2.reg
DelReg=common.delreg
;CpyFiles=BCM43XX.sys.files
[BCM43XX.win.reg]
HKR, Ndi, DeviceID, , "PCI\VEN_14E4&DEV_4307"
HKR, , EnumPropPages, 0, "netdi.dll,EnumPropPages"
HKR, NDIS, MajorNdisVersion, 1, 03
HKR, NDIS, MinorNdisVersion, 1, 0A
HKR, NDIS, LogDriverName, , "BCM43XX"
HKR, NDIS, MajorDriverVersion, 1, 1
HKR, NDIS, MinorDriverVersion, 1, 0
HKR, Ndi\Install, , , "BCM43XX.ndi.install"
HKR, Ndi\Interfaces, DefUpper, 0, "ndis3"
HKR, Ndi\Interfaces, DefLower, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis3"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
[BCM43XX.hlp.reg]
HKR, Ndi, HelpText, , %BCM43XX_HELP%
[BCM43XX.ndi.install]
AddReg=BCM43XX.ndi.reg
[BCM43XX.ndi.reg]
HKR, , DevLoader, 0, "*ndis"
HKR, , DeviceVxDs, 0, "BCMWL5.SYS"
[BCM43XX_NT60.Service.NTamd64]
DisplayName=%BCM43XX_Service_DispName%
ServiceType=1 ; %SERVICE_KERNEL_DRIVER%
StartType=3 ; %SERVICE_DEMAND_START%
ErrorControl=1 ; %SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\bcmwl664.sys
LoadOrderGroup=NDIS
[BCM43XX_NT60.Service.NTx86]
DisplayName=%BCM43XX_Service_DispName%
ServiceType=1 ; %SERVICE_KERNEL_DRIVER%
StartType=3 ; %SERVICE_DEMAND_START%
ErrorControl=1 ; %SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\bcmwl6.sys
LoadOrderGroup=NDIS
[BCM43XX.Service.NTamd64]
DisplayName=%BCM43XX_Service_DispName%
ServiceType=1 ; %SERVICE_KERNEL_DRIVER%
StartType=3 ; %SERVICE_DEMAND_START%
ErrorControl=1 ; %SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\bcmwl564.sys
LoadOrderGroup=NDIS
[BCM43XX.Service.NT]
DisplayName=%BCM43XX_Service_DispName%
ServiceType=1 ; %SERVICE_KERNEL_DRIVER%
StartType=3 ; %SERVICE_DEMAND_START%
ErrorControl=1 ; %SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\bcmwl5.sys
LoadOrderGroup=NDIS
[BCM43XX.Service]
DisplayName=%BCM43XX_Service_DispName%
ServiceType=1 ; %SERVICE_KERNEL_DRIVER%
StartType=3 ; %SERVICE_DEMAND_START%
ErrorControl=1 ; %SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\bcmwl5.sys
LoadOrderGroup=NDIS
[BCM43XX_NT60.files.NTamd64]
BCMWL664.SYS,,,6
[BCM43XX_NT60.files.NTx86]
BCMWL6.SYS,,,6
[BCM43XX.files.NTamd64]
[BCM43XX.files.NT]
[BCM43XX.sys.files]
[BCMIHV.files.NTamd64]
bcmihvsrv64.dll,,,6
bcmihvui64.dll,,,6
[BCMIHV.files.NTx86]
[BCMIHVUI.regsrv.NTamd64]
11,,bcmihvui64.dll,1
[BCMIHVUI.regsrv.NTx86]
[CoInstall.CopyFiles.NTamd64]
[CoInstall.CopyFiles.NTx86]
[CoInstallers.AddReg]
[DestinationDirs]
DefaultDestDir=11
BCM43XX.sys.files=11
BCM43XX.files.NT=12
BCM43XX.files.NTamd64=12
BCM43XX_NT60.files.NTx86=12
BCM43XX_NT60.files.NTamd64=12
BCMIHV.files.NTx86=11
BCMIHV.files.NTamd64=11
CoInstall.CopyFiles.NTamd64=11
CoInstall.CopyFiles.NTx86=11
[SourceDisksNames]
1=%BCM43XX_DiskName%,,
[SourceDisksFiles.amd64]
bcmwl664.sys=1
bcmihvsrv64.dll=1
bcmihvui64.dll=1
bcmwlcoi64.dll=1
[SourceDisksFiles.x86]
bcmwl6.sys=1
[SourceDisksFiles]
bcmwl6.sys=1
[Cleanup]
UnregisterDlls=BCMIHVUI.regsrv.NTamd64, BCMIHVUI.regsrv.NTx86
;DlFiles=BCMIHV.files.NTamd64, BCMIHV.files.NTx86
[common.vista.delreg]
HKR,,"MPC"
HKR, Ndi\params\vlan_mode
HKR,,vlan_mode
HKR, Ndi\params\PowerSaveMode
[common.delreg]
HKR,,"gpiotimerval"
HKR,,"gpio3"
HKR,,"gpio2"
HKR,,"gpio1"
HKR,,"gpio0"
HKR, Ndi\params\Locale
HKR,,Locale
HKR, Ndi\params\Country
HKR,,Country
HKR, Ndi\params\Channel
HKR,,Channel
HKR, Ndi\params\Chanspec
HKR,,Chanspec
HKR, Ndi\params\BTCoexist
HKR,,BTCoexist
HKR, Ndi\params\AssocPref
HKR, Ndi\params\RoamPref
HKR, Ndi\params\RoamTrigger
HKR, Ndi\params\WME
HKR, Ndi\params\MixedCell
HKR,,"abcap"
HKR, Ndi\params\IBSSGMode
HKR,,IBSSGMode
HKR, Ndi\params\IBSSMode
HKR, Ndi\params\IBSSGProtection
HKR, Ndi\params\WZCCoexist
HKR, Ndi\params\BtAmp
HKLM, Software\Broadcom\802.11,"SupportedApps"
[rate.delreg]
HKR, Ndi\params\Rate
HKR, Ndi\params\RateA
[BCMIHV.reg.NTamd64]
HKR, Ndi\IHVExtensions, ExtensibilityDLL, 0, "%%SystemRoot%%\System32\bcmihvsrv64.dll"
HKR, Ndi\IHVExtensions, UIExtensibilityCLSID, 0, "{AAA6DEE9-31B9-4f18-AB39-82EF9B06EB73}"
HKR, Ndi\IHVExtensions, AdapterOUI, 0x00010001, 0x001018
[BCMIHV.reg.NTx86]
HKR, Ndi\IHVExtensions, UIExtensibilityCLSID, 0, "{AAA6DEE9-31B9-4f18-AB39-82EF9B06EB73}"
HKR, Ndi\IHVExtensions, AdapterOUI, 0x00010001, 0x001018
[common.vista.reg]
HKR, Ndi\params\*PriorityVLANTag, ParamDesc, 0, %PriorityVLANTag%
HKR, Ndi\params\*PriorityVLANTag, type, 0, "enum"
HKR, Ndi\params\*PriorityVLANTag\enum, "0", 0, %PriorityAndVLANDisabled%
HKR, Ndi\params\*PriorityVLANTag\enum, "1", 0, %PriorityEnabled%
HKR, Ndi\params\*PriorityVLANTag\enum, "2", 0, %VLANEnabled%
HKR, Ndi\params\*PriorityVLANTag\enum, "3", 0, %PriorityAndVLANEnabled%
HKR, Ndi\params\*PriorityVLANTag,default,,"0"
HKR, Ndi\params\*PriorityVLANTag,optional,,"0"
HKR, ,"PowerSaveMode", 0, "2"
HKR, ,"MPC", 0, "1"
[common.prevista.reg]
HKR, Ndi\params\ssid_auto_promote, ParamDesc, 0, %SSIDAutoPromote%
HKR, Ndi\params\ssid_auto_promote, type, 0, "enum"
HKR, Ndi\params\ssid_auto_promote\enum, "0", 0, %Disabled%
HKR, Ndi\params\ssid_auto_promote\enum, "1", 0, %Enabled%
HKR, Ndi\params\ssid_auto_promote,default,,"0"
HKR, ,"Managed", 0, "1"
HKR, Ndi\params\vlan_mode, ParamDesc,0, %vlan_mode%
HKR, Ndi\params\vlan_mode, type, 0, "enum"
HKR, Ndi\params\vlan_mode\enum, "-1",0, %Auto%
HKR, Ndi\params\vlan_mode\enum, "1", 0, %Enabled%
HKR, Ndi\params\vlan_mode\enum, "0", 0, %Disabled%
HKR, Ndi\params\vlan_mode,default,,"-1"
HKR, Ndi\params\PowerSaveMode, ParamDesc, 0, %PowerSaveMode%
HKR, Ndi\params\PowerSaveMode, type, 0, "enum"
HKR, Ndi\params\PowerSaveMode\enum, "0", 0, %Disabled%
HKR, Ndi\params\PowerSaveMode\enum, "1", 0, %MaxPowerSavings%
HKR, Ndi\params\PowerSaveMode\enum, "2", 0, %HighPerformance%
HKR, Ndi\params\PowerSaveMode,default,,"2"
[common.reg]
HKR, Ndi\params\frag, ParamDesc, 0, %FragmentationThreshold%
HKR, Ndi\params\frag,type,0,"dword"
HKR, Ndi\params\frag,min,,"256"
HKR, Ndi\params\frag,max,,"2346"
HKR, Ndi\params\frag,default,,"2346"
HKR, Ndi\params\rts, ParamDesc, 0, %RTSThreshold%
HKR, Ndi\params\rts,type,0,"dword"
HKR, Ndi\params\rts,min,,"0"
HKR, Ndi\params\rts,max,,"2347"
HKR, Ndi\params\rts,default,,"2347"
HKR, Ndi\params\MPC, ParamDesc, 0, %MinimumPowerConsumption%
HKR, Ndi\params\MPC, type, 0, "enum"
HKR, Ndi\params\MPC\enum, "0", 0, %Disabled%
HKR, Ndi\params\MPC\enum, "1", 0, %Enabled%
HKR, Ndi\params\MPC,default,,"1"
HKR, Ndi\params\RoamDelta, ParamDesc, 0, %RoamingTendency%
HKR, Ndi\params\RoamDelta, type, 0, "enum"
HKR, Ndi\params\RoamDelta\enum, "0", 0, %Aggressive%
HKR, Ndi\params\RoamDelta\enum, "1", 0, %Moderate%
HKR, Ndi\params\RoamDelta\enum, "2", 0, %Conservative%
HKR, Ndi\params\RoamDelta,default,,"1"
HKR, Ndi\params\NetworkAddress, ParamDesc, 0, %LocallyAdministeredMACAddress%
HKR, Ndi\params\NetworkAddress, type, 0, "edit"
HKR, Ndi\params\NetworkAddress, LimitText, 0, "12"
HKR, Ndi\params\NetworkAddress, UpperCase, 0, "1"
HKR, Ndi\params\NetworkAddress, default, 0, ""
HKR, Ndi\params\NetworkAddress, optional, 0, "1"
HKR, Ndi\params\PwrOut, ParamDesc, 0, %PowerOutput%
HKR, Ndi\params\PwrOut, type, 0, "enum"
HKR, Ndi\params\PwrOut\enum, "100", 0, "100%"
HKR, Ndi\params\PwrOut\enum, "75", 0, "75%"
HKR, Ndi\params\PwrOut\enum, "50", 0, "50%"
HKR, Ndi\params\PwrOut\enum, "25", 0, "25%"
HKR, Ndi\params\PwrOut,default,,"100"
HKR, Ndi\params\FrameBursting, ParamDesc, 0, %XPress_Technology%
HKR, Ndi\params\FrameBursting, type, 0, "enum"
HKR, Ndi\params\FrameBursting\enum, "0", 0, %Disabled%
HKR, Ndi\params\FrameBursting\enum, "1", 0, %Enabled%
HKR, Ndi\params\FrameBursting,default,,"1"
HKR, Ndi\params\BTCoexist, ParamDesc, 0, %BlueToothCollaboration%
HKR, Ndi\params\BTCoexist, type, 0, "enum"
HKR, Ndi\params\BTCoexist\enum, "0", 0, %Disable%
HKR, Ndi\params\BTCoexist\enum, "1", 0, %Enable%
HKR, Ndi\params\BTCoexist\enum, "3", 0, %Auto%
HKR, Ndi\params\BTCoexist,default,,"3"
HKR, ,"EnableSoftAP", 0, "0"
HKR, ,"EnableAutoConnect", 0, "0"
HKR, ,"leddc", 0, "0xa0000"
HKR, ,"WEP", 0, ""
HKR, ,"NetworkType", 0, "-1"
HKR, ,"SSID", 0, ""
HKR, ,"scan_channel_time", 0, "-1"
HKR, ,"scan_unassoc_time", 0, "-1"
HKR, ,"scan_home_time", 0, "-1"
HKR, ,"scan_passes", 0, "-1"
HKR, ,"BadFramePreempt", 0, "0"
HKR, ,"Interference_Mode", 0, "-1"
HKR, ,"Chanspec", 0, "11"
HKR, ,"ccx_rm", 0, "1"
HKR, ,"ccx_rm_limit", 0, "300"
HKR, ,"IBSSMode", 0, "0"
HKR, ,"EFCEnable", 0, "0"
HKR, Ndi\params\WME, ParamDesc, 0, %WME%
HKR, Ndi\params\WME, type, 0, "enum"
HKR, Ndi\params\WME\enum, "-1", 0, %Auto%
HKR, Ndi\params\WME\enum, "1", 0, %Enabled%
HKR, Ndi\params\WME\enum, "0", 0, %Disabled%
HKR, Ndi\params\WME,default,,"-1"
HKR, ,"WME",0,"-1"
HKR, Ndi\params\MixedCell, ParamDesc,0, %MixedCell%
HKR, Ndi\params\MixedCell, type, 0, "enum"
HKR, Ndi\params\MixedCell\enum, "0", 0, %Disabled%
HKR, Ndi\params\MixedCell\enum, "1", 0, %Enabled%
HKR, Ndi\params\MixedCell,default,,"0"
HKR, Ndi\params\BtAmp, ParamDesc, 0, "BT-AMP"
HKR, Ndi\params\BtAmp, type, 0, "enum"
HKR, Ndi\params\BtAmp\enum, "0", 0, %Disabled%
HKR, Ndi\params\BtAmp\enum, "1", 0, %Enabled%
HKR, Ndi\params\BtAmp,default,,"1"
[us.reg]
HKR, Ndi\params\Country, ParamDesc, 0, %Location%
HKR, Ndi\params\Country, type, 0, "enum"
HKR, Ndi\params\Country, default, 0, "US"
HKR, ,"Country", 0, "US"
HKR, Ndi\params\Country\enum, "US", 0, %UnitedStates%
[jp.reg]
HKR, Ndi\params\Country, ParamDesc, 0, %Location%
HKR, Ndi\params\Country, type, 0, "enum"
HKR, Ndi\params\Country, default, 0, "JP"
HKR, ,"Country", 0, "JP"
HKR, Ndi\params\Country\enum, "JP", 0, %Japan%
[il.reg]
HKR, Ndi\params\Country, ParamDesc, 0, %Location%
HKR, Ndi\params\Country, type, 0, "enum"
HKR, Ndi\params\Country, default, 0, "IL"
HKR, ,"Country", 0, "IL"
HKR, Ndi\params\Country\enum, "IL", 0, %Israel%
[cc.reg]
HKR, Ndi\params\Country, ParamDesc, 0, %Location%
HKR, Ndi\params\Country, type, 0, "enum"
HKR, Ndi\params\Country, default, 0, %CountryCode%
HKR, ,"Country", 0, %CountryCode%
[cc_fixed.reg]
HKR, Ndi\params\Country\enum, "XX", 0, %CountryCode%
[cc_row.reg]
HKR, Ndi\params\Country\enum, "AG", 0, %AntiguaandBarbuda%
HKR, Ndi\params\Country\enum, "AR", 0, %Argentina%
HKR, Ndi\params\Country\enum, "AW", 0, %Aruba%
HKR, Ndi\params\Country\enum, "AU", 0, %Australia%
HKR, Ndi\params\Country\enum, "AT", 0, %Austria%
HKR, Ndi\params\Country\enum, "BS", 0, %BahamasThe%
HKR, Ndi\params\Country\enum, "BH", 0, %Bahrain%
HKR, Ndi\params\Country\enum, "BD", 0, %Bangladesh%
HKR, Ndi\params\Country\enum, "BB", 0, %Barbados%
HKR, Ndi\params\Country\enum, "BY", 0, %Belarus%
HKR, Ndi\params\Country\enum, "BE", 0, %Belgium%
HKR, Ndi\params\Country\enum, "BM", 0, %Bermuda%
HKR, Ndi\params\Country\enum, "BO", 0, %Bolivia%
HKR, Ndi\params\Country\enum, "BA", 0, %BosniaandHerzegovina%
HKR, Ndi\params\Country\enum, "BR", 0, %Brazil%
HKR, Ndi\params\Country\enum, "BN", 0, %Brunei%
HKR, Ndi\params\Country\enum, "BG", 0, %Bulgaria%
HKR, Ndi\params\Country\enum, "CA", 0, %Canada%
HKR, Ndi\params\Country\enum, "KY", 0, %CaymanIslands%
HKR, Ndi\params\Country\enum, "CL", 0, %Chile%
HKR, Ndi\params\Country\enum, "CN", 0, %China%
HKR, Ndi\params\Country\enum, "CO", 0, %Colombia%
HKR, Ndi\params\Country\enum, "CR", 0, %CostaRica%
HKR, Ndi\params\Country\enum, "HR", 0, %Croatia%
HKR, Ndi\params\Country\enum, "CY", 0, %Cyprus%
HKR, Ndi\params\Country\enum, "CZ", 0, %CzechRepublic%
HKR, Ndi\params\Country\enum, "DK", 0, %Denmark%
HKR, Ndi\params\Country\enum, "DO", 0, %DominicanRepublic%
HKR, Ndi\params\Country\enum, "EC", 0, %Ecuador%
HKR, Ndi\params\Country\enum, "EG", 0, %Egypt%
HKR, Ndi\params\Country\enum, "SV", 0, %ElSalvador%
HKR, Ndi\params\Country\enum, "EE", 0, %Estonia%
HKR, Ndi\params\Country\enum, "FI", 0, %Finland%
HKR, Ndi\params\Country\enum, "FR", 0, %France%
HKR, Ndi\params\Country\enum, "DE", 0, %Germany%
HKR, Ndi\params\Country\enum, "GR", 0, %Greece%
HKR, Ndi\params\Country\enum, "GU", 0, %Guam%
HKR, Ndi\params\Country\enum, "GT", 0, %Guatemala%
HKR, Ndi\params\Country\enum, "HT", 0, %Haiti%
HKR, Ndi\params\Country\enum, "HN", 0, %Honduras%
HKR, Ndi\params\Country\enum, "HK", 0, %HongKongSAR%
HKR, Ndi\params\Country\enum, "HU", 0, %Hungary%
HKR, Ndi\params\Country\enum, "IS", 0, %Iceland%
HKR, Ndi\params\Country\enum, "IN", 0, %India%
HKR, Ndi\params\Country\enum, "ID", 0, %Indonesia%
HKR, Ndi\params\Country\enum, "IE", 0, %Ireland%
HKR, Ndi\params\Country\enum, "IL", 0, %Israel%
HKR, Ndi\params\Country\enum, "IT", 0, %Italy%
HKR, Ndi\params\Country\enum, "JP", 0, %Japan%
HKR, Ndi\params\Country\enum, "JO", 0, %Jordan%
HKR, Ndi\params\Country\enum, "KR", 0, %Korea%
HKR, Ndi\params\Country\enum, "LV", 0, %Latvia%
HKR, Ndi\params\Country\enum, "LI", 0, %Liechtenstein%
HKR, Ndi\params\Country\enum, "LT", 0, %Lithuania%
HKR, Ndi\params\Country\enum, "LU", 0, %Luxembourg%
HKR, Ndi\params\Country\enum, "MO", 0, %MacauSAR%
HKR, Ndi\params\Country\enum, "MY", 0, %Malaysia%
HKR, Ndi\params\Country\enum, "MT", 0, %Malta%
HKR, Ndi\params\Country\enum, "MX", 0, %Mexico%
HKR, Ndi\params\Country\enum, "MC", 0, %Monaco%
HKR, Ndi\params\Country\enum, "MA", 0, %Morocco%
HKR, Ndi\params\Country\enum, "AN", 0, %NetherlandsAntilles%
HKR, Ndi\params\Country\enum, "NL", 0, %NetherlandsThe%
HKR, Ndi\params\Country\enum, "NZ", 0, %NewZealand%
HKR, Ndi\params\Country\enum, "NI", 0, %Nicaragua%
HKR, Ndi\params\Country\enum, "NG", 0, %Nigeria%
HKR, Ndi\params\Country\enum, "NO", 0, %Norway%
HKR, Ndi\params\Country\enum, "PK", 0, %Pakistan%
HKR, Ndi\params\Country\enum, "PA", 0, %Panama%
HKR, Ndi\params\Country\enum, "PY", 0, %Paraguay%
HKR, Ndi\params\Country\enum, "PE", 0, %Peru%
HKR, Ndi\params\Country\enum, "PH", 0, %Philippines%
HKR, Ndi\params\Country\enum, "PL", 0, %Poland%
HKR, Ndi\params\Country\enum, "PT", 0, %Portugal%
HKR, Ndi\params\Country\enum, "RO", 0, %Romania%
HKR, Ndi\params\Country\enum, "RU", 0, %Russia%
HKR, Ndi\params\Country\enum, "SA", 0, %SaudiArabia%
HKR, Ndi\params\Country\enum, "SG", 0, %Singapore%
HKR, Ndi\params\Country\enum, "SK", 0, %Slovakia%
HKR, Ndi\params\Country\enum, "SI", 0, %Slovenia%
HKR, Ndi\params\Country\enum, "ZA", 0, %SouthAfrica%
HKR, Ndi\params\Country\enum, "ES", 0, %Spain%
HKR, Ndi\params\Country\enum, "LK", 0, %SriLanka%
HKR, Ndi\params\Country\enum, "SE", 0, %Sweden%
HKR, Ndi\params\Country\enum, "CH", 0, %Switzerland%
HKR, Ndi\params\Country\enum, "TW", 0, %Taiwan%
HKR, Ndi\params\Country\enum, "TZ", 0, %Tanzania%
HKR, Ndi\params\Country\enum, "TH", 0, %Thailand%
HKR, Ndi\params\Country\enum, "TN", 0, %Tunisia%
HKR, Ndi\params\Country\enum, "TR", 0, %Turkey%
HKR, Ndi\params\Country\enum, "UA", 0, %Ukraine%
HKR, Ndi\params\Country\enum, "AE", 0, %UnitedArabEmirates%
HKR, Ndi\params\Country\enum, "GB", 0, %UnitedKingdom%
HKR, Ndi\params\Country\enum, "UM", 0, %UnitedStatesMinorOutlyingIslands%
HKR, Ndi\params\Country\enum, "UY", 0, %Uruguay%
HKR, Ndi\params\Country\enum, "VE", 0, %Venezuela%
HKR, Ndi\params\Country\enum, "VN", 0, %VietNam%
HKR, Ndi\params\Country\enum, "YU", 0, %Yugoslavia%
[b.reg]
HKR, ,"ledbh0", 0, "5"
HKR, Ndi\params\PLCPHeader, ParamDesc, 0, %PLCPHeader%
HKR, Ndi\params\PLCPHeader, type, 0, "enum"
HKR, Ndi\params\PLCPHeader\enum, "-1", 0, %Long%
HKR, Ndi\params\PLCPHeader\enum, "0", 0, %AutoShortLong%
HKR, Ndi\params\PLCPHeader,default,,"0"
HKR, Ndi\params\Rate, ParamDesc, 0, %Rate%
HKR, Ndi\params\Rate, type, 0, "enum"
HKR, Ndi\params\Rate\enum, "0", 0, %Usebestrate%
HKR, Ndi\params\Rate\enum, "2", 0, " 1"
HKR, Ndi\params\Rate\enum, "4", 0, " 2"
HKR, Ndi\params\Rate\enum, "11", 0, " 5.5"
HKR, Ndi\params\Rate\enum, "22", 0, "11"
HKR, Ndi\params\Rate,default,,"0"
HKR, Ndi\params\ApCompatMode, ParamDesc, 0, %ApCompatibilityMode%
HKR, Ndi\params\ApCompatMode, type, 0, "enum"
HKR, Ndi\params\ApCompatMode\enum, "1", 0, %BroaderCompat%
HKR, Ndi\params\ApCompatMode\enum, "0", 0, %HigherPerf%
HKR, Ndi\params\ApCompatMode,default,,"0"
[g.reg]
HKR, Ndi\params\Afterburner, ParamDesc, 0, %Afterburner%
HKR, Ndi\params\Afterburner, type, 0, "enum"
HKR, Ndi\params\Afterburner\enum, "0", 0, %Disabled%
HKR, Ndi\params\Afterburner\enum, "1", 0, %Enabled%
HKR, Ndi\params\Afterburner,default,,"1"
HKR, Ndi\params\RoamTrigger, ParamDesc, 0, %RoamingDecision%
HKR, Ndi\params\RoamTrigger, type, 0, "enum"
HKR, Ndi\params\RoamTrigger\enum, "1", 0, %OptimizeBandwidth%
HKR, Ndi\params\RoamTrigger\enum, "0", 0, %Default%
HKR, Ndi\params\RoamTrigger\enum, "2", 0, %OptimizeDistance%
HKR, Ndi\params\RoamTrigger,default,,"0"
HKR, Ndi\params\PLCPHeader, ParamDesc, 0, %BSSPLCPHeader%
HKR, Ndi\params\PLCPHeader, type, 0, "enum"
HKR, Ndi\params\PLCPHeader\enum, "-1", 0, %Long%
HKR, Ndi\params\PLCPHeader\enum, "0", 0, %AutoShortLong%
HKR, Ndi\params\PLCPHeader,default,,"0"
HKR, Ndi\params\Rate, ParamDesc, 0, %Rate%
HKR, Ndi\params\Rate, type, 0, "enum"
HKR, Ndi\params\Rate\enum, "0", 0, %Usebestrate%
HKR, Ndi\params\Rate\enum, "2", 0, " 1"
HKR, Ndi\params\Rate\enum, "4", 0, " 2"
HKR, Ndi\params\Rate\enum, "11", 0, " 5.5"
HKR, Ndi\params\Rate\enum, "12", 0, " 6"
HKR, Ndi\params\Rate\enum, "18", 0, " 9"
HKR, Ndi\params\Rate\enum, "22", 0, "11"
HKR, Ndi\params\Rate\enum, "24", 0, "12"
HKR, Ndi\params\Rate\enum, "36", 0, "18"
HKR, Ndi\params\Rate\enum, "48", 0, "24"
HKR, Ndi\params\Rate\enum, "72", 0, "36"
HKR, Ndi\params\Rate\enum, "96", 0, "48"
HKR, Ndi\params\Rate\enum, "108", 0, "54"
HKR, Ndi\params\Rate,default,,"0"
HKR, Ndi\params\ApCompatMode, ParamDesc, 0, %ApCompatibilityMode%
HKR, Ndi\params\ApCompatMode, type, 0, "enum"
HKR, Ndi\params\ApCompatMode\enum, "1", 0, %BroaderCompat%
HKR, Ndi\params\ApCompatMode\enum, "0", 0, %HigherPerf%
HKR, Ndi\params\ApCompatMode,default,,"0"
[gt.reg]
HKR, ,"featureflag", 65537, "0x00000001"
[bg0.reg]
HKR, Ndi\params\Chanspec, ParamDesc, 0, %IBSSChannelNumber%
HKR, Ndi\params\Chanspec, default, 0, "11"
HKR, Ndi\params\Chanspec, min, 0, %IBSSChanMin%
HKR, Ndi\params\Chanspec, step, 0, "1"
HKR, Ndi\params\Chanspec, base, 0, "10"
HKR, Ndi\params\Chanspec, type, 0, "int"
[bg.loc.reg]
HKR, Ndi\params\Chanspec, max, 0, %IBSSChanMax%
[bg1.reg]
HKR, Ndi\params\Chanspec, max, 0, "11"
[bg2.reg]
HKR, Ndi\params\Chanspec, max, 0, "13"
[bg3.reg]
HKR, Ndi\params\Chanspec, max, 0, "14"
[bag.reg]
HKR, Ndi\params\Afterburner, ParamDesc, 0, %Afterburner%
HKR, Ndi\params\Afterburner, type, 0, "enum"
HKR, Ndi\params\Afterburner\enum, "0", 0, %Disabled%
HKR, Ndi\params\Afterburner\enum, "1", 0, %Enabled%
HKR, Ndi\params\Afterburner,default,,"1"
HKR, Ndi\params\RoamTrigger, ParamDesc, 0, %RoamingDecision%
HKR, Ndi\params\RoamTrigger, type, 0, "enum"
HKR, Ndi\params\RoamTrigger\enum, "1", 0, %OptimizeBandwidth%
HKR, Ndi\params\RoamTrigger\enum, "0", 0, %Default%
HKR, Ndi\params\RoamTrigger\enum, "2", 0, %OptimizeDistance%
HKR, Ndi\params\RoamTrigger,default,,"0"
HKR, Ndi\params\PLCPHeader, ParamDesc, 0, %BSSPLCPHeader%
HKR, Ndi\params\PLCPHeader, type, 0, "enum"
HKR, Ndi\params\PLCPHeader\enum, "-1", 0, %Long%
HKR, Ndi\params\PLCPHeader\enum, "0", 0, %AutoShortLong%
HKR, Ndi\params\PLCPHeader,default,,"0"
HKR, Ndi\params\band, ParamDesc, 0, %DisableBands%
HKR, Ndi\params\band, type, 0, "enum"
HKR, Ndi\params\band\enum, "0", 0, %None%
HKR, Ndi\params\band\enum, "1", 0, %Disable80211gb%
HKR, Ndi\params\band\enum, "2", 0, %Disable80211a%
HKR, Ndi\params\band,default,,"0"
HKR, Ndi\params\BandPref, ParamDesc, 0, %BandPreference%
HKR, Ndi\params\BandPref, type, 0, "enum"
HKR, Ndi\params\BandPref\enum, "0", 0, %None%
HKR, Ndi\params\BandPref\enum, "1", 0, %Prefer80211a%
HKR, Ndi\params\BandPref\enum, "2", 0, %Prefer80211gb%
HKR, Ndi\params\BandPref,default,,"0"
HKR, Ndi\params\AssocRoamPref, ParamDesc, 0, %AssociationRoamPreference%
HKR, Ndi\params\AssocRoamPref, type, 0, "enum"
HKR, Ndi\params\AssocRoamPref\enum, "0", 0, %Disabled%
HKR, Ndi\params\AssocRoamPref\enum, "1", 0, %Enabled%
HKR, Ndi\params\AssocRoamPref,default,,"0"
HKR, Ndi\params\RateA, ParamDesc, 0, %Rate_802_11a%
HKR, Ndi\params\RateA, type, 0, "enum"
HKR, Ndi\params\RateA\enum, "0", 0, %Usebestrate%
HKR, Ndi\params\RateA\enum, "12", 0, " 6"
HKR, Ndi\params\RateA\enum, "18", 0, " 9"
HKR, Ndi\params\RateA\enum, "24", 0, "12"
HKR, Ndi\params\RateA\enum, "36", 0, "18"
HKR, Ndi\params\RateA\enum, "48", 0, "24"
HKR, Ndi\params\RateA\enum, "72", 0, "36"
HKR, Ndi\params\RateA\enum, "96", 0, "48"
HKR, Ndi\params\RateA\enum, "108", 0, "54"
HKR, Ndi\params\RateA,default,,"0"
HKR, Ndi\params\Rate, ParamDesc, 0, %Rate_802_11bg%
HKR, Ndi\params\Rate, type, 0, "enum"
HKR, Ndi\params\Rate\enum, "0", 0, %Usebestrate%
HKR, Ndi\params\Rate\enum, "2", 0, " 1"
HKR, Ndi\params\Rate\enum, "4", 0, " 2"
HKR, Ndi\params\Rate\enum, "11", 0, " 5.5"
HKR, Ndi\params\Rate\enum, "12", 0, " 6"
HKR, Ndi\params\Rate\enum, "18", 0, " 9"
HKR, Ndi\params\Rate\enum, "22", 0, "11"
HKR, Ndi\params\Rate\enum, "24", 0, "12"
HKR, Ndi\params\Rate\enum, "36", 0, "18"
HKR, Ndi\params\Rate\enum, "48", 0, "24"
HKR, Ndi\params\Rate\enum, "72", 0, "36"
HKR, Ndi\params\Rate\enum, "96", 0, "48"
HKR, Ndi\params\Rate\enum, "108", 0, "54"
HKR, Ndi\params\Rate,default,,"0"
HKR, Ndi\params\Chanspec, ParamDesc, 0, %IBSSChannelNumber%
HKR, Ndi\params\Chanspec, type, 0, "enum"
HKR, Ndi\params\Chanspec\enum, "1", 0, " 1"
HKR, Ndi\params\Chanspec\enum, "2", 0, " 2"
HKR, Ndi\params\Chanspec\enum, "3", 0, " 3"
HKR, Ndi\params\Chanspec\enum, "4", 0, " 4"
HKR, Ndi\params\Chanspec\enum, "5", 0, " 5"
HKR, Ndi\params\Chanspec\enum, "6", 0, " 6"
HKR, Ndi\params\Chanspec\enum, "7", 0, " 7"
HKR, Ndi\params\Chanspec\enum, "8", 0, " 8"
HKR, Ndi\params\Chanspec\enum, "9", 0, " 9"
HKR, Ndi\params\Chanspec\enum, "10", 0, " 10"
HKR, Ndi\params\Chanspec\enum, "11", 0, " 11"
HKR, Ndi\params\Chanspec, default, 0, "11"
HKR, Ndi\params\ApCompatMode, ParamDesc, 0, %ApCompatibilityMode%
HKR, Ndi\params\ApCompatMode, type, 0, "enum"
HKR, Ndi\params\ApCompatMode\enum, "1", 0, %BroaderCompat%
HKR, Ndi\params\ApCompatMode\enum, "0", 0, %HigherPerf%
HKR, Ndi\params\ApCompatMode,default,,"0"
[bagn.reg]
HKR, Ndi\params\Afterburner, ParamDesc, 0, %Afterburner%
HKR, Ndi\params\Afterburner, type, 0, "enum"
HKR, Ndi\params\Afterburner\enum, "0", 0, %Disabled%
HKR, Ndi\params\Afterburner\enum, "1", 0, %Enabled%
HKR, Ndi\params\Afterburner,default,,"1"
HKR, Ndi\params\RoamTrigger, ParamDesc, 0, %RoamingDecision%
HKR, Ndi\params\RoamTrigger, type, 0, "enum"
HKR, Ndi\params\RoamTrigger\enum, "1", 0, %OptimizeBandwidth%
HKR, Ndi\params\RoamTrigger\enum, "0", 0, %Default%
HKR, Ndi\params\RoamTrigger\enum, "2", 0, %OptimizeDistance%
HKR, Ndi\params\RoamTrigger,default,,"0"
HKR, Ndi\params\PLCPHeader, ParamDesc, 0, %BSSPLCPHeader%
HKR, Ndi\params\PLCPHeader, type, 0, "enum"
HKR, Ndi\params\PLCPHeader\enum, "-1", 0, %Long%
HKR, Ndi\params\PLCPHeader\enum, "0", 0, %AutoShortLong%
HKR, Ndi\params\PLCPHeader,default,,"0"
HKR, Ndi\params\band, ParamDesc, 0, %DisableBands%
HKR, Ndi\params\band, type, 0, "enum"
HKR, Ndi\params\band\enum, "0", 0, %None%
HKR, Ndi\params\band\enum, "1", 0, %Disable80211gb%
HKR, Ndi\params\band\enum, "2", 0, %Disable80211a%
HKR, Ndi\params\band,default,,"0"
HKR, Ndi\params\BandPref, ParamDesc, 0, %BandPreference%
HKR, Ndi\params\BandPref, type, 0, "enum"
HKR, Ndi\params\BandPref\enum, "0", 0, %None%
HKR, Ndi\params\BandPref\enum, "1", 0, %Prefer80211a%
HKR, Ndi\params\BandPref\enum, "2", 0, %Prefer80211gb%
HKR, Ndi\params\BandPref,default,,"0"
HKR, Ndi\params\AssocRoamPref, ParamDesc, 0, %AssociationRoamPreference%
HKR, Ndi\params\AssocRoamPref, type, 0, "enum"
HKR, Ndi\params\AssocRoamPref\enum, "0", 0, %Disabled%
HKR, Ndi\params\AssocRoamPref\enum, "1", 0, %Enabled%
HKR, Ndi\params\AssocRoamPref,default,,"0"
HKR, Ndi\params\RateA, ParamDesc, 0, %Rate_802_11a%
HKR, Ndi\params\RateA, type, 0, "enum"
HKR, Ndi\params\RateA\enum, "0", 0, %Usebestrate%
HKR, Ndi\params\RateA\enum, "12", 0, " 6"
HKR, Ndi\params\RateA\enum, "18", 0, " 9"
HKR, Ndi\params\RateA\enum, "24", 0, "12"
HKR, Ndi\params\RateA\enum, "36", 0, "18"
HKR, Ndi\params\RateA\enum, "48", 0, "24"
HKR, Ndi\params\RateA\enum, "72", 0, "36"
HKR, Ndi\params\RateA\enum, "96", 0, "48"
HKR, Ndi\params\RateA\enum, "108", 0, "54"
HKR, Ndi\params\RateA,default,,"0"
HKR, Ndi\params\Rate, ParamDesc, 0, %Rate_802_11bg%
HKR, Ndi\params\Rate, type, 0, "enum"
HKR, Ndi\params\Rate\enum, "0", 0, %Usebestrate%
HKR, Ndi\params\Rate\enum, "2", 0, " 1"
HKR, Ndi\params\Rate\enum, "4", 0, " 2"
HKR, Ndi\params\Rate\enum, "11", 0, " 5.5"
HKR, Ndi\params\Rate\enum, "12", 0, " 6"
HKR, Ndi\params\Rate\enum, "18", 0, " 9"
HKR, Ndi\params\Rate\enum, "22", 0, "11"
HKR, Ndi\params\Rate\enum, "24", 0, "12"
HKR, Ndi\params\Rate\enum, "36", 0, "18"
HKR, Ndi\params\Rate\enum, "48", 0, "24"
HKR, Ndi\params\Rate\enum, "72", 0, "36"
HKR, Ndi\params\Rate\enum, "96", 0, "48"
HKR, Ndi\params\Rate\enum, "108", 0, "54"
HKR, Ndi\params\Rate,default,,"0"
HKR, Ndi\params\Chanspec, ParamDesc, 0, %IBSSChannelNumber%
HKR, Ndi\params\Chanspec, type, 0, "enum"
HKR, Ndi\params\Chanspec\enum, "1", 0, " 1"
HKR, Ndi\params\Chanspec\enum, "2", 0, " 2"
HKR, Ndi\params\Chanspec\enum, "3", 0, " 3"
HKR, Ndi\params\Chanspec\enum, "4", 0, " 4"
HKR, Ndi\params\Chanspec\enum, "5", 0, " 5"
HKR, Ndi\params\Chanspec\enum, "6", 0, " 6"
HKR, Ndi\params\Chanspec\enum, "7", 0, " 7"
HKR, Ndi\params\Chanspec\enum, "8", 0, " 8"
HKR, Ndi\params\Chanspec\enum, "9", 0, " 9"
HKR, Ndi\params\Chanspec\enum, "10", 0, " 10"
HKR, Ndi\params\Chanspec\enum, "11", 0, " 11"
HKR, Ndi\params\Chanspec, default, 0, "11"
HKR, Ndi\params\ApCompatMode, ParamDesc, 0, %ApCompatibilityMode%
HKR, Ndi\params\ApCompatMode, type, 0, "enum"
HKR, Ndi\params\ApCompatMode\enum, "1", 0, %BroaderCompat%
HKR, Ndi\params\ApCompatMode\enum, "0", 0, %HigherPerf%
HKR, Ndi\params\ApCompatMode,default,,"0"
HKR, Ndi\params\11NPreamble, ParamDesc, 0, "802.11n Preamble"
HKR, Ndi\params\11NPreamble, type, 0, "enum"
HKR, Ndi\params\11NPreamble\enum, "-1", 0, %Green_Field_Mode%
HKR, Ndi\params\11NPreamble\enum, "0", 0, %Mixed_Mode%
HKR, Ndi\params\11NPreamble,default,,"-1"
HKR, Ndi\params\BandwidthCap, ParamDesc, 0, "Bandwidth Capability"
HKR, Ndi\params\BandwidthCap, type, 0, "enum"
HKR, Ndi\params\BandwidthCap\enum, "0", 0, "11a/b/g:20MHz"
HKR, Ndi\params\BandwidthCap\enum, "1", 0, "11a/b/g:20/40MHz"
HKR, Ndi\params\BandwidthCap\enum, "2", 0, "11a:20/40;11bg:20MHz"
HKR, Ndi\params\BandwidthCap,default,,"2"
[gn.reg]
HKR, Ndi\params\Afterburner, ParamDesc, 0, %Afterburner%
HKR, Ndi\params\Afterburner, type, 0, "enum"
HKR, Ndi\params\Afterburner\enum, "0", 0, %Disabled%
HKR, Ndi\params\Afterburner\enum, "1", 0, %Enabled%
HKR, Ndi\params\Afterburner,default,,"1"
HKR, Ndi\params\RoamTrigger, ParamDesc, 0, %RoamingDecision%
HKR, Ndi\params\RoamTrigger, type, 0, "enum"
HKR, Ndi\params\RoamTrigger\enum, "1", 0, %OptimizeBandwidth%
HKR, Ndi\params\RoamTrigger\enum, "0", 0, %Default%
HKR, Ndi\params\RoamTrigger\enum, "2", 0, %OptimizeDistance%
HKR, Ndi\params\RoamTrigger,default,,"0"
HKR, Ndi\params\PLCPHeader, ParamDesc, 0, %BSSPLCPHeader%
HKR, Ndi\params\PLCPHeader, type, 0, "enum"
HKR, Ndi\params\PLCPHeader\enum, "-1", 0, %Long%
HKR, Ndi\params\PLCPHeader\enum, "0", 0, %AutoShortLong%
HKR, Ndi\params\PLCPHeader,default,,"0"
HKR, Ndi\params\AssocRoamPref, ParamDesc, 0, %AssociationRoamPreference%
HKR, Ndi\params\AssocRoamPref, type, 0, "enum"
HKR, Ndi\params\AssocRoamPref\enum, "0", 0, %Disabled%
HKR, Ndi\params\AssocRoamPref\enum, "1", 0, %Enabled%
HKR, Ndi\params\AssocRoamPref,default,,"0"
HKR, Ndi\params\Rate, ParamDesc, 0, %Rate_802_11bg%
HKR, Ndi\params\Rate, type, 0, "enum"
HKR, Ndi\params\Rate\enum, "0", 0, %Usebestrate%
HKR, Ndi\params\Rate\enum, "2", 0, " 1"
HKR, Ndi\params\Rate\enum, "4", 0, " 2"
HKR, Ndi\params\Rate\enum, "11", 0, " 5.5"
HKR, Ndi\params\Rate\enum, "12", 0, " 6"
HKR, Ndi\params\Rate\enum, "18", 0, " 9"
HKR, Ndi\params\Rate\enum, "22", 0, "11"
HKR, Ndi\params\Rate\enum, "24", 0, "12"
HKR, Ndi\params\Rate\enum, "36", 0, "18"
HKR, Ndi\params\Rate\enum, "48", 0, "24"
HKR, Ndi\params\Rate\enum, "72", 0, "36"
HKR, Ndi\params\Rate\enum, "96", 0, "48"
HKR, Ndi\params\Rate\enum, "108", 0, "54"
HKR, Ndi\params\Rate,default,,"0"
HKR, Ndi\params\Chanspec, ParamDesc, 0, %IBSSChannelNumber%
HKR, Ndi\params\Chanspec, type, 0, "enum"
HKR, Ndi\params\Chanspec\enum, "1", 0, " 1"
HKR, Ndi\params\Chanspec\enum, "2", 0, " 2"
HKR, Ndi\params\Chanspec\enum, "3", 0, " 3"
HKR, Ndi\params\Chanspec\enum, "4", 0, " 4"
HKR, Ndi\params\Chanspec\enum, "5", 0, " 5"
HKR, Ndi\params\Chanspec\enum, "6", 0, " 6"
HKR, Ndi\params\Chanspec\enum, "7", 0, " 7"
HKR, Ndi\params\Chanspec\enum, "8", 0, " 8"
HKR, Ndi\params\Chanspec\enum, "9", 0, " 9"
HKR, Ndi\params\Chanspec\enum, "10", 0, " 10"
HKR, Ndi\params\Chanspec\enum, "11", 0, " 11"
HKR, Ndi\params\Chanspec, default, 0, "11"
HKR, Ndi\params\ApCompatMode, ParamDesc, 0, %ApCompatibilityMode%
HKR, Ndi\params\ApCompatMode, type, 0, "enum"
HKR, Ndi\params\ApCompatMode\enum, "1", 0, %BroaderCompat%
HKR, Ndi\params\ApCompatMode\enum, "0", 0, %HigherPerf%
HKR, Ndi\params\ApCompatMode,default,,"0"
HKR, Ndi\params\11NPreamble, ParamDesc, 0, "802.11n Preamble"
HKR, Ndi\params\11NPreamble, type, 0, "enum"
HKR, Ndi\params\11NPreamble\enum, "-1", 0, %Green_Field_Mode%
HKR, Ndi\params\11NPreamble\enum, "0", 0, %Mixed_Mode%
HKR, Ndi\params\11NPreamble,default,,"-1"
HKR, Ndi\params\BandwidthCap, ParamDesc, 0, "Bandwidth Capability"
HKR, Ndi\params\BandwidthCap, type, 0, "enum"
HKR, Ndi\params\BandwidthCap\enum, "0", 0, "11b/g:20MHz"
HKR, Ndi\params\BandwidthCap\enum, "1", 0, "11b/g:20/40MHz"
HKR, Ndi\params\BandwidthCap,default,,"0"
[gn20.reg]
HKR, Ndi\params\Afterburner, ParamDesc, 0, %Afterburner%
HKR, Ndi\params\Afterburner, type, 0, "enum"
HKR, Ndi\params\Afterburner\enum, "0", 0, %Disabled%
HKR, Ndi\params\Afterburner\enum, "1", 0, %Enabled%
HKR, Ndi\params\Afterburner,default,,"1"
HKR, Ndi\params\RoamTrigger, ParamDesc, 0, %RoamingDecision%
HKR, Ndi\params\RoamTrigger, type, 0, "enum"
HKR, Ndi\params\RoamTrigger\enum, "1", 0, %OptimizeBandwidth%
HKR, Ndi\params\RoamTrigger\enum, "0", 0, %Default%
HKR, Ndi\params\RoamTrigger\enum, "2", 0, %OptimizeDistance%
HKR, Ndi\params\RoamTrigger,default,,"0"
HKR, Ndi\params\PLCPHeader, ParamDesc, 0, %BSSPLCPHeader%
HKR, Ndi\params\PLCPHeader, type, 0, "enum"
HKR, Ndi\params\PLCPHeader\enum, "-1", 0, %Long%
HKR, Ndi\params\PLCPHeader\enum, "0", 0, %AutoShortLong%
HKR, Ndi\params\PLCPHeader,default,,"0"
HKR, Ndi\params\AssocRoamPref, ParamDesc, 0, %AssociationRoamPreference%
HKR, Ndi\params\AssocRoamPref, type, 0, "enum"
HKR, Ndi\params\AssocRoamPref\enum, "0", 0, %Disabled%
HKR, Ndi\params\AssocRoamPref\enum, "1", 0, %Enabled%
HKR, Ndi\params\AssocRoamPref,default,,"0"
HKR, Ndi\params\Rate, ParamDesc, 0, %Rate_802_11bg%
HKR, Ndi\params\Rate, type, 0, "enum"
HKR, Ndi\params\Rate\enum, "0", 0, %Usebestrate%
HKR, Ndi\params\Rate\enum, "2", 0, " 1"
HKR, Ndi\params\Rate\enum, "4", 0, " 2"
HKR, Ndi\params\Rate\enum, "11", 0, " 5.5"
HKR, Ndi\params\Rate\enum, "12", 0, " 6"
HKR, Ndi\params\Rate\enum, "18", 0, " 9"
HKR, Ndi\params\Rate\enum, "22", 0, "11"
HKR, Ndi\params\Rate\enum, "24", 0, "12"
HKR, Ndi\params\Rate\enum, "36", 0, "18"
HKR, Ndi\params\Rate\enum, "48", 0, "24"
HKR, Ndi\params\Rate\enum, "72", 0, "36"
HKR, Ndi\params\Rate\enum, "96", 0, "48"
HKR, Ndi\params\Rate\enum, "108", 0, "54"
HKR, Ndi\params\Rate,default,,"0"
HKR, Ndi\params\Chanspec, ParamDesc, 0, %IBSSChannelNumber%
HKR, Ndi\params\Chanspec, type, 0, "enum"
HKR, Ndi\params\Chanspec\enum, "1", 0, " 1"
HKR, Ndi\params\Chanspec\enum, "2", 0, " 2"
HKR, Ndi\params\Chanspec\enum, "3", 0, " 3"
HKR, Ndi\params\Chanspec\enum, "4", 0, " 4"
HKR, Ndi\params\Chanspec\enum, "5", 0, " 5"
HKR, Ndi\params\Chanspec\enum, "6", 0, " 6"
HKR, Ndi\params\Chanspec\enum, "7", 0, " 7"
HKR, Ndi\params\Chanspec\enum, "8", 0, " 8"
HKR, Ndi\params\Chanspec\enum, "9", 0, " 9"
HKR, Ndi\params\Chanspec\enum, "10", 0, " 10"
HKR, Ndi\params\Chanspec\enum, "11", 0, " 11"
HKR, Ndi\params\Chanspec, default, 0, "11"
HKR, Ndi\params\ApCompatMode, ParamDesc, 0, %ApCompatibilityMode%
HKR, Ndi\params\ApCompatMode, type, 0, "enum"
HKR, Ndi\params\ApCompatMode\enum, "1", 0, %BroaderCompat%
HKR, Ndi\params\ApCompatMode\enum, "0", 0, %HigherPerf%
HKR, Ndi\params\ApCompatMode,default,,"0"
HKR, Ndi\params\11NPreamble, ParamDesc, 0, "802.11n Preamble"
HKR, Ndi\params\11NPreamble, type, 0, "enum"
HKR, Ndi\params\11NPreamble\enum, "-1", 0, %Green_Field_Mode%
HKR, Ndi\params\11NPreamble\enum, "0", 0, %Mixed_Mode%
HKR, Ndi\params\11NPreamble,default,,"-1"
[gpiotype1.reg]
HKR, ,"ledbh0", 0, "3"
HKR, ,"ledbh1", 0, "2"
HKR, ,"ledbh2", 0, "0"
HKR, ,"ledbh3", 0, "0"
[gpiotype2.reg]
HKR, ,"ledbh0", 0, "-1"
HKR, ,"ledbh1", 0, "-1"
HKR, ,"ledbh2", 0, "-1"
HKR, ,"ledbh3", 0, "-1"
[chans.thru64.reg]
HKR, Ndi\params\Chanspec\enum, "36", 0, " 36"
HKR, Ndi\params\Chanspec\enum, "40", 0, " 40"
HKR, Ndi\params\Chanspec\enum, "44", 0, " 44"
HKR, Ndi\params\Chanspec\enum, "48", 0, " 48"
HKR, Ndi\params\Chanspec\enum, "52", 0, " 52"
HKR, Ndi\params\Chanspec\enum, "56", 0, " 56"
HKR, Ndi\params\Chanspec\enum, "60", 0, " 60"
HKR, Ndi\params\Chanspec\enum, "64", 0, " 64"
[chans.a.row.reg]
HKR, Ndi\params\Chanspec\enum, "100", 0, "100"
HKR, Ndi\params\Chanspec\enum, "104", 0, "104"
HKR, Ndi\params\Chanspec\enum, "108", 0, "108"
HKR, Ndi\params\Chanspec\enum, "112", 0, "112"
HKR, Ndi\params\Chanspec\enum, "116", 0, "116"
HKR, Ndi\params\Chanspec\enum, "120", 0, "120"
HKR, Ndi\params\Chanspec\enum, "124", 0, "124"
HKR, Ndi\params\Chanspec\enum, "128", 0, "128"
HKR, Ndi\params\Chanspec\enum, "132", 0, "132"
HKR, Ndi\params\Chanspec\enum, "136", 0, "136"
HKR, Ndi\params\Chanspec\enum, "140", 0, "140"
[chans.a.jp.reg]
HKR, Ndi\params\Chanspec\enum, "34", 0, " 34"
HKR, Ndi\params\Chanspec\enum, "38", 0, " 38"
HKR, Ndi\params\Chanspec\enum, "42", 0, " 42"
HKR, Ndi\params\Chanspec\enum, "46", 0, " 46"
[chans.thru13.reg]
HKR, Ndi\params\Chanspec\enum, "12", 0, " 12"
HKR, Ndi\params\Chanspec\enum, "13", 0, " 13"
[chans.thru14.reg]
HKR, Ndi\params\Chanspec\enum, "12", 0, " 12"
HKR, Ndi\params\Chanspec\enum, "13", 0, " 13"
HKR, Ndi\params\Chanspec\enum, "14", 0, " 14"
[hiband.reg]
HKR, Ndi\params\Chanspec\enum, "149", 0, "149"
HKR, Ndi\params\Chanspec\enum, "153", 0, "153"
HKR, Ndi\params\Chanspec\enum, "157", 0, "157"
HKR, Ndi\params\Chanspec\enum, "161", 0, "161"
HKR, Ndi\params\Chanspec\enum, "165", 0, "165"
[enabled.11h.reg]
HKR, Ndi\params\11HNetworks, ParamDesc, 0, "802.11h+d"
HKR, Ndi\params\11HNetworks, type, 0, "enum"
HKR, Ndi\params\11HNetworks\enum, "1", 0, %Loose_11h%
HKR, Ndi\params\11HNetworks\enum, "2", 0, %Strict_11h%
HKR, Ndi\params\11HNetworks\enum, "4", 0, %Loose_11h_and_11d%
HKR, Ndi\params\11HNetworks,default,,"1"
[disabled.11h.reg]
HKR, Ndi\params\11HNetworks, ParamDesc, 0, "802.11h+d"
HKR, Ndi\params\11HNetworks, type, 0, "enum"
HKR, Ndi\params\11HNetworks\enum, "1", 0, %Loose_11h%
HKR, Ndi\params\11HNetworks\enum, "2", 0, %Strict_11h%
HKR, Ndi\params\11HNetworks\enum, "4", 0, %Loose_11h_and_11d%
HKR, Ndi\params\11HNetworks,default,,"1"
[strings]
CountryCode="US"
IBSSChanMin="1"
IBSSChanMax="11"
V_BCM="Broadcom"
BCM430G_DeviceDesc="Broadcom 802.11b/g WLAN"
BCM430M_DeviceDesc="Broadcom 802.11a/b/g WLAN"
BCM43XX_HELP="The Broadcom 802.11 Network Adapter provides wireless local area networking."
BCM43XX_Service_DispName="Broadcom 802.11 Network Adapter Driver"
BCM43XX_DiskName="802.11 Network Adapter Install Disk"
BCM430NM_DeviceDesc="Broadcom 4321AG 802.11a/b/g/draft-n Wi-Fi Adapter"
BCM4322NM_DeviceDesc="Broadcom 4322AG 802.11a/b/g/draft-n Wi-Fi Adapter"
BCM43224NM_DeviceDesc="Broadcom 43224AG 802.11a/b/g/draft-n Wi-Fi Adapter"
BCM4313NG_DeviceDesc="Broadcom 4313 802.11b/g/n"
BCM43225NG_DeviceDesc="Broadcom 43225 802.11b/g/n"
AntiguaandBarbuda="Antigua and Barbuda"
Argentina="Argentina"
Aruba="Aruba"
Australia="Australia"
Austria="Austria"
BahamasThe="Bahamas, The"
Bahrain="Bahrain"
Bangladesh="Bangladesh"
Barbados="Barbados"
Belarus="Belarus"
Belgium="Belgium"
Bermuda="Bermuda"
Bolivia="Bolivia"
BosniaandHerzegovina="Bosnia and Herzegovina"
Brazil="Brazil"
Brunei="Brunei"
Bulgaria="Bulgaria"
Canada="Canada"
CaymanIslands="Cayman Islands"
Chile="Chile"
China="China"
Colombia="Colombia"
CostaRica="Costa Rica"
Croatia="Croatia"
Cyprus="Cyprus"
CzechRepublic="Czech Republic"
Denmark="Denmark"
DominicanRepublic="Dominican Republic"
Ecuador="Ecuador"
Egypt="Egypt"
ElSalvador="El Salvador"
Estonia="Estonia"
Finland="Finland"
France="France"
Germany="Germany"
Greece="Greece"
Guam="Guam"
Guatemala="Guatemala"
Haiti="Haiti"
Honduras="Honduras"
HongKongSAR="Hong Kong S.A.R."
Hungary="Hungary"
Iceland="Iceland"
India="India"
Indonesia="Indonesia"
Ireland="Ireland"
Italy="Italy"
Korea="Korea"
Latvia="Latvia"
Liechtenstein="Liechtenstein"
Lithuania="Lithuania"
Luxembourg="Luxembourg"
MacauSAR="Macau S.A.R."
Malaysia="Malaysia"
Malta="Malta"
Mexico="Mexico"
Monaco="Monaco"
Morocco="Morocco"
NetherlandsAntilles="Netherlands Antilles"
NetherlandsThe="Netherlands, The"
NewZealand="New Zealand"
Nicaragua="Nicaragua"
Nigeria="Nigeria"
Norway="Norway"
Pakistan="Pakistan"
Panama="Panama"
Paraguay="Paraguay"
Peru="Peru"
Philippines="Philippines"
Poland="Poland"
Portugal="Portugal"
Romania="Romania"
Russia="Russia"
SaudiArabia="Saudi Arabia"
Singapore="Singapore"
Slovakia="Slovakia"
Slovenia="Slovenia"
SouthAfrica="South Africa"
Spain="Spain"
SriLanka="Sri Lanka"
Sweden="Sweden"
Switzerland="Switzerland"
Taiwan="Taiwan"
Tanzania="Tanzania"
Tunisia="Tunisia"
Turkey="Turkey"
Ukraine="Ukraine"
UnitedArabEmirates="United Arab Emirates"
UnitedKingdom="United Kingdom"
UnitedStatesMinorOutlyingIslands="US Minor Outlying Islands"
UnitedStates="United States"
Uruguay="Uruguay"
Venezuela="Venezuela"
VietNam="Viet Nam"
Yugoslavia="Yugoslavia"
Israel="Israel"
Japan="Japan"
Jordan="Jordan"
Thailand="Thailand"
Auto="Auto"
AutoShortLong="Auto (Short/Long)"
BSSPLCPHeader="BSS PLCP Header"
BlueToothCollaboration="Bluetooth Collaboration"
Default="Default"
Disable="Disable"
Disable80211a="Disable 802.11a"
Disable80211gb="Disable 802.11g/b"
DisableBands="Disable Bands"
Disabled="Disabled"
Enable="Enable"
Enabled="Enabled"
FragmentationThreshold="Fragmentation Threshold"
LocallyAdministeredMACAddress="Locally Administered MAC Address"
Long="Long"
None="None"
OptimizeBandwidth="Optimize Bandwidth"
OptimizeDistance="Optimize Distance"
PLCPHeader="PLCP Header"
PowerOutput="Power Output"
PowerSaveMode="Power Save Mode"
Prefer80211a="Prefer 802.11a"
Prefer80211gb="Prefer 802.11g/b"
RTSThreshold="RTS Threshold"
Rate="Rate"
RoamingDecision="Roaming Decision"
XPress_Technology="XPress (TM) Technology"
Location="Location"
MaxPowerSavings="Max Power Savings"
HighPerformance="High Performance"
MinimumPowerConsumption="Minimum Power Consumption"
AssociationRoamPreference="Association Roam Preference"
BandPreference="Band Preference"
RoamingTendency="Roam Tendency"
Aggressive="Aggressive"
Moderate="Moderate"
Conservative="Conservative"
ApCompatibilityMode="AP Compatibility Mode"
BroaderCompat="Broader Compatibility"
HigherPerf="Higher Performance"
WME="WMM"
Afterburner="Afterburner"
Rate_802_11a="Rate (802.11a)"
Rate_802_11bg="Rate (802.11b/g)"
SSIDAutoPromote="SSID Autopromote"
IBSSChannelNumber="WZC IBSS Channel Number"
Loose_11h_and_11d="Loose 11h+d"
Loose_11h="Loose 11h"
Strict_11h="Strict 11h"
MixedCell="Mixed Cell Support"
vlan_mode="VLAN Priority Support"
PriorityVLANTag="Priority & VLAN"
PriorityAndVLANDisabled="Priority & VLAN Disabled"
PriorityAndVLANEnabled="Priority & VLAN Enabled"
PriorityEnabled="Priority Enabled"
VLANEnabled="VLAN Enabled"
Usebestrate="Best Rate"
Green_Field_Mode="Green Field Mode"
Mixed_Mode="Mixed Mode"

