
[Version]
DriverVer=02/12/2009, 2.01.01.0015
Signature="$Chicago$"
Compatible=1
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%Provider%
CatalogFile=rt2500usb.CAT ;for WHQL certified
[ControlFlags]
[Manufacturer]
%Ralink%=Ralink
%ALLWIN%=ALLWIN
%Belkin%=Belkin
%BUFFALO%=BUFFALO
%LinkSys%=LinkSys
%HERCULES%=Hercules
[Ralink]
[ALLWIN]
%ALLWIN.DeviceDesc%=ALLWIN.ndi, USB\VID_8516&PID_2500
[Belkin]
%Belkin_7050.DeviceDesc%=Belkin_7050.ndi, USB\VID_050D&PID_7050
%Belkin_705A.DeviceDesc%=Belkin_705A.ndi, USB\VID_050D&PID_705A
[BUFFALO]
%BUFFALO_5E.DeviceDesc%=BUFFALO_5E.ndi, USB\VID_0411&PID_008B
[LinkSys]
%HU200.DeviceDesc%=HU200.ndi, USB\VID_13B1&PID_001A
%WUSB54GPv4.DeviceDesc%=WUSB54GPv4.ndi, USB\VID_13B1&PID_0011
%WUSB54Gv4.DeviceDesc%=WUSB54Gv4.ndi, USB\VID_13B1&PID_000D
[Hercules]
%Hercules.DeviceDesc%=HERCULES.ndi, USB\VID_06F8&PID_E000
[RALINK.ndi]
AddReg=USB_184F_2570.ndi.reg, Common.reg, USB9X.ndi.reg
;CpyFiles=win9x.CopyFiles
[ALLWIN.ndi]
AddReg=USB_8516_2500.ndi.reg, Common.reg, USB9X.ndi.reg
;CpyFiles=win9x.CopyFiles
[Belkin_7050.ndi]
AddReg=USB_050D_7050.ndi.reg, Common.reg, USB9X.ndi.reg
;CpyFiles=win9x.CopyFiles
[Belkin_705A.ndi]
AddReg=USB_050D_705A.ndi.reg, Common.reg, USB9X.ndi.reg
;CpyFiles=win9x.CopyFiles
[BUFFALO_5E.ndi]
AddReg=USB_0411_005E.ndi.reg, Common.reg, USB9X.ndi.reg
;CpyFiles=win9x.CopyFiles
[HU200.ndi]
AddReg=USB_13B1_001A.ndi.reg, Common.reg, USB9X.ndi.reg
;CpyFiles=win9x.CopyFiles
[WUSB54GPv4.ndi]
AddReg=USB_13B1_0011.ndi.reg, Common.reg, USB9X.ndi.reg
;CpyFiles=win9x.CopyFiles
[WUSB54Gv4.ndi]
AddReg=USB_13B1_000D.ndi.reg, Common.reg, USB9X.ndi.reg
;CpyFiles=win9x.CopyFiles
[Hercules.ndi]
AddReg=USB_06F8_E000.ndi.reg, Common.reg, USB9X.ndi.reg
;CpyFiles=win9x.CopyFiles
[RALINK.ndi.NT]
AddReg=Common.reg, RTUSB.ndi.NT.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=15 ;USB
;CpyFiles=NT.CopyFiles
[ALLWIN.ndi.NT]
AddReg=Common.reg, RTUSB.ndi.NT.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=15 ;USB
;CpyFiles=NT.CopyFiles
[Belkin_7050.ndi.NT]
AddReg=Common.reg, RTUSB.ndi.NT.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=15 ;USB
;CpyFiles=NT.CopyFiles
[Belkin_705A.ndi.NT]
AddReg=Common.reg, RTUSB.ndi.NT.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=15 ;USB
;CpyFiles=NT.CopyFiles
[BUFFALO_5E.ndi.NT]
AddReg=Common.reg, RTUSB.ndi.NT.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=15 ;USB
;CpyFiles=NT.CopyFiles
[HU200.ndi.NT]
AddReg=Common.reg, RTUSB.ndi.NT.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=15 ;USB
;CpyFiles=NT.CopyFiles
[WUSB54GPv4.ndi.NT]
AddReg=Common.reg, RTUSB.ndi.NT.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=15 ;USB
;CpyFiles=NT.CopyFiles
[WUSB54Gv4.ndi.NT]
AddReg=Common.reg, RTUSB.ndi.NT.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=15 ;USB
;CpyFiles=NT.CopyFiles
[Hercules.ndi]
AddReg=Common.reg, RTUSB.ndi.NT.reg
Characteristics=0x84 ; NCF_REMOVABLE | NCF_HAS_UI | NCF_PHYSICAL
BusType=15 ;USB
;CpyFiles=NT.CopyFiles
[RALINK.ndi.NT.Services]
AddService=RT2500USB, 2, RALINK.Service, common.EventLog
[ALLWIN.ndi.NT.Services]
AddService=RT2500USB, 2, ALLWIN.Service, common.EventLog
[Belkin_7050.ndi.NT.Services]
AddService=RT2500USB, 2, Belkin_7050.Service, common.EventLog
[Belkin_705A.ndi.NT.Services]
AddService=RT2500USB, 2, Belkin_705A.Service, common.EventLog
[BUFFALO_5E.ndi.NT.Services]
AddService=RT2500USB, 2, BUFFALO.Service, common.EventLog
[HU200.ndi.NT.Services]
AddService=RT2500USB, 2, HU200.Service, common.EventLog
[WUSB54GPv4.ndi.NT.Services]
AddService=RT2500USB, 2, WUSB54GPv4.Service, common.EventLog
[WUSB54Gv4.ndi.NT.Services]
AddService=RT2500USB, 2, WUSB54Gv4.Service, common.EventLog
[Hercules.ndi.NT.Services]
AddService=RT2500USB, 2, Hercules.Service, common.EventLog
[Common.reg]
HKR, , CurProfile, 0,""
HKR, Default, CurProfile, 0,""
HKR, , Radio, 0, "0"
HKR, NDI\params\Radio, ParamDesc, 0, "Radio On/Off"
HKR, NDI\params\Radio, type, 0, "enum"
HKR, NDI\params\Radio, default, 0, "0"
HKR, NDI\params\Radio\enum, 1, 0, "Disable"
HKR, NDI\params\Radio\enum, 0, 0, "Enable"
HKR, , AutoReconnect, 0, "1"
HKR, NDI\params\AutoReconnect, ParamDesc, 0, "Auto Reconnect Mode"
HKR, NDI\params\AutoReconnect, type, 0, "enum"
HKR, NDI\params\AutoReconnect, default, 0, "1"
HKR, NDI\params\AutoReconnect\enum, 0, 0, "Disable"
HKR, NDI\params\AutoReconnect\enum, 1, 0, "Enable"
HKR, , ShowHiddenSSID, 0, "0" ; 0=disable(default), 1=enable
HKR, , ConfigSelect, 0, "0" ; 0=RaConfig, 1=ZeroConfig
HKR, , CountryRegion, 0, "0"
HKR, , WirelessMode, 0, "0"
HKR, , TXBurst, 0, "0"
HKR, , ShortSlot, 0, "0"
HKR, , TurboRate, 0, "0"
HKR, , AdhocOfdm, 0, "0"
HKR, , BGProtection, 0, "0"
HKR, , VendorDesc, 0, %VENDOR_DESC_DEF_STR%
HKR, Default, VendorDesc, 0, %VENDOR_DESC_DEF_STR%
HKR, , PSPXlink, 0, "0"
HKR, NDI\params\PSPXlink, ParamDesc, 0, "PSP Xlink Mode"
HKR, NDI\params\PSPXlink, type, 0, "enum"
HKR, NDI\params\PSPXlink, default, 0, "0"
HKR, NDI\params\PSPXlink\enum, 0, 0, "Disable"
HKR, NDI\params\PSPXlink\enum, 1, 0, "Enable"
HKR, , NetworkType, 0, %NETWORK_TYPE_DEF_STR%
HKR, Default, NetworkType, 0, %NETWORK_TYPE_DEF_STR%
HKR, NDI\params\NetworkType, ParamDesc, 0, "Network Type"
HKR, NDI\params\NetworkType, type, 0, "enum"
HKR, NDI\params\NetworkType, default, 0, %NETWORK_TYPE_DEF_STR%
HKR, NDI\params\NetworkType\enum, 0, 0, "802.11 Ad Hoc"
HKR, NDI\params\NetworkType\enum, 1, 0, "Infrastructure"
HKR, , Channel, 0, %CHANNEL%
HKR, Default, Channel, 0, %CHANNEL%
HKR, , NetworkAddress, 0, ""
HKR, Default, NetworkAddress, 0, ""
HKR, NDI\params\NetworkAddress, ParamDesc, 0, "Local Administration MAC Network Address"
HKR, NDI\params\NetworkAddress, type, 0, "edit"
HKR, NDI\params\NetworkAddress, limitText, 0, "12"
HKR, NDI\params\NetworkAddress, default, 0, ""
HKR, NDI\params\NetworkAddress, optional, 0, "1"
HKR, , PSMode, 0, "0"
HKR, Default, PSMode, 0, "0"
HKR, NDI\params\PSMode, ParamDesc, 0, "Power Saving Mode"
HKR, NDI\params\PSMode, type, 0, "enum"
HKR, NDI\params\PSMode, default, 0, "0"
HKR, NDI\params\PSMode\enum, 0, 0, "CAM (Constantly Awake Mode)"
HKR, NDI\params\PSMode\enum, 1, 0, "Max_PSP (Max Power Savings)"
HKR, NDI\params\PSMode\enum, 2, 0, "Fast_PSP (Power Save Mode)"
HKR, , ACPowerCam, 0, "0"
HKR, Default, ACPowerCam, 0, "0"
HKR, NDI\params\ACPowerCam, ParamDesc, 0, "CAM when AC Power"
HKR, NDI\params\ACPowerCam, type, 0, "enum"
HKR, NDI\params\ACPowerCam, default, 0, "0"
HKR, NDI\params\ACPowerCam\enum, 0, 0, "Disable"
HKR, NDI\params\ACPowerCam\enum, 1, 0, "Enable"
HKR, , PreambleType, 0, "0"
HKR, Default, PreambleType, 0, "0"
HKR, , TXPower, 0, "0"
HKR, Default, TXPower, 0, "0"
HKR, , RTSThresh, 0, "2347"
HKR, Default, RTSThresh, 0, "2347"
HKR, NDI\params\RTSThresh, ParamDesc, 0, "RTS Threshold"
HKR, NDI\params\RTSThresh, type, 0, "int"
HKR, Ndi\params\RTSThresh, default, 0, "2347"
HKR, NDI\params\RTSThresh, min, 0, "0"
HKR, NDI\params\RTSThresh, max, 0, "2347"
HKR, NDI\params\RTSThresh, step, 0, "1"
HKR, NDI\params\RTSThresh, optional, 0, "0"
HKR, , FragThresh, 0, "2346"
HKR, Default, FragThresh, 0, "2346"
HKR, NDI\params\FragThresh, ParamDesc, 0, "Fragment Threshold"
HKR, NDI\params\FragThresh, type, 0, "int"
HKR, Ndi\params\FragThresh, default, 0, "2346"
HKR, NDI\params\FragThresh, min, 0, "256"
HKR, NDI\params\FragThresh, max, 0, "2346"
HKR, NDI\params\FragThresh, step, 0, "1"
HKR, NDI\params\FragThresh, optional, 0, "0"
HKR, , AuthenType, 0, "0" ; Open System
HKR, Default, AuthenType, 0, "0"
HKR, , Encryption, 0, "1" ; Disable
HKR, Default, Encryption, 0, "1"
HKR, , WEPKeyLen, 0, "0"
HKR, Default, WEPKeyLen, 0, "0"
HKR, , WEPKeyUse, 0,"1"
HKR, Default, WEPKeyUse, 0,"1"
HKR, , WEPKey1, 0,""
HKR, Default, WEPKey1, 0,""
HKR, , WEPKey2, 0,""
HKR, Default, WEPKey2, 0,""
HKR, , WEPKey3, 0,""
HKR, Default, WEPKey3, 0,""
HKR, , WEPKey4, 0,""
HKR, Default, WEPKey4, 0,""
HKR, , WPAPSK, 0, ""
HKR, Default, WPAPSK, 0, ""
HKR, , Use8021X, 0, "0"
HKR, Default, Use8021X, 0, "0"
HKR, , AuthenProtocol, 0, "0"
HKR, Default, AuthenProtocol, 0, "0"
HKR, , TunnelProtocol, 0, "3"
HKR, Default, TunnelProtocol, 0, "3"
HKR, , ID, 0, ""
HKR, Default, ID, 0, ""
HKR, , Password, 0, ""
HKR, Default, Password, 0, ""
HKR, , TunnelID, 0, ""
HKR, Default, TunnelID, 0, ""
HKR, , TunnelPassword, 0, ""
HKR, Default, TunnelPassword, 0, ""
HKR, , SessionResumption, 0, "0"
HKR, Default, SessionResumption, 0, "0"
HKR, , PasswordMode, 0, "1"
HKR, Default, PasswordMode, 0, "1"
HKR, , UseClientCert, 0, "0"
HKR, Default, UseClientCert, 0, "0"
HKR, , UseServerCert, 0, "0"
HKR, Default, UseServerCert, 0, "0"
HKR, , ClientCertLen, 0, "0"
HKR, Default, ClientCertLen, 0, "0"
HKR, , ClientCertData, 0, ""
HKR, Default, ClientCertData, 0, ""
HKR, , ServerCertLen, 0, "0"
HKR, Default, ServerCertLen, 0, "0"
HKR, , ServerCertData, 0, ""
HKR, Default, ServerCertData, 0, ""
HKR, , ServerName, 0, ""
HKR, Default, ServerName, 0, ""
HKR, , NameRule, 0, "0"
HKR, Default, NameRule, 0, "0"
HKR, , IntermediateCert, 0, "0"
HKR, Default, IntermediateCert, 0, "0"
HKR, , LeapEnabled, 0, "0"
HKR, Default, LeapEnabled, 0, "0"
HKR, , LeapUserName, 0, ""
HKR, Default, LeapUserName, 0, ""
HKR, , LeapPassword, 0, ""
HKR, Default, LeapPassword, 0, ""
HKR, , RekeyInterval, 0, "60"
HKR, , RekeyMethod, 0, "0"
[USB_184F_2570.ndi.reg]
HKR, Ndi, DeviceID, 0, "USB\VID_148F&PID_2570"
[USB_0411_005E.ndi.reg]
HKR, Ndi, DeviceID, 0, "USB\VID_0411&PID_008B"
[USB_13B1_001A.ndi.reg]
HKR, Ndi, DeviceID, 0, "USB\VID_13B1&PID_001A"
[USB_13B1_0011.ndi.reg]
HKR, Ndi, DeviceID, 0, "USB\VID_13B1&PID_0011"
[USB_13B1_000D.ndi.reg]
HKR, Ndi, DeviceID, 0, "USB\VID_13B1&PID_000D"
[USB_8516_2500.ndi.reg]
HKR, Ndi, DeviceID, 0, "USB\VID_8516&PID_2500"
[USB_050D_7050.ndi.reg]
HKR, Ndi, DeviceID, 0, "USB\VID_050D&PID_7050"
[USB_050D_705A.ndi.reg]
HKR, Ndi, DeviceID, 0, "USB\VID_050D&PID_705A"
[USB_06F8_E000.ndi.reg]
HKR, Ndi, DeviceID, 0, "USB\VID_06F8&PID_E000"
[USB9X.ndi.reg]
HKR, , NTMPDriver, 0, rt25u98.sys
HKR, , BusType, 0, 15
HKR, NDI, CardType, 0, "PNP"
HKR, , RunningWin9X, 0, "1"
HKR, , DevLoader, 0, "*ndis"
HKR, , DeviceVxDs, 0, "rt25u98.sys"
HKR, , EnumPropPages, 0, "netdi.dll,EnumPropPages"
HKR, Ndi\Interfaces, DefUpper, 0, "ndis3"
HKR, Ndi\Interfaces, DefLower, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis3"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, NDIS, LogDriverName, 0, "rt25u98"
HKR, NDIS, MajorNdisVersion, 1, 03
HKR, NDIS, MinorNdisVersion, 1, 0A
[DestinationDirs]
NT.CopyFiles=12 ; system32\drivers subdirectory on NT
win9x.CopyFiles=11 ; system32 subdirectory on win9x
[NT.CopyFiles]
rt2500usb.sys ; NT Installation
[win9x.CopyFiles]
rt25u98.sys ; Win9x Installation
[SourceDisksNames]
1=%INSTALL_DISK_STR%,,,
[SourceDisksFiles]
rt2500usb.sys=1
rt25u98.sys=1
[RTUSB.ndi.NT.reg]
HKR, Ndi, Service, 0, "rt2500usb"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
[Ralink.Service]
DisplayName=%Ralink.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_AUTO_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\rt2500usb.sys
LoadOrderGroup=NDIS
[ALLWIN.Service]
DisplayName=%ALLWIN.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_AUTO_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\rt2500usb.sys
LoadOrderGroup=NDIS
[Belkin_7050.Service]
DisplayName=%Belkin_7050.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_AUTO_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\rt2500usb.sys
LoadOrderGroup=NDIS
[Belkin_705A.Service]
DisplayName=%Belkin_705A.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_AUTO_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\rt2500usb.sys
LoadOrderGroup=NDIS
[BUFFALO.Service]
DisplayName=%BUFFALO.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_AUTO_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\rt2500usb.sys
LoadOrderGroup=NDIS
[HU200.Service]
DisplayName=%HU200.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_AUTO_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\rt2500usb.sys
LoadOrderGroup=NDIS
[WUSB54GPv4.Service]
DisplayName=%WUSB54GPv4.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_AUTO_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\rt2500usb.sys
LoadOrderGroup=NDIS
[WUSB54Gv4.Service]
DisplayName=%WUSB54Gv4.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_AUTO_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\rt2500usb.sys
LoadOrderGroup=NDIS
[Hercules.Service]
DisplayName=%Hercules.Service.DispName%
ServiceType=1 ;%SERVICE_KERNEL_DRIVER%
StartType=3 ;%SERVICE_AUTO_START%
ErrorControl=1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\rt2500usb.sys
LoadOrderGroup=NDIS
[common.EventLog]
AddReg=common.AddEventLog.reg
[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000,"%%SystemRoot%%\System32\netevent.dll,%%SystemRoot%%\System32\drivers\rt2500usb.sys"
HKR, , TypesSupported, 0x00010001, 7
[strings]
Provider="Ralink"
Ralink="Ralink Technology Corp."
ALLWIN="ALLWIN"
Belkin="Belkin Components"
BUFFALO="BUFFALO INC."
Linksys="Linksys, A Division of Cisco Systems, Inc."
HERCULES="Hercules"
RALINK.DeviceDesc="RT2500 USB Wireless LAN Card"
ALLWIN.DeviceDesc="ALLWIN Wireless LAN Card ¡V2500"
Belkin_7050.DeviceDesc="Belkin Wireless G USB Adapter"
Belkin_705A.DeviceDesc="Belkin Wireless G USB Adapter"
BUFFALO_5E.DeviceDesc="Nintendo WiFi USB Adapter"
HU200.DeviceDesc="Linksys Home Wireless-G USB Adapter"
WUSB54GPv4.DeviceDesc="Wireless-G Portable USB Adapter"
WUSB54Gv4.DeviceDesc="Linksys Wireless-G USB Network Adapter"
Hercules.DeviceDesc="Hercules Wireless G USB2"
INSTALL_DISK_STR="Wireless 11g USB Installation Disk"
RALINK.Service.DispName="RT2500 USB Wireless LAN Driver"
ALLWIN.Service.DispName="RT2500 USB Wireless LAN Driver"
Belkin_7050.DispName="Belkin Wireless G USB Network Adapter Driver"
Belkin_705A.DispName="Belkin Wireless G USB Network Adapter Driver"
BUFFALO.Service.DispName="BUFFALO WLI-U2-KG54 RT2500 USB Wireless Driver"
HU200.Service.DispName="Linksys Home Wireless-G USB Adaptor Driver"
WUSB54GPv4.Service.DispName="Linksys Wireless-G Portable USB Adapter Driver"
WUSB54Gv4.Service.DispName="Linksys Wireless-G USB Network Adapter Driver"
Hercules.Service.DispName="Hercules Wireless USB Dongle Driver"
VENDOR_DESC_DEF_STR=""
NETWORK_TYPE_DEF_STR="1"
CHANNEL="1"
