
[Version]
DriverVer=12/09/2003, 1.0.5.1000
Signature="$Chicago$"
Compatible=1
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%VER_VENDOR_STR%
[ControlFlags]
ExcludeFromSelect=*
[Manufacturer]
%VER_VENDOR_NAME_STR%=DeviceList
[DeviceList]
%A021_DESC_STR%=COWUGT_A021, USB\VID_07AA&PID_001C
[COWUGT_A021] ; Win9x
AddReg=COWUGT_A021.reg, COMMON_A02.reg, COMMON_NDIS.reg, COMMON.reg
;CpyFiles=COWUGT_DRIVER.copy
[COWUGT_A021.NT] ; Win2k
AddReg=COWUGT_A021.reg, COMMON_A02.reg.NT, COMMON_NDIS.reg.NT, COMMON.reg
;CpyFiles=COWUGT_DRIVER.copy.NT
BusType=0
Characteristics= 0x84
[COWUGT_A021.NT.Services]
AddService= "COWUGT", 2, COWUGT_DRIVER_A02.Service, COWUGT_DRIVER.EventLog
[COWUGT_A021.reg]
HKR,Ndi,DeviceID,0,"USB\VID_07AA&PID_001C"
HKR,,PlatformID,0,14480
HKR,,VendorDesc,0,%A021_DESC_STR%
HKR,,FWFileName,0,"PRISMA02.arm"
[COWUGT_DRIVER_A02.Service]
DisplayName=%A02_SERVICE_STR%
ServiceType=1 ; SERVICE_KERNEL_DRIVER
StartType=3 ; SERVICE_DEMAND_START
ErrorControl=1 ; NORMAL
ServiceBinary=%12%\COWUGT5.sys
LoadOrderGroup=NDIS
[COWUGT_DRIVER.EventLog]
AddReg=COWUGT_DRIVER.EventLog.reg
[COWUGT_DRIVER.EventLog.reg]
HKR, ,EventMessageFile ,0x00020000 ,"%%SystemRoot%%\System32\netevent.dll"
HKR, ,TypesSupported ,0x00010001 ,7
[COMMON_A02.reg]
HKR,NDI ,Service ,0 ,"COWUGT"
HKR,NDI ,CardType ,0 ,"USB"
HKR, ,BusType ,0 ,"0"
HKR, ,DeviceVxDs ,0 ,"COWUGT3.sys"
[COMMON_A02.reg.NT]
HKR,NDI ,Service ,0 ,"COWUGT"
HKR,NDI ,CardType ,0 ,"USB"
HKR, ,BusType ,0 ,"0"
HKR, ,DeviceVxDs ,0 ,"COWUGT5.sys"
[COMMON_NDIS.reg]
HKR, ,RunningWin9X ,0 ,"1"
HKR, ,DevLoader ,0 ,"*ndis"
HKR, ,EnumPropPages ,0 ,"netdi.dll,EnumPropPages"
HKR,NDI\Interfaces ,UpperRange ,0 ,"ndis3"
HKR,NDI\Interfaces ,LowerRange ,0 ,"ethernet"
HKR,NDI\Interfaces ,DefUpper ,0 ,"ndis3"
HKR,NDI\Interfaces ,DefLower ,0 ,"ethernet"
HKR,NDIS ,LogDriverName ,0 ,"COWUGT3"
HKR,NDIS ,MajorNdisVersion ,1 ,03
HKR,NDIS ,MinorNdisVersion ,1 ,0a
[COMMON_NDIS.reg.NT]
HKR,NDI\Interfaces ,UpperRange ,0 ,"ndis5"
HKR,NDI\Interfaces ,LowerRange ,0 ,"ethernet"
[COMMON.reg]
HKR, ,SSID ,0 ,"corega"
HKR, ,COWUGT ,0 ,"1"
HKR, ,SilentInstall ,0 ,"1"
HKR,NDI\params\ShortRetryLimit,,0,7
HKR,NDI\params\ShortRetryLimit,default,0,7
HKR,NDI\params\ShortRetryLimit,ParamDesc,,%SHORT_RETRY_STR%
HKR,NDI\params\ShortRetryLimit,type,,int
HKR,NDI\params\ShortRetryLimit,min,0,1
HKR,NDI\params\ShortRetryLimit,max,0,255
HKR,NDI\params\ShortRetryLimit,step,0,1
HKR,NDI\params\ShortRetryLimit,optional,0,1
HKR,NDI\params\LongRetryLimit,,0,4
HKR,NDI\params\LongRetryLimit,default,0,4
HKR,NDI\params\LongRetryLimit,ParamDesc,,%LONG_RETRY_STR%
HKR,NDI\params\LongRetryLimit,type,0,int
HKR,NDI\params\LongRetryLimit,min,0,1
HKR,NDI\params\LongRetryLimit,max,0,255
HKR,NDI\params\LongRetryLimit,step,0,1
HKR,NDI\params\LongRetryLimit,optional,0,1
HKR, ,ConfigProfile ,0 ,"256"
[DestinationDirs]
DefaultDestDir=11 ; Win9x=%windir%\system Win2k=%windir%\system32
COWUGT_DRIVER.copy=11 ; Win9x=%windir%\system
COWUGT_DRIVER.copy.NT=12 ; Win2k=%windir%\system32\drivers
[COWUGT_DRIVER.copy]
COWUGT3.sys
COWUGT.vxd ; Win9x Ioctl interface
[COWUGT_DRIVER.copy.NT]
COWUGT5.sys
[SourceDisksNames]
1=%INSTALL_DISK_STR%,,,
[SourceDisksFiles] ; Win9x
[SourceDisksFiles.X86] ; Win2k/Xp
COWUGT5.sys=1
[Strings]
VER_VENDOR_STR="corega"
VER_VENDOR_NAME_STR="corega"
INSTALL_DISK_STR="CG-WLUSB2GT Install Disk"
A021_DESC_STR="CG-WLUSB2GT"
A02_SERVICE_STR="CG-WLUSB2GT"
ON_STR="On"
OFF_STR="Off"
SHORT_RETRY_STR="Short Retry Limit"
LONG_RETRY_STR="Long Retry Limit"
CONFIG_PROFILE="Configuration Profile"
CONFIG_PROF_B_ONLY="B only"
CONFIG_PROF_MIXED="Mixed"
CONFIG_PROF_MIXED_LONG="Mixed Long"
CONFIG_PROF_G_ONLY="G only"
CONFIG_PROF_TEST="Test"
CONFIG_PROF_B_WIFI="B WiFi"
CONFIG_PROF_MIXED_SHORT="Mixed Short"
CONFIG_PROF_WIFI_SPEC="WiFi Spec"

