
[Version]
DriverVer=01/07/2002, 1.13.1.0
Signature="$Chicago$"
Compatible=1
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%VER_VENDOR_STR%
CatalogFile=NETIMWEB.cat
MillenniumPreferred=.ME
[Manufacturer]
%VER_VENDOR_NAME_STR%=DeviceList,NTx86.5.1
%VER_VENDOR_NAME_STR%=DeviceList
[DeviceList.NTx86.5.1]
%IMWEB_PCI1_STR%=IMWEB_PCI1.NT.5.1,PCI\VEN_1260&DEV_3873&SUBSYS_25108086
%IMWEB_PCI1_STR%=IMWEB_PCI1.NT.5.1,PCI\VEN_1260&DEV_3873&SUBSYS_25138086
%IMWEB_PCI1_STR%=IMWEB_PCI1.NT.5.1,PCI\VEN_1260&DEV_3873&SUBSYS_25148086
%IMWEB_PCI1_STR%=IMWEB_PCI1.NT.5.1,PCI\VEN_1260&DEV_3873&SUBSYS_25158086
%IMWEB_PCI1_STR%=IMWEB_PCI1.NT.5.1,PCI\VEN_1260&DEV_3873&SUBSYS_25168086
%IMWEB_PCI1_STR%=IMWEB_PCI1.NT.5.1,PCI\VEN_1260&DEV_3873&SUBSYS_25178086
%IMWEB_PCI1_STR%=IMWEB_PCI1.NT.5.1,PCI\VEN_1260&DEV_3873&SUBSYS_25133274
%IMWEB_PCI2_STR%=IMWEB_PCI2.NT.5.1,PCI\VEN_1260&DEV_3873&SUBSYS_25118086
[DeviceList]
%IMWEB_PCI1_STR%=IMWEB_PCI1,PCI\VEN_1260&DEV_3873&SUBSYS_25108086
%IMWEB_PCI1_STR%=IMWEB_PCI1,PCI\VEN_1260&DEV_3873&SUBSYS_25138086
%IMWEB_PCI1_STR%=IMWEB_PCI1,PCI\VEN_1260&DEV_3873&SUBSYS_25148086
%IMWEB_PCI1_STR%=IMWEB_PCI1,PCI\VEN_1260&DEV_3873&SUBSYS_25158086
%IMWEB_PCI1_STR%=IMWEB_PCI1,PCI\VEN_1260&DEV_3873&SUBSYS_25168086
%IMWEB_PCI1_STR%=IMWEB_PCI1,PCI\VEN_1260&DEV_3873&SUBSYS_25178086
%IMWEB_PCI1_STR%=IMWEB_PCI1,PCI\VEN_1260&DEV_3873&SUBSYS_25133274
%IMWEB_PCI2_STR%=IMWEB_PCI2,PCI\VEN_1260&DEV_3873&SUBSYS_25118086
[ControlFlags]
ExcludeFromSelect=PCI\VEN_1260&DEV_3873&SUBSYS_25108086
ExcludeFromSelect=PCI\VEN_1260&DEV_3873&SUBSYS_25118086
ExcludeFromSelect=PCI\VEN_1260&DEV_3873&SUBSYS_25138086
ExcludeFromSelect=PCI\VEN_1260&DEV_3873&SUBSYS_25148086
ExcludeFromSelect=PCI\VEN_1260&DEV_3873&SUBSYS_25158086
ExcludeFromSelect=PCI\VEN_1260&DEV_3873&SUBSYS_25168086
ExcludeFromSelect=PCI\VEN_1260&DEV_3873&SUBSYS_25178086
ExcludeFromSelect=PCI\VEN_1260&DEV_3873&SUBSYS_25133274
[IMWEB_PCI1] ; Win9x
AddReg=IMWEB_PCI1.reg, COMMON_PCI.reg, COMMON_NDIS.reg, COMMON.reg
;CpyFiles=IMWEB_DRIVER.copy, IMWEB_APPLET.copy, IMWEB_NDI.copy
[IMWEB_PCI1.ME] ; WinMe
AddReg=IMWEB_PCI1.reg, COMMON_PCI.reg, COMMON_NDIS.reg.ME, COMMON.reg
;CpyFiles=IMWEB_DRIVER.copy.ME, IMWEB_APPLET.copy.ME, IMWEB_NDI.copy.ME
BusType=5 ; PCI
Characteristics= 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[IMWEB_PCI1.ME.ME] ; WinMe - Same as .ME (Needed for Update Driver)
AddReg=IMWEB_PCI1.reg, COMMON_PCI.reg, COMMON_NDIS.reg.ME, COMMON.reg
;CpyFiles=IMWEB_DRIVER.copy.ME, IMWEB_APPLET.copy.ME, IMWEB_NDI.copy.ME
BusType=5 ; PCI
Characteristics= 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[IMWEB_PCI1.NT] ; Win2k
AddReg=IMWEB_PCI1.reg, COMMON_PCI.reg, COMMON_NDIS.reg.NT, COMMON.reg
;CpyFiles=IMWEB_DRIVER.copy.NT, IMWEB_APPLET.copy.NT
BusType=5 ; PCI
Characteristics= 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[IMWEB_PCI1.NT.5.1] ; WinXP
AddReg=IMWEB_PCI1.reg, COMMON_PCI.reg.NT.5.1, COMMON_NDIS.reg.NT, COMMON.reg
;CpyFiles=IMWEB_DRIVER.copy.NT.5.1, IMWEB_APPLET.copy.NT
BusType=5 ; PCI
Characteristics= 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[IMWEB_PCI1.ME.Services]
AddService="IMWEB", 2, IMWEB_DRIVER.Service, IMWEB_DRIVER.EventLog
[IMWEB_PCI1.ME.CoInstallers]
;CpyFiles=IMWEB_COINSTALL.copy.NT
AddReg=IMWEB_COINSTALL.reg.NT
[IMWEB_PCI1.NT.Services]
AddService="IMWEB", 2, IMWEB_DRIVER.Service, IMWEB_DRIVER.EventLog
[IMWEB_PCI1.NT.CoInstallers]
;CpyFiles=IMWEB_COINSTALL.copy.NT
AddReg=IMWEB_COINSTALL.reg.NT
[IMWEB_PCI1.NT.5.1.Services]
AddService="IMWEB", 2, IMWEB_DRIVER.NT.5.1.Service, IMWEB_DRIVER.EventLog
[IMWEB_PCI1.NT.5.1.CoInstallers]
;CpyFiles=IMWEB_COINSTALL.copy.NT
AddReg=IMWEB_COINSTALL.reg.NT
[IMWEB_PCI1.reg]
HKR,Ndi ,DeviceID,0,"PCI\VEN_1260&DEV_3873&SUBSYS_25108086"
[IMWEB_PCI2] ; Win9x
AddReg=IMWEB_PCI2.reg, COMMON_PCI.reg, COMMON_NDIS.reg, COMMON.reg
;CpyFiles=IMWEB_DRIVER.copy, IMWEB_APPLET.copy, IMWEB_NDI.copy
[IMWEB_PCI2.ME] ; WinMe
AddReg=IMWEB_PCI2.reg, COMMON_PCI.reg, COMMON_NDIS.reg.ME, COMMON.reg
;CpyFiles=IMWEB_DRIVER.copy.ME, IMWEB_APPLET.copy.ME, IMWEB_NDI.copy.ME
BusType=5 ; PCI
Characteristics= 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[IMWEB_PCI2.ME.ME] ; WinMe - Same as .ME (Needed for Update Driver)
AddReg=IMWEB_PCI2.reg, COMMON_PCI.reg, COMMON_NDIS.reg.ME, COMMON.reg
;CpyFiles=IMWEB_DRIVER.copy.ME, IMWEB_APPLET.copy.ME, IMWEB_NDI.copy.ME
BusType=5 ; PCI
Characteristics= 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[IMWEB_PCI2.NT] ; Win2k
AddReg=IMWEB_PCI2.reg, COMMON_PCI.reg, COMMON_NDIS.reg.NT, COMMON.reg
;CpyFiles=IMWEB_DRIVER.copy.NT, IMWEB_APPLET.copy.NT
BusType=5 ; PCI
Characteristics= 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[IMWEB_PCI2.NT.5.1] ; WinXP
AddReg=IMWEB_PCI2.reg, COMMON_PCI.reg.NT.5.1, COMMON_NDIS.reg.NT, COMMON.reg
;CpyFiles=IMWEB_DRIVER.copy.NT.5.1, IMWEB_APPLET.copy.NT
BusType=5 ; PCI
Characteristics= 0x84 ; NCF_PHYSICAL | NCF_HAS_UI
[IMWEB_PCI2.ME.Services]
AddService="IMWEB", 2, IMWEB_DRIVER.Service, IMWEB_DRIVER.EventLog
[IMWEB_PCI2.NT.Services]
AddService="IMWEB", 2, IMWEB_DRIVER.Service, IMWEB_DRIVER.EventLog
[IMWEB_PCI2.NT.5.1.Services]
AddService="IMWEB", 2, IMWEB_DRIVER.NT.5.1.Service, IMWEB_DRIVER.EventLog
[IMWEB_PCI2.ME.CoInstallers]
;CpyFiles=IMWEB_COINSTALL.copy.NT
AddReg=IMWEB_COINSTALL.reg.NT
[IMWEB_PCI2.NT.CoInstallers]
;CpyFiles=IMWEB_COINSTALL.copy.NT
AddReg=IMWEB_COINSTALL.reg.NT
[IMWEB_PCI2.NT.5.1.CoInstallers]
;CpyFiles=IMWEB_COINSTALL.copy.NT
AddReg=IMWEB_COINSTALL.reg.NT
[IMWEB_PCI2.reg]
HKR,Ndi ,DeviceID,0,"PCI\VEN_1260&DEV_3873&SUBSYS_25118086"
[IMWEB_COINSTALL.reg.NT]
[IMWEB_DRIVER.Service]
DisplayName=%IMWEB_SERVICE_DISPLAY%
ServiceType=1 ; SERVICE_KERNEL_DRIVER
StartType=3 ; SERVICE_DEMAND_START
ErrorControl=1 ; NORMAL
ServiceBinary=%12%\IMWEBN5.sys
LoadOrderGroup=NDIS
[IMWEB_DRIVER.NT.5.1.Service]
DisplayName=%IMWEB_SERVICE_DISPLAY%
ServiceType=1 ; SERVICE_KERNEL_DRIVER
StartType=3 ; SERVICE_DEMAND_START
ErrorControl=1 ; NORMAL
ServiceBinary=%12%\IMWEBN5.sys
LoadOrderGroup=NDIS
[IMWEB_DRIVER.EventLog]
AddReg=IMWEB_DRIVER.EventLog.reg
[IMWEB_DRIVER.EventLog.reg]
HKR, ,EventMessageFile ,0x00020000 ,"%%SystemRoot%%\System32\netevent.dll"
HKR, ,TypesSupported ,0x00010001 ,7
[IMWEB_DRIVER.ME.EventLog]
AddReg=IMWEB_DRIVER.ME.EventLog.reg
[IMWEB_DRIVER.ME.EventLog.reg]
HKR, ,EventMessageFile ,0x00020000 ,"%%SystemRoot%%\System32\netevent.dll"
HKR, ,TypesSupported ,0x00010001 ,7
[COMMON_PCI.reg]
HKR,NDI ,Service ,0 ,"IMWEB"
HKR,NDI ,CardType ,0 ,"PCI"
HKR, ,BusType ,0 ,"5"
HKR, ,DeviceVxDs ,0 ,"IMWEBN5.sys"
HKR, ,EnableIRQSharing ,1 ,01,00,00,00
HKR, ,IOBaseAddress ,1 ,02,00,00,00
HKR, ,InterruptNumber ,1 ,04,00,00,00
[COMMON_PCI.reg.NT.5.1]
HKR,NDI ,Service ,0 ,"IMWEB"
HKR,NDI ,CardType ,0 ,"PCI"
HKR, ,BusType ,0 ,"5"
HKR, ,DeviceVxDs ,0 ,"IMWEBN5.sys"
HKR, ,EnableIRQSharing ,1 ,01,00,00,00
HKR, ,IOBaseAddress ,1 ,02,00,00,00
HKR, ,InterruptNumber ,1 ,04,00,00,00
[COMMON_NDIS.reg]
HKR, ,RunningWin9X ,0 ,"1"
HKR, ,DevLoader ,0 ,"*ndis"
HKR, ,EnumPropPages ,0 ,"netdi.dll,EnumPropPages"
HKR,NDI ,NdiInstaller ,0 ,"IMWEBCFG.dll,NdiProc"
HKR,NDI\Interfaces ,UpperRange ,0 ,"ndis3"
HKR,NDI\Interfaces ,LowerRange ,0 ,"ethernet"
HKR,NDI\Interfaces ,DefUpper ,0 ,"ndis3"
HKR,NDI\Interfaces ,DefLower ,0 ,"ethernet"
HKR,NDIS ,LogDriverName ,0 ,"IMWEB"
HKR,NDIS ,MajorNdisVersion ,1 ,03
HKR,NDIS ,MinorNdisVersion ,1 ,0a
[COMMON_NDIS.reg.ME]
HKR, ,RunningWin9X ,0 ,"1"
HKR, ,DevLoader ,0 ,"*ndis"
HKR, ,EnumPropPages ,0 ,"netdi.dll,EnumPropPages"
HKR,NDI ,NdiInstaller ,0 ,"IMWEBCFG.dll,NdiProc"
HKR,NDI\Interfaces ,UpperRange ,0 ,"ndis3"
HKR,NDI\Interfaces ,LowerRange ,0 ,"ethernet"
HKR,NDI\Interfaces ,DefUpper ,0 ,"ndis3"
HKR,NDI\Interfaces ,DefLower ,0 ,"ethernet"
HKR,NDIS ,LogDriverName ,0 ,"IMWEB"
HKR,NDIS ,MajorNdisVersion ,1 ,03
HKR,NDIS ,MinorNdisVersion ,1 ,0a
[COMMON_NDIS.reg.NT]
HKR,NDI\Interfaces ,UpperRange ,0 ,"ndis5"
HKR,NDI\Interfaces ,LowerRange ,0 ,"ethernet"
[COMMON.reg]
HKR, ,ListenInterval ,0 ,"3"
HKR, ,RTSThresh ,0 ,"2432"
HKR, ,FragThresh ,0 ,"2432"
HKR, ,PreambleMode ,0 ,"2"
HKR, ,AuthentAlg ,0 ,"65535"
HKR, ,IMWEBIOC ,0 ,"1"
HKR,defaults,ListenInterval,0,3
HKR,Ndi\params\ListenInterval,default,0,3
HKR,NDI\params\ListenInterval,ParamDesc,,%LISTENINTERVAL_STR%
HKR,NDI\params\ListenInterval,type,,int
HKR,NDI\params\ListenInterval,flag,1,30,00,00,00
HKR,NDI\params\ListenInterval,min,0,0
HKR,NDI\params\ListenInterval,max,0,77
HKR,NDI\params\ListenInterval,step,0,1
HKR,NDI\params\ListenInterval,optional,0,1
HKR,defaults,RTSThresh,0,2432
HKR,Ndi\params\RTSThresh,default,0,2432
HKR,NDI\params\RTSThresh,ParamDesc,0,%RTSTHRESH_STR%
HKR,NDI\params\RTSThresh,type,0,int
HKR,NDI\params\RTSThresh,flag,1,20,00,00,00
HKR,NDI\params\RTSThresh,min,0,0
HKR,NDI\params\RTSThresh,max,0,2432
HKR,NDI\params\RTSThresh,step,0,64
HKR,NDI\params\RTSThresh,optional,0,1
HKR,defaults,FragThresh,0,2432
HKR,Ndi\params\FragThresh,default,0,2432
HKR,NDI\params\FragThresh,ParamDesc,0,%FRAGTHRESH_STR%
HKR,NDI\params\FragThresh,type,0,int
HKR,NDI\params\FragThresh,flag,1,20,00,00,00
HKR,NDI\params\FragThresh,min,0,256
HKR,NDI\params\FragThresh,max,0,2432
HKR,NDI\params\FragThresh,step,0,128
HKR,NDI\params\FragThresh,optional,0,1
HKR,defaults,PreambleMode,0,2
HKR,Ndi\params\PreambleMode,default,0,2
HKR,NDI\params\PreambleMode,ParamDesc,,%SHORT_PREAM_STR%
HKR,NDI\params\PreambleMode,type,,enum
HKR,NDI\params\PreambleMode,flag,1,30,00,00,00
HKR,NDI\params\PreambleMode\enum,2,,"Short Tx Preamble"
HKR,NDI\params\PreambleMode\enum,0,,"Long Tx Preamble"
HKR,NDI\params\PreambleMode,optional,0,1
HKR,defaults,AuthentAlg,0,65535
HKR,NDI\params\AuthentAlg,default,0,65535
HKR,NDI\params\AuthentAlg,ParamDesc,,%AUTHENT_TYPE_STR%
HKR,NDI\params\AuthentAlg,type,,enum
HKR,NDI\params\AuthentAlg,flag,1,30,00,00,00
HKR,NDI\params\AuthentAlg\enum,0,,"WECA Compliant (always use Open)"
HKR,NDI\params\AuthentAlg\enum,1,,"Must use Shared with WEP"
HKR,NDI\params\AuthentAlg\enum,65535,,"Automatic based on WEP setting"
HKR,NDI\params\AuthentAlg,optional,0,1
[DestinationDirs]
DefaultDestDir=11 ; Win9x=%windir%\system Win2k=%windir%\system32
IMWEB_DRIVER.copy=11 ; Win9x=%windir%\system
IMWEB_DRIVER.copy.ME=11 ; Win9x=%windir%\system
IMWEB_DRIVER.copy.NT=12 ; Win2k=%windir%\system32\drivers
IMWEB_DRIVER.copy.NT.5.1=12 ; WinXP=%windir%\system32\drivers
[IMWEB_NDI.copy]
IMWEBR16.dll ; Win9x NDI
IMWEBCFG.dll ; Win9x NDI
[IMWEB_NDI.copy.ME]
IMWEBR16.dll ; Win9x NDI
IMWEBCFG.dll ; Win9x NDI
[IMWEB_COINSTALL.copy.ME]
[IMWEB_COINSTALL.copy.NT]
[IMWEB_DRIVER.copy]
IMWEBN5.sys
IMWEBIOC.vxd ; Win9x Ioctl interface
[IMWEB_DRIVER.copy.ME]
IMWEBN5.sys
IMWEBIOC.vxd ; Win9x Ioctl interface
[IMWEB_DRIVER.copy.NT]
IMWEBN5.sys
[IMWEB_DRIVER.copy.NT.5.1]
IMWEBN5.sys
[IMWEB_APPLET.copy]
[IMWEB_APPLET.copy.ME]
[IMWEB_APPLET.copy.NT]
[SourceDisksNames]
1=%INSTALL_DISK_STR%,,,
[SourceDisksFiles] ; Win9x
IMWEBN5.sys=1
[SourceDisksFiles.ME] ; WinMe
IMWEBN5.sys=1
[SourceDisksFiles.X86] ; Win2k
IMWEBN5.sys=1
[SourceDisksFiles.NT.5.1] ; WinXP
IMWEBN5.sys=1
[Strings]
VER_VENDOR_STR="Intel"
VER_VENDOR_NAME_STR="Intel Corporation"
IMWEB_PCI1_STR="Intel(R) PRO/Wireless 2011b LAN 3A Mini PCI Adapter"
IMWEB_PCI2_STR="Intel(R) PRO/Wireless 2011b LAN 3B Mini PCI Adapter"
IMWEB_SERVICE_DISPLAY="Intel(R) PRO/Wireless 2011b LAN Mini PCI LAN Driver"
INSTALL_DISK_STR="Intel(R) PRO/Wireless 2011b LAN Mini PCI Install Disk"
ADHOC_DEMO_STR="Adhoc Demo Mode"
SHORT_PREAM_STR="Preamble Mode"
RTSTHRESH_STR="RTS Threshold"
FRAGTHRESH_STR="Fragmentation Threshold"
AUTHENT_TYPE_STR="Authentication Algorithm"
LISTENINTERVAL_STR="Listen Interval"

