
[Version]
DriverVer=11/13/2003, 1.0.5.1000
Signature="$Chicago$"
Compatible=1
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%VER_VENDOR_STR%
[ControlFlags]
ExcludeFromSelect=*
[Manufacturer]
%VER_VENDOR_NAME_STR%=DeviceList,NTx86
[DeviceList]
[DeviceList.NTx86]
%A021_DESC_STR%=WG121_A021, USB\VID_0846&PID_4200
%A021_DESC_STR%=WG121_A022, USB\VID_0846&PID_4210
[WG121_A021] ; Win9x
AddReg=WG121_A021.reg, COMMON_A02.reg, COMMON_NDIS.reg, COMMON.reg
;CpyFiles=WG121_DRIVER.copy
[WG121_A022] ; Win9x
AddReg=WG121_A022.reg, COMMON_A02.reg, COMMON_NDIS.reg, COMMON.reg
;CpyFiles=WG121_DRIVER.copy
[WG121_A021.NT] ; Win2k
AddReg=WG121_A021.reg, COMMON_A02.reg.NT, COMMON_NDIS.reg.NT, COMMON.reg
;CpyFiles=WG121_DRIVER.copy.NT
BusType=0
Characteristics= 0x84
[WG121_A022.NT] ; Win2k
AddReg=WG121_A022.reg, COMMON_A02.reg.NT, COMMON_NDIS.reg.NT, COMMON.reg
;CpyFiles=WG121_DRIVER.copy.NT
BusType=0
Characteristics= 0x84
[WG121_A021.NT.Services]
AddService= "wg121", 2, WG121_DRIVER_A02.Service, WG121_DRIVER.EventLog
[WG121_A022.NT.Services]
AddService= "wg121", 2, WG121_DRIVER_A02.Service, WG121_DRIVER.EventLog
[WG121_A021.reg]
HKR,Ndi,DeviceID,0,"USB\VID_0846&PID_4200"
HKR,,PlatformID,0,14480
HKR,,VendorDesc,0,%A021_DESC_STR%
HKR,,FWFileName,0,"PRISMA02.arm"
[WG121_A022.reg]
HKR,Ndi,DeviceID,0,"USB\VID_0846&PID_4210"
HKR,,PlatformID,0,14480
HKR,,VendorDesc,0,%A021_DESC_STR%
HKR,,FWFileName,0,"PRISMA02.arm"
[WG121_DRIVER_A02.Service]
DisplayName=%A02_SERVICE_STR%
ServiceType=1 ; SERVICE_KERNEL_DRIVER
StartType=3 ; SERVICE_DEMAND_START
ErrorControl=1 ; NORMAL
ServiceBinary=%12%\wg121nd5.sys
LoadOrderGroup=NDIS
[WG121_DRIVER.EventLog]
AddReg=WG121_DRIVER.EventLog.reg
[WG121_DRIVER.EventLog.reg]
HKR, ,EventMessageFile ,0x00020000 ,"%%SystemRoot%%\System32\netevent.dll"
HKR, ,TypesSupported ,0x00010001 ,7
[COMMON_A02.reg]
HKR,NDI ,Service ,0 ,"wg121"
HKR,NDI ,CardType ,0 ,"USB"
HKR, ,BusType ,0 ,"0"
HKR, ,DeviceVxDs ,0 ,"wg121_9x.sys"
[COMMON_A02.reg.NT]
HKR,NDI ,Service ,0 ,"wg121"
HKR,NDI ,CardType ,0 ,"USB"
HKR, ,BusType ,0 ,"0"
HKR, ,DeviceVxDs ,0 ,"wg121nd5.sys"
[COMMON_NDIS.reg]
HKR, ,RunningWin9X ,0 ,"1"
HKR, ,DevLoader ,0 ,"*ndis"
HKR, ,EnumPropPages ,0 ,"netdi.dll,EnumPropPages"
HKR,NDI\Interfaces ,UpperRange ,0 ,"ndis3"
HKR,NDI\Interfaces ,LowerRange ,0 ,"ethernet"
HKR,NDI\Interfaces ,DefUpper ,0 ,"ndis3"
HKR,NDI\Interfaces ,DefLower ,0 ,"ethernet"
HKR,NDIS ,LogDriverName ,0 ,"wg121_9x"
HKR,NDIS ,MajorNdisVersion ,1 ,03
HKR,NDIS ,MinorNdisVersion ,1 ,0a
[COMMON_NDIS.reg.NT]
HKR,NDI\Interfaces ,UpperRange ,0 ,"ndis5"
HKR,NDI\Interfaces ,LowerRange ,0 ,"ethernet"
[COMMON.reg]
HKR, ,wg121 ,0 ,"1"
HKR, ,SilentInstall ,0 ,"1"
HKR,NDI\params\ShortRetryLimit,,0,7
HKR,NDI\params\ShortRetryLimit,default,0,7
HKR,NDI\params\ShortRetryLimit,ParamDesc,,%SHORT_RETRY_STR%
HKR,NDI\params\ShortRetryLimit,type,,int
HKR,NDI\params\ShortRetryLimit,min,0,1
HKR,NDI\params\ShortRetryLimit,max,0,255
HKR,NDI\params\ShortRetryLimit,step,0,1
HKR,NDI\params\ShortRetryLimit,optional,0,1
HKR,NDI\params\LongRetryLimit,,0,4
HKR,NDI\params\LongRetryLimit,default,0,4
HKR,NDI\params\LongRetryLimit,ParamDesc,,%LONG_RETRY_STR%
HKR,NDI\params\LongRetryLimit,type,0,int
HKR,NDI\params\LongRetryLimit,min,0,1
HKR,NDI\params\LongRetryLimit,max,0,255
HKR,NDI\params\LongRetryLimit,step,0,1
HKR,NDI\params\LongRetryLimit,optional,0,1
HKR, ,ConfigProfile ,0 ,"256"
[DestinationDirs]
DefaultDestDir=11 ; Win9x=%windir%\system Win2k=%windir%\system32
WG121_DRIVER.copy=11 ; Win9x=%windir%\system
WG121_DRIVER.copy.NT=12 ; Win2k=%windir%\system32\drivers
[WG121_DRIVER.copy]
wg121_9x.sys
wg121.vxd ; Win9x Ioctl interface
[WG121_DRIVER.copy.NT]
wg121nd5.sys
[SourceDisksNames]
1=%INSTALL_DISK_STR%,,,
[SourceDisksFiles] ; Win9x
wg121.vxd=1
wg121_9x.sys=1
[SourceDisksFiles.X86] ; Win2k/Xp
wg121nd5.sys=1
[Strings]
VER_VENDOR_STR="NETGEAR, Inc."
VER_VENDOR_NAME_STR="NETGEAR, Inc."
INSTALL_DISK_STR="NETGEAR WG121 Wireless LAN Install Disk"
A021_DESC_STR="NETGEAR WG121 802.11g Wireless USB2.0 Adapter"
A02_SERVICE_STR="NETGEAR WG121 802.11g Wireless USB2.0 Adapter"
ON_STR="On"
OFF_STR="Off"
SHORT_RETRY_STR="Short Retry Limit"
LONG_RETRY_STR="Long Retry Limit"
CONFIG_PROFILE="Configuration Profile"
CONFIG_PROF_B_ONLY="B only"
CONFIG_PROF_MIXED="Mixed"
CONFIG_PROF_MIXED_LONG="Mixed Long"
CONFIG_PROF_G_ONLY="G only"
CONFIG_PROF_TEST="Test"
CONFIG_PROF_B_WIFI="B WiFi"
CONFIG_PROF_MIXED_SHORT="Mixed Short"
CONFIG_PROF_WIFI_SPEC="WiFi Spec"

