
[Version]
Signature="$Chicago$"
Compatible=1
Class=Net
ClassGUID={4d36e972-e325-11ce-bfc1-08002be10318}
MillenniumPreferred=.ME
Provider=%INFProvider%
CatalogFile=zd1201u.cat ; for WHQL certified
DriverVer=01/06/2004, 1.97.106.2004
[Manufacturer]
%Manufacturer%=ZyDAS, NT.5.1
[ControlFlags]
[ZyDAS]
%ZD1201_50U_DESC%=ZD1201_50U.ndi, USB\VID_0ACE&PID_1201
[ZyDAS.NT.5.1]
%ZD1201_50U_DESC%=ZD1201XP_50U.ndi, USB\VID_0ACE&PID_1201
[ZD1201_50U.ndi]
AddReg=ZD1201_Win9x.reg, ZD1201_Common.reg, UnZDRegistryUSB.reg
;CpyFiles=ZD1201.CopyFiles98
DriverVer=01/06/2004, 1.97.106.2004
[ZD1201_Win9x.reg]
HKR,NDI, DeviceID, 0, %ZD1201_50U_PNP%
HKR,NDI, CardType, 0, %CardType%
HKR,, DevLoader, 0, "*ndis"
HKR,, DeviceVxDs, 0, %DriverFileName%
HKR,NDIS, MajorNdisVersion, 1, 03
HKR,NDIS, MinorNdisVersion, 1, 0A
HKR,NDIS, LogDriverName, 0, %CustomServiceName%(%Manufacturer%)
HKR,NDI\Interfaces, DefUpper, 0, "ndis3"
HKR,NDI\Interfaces, DefLower, 0, "ethernet"
HKR,NDI\Interfaces, UpperRange, 0, "ndis3"
HKR,NDI\Interfaces, LowerRange, 0, "ethernet"
HKR,, BusType, 0, 15
HKR,, IOBaseAddress, 1, 02,00,00,00
HKR,, InterruptNumber, 1, 04,00,00,00
HKR,, EnumPropPages, 0, "netdi.dll,EnumPropPages"
HKR,NDI\Install, ndis3, 0, "ZD1201.ndis3"
HKR,, VendorDesc, 0, %VendorDesc%
[ZD1201.CopyFiles98]
ZD1201U.sys,ZD1U98.sys,,2
[ZD1201_50U.ndi.ME]
Characteristics=0x84
BusType=15
AddReg=ZD1201_WinMe.reg, ZD1201_Common.reg, UnZDRegistryUSB.reg
;CpyFiles=ZD1201.CopyFilesMe
[ZD1201_50U.ndi.ME.Services]
AddService=%CustomServiceName%(%Manufacturer%), 2, ZD1201U_ME.Service, ZD1201U.EventLog
[ZD1201_WinMe.reg]
HKR,NDI, Service, 0, %CustomServiceName%(%Manufacturer%)
HKR,, DevLoader, 0, "*ndis"
HKR,, DeviceVxDs, 0, %DriverFileName%
HKR,, EnumPropPages, 0, "netdi.dll,EnumPropPages"
HKR,NDIS, MajorNdisVersion, 1, 05
HKR,NDIS, MinorNdisVersion, 1, 00
HKR,NDIS, LogDriverName, 0, %CustomServiceName%(%Manufacturer%)
HKR,NDI\Interfaces, DefUpper, 0, "ndis5"
HKR,NDI\Interfaces, DefLower, 0, "ethernet"
HKR,NDI\Interfaces, UpperRange, 0, "ndis5"
HKR,NDI\Interfaces, LowerRange, 0, "ethernet"
HKR,NDI\Install, ndis3, 0, "ZD1201.ndis5me"
HKR,, VendorDesc, 0, %VendorDesc%
[ZD1201.ndis5me]
;CpyFiles=ZD1201.CopyFilesMe
[ZD1201.CopyFilesMe]
ZD1201U.sys,ZD1UME.sys,,2
[ZD1201U_ME.Service]
DisplayName=%ZD1201U.Service.DispName%(%Manufacturer%)
ServiceType=1 ; %SERVICE_KERNEL_DRIVER%
StartType=3 ; %SERVICE_DEMAND_START%
ErrorControl=1 ; %SERVICE_ERROR_NORMAL%
ServiceBinary=%11%\%DriverFileName% ; %11%\zd1201u.sys
LoadOrderGroup=NDIS
[ZD1201_50U.ndi.NTx86]
Characteristics=0x84
BusType=15
AddReg=ZD1201_Win2K.reg, ZD1201_Common.reg, UnZDRegistryUSB.reg
;CpyFiles=ZD1201.CopyFiles2K
[ZD1201_50U.ndi.NTx86.Services]
AddService=%CustomServiceName%(%Manufacturer%), 2, ZD1201U_NT.Service, ZD1201U.EventLog
[ZD1201_Win2K.reg]
HKR,NDI\Interfaces, UpperRange, 0, "ndis5"
HKR,NDI\Interfaces, LowerRange, 0, "ethernet"
HKR,NDI, Service, 0, %CustomServiceName%(%Manufacturer%)
HKR,, VendorDesc, 0, %VendorDesc%
[ZD1201.CopyFiles2K]
ZD1201U.sys,ZD1U2K.sys,,2
[ZD1201XP_50U.ndi.NTx86]
Characteristics=0x84
BusType=15
AddReg=ZD1201_WinXP.reg, ZD1201_Common.reg, UnZDRegistryUSB.reg
;CpyFiles=ZD1201.CopyFilesXP
[ZD1201XP_50U.ndi.NTx86.Services]
AddService=%CustomServiceName%(%Manufacturer%), 2, ZD1201U_NT.Service, ZD1201U.EventLog
[ZD1201_WinXP.reg]
HKR,NDI\Interfaces, UpperRange, 0, "ndis5"
HKR,NDI\Interfaces, LowerRange, 0, "ethernet"
HKR,NDI, Service, 0, %CustomServiceName%(%Manufacturer%)
HKR,, VendorDesc, 0, %VendorDesc%
[ZD1201.CopyFilesXP]
ZD1201U.sys,ZD1UXP.sys,,2
[ZD1201U_NT.Service]
DisplayName=%ZD1201U.Service.DispName%(%Manufacturer%)
ServiceType=1 ; %SERVICE_KERNEL_DRIVER%
StartType=3 ; %SERVICE_DEMAND_START%
ErrorControl=1 ; %SERVICE_ERROR_NORMAL%
ServiceBinary=%12%\%DriverFileName% ; %12%\%DriverFileName%
LoadOrderGroup=NDIS
[ZD1201U.EventLog]
Addreg=ZD1201U.AddEventLog.reg
[ZD1201U.AddEventLog.reg]
HKR,, EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR,, TypesSupported, 0x00010001, 7
[DestinationDirs]
ZD1201.CopyFiles98=11 ; system subdirectory on Win 98
ZD1201.CopyFilesMe=11 ; system subdirectory on Win Me
ZD1201.CopyFiles2K=12 ; system32\drivers subdirectory on Win NT/2000
ZD1201.CopyFilesXP=12 ; system32\drivers subdirectory on Win XP
[SourceDisksNames]
1=%DISKNAME%,,,
[SourceDisksFiles]
ZD1U98.sys=1
ZD1UME.sys=1
ZD1U2K.sys=1
ZD1UXP.sys=1
[ZD1201_Common.reg]
HKR,, NetworkType, 0, "1"
HKR,NDI\params\NetworkType, ParamDesc, 0, "Network Type"
HKR,NDI\params\NetworkType, type, 0, "enum"
HKR,NDI\params\NetworkType, flag, 1, 30,00,00,00
HKR,NDI\params\NetworkType, default, 0, "1"
HKR,NDI\params\NetworkType\enum, "0", 0, "Ad-Hoc"
HKR,NDI\params\NetworkType\enum, "1", 0, "Infrastructure"
HKR,NDI\params\NetworkType\enum, "3", 0, "Pseudo IBSS"
HKR,NDI\params\NetworkAddress, ParamDesc, 0, "Network Address"
HKR,NDI\params\NetworkAddress, type, 0, "edit"
HKR,NDI\params\NetworkAddress, default, 0, "000000000000"
HKR,NDI\params\NetworkAddress, LimitText, 0, "12"
HKR,NDI\params\NetworkAddress, UpperCase, 0, "1"
HKR,NDI\params\NetworkAddress, Optional, 0, "1"
HKR,, SSID, 0, %Def_SSID%
HKR,NDI\params\SSID, ParamDesc, 0, "SSID"
HKR,NDI\params\SSID, type, 0, "edit"
HKR,NDI\params\SSID, flag, 1, 30,00,00,00
HKR,NDI\params\SSID, default, 0, %Def_SSID%
HKR,NDI\params\SSID, limitText, 0, "32"
HKR,, RFChannel, 0, %Def_Channel%
HKR,NDI\params\RFChannel, ParamDesc, 0, "Channel"
HKR,NDI\params\RFChannel, type, 0, "enum"
HKR,NDI\params\RFChannel, flag, 1, 30,00,00,00
HKR,NDI\params\RFChannel, default, 0, %Def_Channel%
HKR,NDI\params\RFChannel\enum, "1", 0, "Channel 1"
HKR,NDI\params\RFChannel\enum, "2", 0, "Channel 2"
HKR,NDI\params\RFChannel\enum, "3", 0, "Channel 3"
HKR,NDI\params\RFChannel\enum, "4", 0, "Channel 4"
HKR,NDI\params\RFChannel\enum, "5", 0, "Channel 5"
HKR,NDI\params\RFChannel\enum, "6", 0, "Channel 6"
HKR,NDI\params\RFChannel\enum, "7", 0, "Channel 7"
HKR,NDI\params\RFChannel\enum, "8", 0, "Channel 8"
HKR,NDI\params\RFChannel\enum, "9", 0, "Channel 9"
HKR,NDI\params\RFChannel\enum, "10", 0, "Channel 10"
HKR,NDI\params\RFChannel\enum, "11", 0, "Channel 11"
HKR,NDI\params\RFChannel\enum, "12", 0, "Channel 12"
HKR,NDI\params\RFChannel\enum, "13", 0, "Channel 13"
HKR,NDI\params\RFChannel\enum, "14", 0, "Channel 14"
HKR,, TxDataRate, 0, %Def_TxDataRate%
HKR,NDI\params\TxDataRate, ParamDesc, 0, "Transmit Data Rate"
HKR,NDI\params\TxDataRate, type, 0, "enum"
HKR,NDI\params\TxDataRate, flag, 1, 30,00,00,00
HKR,NDI\params\TxDataRate, default, 0, %Def_TxDataRate%
HKR,NDI\params\TxDataRate\enum, "1", 0, "1M bps "
HKR,NDI\params\TxDataRate\enum, "2", 0, "2M bps "
HKR,NDI\params\TxDataRate\enum, "4", 0, "5.5M bps"
HKR,NDI\params\TxDataRate\enum, "8", 0, "11M bps "
HKR,NDI\params\TxDataRate\enum, "15", 0, "Auto "
HKR,, RTSCTSThreshold, 0, "2305"
HKR,NDI\Params\RTSCTSThreshold, ParamDesc, 0, "RTS/CTS Threshold"
HKR,NDI\Params\RTSCTSThreshold, Type, 0, "int"
HKR,NDI\params\RTSCTSThreshold, flag, 1, 30,00,00,00
HKR,NDI\Params\RTSCTSThreshold, Default, 0, "2305"
HKR,NDI\Params\RTSCTSThreshold, Min, 0, "0"
HKR,NDI\Params\RTSCTSThreshold, Max, 0, "2305"
HKR,NDI\Params\RTSCTSThreshold, Step, 0, "1"
HKR,NDI\Params\RTSCTSThreshold, Base, 0, "10"
HKR,, FragmentThreshold, 0, "2305"
HKR,NDI\Params\FragmentThreshold, ParamDesc, 0, "Fragmentation Threshold"
HKR,NDI\Params\FragmentThreshold, Type, 0, "int"
HKR,NDI\params\FragmentThreshold, flag, 1, 30,00,00,00
HKR,NDI\Params\FragmentThreshold, Default, 0, "2305"
HKR,NDI\Params\FragmentThreshold, Min, 0, "0"
HKR,NDI\Params\FragmentThreshold, Max, 0, "2305"
HKR,NDI\Params\FragmentThreshold, Step, 0, "1"
HKR,NDI\Params\FragmentThreshold, Base, 0, "10"
HKR,, PowerSaveMode, 0, "0"
HKR,NDI\params\PowerSaveMode, ParamDesc, 0, "Power Save Mode"
HKR,NDI\params\PowerSaveMode, type, 0, "enum"
HKR,NDI\params\PowerSaveMode, flag, 1, 30,00,00,00
HKR,NDI\params\PowerSaveMode, default, 0, "0"
HKR,NDI\params\PowerSaveMode\enum, "0", 0, "Disabled"
HKR,NDI\params\PowerSaveMode\enum, "1", 0, "Enabled "
HKR,, PowerSaveLevel, 0, "0"
HKR,NDI\params\PowerSaveLevel, ParamDesc, 0, "Power Save Level"
HKR,NDI\params\PowerSaveLevel, type, 0, "enum"
HKR,NDI\params\PowerSaveLevel, flag, 1, 30,00,00,00
HKR,NDI\params\PowerSaveLevel, default, 0, "0"
HKR,NDI\params\PowerSaveLevel\enum, "0", 0, "Level 0"
HKR,NDI\params\PowerSaveLevel\enum, "1", 0, "Level 1"
HKR,, AuthentMode, 0, "3"
HKR,NDI\params\AuthentMode, ParamDesc, 0, "Authentication Mode"
HKR,NDI\params\AuthentMode, type, 0, "enum"
HKR,NDI\params\AuthentMode, flag, 1, 30,00,00,00
HKR,NDI\params\AuthentMode, default, 0, "3"
HKR,NDI\params\AuthentMode\enum, "1", 0, "Open system"
HKR,NDI\params\AuthentMode\enum, "2", 0, "Shared key"
HKR,NDI\params\AuthentMode\enum, "3", 0, "Auto"
HKR,, WEPStatus, 0, "0"
HKR,NDI\params\WEPStatus, ParamDesc, 0, "WEP Encryption"
HKR,NDI\params\WEPStatus, type, 0, "enum"
HKR,NDI\params\WEPStatus, flag, 1, 30,00,00,00
HKR,Ndi\params\WEPStatus, default, 0, "0"
HKR,NDI\params\WEPStatus\enum, 0, 0, "Disabled"
HKR,NDI\params\WEPStatus\enum, 2, 0, "Enabled (64 bit)"
HKR,NDI\params\WEPStatus\enum, 6, 0, "Enabled (128 bit)"
HKR,, FirmwareName, 0, %FirmwareFileName%
HKR,, WEPDefaultKeyId, 0, 1
HKR,, WEPDefaultKeys, 0, "1011121314101112131410111213141011121314"
HKR,, WEPEncryptInDriver,0, 1
HKR,, WEPDecryptInDriver,0, 0
HKR,, ATIMWindow, 0, 0
HKR,, TxPowerControl, 0, 1 ; Enable Tx Power Control process.
HKR,, AntennaSelect, 0, 2 ; Tx/Rx all use Antenna 2. Antenna auto select process is active.
[UnZDRegistryUSB.reg]
HKLM,SOFTWARE\Microsoft\Windows\CurrentVersion\Uninstall\UNZD1201%InterfaceType%,DEL_HKR_0000,0,"ENUM\"%ZD1201_50U_PNP%
[Strings]
INFProvider="ZyDAS"
Manufacturer="ZyDAS"
DISKNAME="ZyDAS ZD1201 IEEE 802.11b Wireless LAN Driver (USB) Installation Disk"
DriverFileName="zd1201u.sys"
InterfaceType="USB"
CardType="PNP"
VendorDesc="ZyDAS ZD1201 802.11b Wireless LAN"
CustomServiceName="ZD1201U"
ZD1201_50U_DESC="(ZD1201)IEEE 802.11b USB Adapter"
ZD1201_50U_PNP="USB\VID_0ACE&PID_1201"
Def_SSID=""
Def_Channel="6"
Def_TxDataRate="15"
ZD1201U.Service.DispName="ZyDAS ZD1201 IEEE 802.11b Wireless LAN Driver (USB)"
