PCTV Systems TVCenter

LESMEG-fil for programversjon  6.4.9                 2014-10-31 

------------------------------------------------------------------------------------------------------

Denne filen inneholder viktig informasjon for bruk av PCTV Systems TVCenter. Vennligst les både manualen og denne filen hvis det oppstår problemer med programvaren.

Innhold:

1.00  Viktige tips
1.1 DistanTV mobile
1.2 TVCenter long start delay
2.00  Støttet maskinvare
   2.1 Broadway 2T
3.00  Støttede operativsystemer
4.00  Tips om bruk
5.00  Kjente begrensninger
6.00  Endringer
7.00  PCTV Systems Support
8.00  Additional License Information

-----------------------------------------------------------------------------------------------------

1.00 Viktige tips

1.1 DistanTV mobile

1.1.1 Supported operating systems on client devices
DistanTV mobile supports TV streaming to both Windows and Macintosh systems. Following the list of supported operating systems:
§	Microsoft Windows XP - with Service Pack 3 or higher (32bit)
§	Microsoft Windows Media Center Edition 2005 - with Service Pack 3 or higher (32bit)
§	Microsoft Windows Vista - with Service Pack 2 or higher 
§	Microsoft Windows 7
§	Microsoft Windows 8
§	MAC OS 10.5 (Leopard) - with installed Adobe Flash Player
§	MAC OS 10.6 (Snow Leopard)

1.1.2 Operation tips for users outside the USA
Please make sure you only select SD (standard definition) TV channels when using DistanTV mobile (live TV streaming). Example: Instead of selecting the channel “Arte HD”, you should select the corresponding channel in SD (“Arte”). Don’t worry, there is no negative impact on the picture and sound quality you get on your streaming client device (e.g. iPad) when selecting an SDTV instead of an HDTV channel.

1.1.3 Known limitations
Distorted DistanTV mobile user interface during local network streaming with Internet Explorer 8
If you are using DistanTV mobile in your local network with Internet Explorer 8 on a Windows XP system, the DistanTV mobile UI may look distorted (showing wrong colors and missing text). The root cause of this issue is a malfunction of Internet Explorer 8 (IE8) in “Local intranet” mode. 
To solve this problem, the automatic detection of the Intranet has to be disabled. To do so follow these steps:
- from the IE8 command bar, select Tools > Internet Options > Security
- select Local intranet 
- click on the Sites-button
- disable all check boxes for automatic intranet detection. 
Alternatively, you can connect to the server PC by typing in the address-field of the browser its IP address instead of the server name. Here you can find the IP-address of the server: TVCenter Settings > DistanTV mobile > Summary > Local Access. 

1.2 TVCenter long start delay 
The long start delay can be caused by certificate verification of .Net framework without a valid internet connection.
Workaround: 
uncheck the option Check for publisher's certificate revocation in the MS Internet Explorer. 
To do so follow these steps:
- open Internet Explorer 
- form the menu bar select Tools > Internet Options > Advanced 
- scroll in the list to Security 
- uncheck the option Check for publisher's certificate revocation

-----------------------------------------------------------------------------------------------------

2.00 Støttet maskinvare

Broadway 2T
PCTV 73A
PCTV 73e Solo
PCTV 73e 
PCTV 74e
PCTV 76e
PCTV 77e
PCTV 78e
PCTV 79e
PCTV 80e
PCTV 170e
PCTV 171e
PCTV 282e
PCTV 290e
PCTV 292e
PCTV 310i
PCTV 330e
PCTV 340e
PCTV 340eSE
PCTV 460e
PCTV 461e
PCTV 510e
PCTV 520e
PCTV 521e
PCTV 800i
PCTV 801e
PCTV 801eSE
PCTV 2000i
PCTV 2001e
PCTV 2002e
PCTV 4000i

2.1 Broadway 2T

2.1.1 Windows MediaCenter support
- It is recommened to use a LAN or a fast WLAN connection (801.11n ).
- Use one Tuner only.

2.1.2 SSID
- It is recommened not do disable or hide the SSID of your WLAN.

2.1.3 Password characters limitation
- Only the following characters are supported . 
  Letters: 	(a ... z) and (A ... Z)
  Numbers : 	(0 ... 9)
  Special : 	!#$%&()*+,-./:<=>?@ []^_{|}~ 

2.1.4 WAN streaming: advanced router configuration
- Some routers require to enable port triggering for the streaming port of Broadway 2T. 
In this case please enable this feature in your router settings.  

2.1.5 WAN streaming : upload speed
- In most cases you will not reach the theoretic upload performance as promised by your provider. Please check your real upload speed. If you try to stream with a bandwidth higher than your real upload speed, the appliaction can be jerky and/or instable.

-----------------------------------------------------------------------------------------------------

3.00 Støttede operativsystemer

§	Microsoft Windows XP Service Pakke 3 eller høyere (32bit)
§	Microsoft Windows Media Center Edition 2005 with Service Pack 3 or higher (32bit)
§	Microsoft Windows Vista with Service Pack 2 or higher 
§	Microsoft Windows 7
§	Microsoft Windows 8

Installering krever administratorrettigheter. For å bruke programvaren er det nok å være "standardbruker" (gruppe: hovedbrukere) eller høyere.

Det anbefales at alle aktuelle Windows Service Pakker er installert.
In addition to that, following  Microsoft-software should be installed on your PC: 
§ .NET Framework 3.5 Service Pack 1 and 
§ .NET Framework 3.5 Family Update for .NET versions 2.0 through 3.5 (KB951847) x86'
You can download  the software under: http://www.microsoft.com/downloads/details.aspx?FamilyId=AB99342F-5D1A-413D-8319-81DA479AB0D7&displaylang=en

-----------------------------------------------------------------------------------------------------

4.00 Tips om bruk
Merk: Enkelte funksjoner er ikke tilgjengelig i alle produktene. Disse funksjonene er merket med (*)

Microsoft Windows Media Center

§ En tilleggsdriver for MS WMC finnes på CD’en i mappen <Windows Media Center>. Denne driveren lar deg benytte hardware delen i selve WMC uten TVCenterprogramvaren.
§ TV funksjonaliteten i WMC miljøet krever en godkjent DVD dekoder

Kongfigurering av video klargjører

Du kan konfigurer og justere din forhåndsvisning gjennom å velge ulike videooppsett fra din Video klargjøringsmeny.
For å velge et nytt videooppsett, åpner du TVCenter konfigureringsapplikasjon og fra menyen velger du så TV titting > Avanserte konfigurasjoner - Videoutgang > Video klargjører.

Signal Forsterker  (integrert forsterker)*

§ Signalforsterkeren øker mottakelsen av svake signaler, f.eks. når du bruker en bærbar antenne.
§ Dersom signalene er sterke, som f.eks ved bruk av en forsterket takantenne, bør Signalforsterkeren slåes av for å unngå overdreven bruk av denne.

Default video parameter - regarding followiong hardware: 100i, 110i, 300i, 310i

The default value for contrast and saturation is "75" (and not "50", like for the other values)

-----------------------------------------------------------------------------------------------------

5.00 Kjente begrensninger

§ Dersom du kobler fra en USB enhet, anbefaler vi at du venter minst 10 sekunder før du kobler den til igjen. Dette for å unngå at det kan oppstå problem med å identifisere enheten igjen.

-----------------------------------------------------------------------------------------------------

6.00 Endringer

§	6.4.8 à 6.4.9
	§	add EPG language selector
	§	H.264 decoder improvements
	§	AAC audio decoder improved

§	6.4.7 à 6.4.8
	§	add PCTV 79e
	§	add PCTV 292e
	§	Win8.1 improvements

§	6.4.6 à 6.4.7
	§	add PCTV 291e
	§	add PCTV 521e
	§	Win8 improvements

§	6.4.4 à 6.4.5
	§	add PCTV 78e
	§	Win8 support improvements

§	6.4.3 à 6.4.4
	§	add PCTV 77e

§	6.4.2 à 6.4.3
	§	add PCTV 76e

§	6.4.1 à 6.4.2
	§	add PCTV 76e
	§	improve H.264 decoder stability

§	6.4.0 à 6.4.1
	§	add Broadway 2T
	§	improve H.264 decoder stability
	§	add DVB-C support for: Sweden, Denmark and Spain

§	6.3.2 à 6.4.0
	§	add DistanTV mobile 2
	§	add Internal EPG Viewer
	§	add TitanTV support (US only)
	§	add Parental Control (US only)
	§	add Closed caption (US only)
	§	Converter: reworked	
	§	optimized H.264 decoder with DXVA support
	§	expand hardware support

§	6.3.1 à 6.3.2
	§	expand hardware support

§	6.3.0 à 6.3.1
	§	expand hardware support

§	6.2.0 à 6.3.0.
	§	expand hardware support
§	add DistanTV mobile: iPhone® / iPod touch®  TV streaming  
	§	add DVB-S / DVB-S2 support
§	expand scheduler: add recurrence
	§	optimized H.264 decoder  
§	add separat driver installation

§	6.1.0 à 6.2.0.
	§	utvid maskinvarestøtte	
	§	legg til fm radio
§	legg til analog TV support
§	legg til konfigurerbar video klargjører
§	lelg til multi tuner støtte
§	legg til Dolby Digital+ (E-AC3) støtte
§	legg til fjernkontrollstøtte

§	6.0.0 à 6.1.0.
	§	utvid maskinvarestøtte	
	§	legg til radio
	§	legg til DistanTV
	§	legg til Kanal redigeringsfunksjon
	§	forbedring av kanal søketiden
§	utvid språkstøtte

-----------------------------------------------------------------------------------------------------

7.00 PCTV Systems Support

Nye versjoner av PCTV SystemsTVCenter programvare er tilgjengelige på PCTV Systems' nettside:

http://www.pctvsystems.com/

Husk å være klar til å gi følgende opplysninger ved henvendelse til PCTV Systems Support:

  1.  Produkt:
  2.  Serie nummer:
  3.  Programvare  versjon:
  4.  Operativsystem versjon:
  5.  Hovedkort:
  6.  CPU: 	
  7.  RAM: 
  8.  Feiltype:
  9.  Kort beskrivelse av problemet:
10.  Informasjon om hvordan feilen kan gjenskapes:	PCTV Systems TVCenter
Dette finnes på CD-omslaget eller i oppsettet på TV app.
6.4.9 
f.eks. Windows 7 inkl. Service Pakke versjonen
Navn, chip type, BIOS versjon
Type og hastighet (f.eks., Pentium 4, 2.4 GHz)
Størrelsen på hovedminnet (f.eks., 512 MB).
Krasj, problem med videokvalitet, installasjonsproblem osv.

Kontact PCTV Systems Support slik som det beskrives i støtte informasjonsarket som er vedlagt ditt produkt.

-------------------------------------------------------------------------------------------------------

8.00 Additional License Information

PCTV Systems TVCenter Copyright © 2009, 2010, 2011, 2012, 2013, 2014 by PCTV Systems S.à r.l. All Rights Reserved.

Parts of the TVCenter software use: 

§ ffmpeg - under the terms of the GNU Lesser General Public License.
For further details regarding ffmpeg visit: http://ffmpeg.org/index.html

§ md5.js - Copyright (c) 1996 Henri Torgemane 

Parts of Broadway 2T use: 

§ libdvbpsi - under the terms of the GNU General Public License V2
For further details regarding libdvbpsi visit: http://www.videolan.org

§ libiconv - under the terms of the GNU General Public License V2
For further details regarding libiconv visit: http:// "http://www.gnu.org/software/libiconv/" www.gnu.org/software/libiconv/  

§ libhdhomerun - under the terms of the GNU Lesser General Public License V3
For further details regarding libhdhomerun visit: http:// "http://www.silicondust.com" www.silicondust.com

§ goahead - Copyright GoAhead Software Inc., 1995-2000
For further details regarding goahead visit: http:// "http://www.goahead.com" www.goahead.com

For further details please refer to the Legal Information-section of the help or manual file.