PCTV Systems TVCenter

LEIAME para a versão do programa 6.4.9                 2014-10-31

--------------------------------------------------------------------------------------------------------------------

Este arquivo contém informação importante sobre a utilização do PCTV Systems TVCenter. No caso de problemas com o software, leia o manual e este arquivo.

Conteúdo:

1.00  Instruções importantes
1.1 DistanTV mobile
1.2 TVCenter long start delay
2.00  Hardware suportado
  2.1 Broadway 2T
3.00  Sistemas operacionais suportados
4.00  Dicas de funcionamento
5.00  Limitações conhecidas
6.00  Mudanças
7.00  Suporte Técnico da PCTV Systems
8.00  Additional License Information

-----------------------------------------------------------------------------------------------------

1.00 Dicas importantes

1.1 DistanTV mobile

1.1.1 Supported operating systems on client devices
DistanTV mobile supports TV streaming to both Windows and Macintosh systems. Following the list of supported operating systems:
§	Microsoft Windows XP - with Service Pack 3 or higher (32bit)
§	Microsoft Windows Media Center Edition 2005 - with Service Pack 3 or higher (32bit)
§	Microsoft Windows Vista - with Service Pack 2 or higher 
§	Microsoft Windows 7
§	Microsoft Windows 8
§	MAC OS 10.5 (Leopard) - with installed Adobe Flash Player
§	MAC OS 10.6 (Snow Leopard)

1.1.2 Operation tips for users outside the USA
Please make sure you only select SD (standard definition) TV channels when using DistanTV mobile (live TV streaming). Example: Instead of selecting the channel “Arte HD”, you should select the corresponding channel in SD (“Arte”). Don’t worry, there is no negative impact on the picture and sound quality you get on your streaming client device (e.g. iPad) when selecting an SDTV instead of an HDTV channel.

1.1.3 Known limitations
Distorted DistanTV mobile user interface during local network streaming with Internet Explorer 8
If you are using DistanTV mobile in your local network with Internet Explorer 8 on a Windows XP system, the DistanTV mobile UI may look distorted (showing wrong colors and missing text). The root cause of this issue is a malfunction of Internet Explorer 8 (IE8) in “Local intranet” mode. 
To solve this problem, the automatic detection of the Intranet has to be disabled. To do so follow these steps:
- from the IE8 command bar, select Tools > Internet Options > Security
- select Local intranet 
- click on the Sites-button
- disable all check boxes for automatic intranet detection. 
Alternatively, you can connect to the server PC by typing in the address-field of the browser its IP address instead of the server name. Here you can find the IP-address of the server: TVCenter Settings > DistanTV mobile > Summary > Local Access. 

1.2 TVCenter long start delay 
The long start delay can be caused by certificate verification of .Net framework without a valid internet connection.
Workaround: 
uncheck the option Check for publisher's certificate revocation in the MS Internet Explorer. 
To do so follow these steps:
- open Internet Explorer 
- form the menu bar select Tools > Internet Options > Advanced 
- scroll in the list to Security 
- uncheck the option Check for publisher's certificate revocation

-----------------------------------------------------------------------------------------------------

2.00 Hardware suportado

Broadway 2T
PCTV 73A
PCTV 73e Solo
PCTV 73e 
PCTV 74e
PCTV 76e
PCTV 77e
PCTV 78e
PCTV 79e
PCTV 80e
PCTV 170e
PCTV 171e
PCTV 282e
PCTV 290e
PCTV 292e
PCTV 310i
PCTV 330e
PCTV 340e
PCTV 340eSE
PCTV 460e
PCTV 461e
PCTV 510e
PCTV 520e
PCTV 521e
PCTV 800i
PCTV 801e
PCTV 801eSE
PCTV 2000i
PCTV 2001e
PCTV 2002e
PCTV 4000i

2.1 Broadway 2T

2.1.1 Windows MediaCenter support
- It is recommened to use a LAN or a fast WLAN connection (801.11n ).
- Use one Tuner only.

2.1.2 SSID
- It is recommened not do disable or hide the SSID of your WLAN.

2.1.3 Password characters limitation
- Only the following characters are supported . 
  Letters: 	(a ... z) and (A ... Z)
  Numbers : 	(0 ... 9)
  Special : 	!#$%&()*+,-./:<=>?@ []^_{|}~ 

2.1.4 WAN streaming: advanced router configuration
- Some routers require to enable port triggering for the streaming port of Broadway 2T. 
In this case please enable this feature in your router settings.  

2.1.5 WAN streaming : upload speed
- In most cases you will not reach the theoretic upload performance as promised by your provider. Please check your real upload speed. If you try to stream with a bandwidth higher than your real upload speed, the appliaction can be jerky and/or instable.

-----------------------------------------------------------------------------------------------------

3.00 Sistemas operacionais suportados

§	Microsoft Windows XP Service Pack 3 ou superior (32bit)
§	Microsoft Windows Media Center Edition 2005 with Service Pack 3 or higher (32bit)
§	Microsoft Windows Vista with Service Pack 2 or higher 
§	Microsoft Windows 7
§	Microsoft Windows 8

A instalação requer que você tenha direitos de administrador.
Para utilizar os aplicativos, você tem de ser um "usuário padrão" (grupo: usuários principais) ou ter direitos superiores.

É recomendável a instalação prévia do Windows Service Pack atual.
In addition to that, following  Microsoft-software should be installed on your PC: 
§ .NET Framework 3.5 Service Pack 1 and 
§ .NET Framework 3.5 Family Update for .NET versions 2.0 through 3.5 (KB951847) x86'
You can download  the software under: http://www.microsoft.com/downloads/details.aspx?FamilyId=AB99342F-5D1A-413D-8319-81DA479AB0D7&displaylang=en

-----------------------------------------------------------------------------------------------------

4.00 Dicas de funcionamento

Atenção: Algumas funções não estão disponíveis em todos os produtos. Estas estão marcadas com (*)

Microsoft Windows Media Center Edition 2005

§ Encontrará um driver MS MCE2005 adicional no CD na pasta <Windows Media Center>. 
      Este driver permite a você usar o hardware dentro do MCE sem o software TVCenter.

§ É necessário um decodificador de DVD certificado MCE para utilizar a funcionalidade de TV em ambientes MCE 2005.

Configurable video renderer

You can configure and adjust the preview by choosing different video modes from the Video renderer dropdown-menu.
To set the video mode please open the TVCenter-Settings application and from the navigation bar select  TV watching > Advanced settings - Video output > Video renderer.

Signal Booster (integrated amplifier)*

§ The Signal Booster improves the reception of weaker signals, for example when you use a portable antenna.
§ With strong signals from e.g. an amplified rooftop antenna, the Signal Booster should be turned off to avoid potential overdriving of the tuner.

Default video parameter - regarding followiong hardware: 100i, 110i, 300i, 310i

The default value for contrast and saturation is "75" (and not "50", like for the other values)

-----------------------------------------------------------------------------------------------------

5.00 Limitações conhecidas

§	Se você desconectar um dispositivo USB, recomendamos que aguarde pelo menos 10 antes de o conectar novamente; caso contrário, o hardware poderá não ser corretamente reconhecido.

-----------------------------------------------------------------------------------------------------

6.00 Mudanças

§	6.4.8 à 6.4.9
	§	add EPG language selector
	§	H.264 decoder improvements
	§	AAC audio decoder improved

§	6.4.7 à 6.4.8
	§	add PCTV 79e
	§	add PCTV 292e
	§	Win8.1 improvements

§	6.4.6 à 6.4.7
	§	add PCTV 291e
	§	add PCTV 521e
	§	Win8 improvements

§	6.4.5 à 6.4.6
	§	add PCTV 461e
	§	add PCTV 2002e
	§	Win8 improvements

§	6.4.4 à 6.4.5
	§	add PCTV 78e
	§	Win8 support improvements

§	6.4.3 à 6.4.4
	§	add PCTV 77e

§	6.4.2 à 6.4.3
	§	add PCTV 76e

§	6.4.1 à 6.4.2
	§	add 76e
	§	improve H.264 decoder stability

§	6.4.0 à 6.4.1
	§	add Broadway 2T
	§	improve H.264 decoder stability
	§	add DVB-C support for: Sweden, Denmark and Spain

§	6.3.2 à 6.4.0
	§	add DistanTV mobile 2
	§	add Internal EPG Viewer
	§	add TitanTV support (US only)
	§	add Parental Control (US only)
	§	add Closed caption (US only)
	§	Converter: reworked	
	§	optimized H.264 decoder with DXVA support
	§	expand hardware support

§	6.3.1 à 6.3.2
	§	expand hardware support

§	6.3.0 à 6.3.1
	§	expand hardware support

§	6.2.0 à 6.3.0.
	§	expand hardware support
§	add DistanTV mobile: iPhone® / iPod touch®  TV streaming  
	§	add DVB-S / DVB-S2 support
§	expand scheduler: add recurrence
	§	optimized H.264 decoder  
§	add separat driver installation

§	6.1.0 à 6.2.0.
	§	expand hardware support	
	§	add fm radio
§	add analog TV support
§	add configurable video renderer
§	add multi tuner support
§	add Dolby Digital+ (E-AC3) support
§	add remote control support

§	6.0.0 à 6.1.0.
	§	Suporte expandido para hardware	
	§	Rádio
	§	Aplicativo DistanTV
	§	Função de Edição de Canal
	§	Melhoria da duração de busca de canais
	§	Suporte para idiomas

-----------------------------------------------------------------------------------------------------

7.00 Suporte Técnico da PCTV Systems

Estão disponíveis novas versões do software PCTV Systems TVCenter no website da PCTV Systems:

http://www.pctvsystems.com/

Tenha preparada a seguinte informação no contato com o Suporte Técnico da PCTV Systems:

  1. Produto:
  2. Número de série:
  3. Versão do software:
  4. Versão do sistema operacional:
  5. Placa principal:
  6. CPU: 	
  7. RAM: 
  8. Tipo de problema:
  9.  Breve descrição do problema:
10.  Informação sobre como o problema pode ser reproduzido:	PCTV Systems TVCenter
Located on the cover of your CD or in the settings of the TV app.
6.4.9 
e.g. Windows 7 including the Service Pack version
Name, chip set, BIOS version
Type and speed (e.g., Pentium 4, 2.4 GHz)
Size of main memory (e.g., 512 MB).
Crash, problems with video quality, installation problems, etc.

Contate o Suporte Técnico da PCTV Systems da forma descrita na folha de informação de suporte incluída com seu produto.

-------------------------------------------------------------------------------------------------------

8.00 Additional License Information

PCTV Systems TVCenter Copyright © 2009, 2010, 2011, 2012, 2013, 2014 by PCTV Systems S.à r.l. All Rights Reserved.

Parts of the TVCenter software use: 

§ ffmpeg - under the terms of the GNU Lesser General Public License.
For further details regarding ffmpeg visit: http://ffmpeg.org/index.html

§ md5.js - Copyright (c) 1996 Henri Torgemane 

Parts of Broadway 2T use: 

§ libdvbpsi - under the terms of the GNU General Public License V2
For further details regarding libdvbpsi visit: http://www.videolan.org

§ libiconv - under the terms of the GNU General Public License V2
For further details regarding libiconv visit: http:// "http://www.gnu.org/software/libiconv/" www.gnu.org/software/libiconv/  

§ libhdhomerun - under the terms of the GNU Lesser General Public License V3
For further details regarding libhdhomerun visit: http:// "http://www.silicondust.com" www.silicondust.com

§ goahead - Copyright GoAhead Software Inc., 1995-2000
For further details regarding goahead visit: http:// "http://www.goahead.com" www.goahead.com

For further details please refer to the Legal Information-section of the help or manual file.